--- /dev/null
+++ b/drivers/bcmdrivers/usb2h/usbh_cfg.h
@@ -0,0 +1,51 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+
+#ifndef __ISLAND_USBH_CFG_H
+#define __ISLAND_USBH_CFG_H
+
+#define USBH_NUM_PORTS 3
+
+struct usbh_port_cfg {
+	/* GPIO for host power */
+	int pwr_gpio;
+
+	/* GPIO for power fault (over-current) detection */
+	int pwr_flt_gpio;
+
+	/* GPIO for PHY reset */
+	int reset_gpio;
+};
+
+/*
+ * USB Host related HW parameters
+ */
+struct usbh_cfg {
+	/* peripheral clock name string */
+	char *peri_clk_name;
+
+	/* AHB bus clock name string */
+	char *ahb_clk_name;
+
+	/* the block might require optional clock to be enabled */
+	char *opt_clk_name;
+
+	unsigned int num_ports;
+
+	struct usbh_port_cfg port[USBH_NUM_PORTS];
+};
+
+#endif
diff --git a/drivers/bcmdrivers/wdt/.gitignore b/drivers/bcmdrivers/wdt/.gitignore
new file mode 100644
index 0000000..d741861
