--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmotp.h
@@ -0,0 +1,81 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * OTP support.
+ *
+ * $Id: bcmotp.h 321779 2012-03-16 19:39:00Z $
+ */
+
+#ifndef	_bcmotp_h_
+#define	_bcmotp_h_
+
+/* OTP regions */
+#define OTP_HW_RGN	1
+#define OTP_SW_RGN	2
+#define OTP_CI_RGN	4
+#define OTP_FUSE_RGN	8
+#define OTP_ALL_RGN	0xf	/* From h/w region to end of OTP including checksum */
+
+/* OTP Size */
+#define OTP_SZ_MAX		(6144/8)	/* maximum bytes in one CIS */
+
+/* Fixed size subregions sizes in words */
+#define OTPGU_CI_SZ		2
+
+/* OTP usage */
+#define OTP4325_FM_DISABLED_OFFSET	188
+
+#ifdef BCMNVRAMW
+/* Global RDE index for chips not having an OTP PMU resource. */
+#define OTP_GLOBAL_RDE_IDX 0xFF
+#endif
+
+/* Exported functions */
+extern int	otp_status(void *oh);
+extern int	otp_size(void *oh);
+extern uint16	otp_read_bit(void *oh, uint offset);
+extern void*	otp_init(si_t *sih);
+extern int	otp_read_region(si_t *sih, int region, uint16 *data, uint *wlen);
+extern int	otp_read_word(si_t *sih, uint wn, uint16 *data);
+extern int	otp_nvread(void *oh, char *data, uint *len);
+#ifdef BCMNVRAMW
+extern int	otp_write_region(si_t *sih, int region, uint16 *data, uint wlen);
+extern int	otp_write_word(si_t *sih, uint wn, uint16 data);
+extern int	otp_cis_append_region(si_t *sih, int region, char *vars, int count);
+extern int	otp_lock(si_t *sih);
+extern int	otp_nvwrite(void *oh, uint16 *data, uint wlen);
+#endif /* BCMNVRAMW */
+
+#if defined(WLTEST)
+extern int	otp_dump(void *oh, int arg, char *buf, uint size);
+extern int	otp_dumpstats(void *oh, int arg, char *buf, uint size);
+#endif
+
+#if defined(BCMNVRAMW)
+#define otp_write_rde(oh, rde, bit, val)	ipxotp_write_rde(oh, rde, bit, val)
+extern int	ipxotp_write_rde(void *oh, int rde, uint bit, uint val);
+extern int otp_write_bits(void *oh, uint offset, int bits, uint8* data);
+
+#ifdef OTP_DEBUG
+extern int otp_verify1x(void *oh, uint off, uint fuse);
+extern int otp_read1x(void *oh, uint off, uint fuse);
+extern int otp_repair_bit(void *oh, uint off, uint val);
+extern int otp_write_ones(void *oh, uint off, uint bits);
+extern int otp_write_ones_old(void *oh, uint off, uint bits);
+#endif
+
+#endif
+
+#endif /* _bcmotp_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmparams.h b/drivers/bcmdrivers/gmac/src/include/bcmparams.h
new file mode 100755
index 0000000..da6eb4c
