--- a/drivers/rtc/rtc-mv.c
+++ b/drivers/rtc/rtc-mv.c
@@ -12,6 +12,7 @@
 #include <linux/bcd.h>
 #include <linux/io.h>
 #include <linux/platform_device.h>
+#include <linux/of.h>
 #include <linux/delay.h>
 #include <linux/gfp.h>
 #include <linux/module.h>
@@ -294,11 +295,19 @@ static int __exit mv_rtc_remove(struct platform_device *pdev)
 	return 0;
 }
 
+#ifdef CONFIG_OF
+static struct of_device_id rtc_mv_of_match_table[] = {
+	{ .compatible = "mrvl,orion-rtc", },
+	{}
+};
+#endif
+
 static struct platform_driver mv_rtc_driver = {
 	.remove		= __exit_p(mv_rtc_remove),
 	.driver		= {
 		.name	= "rtc-mv",
 		.owner	= THIS_MODULE,
+		.of_match_table = of_match_ptr(rtc_mv_of_match_table),
 	},
 };
 
diff --git a/drivers/rtc/rtc-s35390a.c b/drivers/rtc/rtc-s35390a.c
index f789e00..5208bec 100644
