--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/proto/ethernet.h
@@ -0,0 +1,202 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * From FreeBSD 2.2.7: Fundamental constants relating to ethernet.
+ *
+ * $Id: ethernet.h 316696 2012-02-23 03:29:35Z $
+ */
+
+#ifndef _NET_ETHERNET_H_	  /* use native BSD ethernet.h when available */
+#define _NET_ETHERNET_H_
+
+#ifndef _TYPEDEFS_H_
+#include "typedefs.h"
+#endif
+
+/* This marks the start of a packed structure section. */
+#include <packed_section_start.h>
+
+
+/*
+ * The number of bytes in an ethernet (MAC) address.
+ */
+#define	ETHER_ADDR_LEN		6
+
+/*
+ * The number of bytes in the type field.
+ */
+#define	ETHER_TYPE_LEN		2
+
+/*
+ * The number of bytes in the trailing CRC field.
+ */
+#define	ETHER_CRC_LEN		4
+
+/*
+ * The length of the combined header.
+ */
+#define	ETHER_HDR_LEN		(ETHER_ADDR_LEN * 2 + ETHER_TYPE_LEN)
+
+/*
+ * The minimum packet length.
+ */
+#define	ETHER_MIN_LEN		64
+
+/*
+ * The minimum packet user data length.
+ */
+#define	ETHER_MIN_DATA		46
+
+/*
+ * The maximum packet length.
+ */
+#define	ETHER_MAX_LEN		1518
+
+/*
+ * The maximum packet user data length.
+ */
+#define	ETHER_MAX_DATA		1500
+
+/* ether types */
+#define ETHER_TYPE_MIN		0x0600		/* Anything less than MIN is a length */
+#define	ETHER_TYPE_IP		0x0800		/* IP */
+#define ETHER_TYPE_ARP		0x0806		/* ARP */
+#define ETHER_TYPE_8021Q	0x8100		/* 802.1Q */
+#define	ETHER_TYPE_IPV6		0x86dd		/* IPv6 */
+#define	ETHER_TYPE_BRCM		0x886c		/* Broadcom Corp. */
+#define	ETHER_TYPE_802_1X	0x888e		/* 802.1x */
+#define	ETHER_TYPE_802_1X_PREAUTH 0x88c7	/* 802.1x preauthentication */
+#define ETHER_TYPE_WAI		0x88b4		/* WAI */
+#define ETHER_TYPE_89_0D	0x890d		/* 89-0d frame for TDLS */
+
+#define ETHER_TYPE_PPP_SES	0x8864		/* PPPoE Session */
+
+/* Broadcom subtype follows ethertype;  First 2 bytes are reserved; Next 2 are subtype; */
+#define	ETHER_BRCM_SUBTYPE_LEN	4	/* Broadcom 4 byte subtype */
+
+/* ether header */
+#define ETHER_DEST_OFFSET	(0 * ETHER_ADDR_LEN)	/* dest address offset */
+#define ETHER_SRC_OFFSET	(1 * ETHER_ADDR_LEN)	/* src address offset */
+#define ETHER_TYPE_OFFSET	(2 * ETHER_ADDR_LEN)	/* ether type offset */
+
+/*
+ * A macro to validate a length with
+ */
+#define	ETHER_IS_VALID_LEN(foo)	\
+	((foo) >= ETHER_MIN_LEN && (foo) <= ETHER_MAX_LEN)
+
+#define ETHER_FILL_MCAST_ADDR_FROM_IP(ea, mgrp_ip) {		\
+		((uint8 *)ea)[0] = 0x01;			\
+		((uint8 *)ea)[1] = 0x00;			\
+		((uint8 *)ea)[2] = 0x5e;			\
+		((uint8 *)ea)[3] = ((mgrp_ip) >> 16) & 0x7f;	\
+		((uint8 *)ea)[4] = ((mgrp_ip) >>  8) & 0xff;	\
+		((uint8 *)ea)[5] = ((mgrp_ip) >>  0) & 0xff;	\
+}
+
+#ifndef __INCif_etherh   /* Quick and ugly hack for VxWorks */
+/*
+ * Structure of a 10Mb/s Ethernet header.
+ */
+BWL_PRE_PACKED_STRUCT struct ether_header {
+	uint8	ether_dhost[ETHER_ADDR_LEN];
+	uint8	ether_shost[ETHER_ADDR_LEN];
+	uint16	ether_type;
+} BWL_POST_PACKED_STRUCT;
+
+/*
+ * Structure of a 48-bit Ethernet address.
+ */
+BWL_PRE_PACKED_STRUCT struct	ether_addr {
+	uint8 octet[ETHER_ADDR_LEN];
+} BWL_POST_PACKED_STRUCT;
+#endif	/* !__INCif_etherh Quick and ugly hack for VxWorks */
+
+/*
+ * Takes a pointer, set, test, clear, toggle locally admininistered
+ * address bit in the 48-bit Ethernet address.
+ */
+#define ETHER_SET_LOCALADDR(ea)	(((uint8 *)(ea))[0] = (((uint8 *)(ea))[0] | 2))
+#define ETHER_IS_LOCALADDR(ea) 	(((uint8 *)(ea))[0] & 2)
+#define ETHER_CLR_LOCALADDR(ea)	(((uint8 *)(ea))[0] = (((uint8 *)(ea))[0] & 0xfd))
+#define ETHER_TOGGLE_LOCALADDR(ea)	(((uint8 *)(ea))[0] = (((uint8 *)(ea))[0] ^ 2))
+
+/* Takes a pointer, marks unicast address bit in the MAC address */
+#define ETHER_SET_UNICAST(ea)	(((uint8 *)(ea))[0] = (((uint8 *)(ea))[0] & ~1))
+
+/*
+ * Takes a pointer, returns true if a 48-bit multicast address
+ * (including broadcast, since it is all ones)
+ */
+#define ETHER_ISMULTI(ea) (((const uint8 *)(ea))[0] & 1)
+
+/* Copy an ethernet address in reverse order */
+#define	ether_rcopy(s, d) \
+do { \
+	((uint16 *)(d))[2] = ((uint16 *)(s))[2]; \
+	((uint16 *)(d))[1] = ((uint16 *)(s))[1]; \
+	((uint16 *)(d))[0] = ((uint16 *)(s))[0]; \
+} while (0)
+
+/* compare two ethernet addresses - assumes the pointers can be referenced as shorts */
+#define eacmp(a, b)	((((uint16 *)(a))[0] ^ ((uint16 *)(b))[0]) | \
+	                 (((uint16 *)(a))[1] ^ ((uint16 *)(b))[1]) | \
+	                 (((uint16 *)(a))[2] ^ ((uint16 *)(b))[2]))
+
+#define	ether_cmp(a, b)	eacmp(a, b)
+
+/* copy an ethernet address - assumes the pointers can be referenced as shorts */
+#define eacopy(s, d) \
+do { \
+	((uint16 *)(d))[0] = ((const uint16 *)(s))[0]; \
+	((uint16 *)(d))[1] = ((const uint16 *)(s))[1]; \
+	((uint16 *)(d))[2] = ((const uint16 *)(s))[2]; \
+} while (0)
+
+#define	ether_copy(s, d) eacopy(s, d)
+
+
+static const struct ether_addr ether_bcast = {{255, 255, 255, 255, 255, 255}};
+static const struct ether_addr ether_null = {{0, 0, 0, 0, 0, 0}};
+
+#define ETHER_ISBCAST(ea)	((((const uint8 *)(ea))[0] &		\
+	                          ((const uint8 *)(ea))[1] &		\
+				  ((const uint8 *)(ea))[2] &		\
+				  ((const uint8 *)(ea))[3] &		\
+				  ((const uint8 *)(ea))[4] &		\
+				  ((const uint8 *)(ea))[5]) == 0xff)
+#define ETHER_ISNULLADDR(ea)	((((const uint8 *)(ea))[0] |		\
+				  ((const uint8 *)(ea))[1] |		\
+				  ((const uint8 *)(ea))[2] |		\
+				  ((const uint8 *)(ea))[3] |		\
+				  ((const uint8 *)(ea))[4] |		\
+				  ((const uint8 *)(ea))[5]) == 0)
+
+#define ETHER_ISNULLDEST(da)	((((const uint16 *)(da))[0] |           \
+				  ((const uint16 *)(da))[1] |           \
+				  ((const uint16 *)(da))[2]) == 0)
+
+
+#define ETHER_MOVE_HDR(d, s) \
+do { \
+	struct ether_header t; \
+	t = *(struct ether_header *)(s); \
+	*(struct ether_header *)(d) = t; \
+} while (0)
+
+/* This marks the end of a packed structure section. */
+#include <packed_section_end.h>
+
+#endif /* _NET_ETHERNET_H_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/proto/vlan.h b/drivers/bcmdrivers/gmac/src/include/proto/vlan.h
new file mode 100755
index 0000000..5393070
