--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/sbhnddma.h
@@ -0,0 +1,403 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Generic Broadcom Home Networking Division (HND) DMA engine HW interface
+ * This supports the following chips: BCM42xx, 44xx, 47xx .
+ *
+ * $Id: sbhnddma.h 321146 2012-03-14 08:27:23Z $
+ */
+
+#ifndef	_sbhnddma_h_
+#define	_sbhnddma_h_
+
+/* DMA structure:
+ *  support two DMA engines: 32 bits address or 64 bit addressing
+ *  basic DMA register set is per channel(transmit or receive)
+ *  a pair of channels is defined for convenience
+ */
+
+
+/* 32 bits addressing */
+
+/* dma registers per channel(xmt or rcv) */
+typedef volatile struct {
+	uint32	control;		/* enable, et al */
+	uint32	addr;			/* descriptor ring base address (4K aligned) */
+	uint32	ptr;			/* last descriptor posted to chip */
+	uint32	status;			/* current active descriptor, et al */
+} dma32regs_t;
+
+typedef volatile struct {
+	dma32regs_t	xmt;		/* dma tx channel */
+	dma32regs_t	rcv;		/* dma rx channel */
+} dma32regp_t;
+
+typedef volatile struct {	/* diag access */
+	uint32	fifoaddr;		/* diag address */
+	uint32	fifodatalow;		/* low 32bits of data */
+	uint32	fifodatahigh;		/* high 32bits of data */
+	uint32	pad;			/* reserved */
+} dma32diag_t;
+
+/*
+ * DMA Descriptor
+ * Descriptors are only read by the hardware, never written back.
+ */
+typedef volatile struct {
+	uint32	ctrl;		/* misc control bits & bufcount */
+	uint32	addr;		/* data buffer address */
+} dma32dd_t;
+
+/*
+ * Each descriptor ring must be 4096byte aligned, and fit within a single 4096byte page.
+ */
+#define	D32RINGALIGN_BITS	12
+#define	D32MAXRINGSZ		(1 << D32RINGALIGN_BITS)
+#define	D32RINGALIGN		(1 << D32RINGALIGN_BITS)
+
+#define	D32MAXDD	(D32MAXRINGSZ / sizeof (dma32dd_t))
+
+/* transmit channel control */
+#define	XC_XE		((uint32)1 << 0)	/* transmit enable */
+#define	XC_SE		((uint32)1 << 1)	/* transmit suspend request */
+#define	XC_LE		((uint32)1 << 2)	/* loopback enable */
+#define	XC_FL		((uint32)1 << 4)	/* flush request */
+#define XC_MR_MASK	0x000000C0		/* Multiple outstanding reads */
+#define XC_MR_SHIFT	6
+#define	XC_PD		((uint32)1 << 11)	/* parity check disable */
+#define	XC_AE		((uint32)3 << 16)	/* address extension bits */
+#define	XC_AE_SHIFT	16
+#define XC_BL_MASK	0x001C0000		/* BurstLen bits */
+#define XC_BL_SHIFT	18
+#define XC_PC_MASK	0x00E00000		/* Prefetch control */
+#define XC_PC_SHIFT	21
+#define XC_PT_MASK	0x03000000		/* Prefetch threshold */
+#define XC_PT_SHIFT	24
+
+/* Multiple outstanding reads */
+#define DMA_MR_1	0
+#define DMA_MR_2	1
+/* 2, 3: reserved */
+
+/* DMA Burst Length in bytes */
+#define DMA_BL_16	0
+#define DMA_BL_32	1
+#define DMA_BL_64	2
+#define DMA_BL_128	3
+#define DMA_BL_256	4
+#define DMA_BL_512	5
+#define DMA_BL_1024	6
+
+/* Prefetch control */
+#define DMA_PC_0	0
+#define DMA_PC_4	1
+#define DMA_PC_8	2
+#define DMA_PC_16	3
+/* others: reserved */
+
+/* Prefetch threshold */
+#define DMA_PT_1	0
+#define DMA_PT_2	1
+#define DMA_PT_4	2
+#define DMA_PT_8	3
+
+/* transmit descriptor table pointer */
+#define	XP_LD_MASK	0xfff			/* last valid descriptor */
+
+/* transmit channel status */
+#define	XS_CD_MASK	0x0fff			/* current descriptor pointer */
+#define	XS_XS_MASK	0xf000			/* transmit state */
+#define	XS_XS_SHIFT	12
+#define	XS_XS_DISABLED	0x0000			/* disabled */
+#define	XS_XS_ACTIVE	0x1000			/* active */
+#define	XS_XS_IDLE	0x2000			/* idle wait */
+#define	XS_XS_STOPPED	0x3000			/* stopped */
+#define	XS_XS_SUSP	0x4000			/* suspend pending */
+#define	XS_XE_MASK	0xf0000			/* transmit errors */
+#define	XS_XE_SHIFT	16
+#define	XS_XE_NOERR	0x00000			/* no error */
+#define	XS_XE_DPE	0x10000			/* descriptor protocol error */
+#define	XS_XE_DFU	0x20000			/* data fifo underrun */
+#define	XS_XE_BEBR	0x30000			/* bus error on buffer read */
+#define	XS_XE_BEDA	0x40000			/* bus error on descriptor access */
+#define	XS_AD_MASK	0xfff00000		/* active descriptor */
+#define	XS_AD_SHIFT	20
+
+/* receive channel control */
+#define	RC_RE		((uint32)1 << 0)	/* receive enable */
+#define	RC_RO_MASK	0xfe			/* receive frame offset */
+#define	RC_RO_SHIFT	1
+#define	RC_FM		((uint32)1 << 8)	/* direct fifo receive (pio) mode */
+#define	RC_SH		((uint32)1 << 9)	/* separate rx header descriptor enable */
+#define	RC_OC		((uint32)1 << 10)	/* overflow continue */
+#define	RC_PD		((uint32)1 << 11)	/* parity check disable */
+#define	RC_AE		((uint32)3 << 16)	/* address extension bits */
+#define	RC_AE_SHIFT	16
+#define RC_BL_MASK	0x001C0000		/* BurstLen bits */
+#define RC_BL_SHIFT	18
+#define RC_PC_MASK	0x00E00000		/* Prefetch control */
+#define RC_PC_SHIFT	21
+#define RC_PT_MASK	0x03000000		/* Prefetch threshold */
+#define RC_PT_SHIFT	24
+
+/* receive descriptor table pointer */
+#define	RP_LD_MASK	0xfff			/* last valid descriptor */
+
+/* receive channel status */
+#define	RS_CD_MASK	0x0fff			/* current descriptor pointer */
+#define	RS_RS_MASK	0xf000			/* receive state */
+#define	RS_RS_SHIFT	12
+#define	RS_RS_DISABLED	0x0000			/* disabled */
+#define	RS_RS_ACTIVE	0x1000			/* active */
+#define	RS_RS_IDLE	0x2000			/* idle wait */
+#define	RS_RS_STOPPED	0x3000			/* reserved */
+#define	RS_RE_MASK	0xf0000			/* receive errors */
+#define	RS_RE_SHIFT	16
+#define	RS_RE_NOERR	0x00000			/* no error */
+#define	RS_RE_DPE	0x10000			/* descriptor protocol error */
+#define	RS_RE_DFO	0x20000			/* data fifo overflow */
+#define	RS_RE_BEBW	0x30000			/* bus error on buffer write */
+#define	RS_RE_BEDA	0x40000			/* bus error on descriptor access */
+#define	RS_AD_MASK	0xfff00000		/* active descriptor */
+#define	RS_AD_SHIFT	20
+
+/* fifoaddr */
+#define	FA_OFF_MASK	0xffff			/* offset */
+#define	FA_SEL_MASK	0xf0000			/* select */
+#define	FA_SEL_SHIFT	16
+#define	FA_SEL_XDD	0x00000			/* transmit dma data */
+#define	FA_SEL_XDP	0x10000			/* transmit dma pointers */
+#define	FA_SEL_RDD	0x40000			/* receive dma data */
+#define	FA_SEL_RDP	0x50000			/* receive dma pointers */
+#define	FA_SEL_XFD	0x80000			/* transmit fifo data */
+#define	FA_SEL_XFP	0x90000			/* transmit fifo pointers */
+#define	FA_SEL_RFD	0xc0000			/* receive fifo data */
+#define	FA_SEL_RFP	0xd0000			/* receive fifo pointers */
+#define	FA_SEL_RSD	0xe0000			/* receive frame status data */
+#define	FA_SEL_RSP	0xf0000			/* receive frame status pointers */
+
+/* descriptor control flags */
+#define	CTRL_BC_MASK	0x00001fff		/* buffer byte count, real data len must <= 4KB */
+#define	CTRL_AE		((uint32)3 << 16)	/* address extension bits */
+#define	CTRL_AE_SHIFT	16
+#define	CTRL_PARITY	((uint32)3 << 18)	/* parity bit */
+#define	CTRL_EOT	((uint32)1 << 28)	/* end of descriptor table */
+#define	CTRL_IOC	((uint32)1 << 29)	/* interrupt on completion */
+#define	CTRL_EOF	((uint32)1 << 30)	/* end of frame */
+#define	CTRL_SOF	((uint32)1 << 31)	/* start of frame */
+
+/* control flags in the range [27:20] are core-specific and not defined here */
+#define	CTRL_CORE_MASK	0x0ff00000
+
+/* 64 bits addressing */
+
+/* dma registers per channel(xmt or rcv) */
+typedef volatile struct {
+	uint32	control;		/* enable, et al */
+	uint32	ptr;			/* last descriptor posted to chip */
+	uint32	addrlow;		/* descriptor ring base address low 32-bits (8K aligned) */
+	uint32	addrhigh;		/* descriptor ring base address bits 63:32 (8K aligned) */
+	uint32	status0;		/* current descriptor, xmt state */
+	uint32	status1;		/* active descriptor, xmt error */
+} dma64regs_t;
+
+typedef volatile struct {
+	dma64regs_t	tx;		/* dma64 tx channel */
+	dma64regs_t	rx;		/* dma64 rx channel */
+} dma64regp_t;
+
+typedef volatile struct {		/* diag access */
+	uint32	fifoaddr;		/* diag address */
+	uint32	fifodatalow;		/* low 32bits of data */
+	uint32	fifodatahigh;		/* high 32bits of data */
+	uint32	pad;			/* reserved */
+} dma64diag_t;
+
+/*
+ * DMA Descriptor
+ * Descriptors are only read by the hardware, never written back.
+ */
+typedef volatile struct {
+	uint32	ctrl1;		/* misc control bits */
+	uint32	ctrl2;		/* buffer count and address extension */
+	uint32	addrlow;	/* memory address of the date buffer, bits 31:0 */
+	uint32	addrhigh;	/* memory address of the date buffer, bits 63:32 */
+} dma64dd_t;
+
+/*
+ * Each descriptor ring must be 8kB aligned, and fit within a contiguous 8kB physical addresss.
+ */
+#define D64RINGALIGN_BITS	13
+#define	D64MAXRINGSZ		(1 << D64RINGALIGN_BITS)
+#define	D64RINGBOUNDARY		(1 << D64RINGALIGN_BITS)
+
+#define	D64MAXDD	(D64MAXRINGSZ / sizeof (dma64dd_t))
+
+/* for cores with large descriptor ring support, descriptor ring size can be up to 4096 */
+#define	D64MAXDD_LARGE		((1 << 16) / sizeof (dma64dd_t))
+
+/* for cores with large descriptor ring support (4k descriptors), descriptor ring cannot cross
+ * 64K boundary
+ */
+#define	D64RINGBOUNDARY_LARGE	(1 << 16)
+
+/*
+ * Default DMA Burstlen values for USBRev >= 12 and SDIORev >= 11.
+ * When this field contains the value N, the burst length is 2**(N + 4) bytes.
+ */
+#define D64_DEF_USBBURSTLEN     2
+#define D64_DEF_SDIOBURSTLEN    1
+
+
+#ifndef D64_USBBURSTLEN
+#define D64_USBBURSTLEN	DMA_BL_64
+#endif
+#ifndef D64_SDIOBURSTLEN
+#define D64_SDIOBURSTLEN	DMA_BL_32
+#endif
+
+/* transmit channel control */
+#define	D64_XC_XE		0x00000001	/* transmit enable */
+#define	D64_XC_SE		0x00000002	/* transmit suspend request */
+#define	D64_XC_LE		0x00000004	/* loopback enable */
+#define	D64_XC_FL		0x00000010	/* flush request */
+#define D64_XC_MR_MASK		0x000000C0	/* Multiple outstanding reads */
+#define D64_XC_MR_SHIFT		6
+#define	D64_XC_PD		0x00000800	/* parity check disable */
+#define	D64_XC_AE		0x00030000	/* address extension bits */
+#define	D64_XC_AE_SHIFT		16
+#define D64_XC_BL_MASK		0x001C0000	/* BurstLen bits */
+#define D64_XC_BL_SHIFT		18
+#define D64_XC_PC_MASK		0x00E00000		/* Prefetch control */
+#define D64_XC_PC_SHIFT		21
+#define D64_XC_PT_MASK		0x03000000		/* Prefetch threshold */
+#define D64_XC_PT_SHIFT		24
+
+/* transmit descriptor table pointer */
+#define	D64_XP_LD_MASK		0x00001fff	/* last valid descriptor */
+
+/* transmit channel status */
+#define	D64_XS0_CD_MASK		0x00001fff	/* current descriptor pointer */
+#define	D64_XS0_XS_MASK		0xf0000000     	/* transmit state */
+#define	D64_XS0_XS_SHIFT		28
+#define	D64_XS0_XS_DISABLED	0x00000000	/* disabled */
+#define	D64_XS0_XS_ACTIVE	0x10000000	/* active */
+#define	D64_XS0_XS_IDLE		0x20000000	/* idle wait */
+#define	D64_XS0_XS_STOPPED	0x30000000	/* stopped */
+#define	D64_XS0_XS_SUSP		0x40000000	/* suspend pending */
+
+#define	D64_XS1_AD_MASK		0x00001fff	/* active descriptor */
+#define	D64_XS1_XE_MASK		0xf0000000     	/* transmit errors */
+#define	D64_XS1_XE_SHIFT		28
+#define	D64_XS1_XE_NOERR	0x00000000	/* no error */
+#define	D64_XS1_XE_DPE		0x10000000	/* descriptor protocol error */
+#define	D64_XS1_XE_DFU		0x20000000	/* data fifo underrun */
+#define	D64_XS1_XE_DTE		0x30000000	/* data transfer error */
+#define	D64_XS1_XE_DESRE	0x40000000	/* descriptor read error */
+#define	D64_XS1_XE_COREE	0x50000000	/* core error */
+
+/* receive channel control */
+#define	D64_RC_RE		0x00000001	/* receive enable */
+#define	D64_RC_RO_MASK		0x000000fe	/* receive frame offset */
+#define	D64_RC_RO_SHIFT		1
+#define	D64_RC_FM		0x00000100	/* direct fifo receive (pio) mode */
+#define	D64_RC_SH		0x00000200	/* separate rx header descriptor enable */
+#define	D64_RC_OC		0x00000400	/* overflow continue */
+#define	D64_RC_PD		0x00000800	/* parity check disable */
+#define D64_RC_GE		0x00004000	/* Glom enable */
+#define	D64_RC_AE		0x00030000	/* address extension bits */
+#define	D64_RC_AE_SHIFT		16
+#define D64_RC_BL_MASK		0x001C0000	/* BurstLen bits */
+#define D64_RC_BL_SHIFT		18
+#define D64_RC_PC_MASK		0x00E00000	/* Prefetch control */
+#define D64_RC_PC_SHIFT		21
+#define D64_RC_PT_MASK		0x03000000	/* Prefetch threshold */
+#define D64_RC_PT_SHIFT		24
+
+/* flags for dma controller */
+#define DMA_CTRL_PEN		(1 << 0)	/* partity enable */
+#define DMA_CTRL_ROC		(1 << 1)	/* rx overflow continue */
+#define DMA_CTRL_RXMULTI	(1 << 2)	/* allow rx scatter to multiple descriptors */
+#define DMA_CTRL_UNFRAMED	(1 << 3)	/* Unframed Rx/Tx data */
+#define DMA_CTRL_USB_BOUNDRY4KB_WAR (1 << 4)
+#define DMA_CTRL_DMA_AVOIDANCE_WAR (1 << 5)	/* DMA avoidance WAR for 4331 */
+#define DMA_CTRL_RXSINGLE	(1 << 6)	/* always single buffer */
+
+/* receive descriptor table pointer */
+#define	D64_RP_LD_MASK		0x00001fff	/* last valid descriptor */
+
+/* receive channel status */
+#define	D64_RS0_CD_MASK		0x00001fff	/* current descriptor pointer */
+#define	D64_RS0_RS_MASK		0xf0000000     	/* receive state */
+#define	D64_RS0_RS_SHIFT		28
+#define	D64_RS0_RS_DISABLED	0x00000000	/* disabled */
+#define	D64_RS0_RS_ACTIVE	0x10000000	/* active */
+#define	D64_RS0_RS_IDLE		0x20000000	/* idle wait */
+#define	D64_RS0_RS_STOPPED	0x30000000	/* stopped */
+#define	D64_RS0_RS_SUSP		0x40000000	/* suspend pending */
+
+#define	D64_RS1_AD_MASK		0x0001ffff	/* active descriptor */
+#define	D64_RS1_RE_MASK		0xf0000000     	/* receive errors */
+#define	D64_RS1_RE_SHIFT		28
+#define	D64_RS1_RE_NOERR	0x00000000	/* no error */
+#define	D64_RS1_RE_DPO		0x10000000	/* descriptor protocol error */
+#define	D64_RS1_RE_DFU		0x20000000	/* data fifo overflow */
+#define	D64_RS1_RE_DTE		0x30000000	/* data transfer error */
+#define	D64_RS1_RE_DESRE	0x40000000	/* descriptor read error */
+#define	D64_RS1_RE_COREE	0x50000000	/* core error */
+
+/* fifoaddr */
+#define	D64_FA_OFF_MASK		0xffff		/* offset */
+#define	D64_FA_SEL_MASK		0xf0000		/* select */
+#define	D64_FA_SEL_SHIFT	16
+#define	D64_FA_SEL_XDD		0x00000		/* transmit dma data */
+#define	D64_FA_SEL_XDP		0x10000		/* transmit dma pointers */
+#define	D64_FA_SEL_RDD		0x40000		/* receive dma data */
+#define	D64_FA_SEL_RDP		0x50000		/* receive dma pointers */
+#define	D64_FA_SEL_XFD		0x80000		/* transmit fifo data */
+#define	D64_FA_SEL_XFP		0x90000		/* transmit fifo pointers */
+#define	D64_FA_SEL_RFD		0xc0000		/* receive fifo data */
+#define	D64_FA_SEL_RFP		0xd0000		/* receive fifo pointers */
+#define	D64_FA_SEL_RSD		0xe0000		/* receive frame status data */
+#define	D64_FA_SEL_RSP		0xf0000		/* receive frame status pointers */
+
+/* descriptor control flags 1 */
+#define D64_CTRL_COREFLAGS	0x0ff00000	/* core specific flags */
+#define	D64_CTRL1_EOT		((uint32)1 << 28)	/* end of descriptor table */
+#define	D64_CTRL1_IOC		((uint32)1 << 29)	/* interrupt on completion */
+#define	D64_CTRL1_EOF		((uint32)1 << 30)	/* end of frame */
+#define	D64_CTRL1_SOF		((uint32)1 << 31)	/* start of frame */
+
+/* descriptor control flags 2 */
+#define	D64_CTRL2_BC_MASK	0x00007fff	/* buffer byte count. real data len must <= 16KB */
+#define	D64_CTRL2_AE		0x00030000	/* address extension bits */
+#define	D64_CTRL2_AE_SHIFT	16
+#define D64_CTRL2_PARITY	0x00040000      /* parity bit */
+
+/* control flags in the range [27:20] are core-specific and not defined here */
+#define	D64_CTRL_CORE_MASK	0x0ff00000
+
+#define D64_RX_FRM_STS_LEN	0x0000ffff	/* frame length mask */
+#define D64_RX_FRM_STS_OVFL	0x00800000	/* RxOverFlow */
+#define D64_RX_FRM_STS_DSCRCNT	0x0f000000	/* no. of descriptors used - 1, d11corerev >= 22 */
+#define D64_RX_FRM_STS_DATATYPE	0xf0000000	/* core-dependent data type */
+
+/* receive frame status */
+typedef volatile struct {
+	uint16 len;
+	uint16 flags;
+} dma_rxh_t;
+
+#endif	/* _sbhnddma_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/sbsocram.h b/drivers/bcmdrivers/gmac/src/include/sbsocram.h
new file mode 100755
index 0000000..1afd2e3
