--- a/arch/arm/boot/compressed/head.S
+++ b/arch/arm/boot/compressed/head.S
@@ -18,6 +18,7 @@
  * 100% relocatable.  Any attempt to do so will result in a crash.
  * Please select one of the following when turning on debugging.
  */
+#define DEBUG 1
 #ifdef DEBUG
 
 #if defined(CONFIG_DEBUG_ICEDCC)
diff --git a/arch/arm/boot/dts/accton_as4610_54.dts b/arch/arm/boot/dts/accton_as4610_54.dts
new file mode 100644
index 0000000..9276c0a
