--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/sbchipc.h
@@ -0,0 +1,2517 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * SiliconBackplane Chipcommon core hardware definitions.
+ *
+ * The chipcommon core provides chip identification, SB control,
+ * JTAG, 0/1/2 UARTs, clock frequency control, a watchdog interrupt timer,
+ * GPIO interface, extbus, and support for serial and parallel flashes.
+ *
+ * $Id: sbchipc.h 328955 2012-04-23 09:06:12Z $
+ */
+
+#ifndef	_SBCHIPC_H
+#define	_SBCHIPC_H
+
+#ifndef _LANGUAGE_ASSEMBLY
+
+/* cpp contortions to concatenate w/arg prescan */
+#ifndef PAD
+#define	_PADLINE(line)	pad ## line
+#define	_XSTR(line)	_PADLINE(line)
+#define	PAD		_XSTR(__LINE__)
+#endif	/* PAD */
+
+typedef struct eci_prerev35 {
+	uint32	eci_output;
+	uint32	eci_control;
+	uint32	eci_inputlo;
+	uint32	eci_inputmi;
+	uint32	eci_inputhi;
+	uint32	eci_inputintpolaritylo;
+	uint32	eci_inputintpolaritymi;
+	uint32	eci_inputintpolarityhi;
+	uint32	eci_intmasklo;
+	uint32	eci_intmaskmi;
+	uint32	eci_intmaskhi;
+	uint32	eci_eventlo;
+	uint32	eci_eventmi;
+	uint32	eci_eventhi;
+	uint32	eci_eventmasklo;
+	uint32	eci_eventmaskmi;
+	uint32	eci_eventmaskhi;
+	uint32	PAD[3];
+} eci_prerev35_t;
+
+typedef struct eci_rev35 {
+	uint32	eci_outputlo;
+	uint32	eci_outputhi;
+	uint32	eci_controllo;
+	uint32	eci_controlhi;
+	uint32	eci_inputlo;
+	uint32	eci_inputhi;
+	uint32	eci_inputintpolaritylo;
+	uint32	eci_inputintpolarityhi;
+	uint32	eci_intmasklo;
+	uint32	eci_intmaskhi;
+	uint32	eci_eventlo;
+	uint32	eci_eventhi;
+	uint32	eci_eventmasklo;
+	uint32	eci_eventmaskhi;
+	uint32	eci_auxtx;
+	uint32	eci_auxrx;
+	uint32	eci_datatag;
+	uint32	eci_uartescvalue;
+	uint32	eci_autobaudctr;
+	uint32	eci_uartfifolevel;
+} eci_rev35_t;
+
+typedef struct flash_config {
+	uint32	PAD[19];
+	/* Flash struct configuration registers (0x18c) for BCM4706 (corerev = 31) */
+	uint32 flashstrconfig;
+} flash_config_t;
+
+typedef volatile struct {
+	uint32	chipid;			/* 0x0 */
+	uint32	capabilities;
+	uint32	corecontrol;		/* corerev >= 1 */
+	uint32	bist;
+
+	/* OTP */
+	uint32	otpstatus;		/* 0x10, corerev >= 10 */
+	uint32	otpcontrol;
+	uint32	otpprog;
+	uint32	otplayout;		/* corerev >= 23 */
+
+	/* Interrupt control */
+	uint32	intstatus;		/* 0x20 */
+	uint32	intmask;
+
+	/* Chip specific regs */
+	uint32	chipcontrol;		/* 0x28, rev >= 11 */
+	uint32	chipstatus;		/* 0x2c, rev >= 11 */
+
+	/* Jtag Master */
+	uint32	jtagcmd;		/* 0x30, rev >= 10 */
+	uint32	jtagir;
+	uint32	jtagdr;
+	uint32	jtagctrl;
+
+	/* serial flash interface registers */
+	uint32	flashcontrol;		/* 0x40 */
+	uint32	flashaddress;
+	uint32	flashdata;
+	uint32	otplayoutextension;	/* rev >= 35 */
+
+	/* Silicon backplane configuration broadcast control */
+	uint32	broadcastaddress;	/* 0x50 */
+	uint32	broadcastdata;
+
+	/* gpio - cleared only by power-on-reset */
+	uint32	gpiopullup;		/* 0x58, corerev >= 20 */
+	uint32	gpiopulldown;		/* 0x5c, corerev >= 20 */
+	uint32	gpioin;			/* 0x60 */
+	uint32	gpioout;		/* 0x64 */
+	uint32	gpioouten;		/* 0x68 */
+	uint32	gpiocontrol;		/* 0x6C */
+	uint32	gpiointpolarity;	/* 0x70 */
+	uint32	gpiointmask;		/* 0x74 */
+
+	/* GPIO events corerev >= 11 */
+	uint32	gpioevent;
+	uint32	gpioeventintmask;
+
+	/* Watchdog timer */
+	uint32	watchdog;		/* 0x80 */
+
+	/* GPIO events corerev >= 11 */
+	uint32	gpioeventintpolarity;
+
+	/* GPIO based LED powersave registers corerev >= 16 */
+	uint32  gpiotimerval;		/* 0x88 */
+	uint32  gpiotimeroutmask;
+
+	/* clock control */
+	uint32	clockcontrol_n;		/* 0x90 */
+	uint32	clockcontrol_sb;	/* aka m0 */
+	uint32	clockcontrol_pci;	/* aka m1 */
+	uint32	clockcontrol_m2;	/* mii/uart/mipsref */
+	uint32	clockcontrol_m3;	/* cpu */
+	uint32	clkdiv;			/* corerev >= 3 */
+	uint32	gpiodebugsel;		/* corerev >= 28 */
+	uint32	capabilities_ext;               	/* 0xac  */
+
+	/* pll delay registers (corerev >= 4) */
+	uint32	pll_on_delay;		/* 0xb0 */
+	uint32	fref_sel_delay;
+	uint32	slow_clk_ctl;		/* 5 < corerev < 10 */
+	uint32	PAD;
+
+	/* Instaclock registers (corerev >= 10) */
+	uint32	system_clk_ctl;		/* 0xc0 */
+	uint32	clkstatestretch;
+	uint32	PAD[2];
+
+	/* Indirect backplane access (corerev >= 22) */
+	uint32	bp_addrlow;		/* 0xd0 */
+	uint32	bp_addrhigh;
+	uint32	bp_data;
+	uint32	PAD;
+	uint32	bp_indaccess;
+	/* SPI registers, corerev >= 37 */
+	uint32	gsioctrl;
+	uint32	gsioaddress;
+	uint32	gsiodata;
+
+	/* More clock dividers (corerev >= 32) */
+	uint32	clkdiv2;
+	/* FAB ID (corerev >= 40) */
+	uint32	otpcontrol1;
+	uint32	fabid;			/* 0xf8 */
+
+	/* In AI chips, pointer to erom */
+	uint32	eromptr;		/* 0xfc */
+
+	/* ExtBus control registers (corerev >= 3) */
+	uint32	pcmcia_config;		/* 0x100 */
+	uint32	pcmcia_memwait;
+	uint32	pcmcia_attrwait;
+	uint32	pcmcia_iowait;
+	uint32	ide_config;
+	uint32	ide_memwait;
+	uint32	ide_attrwait;
+	uint32	ide_iowait;
+	uint32	prog_config;
+	uint32	prog_waitcount;
+	uint32	flash_config;
+	uint32	flash_waitcount;
+	uint32  SECI_config;		/* 0x130 SECI configuration */
+	uint32	SECI_status;
+	uint32	SECI_statusmask;
+	uint32	SECI_rxnibchanged;
+
+	union {				/* 0x140 */
+		/* Enhanced Coexistence Interface (ECI) registers (corerev >= 21) */
+		struct eci_prerev35	lt35;
+		struct eci_rev35	ge35;
+		/* Other interfaces */
+		struct flash_config	flashconf;
+		uint32	PAD[20];
+	} eci;
+
+	/* SROM interface (corerev >= 32) */
+	uint32	sromcontrol;		/* 0x190 */
+	uint32	sromaddress;
+	uint32	sromdata;
+	uint32	PAD[1];				/* 0x19C */
+	/* NAND flash registers for BCM4706 (corerev = 31) */
+    uint32  nflashctrl;         /* 0x1a0 */
+    uint32  nflashconf;
+    uint32  nflashcoladdr;
+    uint32  nflashrowaddr;
+    uint32  nflashdata;
+    uint32  nflashwaitcnt0;		/* 0x1b4 */
+    uint32  PAD[2];
+
+	uint32  seci_uart_data;		/* 0x1C0 */
+	uint32  seci_uart_bauddiv;
+	uint32  seci_uart_fcr;
+	uint32  seci_uart_lcr;
+	uint32  seci_uart_mcr;
+	uint32  seci_uart_lsr;
+	uint32  seci_uart_msr;
+	uint32  seci_uart_baudadj;
+	/* Clock control and hardware workarounds (corerev >= 20) */
+	uint32	clk_ctl_st;		/* 0x1e0 */
+	uint32	hw_war;
+	uint32	PAD[70];
+
+	/* UARTs */
+	uint8	uart0data;		/* 0x300 */
+	uint8	uart0imr;
+	uint8	uart0fcr;
+	uint8	uart0lcr;
+	uint8	uart0mcr;
+	uint8	uart0lsr;
+	uint8	uart0msr;
+	uint8	uart0scratch;
+	uint8	PAD[248];		/* corerev >= 1 */
+
+	uint8	uart1data;		/* 0x400 */
+	uint8	uart1imr;
+	uint8	uart1fcr;
+	uint8	uart1lcr;
+	uint8	uart1mcr;
+	uint8	uart1lsr;
+	uint8	uart1msr;
+	uint8	uart1scratch;
+	uint32	PAD[126];
+
+	/* PMU registers (corerev >= 20) */
+	/* Note: all timers driven by ILP clock are updated asynchronously to HT/ALP.
+	 * The CPU must read them twice, compare, and retry if different.
+	 */
+	uint32	pmucontrol;		/* 0x600 */
+	uint32	pmucapabilities;
+	uint32	pmustatus;
+	uint32	res_state;
+	uint32	res_pending;
+	uint32	pmutimer;
+	uint32	min_res_mask;
+	uint32	max_res_mask;
+	uint32	res_table_sel;
+	uint32	res_dep_mask;
+	uint32	res_updn_timer;
+	uint32	res_timer;
+	uint32	clkstretch;
+	uint32	pmuwatchdog;
+	uint32	gpiosel;		/* 0x638, rev >= 1 */
+	uint32	gpioenable;		/* 0x63c, rev >= 1 */
+	uint32	res_req_timer_sel;
+	uint32	res_req_timer;
+	uint32	res_req_mask;
+	uint32	PAD;
+	uint32	chipcontrol_addr;	/* 0x650 */
+	uint32	chipcontrol_data;	/* 0x654 */
+	uint32	regcontrol_addr;
+	uint32	regcontrol_data;
+	uint32	pllcontrol_addr;
+	uint32	pllcontrol_data;
+	uint32	pmustrapopt;		/* 0x668, corerev >= 28 */
+	uint32	pmu_xtalfreq;		/* 0x66C, pmurev >= 10 */
+	uint32	PAD[100];
+	uint16	sromotp[512];		/* 0x800 */
+#ifdef NFLASH_SUPPORT
+	/* Nand flash MLC controller registers (corerev >= 38) */
+	uint32	nand_revision;		/* 0xC00 */
+	uint32	nand_cmd_start;
+	uint32	nand_cmd_addr_x;
+	uint32	nand_cmd_addr;
+	uint32	nand_cmd_end_addr;
+	uint32	nand_cs_nand_select;
+	uint32	nand_cs_nand_xor;
+	uint32	PAD;
+	uint32	nand_spare_rd0;
+	uint32	nand_spare_rd4;
+	uint32	nand_spare_rd8;
+	uint32	nand_spare_rd12;
+	uint32	nand_spare_wr0;
+	uint32	nand_spare_wr4;
+	uint32	nand_spare_wr8;
+	uint32	nand_spare_wr12;
+	uint32	nand_acc_control;
+	uint32	PAD;
+	uint32	nand_config;
+	uint32	PAD;
+	uint32	nand_timing_1;
+	uint32	nand_timing_2;
+	uint32	nand_semaphore;
+	uint32	PAD;
+	uint32	nand_devid;
+	uint32	nand_devid_x;
+	uint32	nand_block_lock_status;
+	uint32	nand_intfc_status;
+	uint32	nand_ecc_corr_addr_x;
+	uint32	nand_ecc_corr_addr;
+	uint32	nand_ecc_unc_addr_x;
+	uint32	nand_ecc_unc_addr;
+	uint32	nand_read_error_count;
+	uint32	nand_corr_stat_threshold;
+	uint32	PAD[2];
+	uint32	nand_read_addr_x;
+	uint32	nand_read_addr;
+	uint32	nand_page_program_addr_x;
+	uint32	nand_page_program_addr;
+	uint32	nand_copy_back_addr_x;
+	uint32	nand_copy_back_addr;
+	uint32	nand_block_erase_addr_x;
+	uint32	nand_block_erase_addr;
+	uint32	nand_inv_read_addr_x;
+	uint32	nand_inv_read_addr;
+	uint32	PAD[2];
+	uint32	nand_blk_wr_protect;
+	uint32	PAD[3];
+	uint32	nand_acc_control_cs1;
+	uint32	nand_config_cs1;
+	uint32	nand_timing_1_cs1;
+	uint32	nand_timing_2_cs1;
+	uint32	PAD[20];
+	uint32	nand_spare_rd16;
+	uint32	nand_spare_rd20;
+	uint32	nand_spare_rd24;
+	uint32	nand_spare_rd28;
+	uint32	nand_cache_addr;
+	uint32	nand_cache_data;
+	uint32	nand_ctrl_config;
+	uint32	nand_ctrl_status;
+#endif /* NFLASH_SUPPORT */
+	uint32  gci_corecaps0; /* GCI starting at 0xC00 */
+	uint32	gci_corecaps1;
+	uint32	gci_corecaps2;
+	uint32	gci_corectrl;
+	uint32	gci_corestat; /* 0xC10 */
+	uint32	PAD[11];
+	uint32	gci_indirect_addr; /* 0xC40 */
+	uint32	PAD[111];
+	uint32	gci_chipctrl; /* 0xE00 */
+} chipcregs_t;
+
+#endif /* _LANGUAGE_ASSEMBLY */
+
+#if	defined(IL_BIGENDIAN) && defined(BCMHND74K)
+/* Selective swapped defines for those registers we need in
+ * big-endian code.
+ */
+#define	CC_CHIPID		4
+#define	CC_CAPABILITIES		0
+#define	CC_CHIPST		0x28
+#define	CC_EROMPTR		0xf8
+
+#else	/* !IL_BIGENDIAN || !BCMHND74K */
+
+#define	CC_CHIPID		0
+#define	CC_CAPABILITIES		4
+#define	CC_CHIPST		0x2c
+#define	CC_EROMPTR		0xfc
+
+#endif	/* IL_BIGENDIAN && BCMHND74K */
+
+#define CC_OTPST		0x10
+#define	CC_JTAGCMD		0x30
+#define	CC_JTAGIR		0x34
+#define	CC_JTAGDR		0x38
+#define	CC_JTAGCTRL		0x3c
+#define	CC_GPIOPU		0x58
+#define	CC_GPIOPD		0x5c
+#define	CC_GPIOIN		0x60
+#define	CC_GPIOOUT		0x64
+#define	CC_GPIOOUTEN		0x68
+#define	CC_GPIOCTRL		0x6c
+#define	CC_GPIOPOL		0x70
+#define	CC_GPIOINTM		0x74
+#define	CC_WATCHDOG		0x80
+#define	CC_CLKC_N		0x90
+#define	CC_CLKC_M0		0x94
+#define	CC_CLKC_M1		0x98
+#define	CC_CLKC_M2		0x9c
+#define	CC_CLKC_M3		0xa0
+#define	CC_CLKDIV		0xa4
+#define	CC_SYS_CLK_CTL		0xc0
+#define	CC_CLK_CTL_ST		SI_CLK_CTL_ST
+#define	PMU_CTL			0x600
+#define	PMU_CAP			0x604
+#define	PMU_ST			0x608
+#define PMU_RES_STATE		0x60c
+#define PMU_TIMER		0x614
+#define	PMU_MIN_RES_MASK	0x618
+#define	PMU_MAX_RES_MASK	0x61c
+#define CC_CHIPCTL_ADDR         0x650
+#define CC_CHIPCTL_DATA         0x654
+#define PMU_REG_CONTROL_ADDR	0x658
+#define PMU_REG_CONTROL_DATA	0x65C
+#define PMU_PLL_CONTROL_ADDR 	0x660
+#define PMU_PLL_CONTROL_DATA 	0x664
+#define CC_SROM_CTRL	0x190
+#define	CC_SROM_OTP		0x800		/* SROM/OTP address space */
+#define CC_GCI_INDIRECT_ADDR_REG	0xC40
+#define CC_GCI_CHIP_CTRL_REG	0xE00
+#define CC_GCI_CC_OFFSET_2	2
+#define CC_GCI_CC_OFFSET_5	5
+
+#ifdef NFLASH_SUPPORT
+/* NAND flash support */
+#define CC_NAND_REVISION	0xC00
+#define CC_NAND_CMD_START	0xC04
+#define CC_NAND_CMD_ADDR	0xC0C
+#define CC_NAND_SPARE_RD_0	0xC20
+#define CC_NAND_SPARE_RD_4	0xC24
+#define CC_NAND_SPARE_RD_8	0xC28
+#define CC_NAND_SPARE_RD_C	0xC2C
+#define CC_NAND_CONFIG		0xC48
+#define CC_NAND_DEVID		0xC60
+#define CC_NAND_DEVID_EXT	0xC64
+#define CC_NAND_INTFC_STATUS	0xC6C
+#endif /* NFLASH_SUPPORT */
+
+/* chipid */
+#define	CID_ID_MASK		0x0000ffff	/* Chip Id mask */
+#define	CID_REV_MASK		0x000f0000	/* Chip Revision mask */
+#define	CID_REV_SHIFT		16		/* Chip Revision shift */
+#define	CID_PKG_MASK		0x00f00000	/* Package Option mask */
+#define	CID_PKG_SHIFT		20		/* Package Option shift */
+#define	CID_CC_MASK		0x0f000000	/* CoreCount (corerev >= 4) */
+#define CID_CC_SHIFT		24
+#define	CID_TYPE_MASK		0xf0000000	/* Chip Type */
+#define CID_TYPE_SHIFT		28
+
+/* capabilities */
+#define	CC_CAP_UARTS_MASK	0x00000003	/* Number of UARTs */
+#define CC_CAP_MIPSEB		0x00000004	/* MIPS is in big-endian mode */
+#define CC_CAP_UCLKSEL		0x00000018	/* UARTs clock select */
+#define CC_CAP_UINTCLK		0x00000008	/* UARTs are driven by internal divided clock */
+#define CC_CAP_UARTGPIO		0x00000020	/* UARTs own GPIOs 15:12 */
+#define CC_CAP_EXTBUS_MASK	0x000000c0	/* External bus mask */
+#define CC_CAP_EXTBUS_NONE	0x00000000	/* No ExtBus present */
+#define CC_CAP_EXTBUS_FULL	0x00000040	/* ExtBus: PCMCIA, IDE & Prog */
+#define CC_CAP_EXTBUS_PROG	0x00000080	/* ExtBus: ProgIf only */
+#define	CC_CAP_FLASH_MASK	0x00000700	/* Type of flash */
+#define	CC_CAP_PLL_MASK		0x00038000	/* Type of PLL */
+#define CC_CAP_PWR_CTL		0x00040000	/* Power control */
+#define CC_CAP_OTPSIZE		0x00380000	/* OTP Size (0 = none) */
+#define CC_CAP_OTPSIZE_SHIFT	19		/* OTP Size shift */
+#define CC_CAP_OTPSIZE_BASE	5		/* OTP Size base */
+#define CC_CAP_JTAGP		0x00400000	/* JTAG Master Present */
+#define CC_CAP_ROM		0x00800000	/* Internal boot rom active */
+#define CC_CAP_BKPLN64		0x08000000	/* 64-bit backplane */
+#define	CC_CAP_PMU		0x10000000	/* PMU Present, rev >= 20 */
+#define	CC_CAP_ECI		0x20000000	/* ECI Present, rev >= 21 */
+#define	CC_CAP_SROM		0x40000000	/* Srom Present, rev >= 32 */
+#define	CC_CAP_NFLASH		0x80000000	/* Nand flash present, rev >= 35 */
+
+#define	CC_CAP2_SECI		0x00000001	/* SECI Present, rev >= 36 */
+#define	CC_CAP2_GSIO		0x00000002	/* GSIO (spi/i2c) present, rev >= 37 */
+
+/* capabilities extension */
+#define CC_CAP_EXT_SECI_PRESENT   0x00000001    /* SECI present */
+
+/* PLL type */
+#define PLL_NONE		0x00000000
+#define PLL_TYPE1		0x00010000	/* 48MHz base, 3 dividers */
+#define PLL_TYPE2		0x00020000	/* 48MHz, 4 dividers */
+#define PLL_TYPE3		0x00030000	/* 25MHz, 2 dividers */
+#define PLL_TYPE4		0x00008000	/* 48MHz, 4 dividers */
+#define PLL_TYPE5		0x00018000	/* 25MHz, 4 dividers */
+#define PLL_TYPE6		0x00028000	/* 100/200 or 120/240 only */
+#define PLL_TYPE7		0x00038000	/* 25MHz, 4 dividers */
+
+/* ILP clock */
+#define	ILP_CLOCK		32000
+
+/* ALP clock on pre-PMU chips */
+#define	ALP_CLOCK		20000000
+
+#define NS_ALP_CLOCK		125000000
+#define NS_SLOW_ALP_CLOCK	100000000
+#define NS_CPU_CLOCK		1000000000
+#define NS_SLOW_CPU_CLOCK	800000000
+#define NS_SI_CLOCK		250000000
+#define NS_SLOW_SI_CLOCK	200000000
+#define NS_FAST_MEM_CLOCK	800000000
+#define NS_MEM_CLOCK		533000000
+#define NS_SLOW_MEM_CLOCK	400000000
+
+/* HT clock */
+#define	HT_CLOCK		80000000
+
+/* corecontrol */
+#define CC_UARTCLKO		0x00000001	/* Drive UART with internal clock */
+#define	CC_SE			0x00000002	/* sync clk out enable (corerev >= 3) */
+#define CC_ASYNCGPIO	0x00000004	/* 1=generate GPIO interrupt without backplane clock */
+#define CC_UARTCLKEN		0x00000008	/* enable UART Clock (corerev > = 21 */
+
+/* 4321 chipcontrol */
+#define CHIPCTRL_4321A0_DEFAULT	0x3a4
+#define CHIPCTRL_4321A1_DEFAULT	0x0a4
+#define CHIPCTRL_4321_PLL_DOWN	0x800000	/* serdes PLL down override */
+
+/* Fields in the otpstatus register in rev >= 21 */
+#define OTPS_OL_MASK		0x000000ff
+#define OTPS_OL_MFG		0x00000001	/* manuf row is locked */
+#define OTPS_OL_OR1		0x00000002	/* otp redundancy row 1 is locked */
+#define OTPS_OL_OR2		0x00000004	/* otp redundancy row 2 is locked */
+#define OTPS_OL_GU		0x00000008	/* general use region is locked */
+#define OTPS_GUP_MASK		0x00000f00
+#define OTPS_GUP_SHIFT		8
+#define OTPS_GUP_HW		0x00000100	/* h/w subregion is programmed */
+#define OTPS_GUP_SW		0x00000200	/* s/w subregion is programmed */
+#define OTPS_GUP_CI		0x00000400	/* chipid/pkgopt subregion is programmed */
+#define OTPS_GUP_FUSE		0x00000800	/* fuse subregion is programmed */
+#define OTPS_READY		0x00001000
+#define OTPS_RV(x)		(1 << (16 + (x)))	/* redundancy entry valid */
+#define OTPS_RV_MASK		0x0fff0000
+#define OTPS_PROGOK     0x40000000
+
+/* Fields in the otpcontrol register in rev >= 21 */
+#define OTPC_PROGSEL		0x00000001
+#define OTPC_PCOUNT_MASK	0x0000000e
+#define OTPC_PCOUNT_SHIFT	1
+#define OTPC_VSEL_MASK		0x000000f0
+#define OTPC_VSEL_SHIFT		4
+#define OTPC_TMM_MASK		0x00000700
+#define OTPC_TMM_SHIFT		8
+#define OTPC_ODM		0x00000800
+#define OTPC_PROGEN		0x80000000
+
+/* Fields in the 40nm otpcontrol register in rev >= 40 */
+#define OTPC_40NM_PROGSEL_SHIFT	0
+#define OTPC_40NM_PCOUNT_SHIFT	1
+#define OTPC_40NM_PCOUNT_WR	0xA
+#define OTPC_40NM_PCOUNT_V1X	0xB
+#define OTPC_40NM_REGCSEL_SHIFT	5
+#define OTPC_40NM_REGCSEL_DEF	0x4
+#define OTPC_40NM_PROGIN_SHIFT	8
+#define OTPC_40NM_R2X_SHIFT	10
+#define OTPC_40NM_ODM_SHIFT	11
+#define OTPC_40NM_DF_SHIFT	15
+#define OTPC_40NM_VSEL_SHIFT	16
+#define OTPC_40NM_VSEL_WR	0xA
+#define OTPC_40NM_VSEL_V1X	0xA
+#define OTPC_40NM_VSEL_R1X	0x5
+#define OTPC_40NM_COFAIL_SHIFT	30
+
+#define OTPC1_CPCSEL_SHIFT	0
+#define OTPC1_CPCSEL_DEF	6
+#define OTPC1_TM_SHIFT		8
+#define OTPC1_TM_WR		0x84
+#define OTPC1_TM_V1X		0x84
+#define OTPC1_TM_R1X		0x4
+
+/* Fields in otpprog in rev >= 21 and HND OTP */
+#define OTPP_COL_MASK		0x000000ff
+#define OTPP_COL_SHIFT		0
+#define OTPP_ROW_MASK		0x0000ff00
+#define OTPP_ROW_SHIFT		8
+#define OTPP_OC_MASK		0x0f000000
+#define OTPP_OC_SHIFT		24
+#define OTPP_READERR		0x10000000
+#define OTPP_VALUE_MASK		0x20000000
+#define OTPP_VALUE_SHIFT	29
+#define OTPP_START_BUSY		0x80000000
+#define	OTPP_READ		0x40000000	/* HND OTP */
+
+/* Fields in otplayout register */
+#define OTPL_HWRGN_OFF_MASK	0x00000FFF
+#define OTPL_HWRGN_OFF_SHIFT	0
+#define OTPL_WRAP_REVID_MASK	0x00F80000
+#define OTPL_WRAP_REVID_SHIFT	19
+#define OTPL_WRAP_TYPE_MASK	0x00070000
+#define OTPL_WRAP_TYPE_SHIFT	16
+#define OTPL_WRAP_TYPE_65NM	0
+#define OTPL_WRAP_TYPE_40NM	1
+
+/* otplayout reg corerev >= 36 */
+#define OTP_CISFORMAT_NEW	0x80000000
+
+/* Opcodes for OTPP_OC field */
+#define OTPPOC_READ		0
+#define OTPPOC_BIT_PROG		1
+#define OTPPOC_VERIFY		3
+#define OTPPOC_INIT		4
+#define OTPPOC_SET		5
+#define OTPPOC_RESET		6
+#define OTPPOC_OCST		7
+#define OTPPOC_ROW_LOCK		8
+#define OTPPOC_PRESCN_TEST	9
+
+/* Opcodes for OTPP_OC field (40NM) */
+#define OTPPOC_READ_40NM	0
+#define OTPPOC_PROG_ENABLE_40NM 1
+#define OTPPOC_PROG_DISABLE_40NM	2
+#define OTPPOC_VERIFY_40NM	3
+#define OTPPOC_WORD_VERIFY_1_40NM	4
+#define OTPPOC_ROW_LOCK_40NM	5
+#define OTPPOC_STBY_40NM	6
+#define OTPPOC_WAKEUP_40NM	7
+#define OTPPOC_WORD_VERIFY_0_40NM	8
+#define OTPPOC_PRESCN_TEST_40NM 9
+#define OTPPOC_BIT_PROG_40NM	10
+#define OTPPOC_WORDPROG_40NM	11
+#define OTPPOC_BURNIN_40NM	12
+#define OTPPOC_AUTORELOAD_40NM	13
+#define OTPPOC_OVST_READ_40NM	14
+#define OTPPOC_OVST_PROG_40NM	15
+
+/* Fields in otplayoutextension */
+#define OTPLAYOUTEXT_FUSE_MASK	0x3FF
+
+
+/* Jtagm characteristics that appeared at a given corerev */
+#define	JTAGM_CREV_OLD		10	/* Old command set, 16bit max IR */
+#define	JTAGM_CREV_IRP		22	/* Able to do pause-ir */
+#define	JTAGM_CREV_RTI		28	/* Able to do return-to-idle */
+
+/* jtagcmd */
+#define JCMD_START		0x80000000
+#define JCMD_BUSY		0x80000000
+#define JCMD_STATE_MASK		0x60000000
+#define JCMD_STATE_TLR		0x00000000	/* Test-logic-reset */
+#define JCMD_STATE_PIR		0x20000000	/* Pause IR */
+#define JCMD_STATE_PDR		0x40000000	/* Pause DR */
+#define JCMD_STATE_RTI		0x60000000	/* Run-test-idle */
+#define JCMD0_ACC_MASK		0x0000f000
+#define JCMD0_ACC_IRDR		0x00000000
+#define JCMD0_ACC_DR		0x00001000
+#define JCMD0_ACC_IR		0x00002000
+#define JCMD0_ACC_RESET		0x00003000
+#define JCMD0_ACC_IRPDR		0x00004000
+#define JCMD0_ACC_PDR		0x00005000
+#define JCMD0_IRW_MASK		0x00000f00
+#define JCMD_ACC_MASK		0x000f0000	/* Changes for corerev 11 */
+#define JCMD_ACC_IRDR		0x00000000
+#define JCMD_ACC_DR		0x00010000
+#define JCMD_ACC_IR		0x00020000
+#define JCMD_ACC_RESET		0x00030000
+#define JCMD_ACC_IRPDR		0x00040000
+#define JCMD_ACC_PDR		0x00050000
+#define JCMD_ACC_PIR		0x00060000
+#define JCMD_ACC_IRDR_I		0x00070000	/* rev 28: return to run-test-idle */
+#define JCMD_ACC_DR_I		0x00080000	/* rev 28: return to run-test-idle */
+#define JCMD_IRW_MASK		0x00001f00
+#define JCMD_IRW_SHIFT		8
+#define JCMD_DRW_MASK		0x0000003f
+
+/* jtagctrl */
+#define JCTRL_FORCE_CLK		4		/* Force clock */
+#define JCTRL_EXT_EN		2		/* Enable external targets */
+#define JCTRL_EN		1		/* Enable Jtag master */
+
+/* Fields in clkdiv */
+#define	CLKD_SFLASH		0x0f000000
+#define	CLKD_SFLASH_SHIFT	24
+#define	CLKD_OTP		0x000f0000
+#define	CLKD_OTP_SHIFT		16
+#define	CLKD_JTAG		0x00000f00
+#define	CLKD_JTAG_SHIFT		8
+#define	CLKD_UART		0x000000ff
+
+#define	CLKD2_SROM		0x00000003
+
+/* intstatus/intmask */
+#define	CI_GPIO			0x00000001	/* gpio intr */
+#define	CI_EI			0x00000002	/* extif intr (corerev >= 3) */
+#define	CI_TEMP			0x00000004	/* temp. ctrl intr (corerev >= 15) */
+#define	CI_SIRQ			0x00000008	/* serial IRQ intr (corerev >= 15) */
+#define	CI_ECI			0x00000010	/* eci intr (corerev >= 21) */
+#define	CI_PMU			0x00000020	/* pmu intr (corerev >= 21) */
+#define	CI_UART			0x00000040	/* uart intr (corerev >= 21) */
+#define	CI_WDRESET		0x80000000	/* watchdog reset occurred */
+
+/* slow_clk_ctl */
+#define SCC_SS_MASK		0x00000007	/* slow clock source mask */
+#define	SCC_SS_LPO		0x00000000	/* source of slow clock is LPO */
+#define	SCC_SS_XTAL		0x00000001	/* source of slow clock is crystal */
+#define	SCC_SS_PCI		0x00000002	/* source of slow clock is PCI */
+#define SCC_LF			0x00000200	/* LPOFreqSel, 1: 160Khz, 0: 32KHz */
+#define SCC_LP			0x00000400	/* LPOPowerDown, 1: LPO is disabled,
+						 * 0: LPO is enabled
+						 */
+#define SCC_FS			0x00000800	/* ForceSlowClk, 1: sb/cores running on slow clock,
+						 * 0: power logic control
+						 */
+#define SCC_IP			0x00001000	/* IgnorePllOffReq, 1/0: power logic ignores/honors
+						 * PLL clock disable requests from core
+						 */
+#define SCC_XC			0x00002000	/* XtalControlEn, 1/0: power logic does/doesn't
+						 * disable crystal when appropriate
+						 */
+#define SCC_XP			0x00004000	/* XtalPU (RO), 1/0: crystal running/disabled */
+#define SCC_CD_MASK		0xffff0000	/* ClockDivider (SlowClk = 1/(4+divisor)) */
+#define SCC_CD_SHIFT		16
+
+/* system_clk_ctl */
+#define	SYCC_IE			0x00000001	/* ILPen: Enable Idle Low Power */
+#define	SYCC_AE			0x00000002	/* ALPen: Enable Active Low Power */
+#define	SYCC_FP			0x00000004	/* ForcePLLOn */
+#define	SYCC_AR			0x00000008	/* Force ALP (or HT if ALPen is not set */
+#define	SYCC_HR			0x00000010	/* Force HT */
+#define SYCC_CD_MASK		0xffff0000	/* ClkDiv  (ILP = 1/(4 * (divisor + 1)) */
+#define SYCC_CD_SHIFT		16
+
+/* Indirect backplane access */
+#define	BPIA_BYTEEN		0x0000000f
+#define	BPIA_SZ1		0x00000001
+#define	BPIA_SZ2		0x00000003
+#define	BPIA_SZ4		0x00000007
+#define	BPIA_SZ8		0x0000000f
+#define	BPIA_WRITE		0x00000100
+#define	BPIA_START		0x00000200
+#define	BPIA_BUSY		0x00000200
+#define	BPIA_ERROR		0x00000400
+
+/* pcmcia/prog/flash_config */
+#define	CF_EN			0x00000001	/* enable */
+#define	CF_EM_MASK		0x0000000e	/* mode */
+#define	CF_EM_SHIFT		1
+#define	CF_EM_FLASH		0		/* flash/asynchronous mode */
+#define	CF_EM_SYNC		2		/* synchronous mode */
+#define	CF_EM_PCMCIA		4		/* pcmcia mode */
+#define	CF_DS			0x00000010	/* destsize:  0=8bit, 1=16bit */
+#define	CF_BS			0x00000020	/* byteswap */
+#define	CF_CD_MASK		0x000000c0	/* clock divider */
+#define	CF_CD_SHIFT		6
+#define	CF_CD_DIV2		0x00000000	/* backplane/2 */
+#define	CF_CD_DIV3		0x00000040	/* backplane/3 */
+#define	CF_CD_DIV4		0x00000080	/* backplane/4 */
+#define	CF_CE			0x00000100	/* clock enable */
+#define	CF_SB			0x00000200	/* size/bytestrobe (synch only) */
+
+/* pcmcia_memwait */
+#define	PM_W0_MASK		0x0000003f	/* waitcount0 */
+#define	PM_W1_MASK		0x00001f00	/* waitcount1 */
+#define	PM_W1_SHIFT		8
+#define	PM_W2_MASK		0x001f0000	/* waitcount2 */
+#define	PM_W2_SHIFT		16
+#define	PM_W3_MASK		0x1f000000	/* waitcount3 */
+#define	PM_W3_SHIFT		24
+
+/* pcmcia_attrwait */
+#define	PA_W0_MASK		0x0000003f	/* waitcount0 */
+#define	PA_W1_MASK		0x00001f00	/* waitcount1 */
+#define	PA_W1_SHIFT		8
+#define	PA_W2_MASK		0x001f0000	/* waitcount2 */
+#define	PA_W2_SHIFT		16
+#define	PA_W3_MASK		0x1f000000	/* waitcount3 */
+#define	PA_W3_SHIFT		24
+
+/* pcmcia_iowait */
+#define	PI_W0_MASK		0x0000003f	/* waitcount0 */
+#define	PI_W1_MASK		0x00001f00	/* waitcount1 */
+#define	PI_W1_SHIFT		8
+#define	PI_W2_MASK		0x001f0000	/* waitcount2 */
+#define	PI_W2_SHIFT		16
+#define	PI_W3_MASK		0x1f000000	/* waitcount3 */
+#define	PI_W3_SHIFT		24
+
+/* prog_waitcount */
+#define	PW_W0_MASK		0x0000001f	/* waitcount0 */
+#define	PW_W1_MASK		0x00001f00	/* waitcount1 */
+#define	PW_W1_SHIFT		8
+#define	PW_W2_MASK		0x001f0000	/* waitcount2 */
+#define	PW_W2_SHIFT		16
+#define	PW_W3_MASK		0x1f000000	/* waitcount3 */
+#define	PW_W3_SHIFT		24
+
+#define PW_W0       		0x0000000c
+#define PW_W1       		0x00000a00
+#define PW_W2       		0x00020000
+#define PW_W3       		0x01000000
+
+/* flash_waitcount */
+#define	FW_W0_MASK		0x0000003f	/* waitcount0 */
+#define	FW_W1_MASK		0x00001f00	/* waitcount1 */
+#define	FW_W1_SHIFT		8
+#define	FW_W2_MASK		0x001f0000	/* waitcount2 */
+#define	FW_W2_SHIFT		16
+#define	FW_W3_MASK		0x1f000000	/* waitcount3 */
+#define	FW_W3_SHIFT		24
+
+/* When Srom support present, fields in sromcontrol */
+#define	SRC_START		0x80000000
+#define	SRC_BUSY		0x80000000
+#define	SRC_OPCODE		0x60000000
+#define	SRC_OP_READ		0x00000000
+#define	SRC_OP_WRITE		0x20000000
+#define	SRC_OP_WRDIS		0x40000000
+#define	SRC_OP_WREN		0x60000000
+#define	SRC_OTPSEL		0x00000010
+#define	SRC_LOCK		0x00000008
+#define	SRC_SIZE_MASK		0x00000006
+#define	SRC_SIZE_1K		0x00000000
+#define	SRC_SIZE_4K		0x00000002
+#define	SRC_SIZE_16K		0x00000004
+#define	SRC_SIZE_SHIFT		1
+#define	SRC_PRESENT		0x00000001
+
+/* Fields in pmucontrol */
+#define	PCTL_ILP_DIV_MASK	0xffff0000
+#define	PCTL_ILP_DIV_SHIFT	16
+#define PCTL_PLL_PLLCTL_UPD	0x00000400	/* rev 2 */
+#define PCTL_NOILP_ON_WAIT	0x00000200	/* rev 1 */
+#define	PCTL_HT_REQ_EN		0x00000100
+#define	PCTL_ALP_REQ_EN		0x00000080
+#define	PCTL_XTALFREQ_MASK	0x0000007c
+#define	PCTL_XTALFREQ_SHIFT	2
+#define	PCTL_ILP_DIV_EN		0x00000002
+#define	PCTL_LPO_SEL		0x00000001
+
+/* Fields in clkstretch */
+#define CSTRETCH_HT		0xffff0000
+#define CSTRETCH_ALP		0x0000ffff
+
+/* gpiotimerval */
+#define GPIO_ONTIME_SHIFT	16
+
+/* clockcontrol_n */
+#define	CN_N1_MASK		0x3f		/* n1 control */
+#define	CN_N2_MASK		0x3f00		/* n2 control */
+#define	CN_N2_SHIFT		8
+#define	CN_PLLC_MASK		0xf0000		/* pll control */
+#define	CN_PLLC_SHIFT		16
+
+/* clockcontrol_sb/pci/uart */
+#define	CC_M1_MASK		0x3f		/* m1 control */
+#define	CC_M2_MASK		0x3f00		/* m2 control */
+#define	CC_M2_SHIFT		8
+#define	CC_M3_MASK		0x3f0000	/* m3 control */
+#define	CC_M3_SHIFT		16
+#define	CC_MC_MASK		0x1f000000	/* mux control */
+#define	CC_MC_SHIFT		24
+
+/* N3M Clock control magic field values */
+#define	CC_F6_2			0x02		/* A factor of 2 in */
+#define	CC_F6_3			0x03		/* 6-bit fields like */
+#define	CC_F6_4			0x05		/* N1, M1 or M3 */
+#define	CC_F6_5			0x09
+#define	CC_F6_6			0x11
+#define	CC_F6_7			0x21
+
+#define	CC_F5_BIAS		5		/* 5-bit fields get this added */
+
+#define	CC_MC_BYPASS		0x08
+#define	CC_MC_M1		0x04
+#define	CC_MC_M1M2		0x02
+#define	CC_MC_M1M2M3		0x01
+#define	CC_MC_M1M3		0x11
+
+/* Type 2 Clock control magic field values */
+#define	CC_T2_BIAS		2		/* n1, n2, m1 & m3 bias */
+#define	CC_T2M2_BIAS		3		/* m2 bias */
+
+#define	CC_T2MC_M1BYP		1
+#define	CC_T2MC_M2BYP		2
+#define	CC_T2MC_M3BYP		4
+
+/* Type 6 Clock control magic field values */
+#define	CC_T6_MMASK		1		/* bits of interest in m */
+#define	CC_T6_M0		120000000	/* sb clock for m = 0 */
+#define	CC_T6_M1		100000000	/* sb clock for m = 1 */
+#define	SB2MIPS_T6(sb)		(2 * (sb))
+
+/* Common clock base */
+#define	CC_CLOCK_BASE1		24000000	/* Half the clock freq */
+#define CC_CLOCK_BASE2		12500000	/* Alternate crystal on some PLLs */
+
+/* Clock control values for 200MHz in 5350 */
+#define	CLKC_5350_N		0x0311
+#define	CLKC_5350_M		0x04020009
+
+/* Flash types in the chipcommon capabilities register */
+#define FLASH_NONE		0x000		/* No flash */
+#define SFLASH_ST		0x100		/* ST serial flash */
+#define SFLASH_AT		0x200		/* Atmel serial flash */
+#define NFLASH			0x300
+#define	PFLASH			0x700		/* Parallel flash */
+#define QSPIFLASH_ST		0x800
+#define QSPIFLASH_AT		0x900
+
+/* Bits in the ExtBus config registers */
+#define	CC_CFG_EN		0x0001		/* Enable */
+#define	CC_CFG_EM_MASK		0x000e		/* Extif Mode */
+#define	CC_CFG_EM_ASYNC		0x0000		/*   Async/Parallel flash */
+#define	CC_CFG_EM_SYNC		0x0002		/*   Synchronous */
+#define	CC_CFG_EM_PCMCIA	0x0004		/*   PCMCIA */
+#define	CC_CFG_EM_IDE		0x0006		/*   IDE */
+#define	CC_CFG_DS		0x0010		/* Data size, 0=8bit, 1=16bit */
+#define	CC_CFG_CD_MASK		0x00e0		/* Sync: Clock divisor, rev >= 20 */
+#define	CC_CFG_CE		0x0100		/* Sync: Clock enable, rev >= 20 */
+#define	CC_CFG_SB		0x0200		/* Sync: Size/Bytestrobe, rev >= 20 */
+#define	CC_CFG_IS		0x0400		/* Extif Sync Clk Select, rev >= 20 */
+
+/* ExtBus address space */
+#define	CC_EB_BASE		0x1a000000	/* Chipc ExtBus base address */
+#define	CC_EB_PCMCIA_MEM	0x1a000000	/* PCMCIA 0 memory base address */
+#define	CC_EB_PCMCIA_IO		0x1a200000	/* PCMCIA 0 I/O base address */
+#define	CC_EB_PCMCIA_CFG	0x1a400000	/* PCMCIA 0 config base address */
+#define	CC_EB_IDE		0x1a800000	/* IDE memory base */
+#define	CC_EB_PCMCIA1_MEM	0x1a800000	/* PCMCIA 1 memory base address */
+#define	CC_EB_PCMCIA1_IO	0x1aa00000	/* PCMCIA 1 I/O base address */
+#define	CC_EB_PCMCIA1_CFG	0x1ac00000	/* PCMCIA 1 config base address */
+#define	CC_EB_PROGIF		0x1b000000	/* ProgIF Async/Sync base address */
+
+
+/* Start/busy bit in flashcontrol */
+#define SFLASH_OPCODE		0x000000ff
+#define SFLASH_ACTION		0x00000700
+#define	SFLASH_CS_ACTIVE	0x00001000	/* Chip Select Active, rev >= 20 */
+#define SFLASH_START		0x80000000
+#define SFLASH_BUSY		SFLASH_START
+
+/* flashcontrol action codes */
+#define	SFLASH_ACT_OPONLY	0x0000		/* Issue opcode only */
+#define	SFLASH_ACT_OP1D		0x0100		/* opcode + 1 data byte */
+#define	SFLASH_ACT_OP3A		0x0200		/* opcode + 3 addr bytes */
+#define	SFLASH_ACT_OP3A1D	0x0300		/* opcode + 3 addr & 1 data bytes */
+#define	SFLASH_ACT_OP3A4D	0x0400		/* opcode + 3 addr & 4 data bytes */
+#define	SFLASH_ACT_OP3A4X4D	0x0500		/* opcode + 3 addr, 4 don't care & 4 data bytes */
+#define	SFLASH_ACT_OP3A1X4D	0x0700		/* opcode + 3 addr, 1 don't care & 4 data bytes */
+
+/* flashcontrol action+opcodes for ST flashes */
+#define SFLASH_ST_WREN		0x0006		/* Write Enable */
+#define SFLASH_ST_WRDIS		0x0004		/* Write Disable */
+#define SFLASH_ST_RDSR		0x0105		/* Read Status Register */
+#define SFLASH_ST_WRSR		0x0101		/* Write Status Register */
+#define SFLASH_ST_READ		0x0303		/* Read Data Bytes */
+#define SFLASH_ST_PP		0x0302		/* Page Program */
+#define SFLASH_ST_SE		0x02d8		/* Sector Erase */
+#define SFLASH_ST_BE		0x00c7		/* Bulk Erase */
+#define SFLASH_ST_DP		0x00b9		/* Deep Power-down */
+#define SFLASH_ST_RES		0x03ab		/* Read Electronic Signature */
+#define SFLASH_ST_CSA		0x1000		/* Keep chip select asserted */
+#define SFLASH_ST_SSE		0x0220		/* Sub-sector Erase */
+
+#define SFLASH_MXIC_RDID	0x0390		/* Read Manufacture ID */
+#define SFLASH_MXIC_MFID	0xc2		/* MXIC Manufacture ID */
+
+/* Status register bits for ST flashes */
+#define SFLASH_ST_WIP		0x01		/* Write In Progress */
+#define SFLASH_ST_WEL		0x02		/* Write Enable Latch */
+#define SFLASH_ST_BP_MASK	0x1c		/* Block Protect */
+#define SFLASH_ST_BP_SHIFT	2
+#define SFLASH_ST_SRWD		0x80		/* Status Register Write Disable */
+
+/* flashcontrol action+opcodes for Atmel flashes */
+#define SFLASH_AT_READ				0x07e8
+#define SFLASH_AT_PAGE_READ			0x07d2
+#define SFLASH_AT_BUF1_READ
+#define SFLASH_AT_BUF2_READ
+#define SFLASH_AT_STATUS			0x01d7
+#define SFLASH_AT_BUF1_WRITE			0x0384
+#define SFLASH_AT_BUF2_WRITE			0x0387
+#define SFLASH_AT_BUF1_ERASE_PROGRAM		0x0283
+#define SFLASH_AT_BUF2_ERASE_PROGRAM		0x0286
+#define SFLASH_AT_BUF1_PROGRAM			0x0288
+#define SFLASH_AT_BUF2_PROGRAM			0x0289
+#define SFLASH_AT_PAGE_ERASE			0x0281
+#define SFLASH_AT_BLOCK_ERASE			0x0250
+#define SFLASH_AT_BUF1_WRITE_ERASE_PROGRAM	0x0382
+#define SFLASH_AT_BUF2_WRITE_ERASE_PROGRAM	0x0385
+#define SFLASH_AT_BUF1_LOAD			0x0253
+#define SFLASH_AT_BUF2_LOAD			0x0255
+#define SFLASH_AT_BUF1_COMPARE			0x0260
+#define SFLASH_AT_BUF2_COMPARE			0x0261
+#define SFLASH_AT_BUF1_REPROGRAM		0x0258
+#define SFLASH_AT_BUF2_REPROGRAM		0x0259
+
+/* Status register bits for Atmel flashes */
+#define SFLASH_AT_READY				0x80
+#define SFLASH_AT_MISMATCH			0x40
+#define SFLASH_AT_ID_MASK			0x38
+#define SFLASH_AT_ID_SHIFT			3
+
+/* SPI register bits, corerev >= 37 */
+#define GSIO_START			0x80000000
+#define GSIO_BUSY			GSIO_START
+
+/*
+ * These are the UART port assignments, expressed as offsets from the base
+ * register.  These assignments should hold for any serial port based on
+ * a 8250, 16450, or 16550(A).
+ */
+
+#define UART_RX		0	/* In:  Receive buffer (DLAB=0) */
+#define UART_TX		0	/* Out: Transmit buffer (DLAB=0) */
+#define UART_DLL	0	/* Out: Divisor Latch Low (DLAB=1) */
+#define UART_IER	1	/* In/Out: Interrupt Enable Register (DLAB=0) */
+#define UART_DLM	1	/* Out: Divisor Latch High (DLAB=1) */
+#define UART_IIR	2	/* In: Interrupt Identity Register  */
+#define UART_FCR	2	/* Out: FIFO Control Register */
+#define UART_LCR	3	/* Out: Line Control Register */
+#define UART_MCR	4	/* Out: Modem Control Register */
+#define UART_LSR	5	/* In:  Line Status Register */
+#define UART_MSR	6	/* In:  Modem Status Register */
+#define UART_SCR	7	/* I/O: Scratch Register */
+#define UART_LCR_DLAB	0x80	/* Divisor latch access bit */
+#define UART_LCR_WLEN8	0x03	/* Word length: 8 bits */
+#define UART_MCR_OUT2	0x08	/* MCR GPIO out 2 */
+#define UART_MCR_LOOP	0x10	/* Enable loopback test mode */
+#define UART_LSR_RX_FIFO 	0x80	/* Receive FIFO error */
+#define UART_LSR_TDHR		0x40	/* Data-hold-register empty */
+#define UART_LSR_THRE		0x20	/* Transmit-hold-register empty */
+#define UART_LSR_BREAK		0x10	/* Break interrupt */
+#define UART_LSR_FRAMING	0x08	/* Framing error */
+#define UART_LSR_PARITY		0x04	/* Parity error */
+#define UART_LSR_OVERRUN	0x02	/* Overrun error */
+#define UART_LSR_RXRDY		0x01	/* Receiver ready */
+#define UART_FCR_FIFO_ENABLE 1	/* FIFO control register bit controlling FIFO enable/disable */
+
+/* Interrupt Identity Register (IIR) bits */
+#define UART_IIR_FIFO_MASK	0xc0	/* IIR FIFO disable/enabled mask */
+#define UART_IIR_INT_MASK	0xf	/* IIR interrupt ID source */
+#define UART_IIR_MDM_CHG	0x0	/* Modem status changed */
+#define UART_IIR_NOINT		0x1	/* No interrupt pending */
+#define UART_IIR_THRE		0x2	/* THR empty */
+#define UART_IIR_RCVD_DATA	0x4	/* Received data available */
+#define UART_IIR_RCVR_STATUS 	0x6	/* Receiver status */
+#define UART_IIR_CHAR_TIME 	0xc	/* Character time */
+
+/* Interrupt Enable Register (IER) bits */
+#define UART_IER_EDSSI	8	/* enable modem status interrupt */
+#define UART_IER_ELSI	4	/* enable receiver line status interrupt */
+#define UART_IER_ETBEI  2	/* enable transmitter holding register empty interrupt */
+#define UART_IER_ERBFI	1	/* enable data available interrupt */
+
+/* pmustatus */
+#define PST_EXTLPOAVAIL	0x0100
+#define PST_WDRESET	0x0080
+#define	PST_INTPEND	0x0040
+#define	PST_SBCLKST	0x0030
+#define	PST_SBCLKST_ILP	0x0010
+#define	PST_SBCLKST_ALP	0x0020
+#define	PST_SBCLKST_HT	0x0030
+#define	PST_ALPAVAIL	0x0008
+#define	PST_HTAVAIL	0x0004
+#define	PST_RESINIT	0x0003
+
+/* pmucapabilities */
+#define PCAP_REV_MASK	0x000000ff
+#define PCAP_RC_MASK	0x00001f00
+#define PCAP_RC_SHIFT	8
+#define PCAP_TC_MASK	0x0001e000
+#define PCAP_TC_SHIFT	13
+#define PCAP_PC_MASK	0x001e0000
+#define PCAP_PC_SHIFT	17
+#define PCAP_VC_MASK	0x01e00000
+#define PCAP_VC_SHIFT	21
+#define PCAP_CC_MASK	0x1e000000
+#define PCAP_CC_SHIFT	25
+#define PCAP5_PC_MASK	0x003e0000	/* PMU corerev >= 5 */
+#define PCAP5_PC_SHIFT	17
+#define PCAP5_VC_MASK	0x07c00000
+#define PCAP5_VC_SHIFT	22
+#define PCAP5_CC_MASK	0xf8000000
+#define PCAP5_CC_SHIFT	27
+
+/* PMU Resource Request Timer registers */
+/* This is based on PmuRev0 */
+#define	PRRT_TIME_MASK	0x03ff
+#define	PRRT_INTEN	0x0400
+#define	PRRT_REQ_ACTIVE	0x0800
+#define	PRRT_ALP_REQ	0x1000
+#define	PRRT_HT_REQ	0x2000
+#define PRRT_HQ_REQ 0x4000
+
+/* PMU resource bit position */
+#define PMURES_BIT(bit)	(1 << (bit))
+
+/* PMU resource number limit */
+#define PMURES_MAX_RESNUM	30
+
+/* PMU chip control0 register */
+#define	PMU_CHIPCTL0		0
+
+/* clock req types */
+#define PMU_CC1_CLKREQ_TYPE_SHIFT	19
+#define PMU_CC1_CLKREQ_TYPE_MASK	(1 << PMU_CC1_CLKREQ_TYPE_SHIFT)
+
+#define CLKREQ_TYPE_CONFIG_OPENDRAIN		0
+#define CLKREQ_TYPE_CONFIG_PUSHPULL		1
+
+/* PMU chip control1 register */
+#define	PMU_CHIPCTL1			1
+#define	PMU_CC1_RXC_DLL_BYPASS		0x00010000
+
+#define PMU_CC1_IF_TYPE_MASK   		0x00000030
+#define PMU_CC1_IF_TYPE_RMII    	0x00000000
+#define PMU_CC1_IF_TYPE_MII     	0x00000010
+#define PMU_CC1_IF_TYPE_RGMII   	0x00000020
+
+#define PMU_CC1_SW_TYPE_MASK    	0x000000c0
+#define PMU_CC1_SW_TYPE_EPHY    	0x00000000
+#define PMU_CC1_SW_TYPE_EPHYMII 	0x00000040
+#define PMU_CC1_SW_TYPE_EPHYRMII	0x00000080
+#define PMU_CC1_SW_TYPE_RGMII   	0x000000c0
+
+/* PMU chip control2 register */
+#define	PMU_CHIPCTL2		2
+
+/* PMU chip control3 register */
+#define	PMU_CHIPCTL3		3
+
+#define PMU_CC3_ENABLE_SDIO_WAKEUP_SHIFT  19
+#define PMU_CC3_ENABLE_RF_SHIFT           22
+#define PMU_CC3_RF_DISABLE_IVALUE_SHIFT   23
+
+
+/* PMU corerev and chip specific PLL controls.
+ * PMU<rev>_PLL<num>_XX where <rev> is PMU corerev and <num> is an arbitrary number
+ * to differentiate different PLLs controlled by the same PMU rev.
+ */
+/* pllcontrol registers */
+/* PDIV, div_phy, div_arm, div_adc, dith_sel, ioff, kpd_scale, lsb_sel, mash_sel, lf_c & lf_r */
+#define	PMU0_PLL0_PLLCTL0		0
+#define	PMU0_PLL0_PC0_PDIV_MASK		1
+#define	PMU0_PLL0_PC0_PDIV_FREQ		25000
+#define PMU0_PLL0_PC0_DIV_ARM_MASK	0x00000038
+#define PMU0_PLL0_PC0_DIV_ARM_SHIFT	3
+#define PMU0_PLL0_PC0_DIV_ARM_BASE	8
+
+/* PC0_DIV_ARM for PLLOUT_ARM */
+#define PMU0_PLL0_PC0_DIV_ARM_110MHZ	0
+#define PMU0_PLL0_PC0_DIV_ARM_97_7MHZ	1
+#define PMU0_PLL0_PC0_DIV_ARM_88MHZ	2
+#define PMU0_PLL0_PC0_DIV_ARM_80MHZ	3 /* Default */
+#define PMU0_PLL0_PC0_DIV_ARM_73_3MHZ	4
+#define PMU0_PLL0_PC0_DIV_ARM_67_7MHZ	5
+#define PMU0_PLL0_PC0_DIV_ARM_62_9MHZ	6
+#define PMU0_PLL0_PC0_DIV_ARM_58_6MHZ	7
+
+/* Wildcard base, stop_mod, en_lf_tp, en_cal & lf_r2 */
+#define	PMU0_PLL0_PLLCTL1		1
+#define	PMU0_PLL0_PC1_WILD_INT_MASK	0xf0000000
+#define	PMU0_PLL0_PC1_WILD_INT_SHIFT	28
+#define	PMU0_PLL0_PC1_WILD_FRAC_MASK	0x0fffff00
+#define	PMU0_PLL0_PC1_WILD_FRAC_SHIFT	8
+#define	PMU0_PLL0_PC1_STOP_MOD		0x00000040
+
+/* Wildcard base, vco_calvar, vco_swc, vco_var_selref, vso_ical & vco_sel_avdd */
+#define	PMU0_PLL0_PLLCTL2		2
+#define	PMU0_PLL0_PC2_WILD_INT_MASK	0xf
+#define	PMU0_PLL0_PC2_WILD_INT_SHIFT	4
+
+/* pllcontrol registers */
+/* ndiv_pwrdn, pwrdn_ch<x>, refcomp_pwrdn, dly_ch<x>, p1div, p2div, _bypass_sdmod */
+#define PMU1_PLL0_PLLCTL0		0
+#define PMU1_PLL0_PC0_P1DIV_MASK	0x00f00000
+#define PMU1_PLL0_PC0_P1DIV_SHIFT	20
+#define PMU1_PLL0_PC0_P2DIV_MASK	0x0f000000
+#define PMU1_PLL0_PC0_P2DIV_SHIFT	24
+
+/* m<x>div */
+#define PMU1_PLL0_PLLCTL1		1
+#define PMU1_PLL0_PC1_M1DIV_MASK	0x000000ff
+#define PMU1_PLL0_PC1_M1DIV_SHIFT	0
+#define PMU1_PLL0_PC1_M2DIV_MASK	0x0000ff00
+#define PMU1_PLL0_PC1_M2DIV_SHIFT	8
+#define PMU1_PLL0_PC1_M3DIV_MASK	0x00ff0000
+#define PMU1_PLL0_PC1_M3DIV_SHIFT	16
+#define PMU1_PLL0_PC1_M4DIV_MASK	0xff000000
+#define PMU1_PLL0_PC1_M4DIV_SHIFT	24
+#define PMU1_PLL0_PC1_M4DIV_BY_9	9
+#define PMU1_PLL0_PC1_M4DIV_BY_18	0x12
+#define PMU1_PLL0_PC1_M4DIV_BY_36	0x24
+
+#define DOT11MAC_880MHZ_CLK_DIVISOR_SHIFT 8
+#define DOT11MAC_880MHZ_CLK_DIVISOR_MASK (0xFF << DOT11MAC_880MHZ_CLK_DIVISOR_SHIFT)
+#define DOT11MAC_880MHZ_CLK_DIVISOR_VAL  (0xE << DOT11MAC_880MHZ_CLK_DIVISOR_SHIFT)
+
+/* m<x>div, ndiv_dither_mfb, ndiv_mode, ndiv_int */
+#define PMU1_PLL0_PLLCTL2		2
+#define PMU1_PLL0_PC2_M5DIV_MASK	0x000000ff
+#define PMU1_PLL0_PC2_M5DIV_SHIFT	0
+#define PMU1_PLL0_PC2_M5DIV_BY_12	0xc
+#define PMU1_PLL0_PC2_M5DIV_BY_18	0x12
+#define PMU1_PLL0_PC2_M5DIV_BY_36	0x24
+#define PMU1_PLL0_PC2_M6DIV_MASK	0x0000ff00
+#define PMU1_PLL0_PC2_M6DIV_SHIFT	8
+#define PMU1_PLL0_PC2_M6DIV_BY_18	0x12
+#define PMU1_PLL0_PC2_M6DIV_BY_36	0x24
+#define PMU1_PLL0_PC2_NDIV_MODE_MASK	0x000e0000
+#define PMU1_PLL0_PC2_NDIV_MODE_SHIFT	17
+#define PMU1_PLL0_PC2_NDIV_MODE_MASH	1
+#define PMU1_PLL0_PC2_NDIV_MODE_MFB	2	/* recommended for 4319 */
+#define PMU1_PLL0_PC2_NDIV_INT_MASK	0x1ff00000
+#define PMU1_PLL0_PC2_NDIV_INT_SHIFT	20
+
+/* ndiv_frac */
+#define PMU1_PLL0_PLLCTL3		3
+#define PMU1_PLL0_PC3_NDIV_FRAC_MASK	0x00ffffff
+#define PMU1_PLL0_PC3_NDIV_FRAC_SHIFT	0
+
+/* pll_ctrl */
+#define PMU1_PLL0_PLLCTL4		4
+
+/* pll_ctrl, vco_rng, clkdrive_ch<x> */
+#define PMU1_PLL0_PLLCTL5		5
+#define PMU1_PLL0_PC5_CLK_DRV_MASK 0xffffff00
+#define PMU1_PLL0_PC5_CLK_DRV_SHIFT 8
+
+/* PMU rev 2 control words */
+#define PMU2_PHY_PLL_PLLCTL		4
+#define PMU2_SI_PLL_PLLCTL		10
+
+/* PMU rev 2 */
+/* pllcontrol registers */
+/* ndiv_pwrdn, pwrdn_ch<x>, refcomp_pwrdn, dly_ch<x>, p1div, p2div, _bypass_sdmod */
+#define PMU2_PLL_PLLCTL0		0
+#define PMU2_PLL_PC0_P1DIV_MASK 	0x00f00000
+#define PMU2_PLL_PC0_P1DIV_SHIFT	20
+#define PMU2_PLL_PC0_P2DIV_MASK 	0x0f000000
+#define PMU2_PLL_PC0_P2DIV_SHIFT	24
+
+/* m<x>div */
+#define PMU2_PLL_PLLCTL1		1
+#define PMU2_PLL_PC1_M1DIV_MASK 	0x000000ff
+#define PMU2_PLL_PC1_M1DIV_SHIFT	0
+#define PMU2_PLL_PC1_M2DIV_MASK 	0x0000ff00
+#define PMU2_PLL_PC1_M2DIV_SHIFT	8
+#define PMU2_PLL_PC1_M3DIV_MASK 	0x00ff0000
+#define PMU2_PLL_PC1_M3DIV_SHIFT	16
+#define PMU2_PLL_PC1_M4DIV_MASK 	0xff000000
+#define PMU2_PLL_PC1_M4DIV_SHIFT	24
+
+/* m<x>div, ndiv_dither_mfb, ndiv_mode, ndiv_int */
+#define PMU2_PLL_PLLCTL2		2
+#define PMU2_PLL_PC2_M5DIV_MASK 	0x000000ff
+#define PMU2_PLL_PC2_M5DIV_SHIFT	0
+#define PMU2_PLL_PC2_M6DIV_MASK 	0x0000ff00
+#define PMU2_PLL_PC2_M6DIV_SHIFT	8
+#define PMU2_PLL_PC2_NDIV_MODE_MASK	0x000e0000
+#define PMU2_PLL_PC2_NDIV_MODE_SHIFT	17
+#define PMU2_PLL_PC2_NDIV_INT_MASK	0x1ff00000
+#define PMU2_PLL_PC2_NDIV_INT_SHIFT	20
+
+/* ndiv_frac */
+#define PMU2_PLL_PLLCTL3		3
+#define PMU2_PLL_PC3_NDIV_FRAC_MASK	0x00ffffff
+#define PMU2_PLL_PC3_NDIV_FRAC_SHIFT	0
+
+/* pll_ctrl */
+#define PMU2_PLL_PLLCTL4		4
+
+/* pll_ctrl, vco_rng, clkdrive_ch<x> */
+#define PMU2_PLL_PLLCTL5		5
+#define PMU2_PLL_PC5_CLKDRIVE_CH1_MASK	0x00000f00
+#define PMU2_PLL_PC5_CLKDRIVE_CH1_SHIFT	8
+#define PMU2_PLL_PC5_CLKDRIVE_CH2_MASK	0x0000f000
+#define PMU2_PLL_PC5_CLKDRIVE_CH2_SHIFT	12
+#define PMU2_PLL_PC5_CLKDRIVE_CH3_MASK	0x000f0000
+#define PMU2_PLL_PC5_CLKDRIVE_CH3_SHIFT	16
+#define PMU2_PLL_PC5_CLKDRIVE_CH4_MASK	0x00f00000
+#define PMU2_PLL_PC5_CLKDRIVE_CH4_SHIFT	20
+#define PMU2_PLL_PC5_CLKDRIVE_CH5_MASK	0x0f000000
+#define PMU2_PLL_PC5_CLKDRIVE_CH5_SHIFT	24
+#define PMU2_PLL_PC5_CLKDRIVE_CH6_MASK	0xf0000000
+#define PMU2_PLL_PC5_CLKDRIVE_CH6_SHIFT	28
+
+/* PMU rev 5 (& 6) */
+#define	PMU5_PLL_P1P2_OFF		0
+#define	PMU5_PLL_P1_MASK		0x0f000000
+#define	PMU5_PLL_P1_SHIFT		24
+#define	PMU5_PLL_P2_MASK		0x00f00000
+#define	PMU5_PLL_P2_SHIFT		20
+#define	PMU5_PLL_M14_OFF		1
+#define	PMU5_PLL_MDIV_MASK		0x000000ff
+#define	PMU5_PLL_MDIV_WIDTH		8
+#define	PMU5_PLL_NM5_OFF		2
+#define	PMU5_PLL_NDIV_MASK		0xfff00000
+#define	PMU5_PLL_NDIV_SHIFT		20
+#define	PMU5_PLL_NDIV_MODE_MASK		0x000e0000
+#define	PMU5_PLL_NDIV_MODE_SHIFT	17
+#define	PMU5_PLL_FMAB_OFF		3
+#define	PMU5_PLL_MRAT_MASK		0xf0000000
+#define	PMU5_PLL_MRAT_SHIFT		28
+#define	PMU5_PLL_ABRAT_MASK		0x08000000
+#define	PMU5_PLL_ABRAT_SHIFT		27
+#define	PMU5_PLL_FDIV_MASK		0x07ffffff
+#define	PMU5_PLL_PLLCTL_OFF		4
+#define	PMU5_PLL_PCHI_OFF		5
+#define	PMU5_PLL_PCHI_MASK		0x0000003f
+
+/* pmu XtalFreqRatio */
+#define	PMU_XTALFREQ_REG_ILPCTR_MASK	0x00001FFF
+#define	PMU_XTALFREQ_REG_MEASURE_MASK	0x80000000
+#define	PMU_XTALFREQ_REG_MEASURE_SHIFT	31
+
+/* Divider allocation in 4716/47162/5356/5357 */
+#define	PMU5_MAINPLL_CPU		1
+#define	PMU5_MAINPLL_MEM		2
+#define	PMU5_MAINPLL_SI			3
+
+/* 4706 PMU */
+#define PMU4706_MAINPLL_PLL0	0
+#define PMU6_4706_PROCPLL_OFF	4	/* The CPU PLL */
+#define PMU6_4706_PROC_P2DIV_MASK		0x000f0000
+#define PMU6_4706_PROC_P2DIV_SHIFT	16
+#define PMU6_4706_PROC_P1DIV_MASK		0x0000f000
+#define PMU6_4706_PROC_P1DIV_SHIFT	12
+#define PMU6_4706_PROC_NDIV_INT_MASK	0x00000ff8
+#define PMU6_4706_PROC_NDIV_INT_SHIFT	3
+#define PMU6_4706_PROC_NDIV_MODE_MASK		0x00000007
+#define PMU6_4706_PROC_NDIV_MODE_SHIFT	0
+
+#define PMU7_PLL_PLLCTL7                7
+#define PMU7_PLL_CTL7_M4DIV_MASK	0xff000000
+#define PMU7_PLL_CTL7_M4DIV_SHIFT 	24
+#define PMU7_PLL_CTL7_M4DIV_BY_6	6
+#define PMU7_PLL_CTL7_M4DIV_BY_12	0xc
+#define PMU7_PLL_CTL7_M4DIV_BY_24	0x18
+#define PMU7_PLL_PLLCTL8                8
+#define PMU7_PLL_CTL8_M5DIV_MASK	0x000000ff
+#define PMU7_PLL_CTL8_M5DIV_SHIFT	0
+#define PMU7_PLL_CTL8_M5DIV_BY_8	8
+#define PMU7_PLL_CTL8_M5DIV_BY_12	0xc
+#define PMU7_PLL_CTL8_M5DIV_BY_24	0x18
+#define PMU7_PLL_CTL8_M6DIV_MASK	0x0000ff00
+#define PMU7_PLL_CTL8_M6DIV_SHIFT	8
+#define PMU7_PLL_CTL8_M6DIV_BY_12	0xc
+#define PMU7_PLL_CTL8_M6DIV_BY_24	0x18
+#define PMU7_PLL_PLLCTL11		11
+#define PMU7_PLL_PLLCTL11_MASK		0xffffff00
+#define PMU7_PLL_PLLCTL11_VAL		0x22222200
+
+/* PMU rev 15 */
+#define PMU15_PLL_PLLCTL0		0
+#define PMU15_PLL_PC0_CLKSEL_MASK	0x00000003
+#define PMU15_PLL_PC0_CLKSEL_SHIFT	0
+#define PMU15_PLL_PC0_FREQTGT_MASK	0x003FFFFC
+#define PMU15_PLL_PC0_FREQTGT_SHIFT	2
+#define PMU15_PLL_PC0_PRESCALE_MASK	0x00C00000
+#define PMU15_PLL_PC0_PRESCALE_SHIFT	22
+#define PMU15_PLL_PC0_KPCTRL_MASK	0x07000000
+#define PMU15_PLL_PC0_KPCTRL_SHIFT	24
+#define PMU15_PLL_PC0_FCNTCTRL_MASK	0x38000000
+#define PMU15_PLL_PC0_FCNTCTRL_SHIFT	27
+#define PMU15_PLL_PC0_FDCMODE_MASK	0x40000000
+#define PMU15_PLL_PC0_FDCMODE_SHIFT	30
+#define PMU15_PLL_PC0_CTRLBIAS_MASK	0x80000000
+#define PMU15_PLL_PC0_CTRLBIAS_SHIFT	31
+
+#define PMU15_PLL_PLLCTL1			1
+#define PMU15_PLL_PC1_BIAS_CTLM_MASK		0x00000060
+#define PMU15_PLL_PC1_BIAS_CTLM_SHIFT		5
+#define PMU15_PLL_PC1_BIAS_CTLM_RST_MASK	0x00000040
+#define PMU15_PLL_PC1_BIAS_CTLM_RST_SHIFT	6
+#define PMU15_PLL_PC1_BIAS_SS_DIVR_MASK		0x0001FF80
+#define PMU15_PLL_PC1_BIAS_SS_DIVR_SHIFT	7
+#define PMU15_PLL_PC1_BIAS_SS_RSTVAL_MASK	0x03FE0000
+#define PMU15_PLL_PC1_BIAS_SS_RSTVAL_SHIFT	17
+#define PMU15_PLL_PC1_BIAS_INTG_BW_MASK		0x0C000000
+#define PMU15_PLL_PC1_BIAS_INTG_BW_SHIFT	26
+#define PMU15_PLL_PC1_BIAS_INTG_BYP_MASK	0x10000000
+#define PMU15_PLL_PC1_BIAS_INTG_BYP_SHIFT	28
+#define PMU15_PLL_PC1_OPENLP_EN_MASK		0x40000000
+#define PMU15_PLL_PC1_OPENLP_EN_SHIFT		30
+
+#define PMU15_PLL_PLLCTL2			2
+#define PMU15_PLL_PC2_CTEN_MASK			0x00000001
+#define PMU15_PLL_PC2_CTEN_SHIFT		0
+
+#define PMU15_PLL_PLLCTL3			3
+#define PMU15_PLL_PC3_DITHER_EN_MASK		0x00000001
+#define PMU15_PLL_PC3_DITHER_EN_SHIFT		0
+#define PMU15_PLL_PC3_DCOCTLSP_MASK		0xFE000000
+#define PMU15_PLL_PC3_DCOCTLSP_SHIFT		25
+#define PMU15_PLL_PC3_DCOCTLSP_DIV2EN_MASK	0x01
+#define PMU15_PLL_PC3_DCOCTLSP_DIV2EN_SHIFT	0
+#define PMU15_PLL_PC3_DCOCTLSP_CH0EN_MASK	0x02
+#define PMU15_PLL_PC3_DCOCTLSP_CH0EN_SHIFT	1
+#define PMU15_PLL_PC3_DCOCTLSP_CH1EN_MASK	0x04
+#define PMU15_PLL_PC3_DCOCTLSP_CH1EN_SHIFT	2
+#define PMU15_PLL_PC3_DCOCTLSP_CH0SEL_MASK	0x18
+#define PMU15_PLL_PC3_DCOCTLSP_CH0SEL_SHIFT	3
+#define PMU15_PLL_PC3_DCOCTLSP_CH1SEL_MASK	0x60
+#define PMU15_PLL_PC3_DCOCTLSP_CH1SEL_SHIFT	5
+#define PMU15_PLL_PC3_DCOCTLSP_CHSEL_OUTP_DIV1	0
+#define PMU15_PLL_PC3_DCOCTLSP_CHSEL_OUTP_DIV2	1
+#define PMU15_PLL_PC3_DCOCTLSP_CHSEL_OUTP_DIV3	2
+#define PMU15_PLL_PC3_DCOCTLSP_CHSEL_OUTP_DIV5	3
+
+#define PMU15_PLL_PLLCTL4			4
+#define PMU15_PLL_PC4_FLLCLK1_DIV_MASK		0x00000007
+#define PMU15_PLL_PC4_FLLCLK1_DIV_SHIFT		0
+#define PMU15_PLL_PC4_FLLCLK2_DIV_MASK		0x00000038
+#define PMU15_PLL_PC4_FLLCLK2_DIV_SHIFT		3
+#define PMU15_PLL_PC4_FLLCLK3_DIV_MASK		0x000001C0
+#define PMU15_PLL_PC4_FLLCLK3_DIV_SHIFT		6
+#define PMU15_PLL_PC4_DBGMODE_MASK		0x00000E00
+#define PMU15_PLL_PC4_DBGMODE_SHIFT		9
+#define PMU15_PLL_PC4_FLL480_CTLSP_LK_MASK	0x00001000
+#define PMU15_PLL_PC4_FLL480_CTLSP_LK_SHIFT	12
+#define PMU15_PLL_PC4_FLL480_CTLSP_MASK		0x000FE000
+#define PMU15_PLL_PC4_FLL480_CTLSP_SHIFT	13
+#define PMU15_PLL_PC4_DINPOL_MASK		0x00100000
+#define PMU15_PLL_PC4_DINPOL_SHIFT		20
+#define PMU15_PLL_PC4_CLKOUT_PD_MASK		0x00200000
+#define PMU15_PLL_PC4_CLKOUT_PD_SHIFT		21
+#define PMU15_PLL_PC4_CLKDIV2_PD_MASK		0x00400000
+#define PMU15_PLL_PC4_CLKDIV2_PD_SHIFT		22
+#define PMU15_PLL_PC4_CLKDIV4_PD_MASK		0x00800000
+#define PMU15_PLL_PC4_CLKDIV4_PD_SHIFT		23
+#define PMU15_PLL_PC4_CLKDIV8_PD_MASK		0x01000000
+#define PMU15_PLL_PC4_CLKDIV8_PD_SHIFT		24
+#define PMU15_PLL_PC4_CLKDIV16_PD_MASK		0x02000000
+#define PMU15_PLL_PC4_CLKDIV16_PD_SHIFT		25
+#define PMU15_PLL_PC4_TEST_EN_MASK		0x04000000
+#define PMU15_PLL_PC4_TEST_EN_SHIFT		26
+
+#define PMU15_PLL_PLLCTL5			5
+#define PMU15_PLL_PC5_FREQTGT_MASK		0x000FFFFF
+#define PMU15_PLL_PC5_FREQTGT_SHIFT		0
+#define PMU15_PLL_PC5_DCOCTLSP_MASK		0x07F00000
+#define PMU15_PLL_PC5_DCOCTLSP_SHIFT		20
+#define PMU15_PLL_PC5_PRESCALE_MASK		0x18000000
+#define PMU15_PLL_PC5_PRESCALE_SHIFT		27
+
+#define PMU15_PLL_PLLCTL6		6
+#define PMU15_PLL_PC6_FREQTGT_MASK	0x000FFFFF
+#define PMU15_PLL_PC6_FREQTGT_SHIFT	0
+#define PMU15_PLL_PC6_DCOCTLSP_MASK	0x07F00000
+#define PMU15_PLL_PC6_DCOCTLSP_SHIFT	20
+#define PMU15_PLL_PC6_PRESCALE_MASK	0x18000000
+#define PMU15_PLL_PC6_PRESCALE_SHIFT	27
+
+#define PMU15_FREQTGT_480_DEFAULT	0x19AB1
+#define PMU15_FREQTGT_492_DEFAULT	0x1A4F5
+#define PMU15_ARM_96MHZ			96000000	/* 96 Mhz */
+#define PMU15_ARM_98MHZ			98400000	/* 98.4 Mhz */
+#define PMU15_ARM_97MHZ			97000000	/* 97 Mhz */
+
+
+#define PMU17_PLLCTL2_NDIVTYPE_MASK		0x00000070
+#define PMU17_PLLCTL2_NDIVTYPE_SHIFT		4
+
+#define PMU17_PLLCTL2_NDIV_MODE_INT		0
+#define PMU17_PLLCTL2_NDIV_MODE_INT1B8		1
+#define PMU17_PLLCTL2_NDIV_MODE_MASH111		2
+#define PMU17_PLLCTL2_NDIV_MODE_MASH111B8	3
+
+#define PMU17_PLLCTL0_BBPLL_PWRDWN		0
+#define PMU17_PLLCTL0_BBPLL_DRST		3
+#define PMU17_PLLCTL0_BBPLL_DISBL_CLK		8
+
+/* PLL usage in 4716/47162 */
+#define	PMU4716_MAINPLL_PLL0		12
+
+/* PLL usage in 5356/5357 */
+#define	PMU5356_MAINPLL_PLL0		0
+#define	PMU5357_MAINPLL_PLL0		0
+
+/* 4716/47162 resources */
+#define RES4716_PROC_PLL_ON		0x00000040
+#define RES4716_PROC_HT_AVAIL		0x00000080
+
+/* 4716/4717/4718 Chip specific ChipControl register bits */
+#define CCTRL_471X_I2S_PINS_ENABLE	0x0080 /* I2S pins off by default, shared w/ pflash */
+
+/* 5357 Chip specific ChipControl register bits */
+/* 2nd - 32-bit reg */
+#define CCTRL_5357_I2S_PINS_ENABLE	0x00040000 /* I2S pins enable */
+#define CCTRL_5357_I2CSPI_PINS_ENABLE	0x00080000 /* I2C/SPI pins enable */
+
+/* 5354 resources */
+#define RES5354_EXT_SWITCHER_PWM	0	/* 0x00001 */
+#define RES5354_BB_SWITCHER_PWM		1	/* 0x00002 */
+#define RES5354_BB_SWITCHER_BURST	2	/* 0x00004 */
+#define RES5354_BB_EXT_SWITCHER_BURST	3	/* 0x00008 */
+#define RES5354_ILP_REQUEST		4	/* 0x00010 */
+#define RES5354_RADIO_SWITCHER_PWM	5	/* 0x00020 */
+#define RES5354_RADIO_SWITCHER_BURST	6	/* 0x00040 */
+#define RES5354_ROM_SWITCH		7	/* 0x00080 */
+#define RES5354_PA_REF_LDO		8	/* 0x00100 */
+#define RES5354_RADIO_LDO		9	/* 0x00200 */
+#define RES5354_AFE_LDO			10	/* 0x00400 */
+#define RES5354_PLL_LDO			11	/* 0x00800 */
+#define RES5354_BG_FILTBYP		12	/* 0x01000 */
+#define RES5354_TX_FILTBYP		13	/* 0x02000 */
+#define RES5354_RX_FILTBYP		14	/* 0x04000 */
+#define RES5354_XTAL_PU			15	/* 0x08000 */
+#define RES5354_XTAL_EN			16	/* 0x10000 */
+#define RES5354_BB_PLL_FILTBYP		17	/* 0x20000 */
+#define RES5354_RF_PLL_FILTBYP		18	/* 0x40000 */
+#define RES5354_BB_PLL_PU		19	/* 0x80000 */
+
+/* 5357 Chip specific ChipControl register bits */
+#define CCTRL5357_EXTPA                 (1<<14) /* extPA in ChipControl 1, bit 14 */
+#define CCTRL5357_ANT_MUX_2o3		(1<<15) /* 2o3 in ChipControl 1, bit 15 */
+#define CCTRL5357_NFLASH		(1<<16) /* Nandflash in ChipControl 1, bit 16 */
+
+/* 4328 resources */
+#define RES4328_EXT_SWITCHER_PWM	0	/* 0x00001 */
+#define RES4328_BB_SWITCHER_PWM		1	/* 0x00002 */
+#define RES4328_BB_SWITCHER_BURST	2	/* 0x00004 */
+#define RES4328_BB_EXT_SWITCHER_BURST	3	/* 0x00008 */
+#define RES4328_ILP_REQUEST		4	/* 0x00010 */
+#define RES4328_RADIO_SWITCHER_PWM	5	/* 0x00020 */
+#define RES4328_RADIO_SWITCHER_BURST	6	/* 0x00040 */
+#define RES4328_ROM_SWITCH		7	/* 0x00080 */
+#define RES4328_PA_REF_LDO		8	/* 0x00100 */
+#define RES4328_RADIO_LDO		9	/* 0x00200 */
+#define RES4328_AFE_LDO			10	/* 0x00400 */
+#define RES4328_PLL_LDO			11	/* 0x00800 */
+#define RES4328_BG_FILTBYP		12	/* 0x01000 */
+#define RES4328_TX_FILTBYP		13	/* 0x02000 */
+#define RES4328_RX_FILTBYP		14	/* 0x04000 */
+#define RES4328_XTAL_PU			15	/* 0x08000 */
+#define RES4328_XTAL_EN			16	/* 0x10000 */
+#define RES4328_BB_PLL_FILTBYP		17	/* 0x20000 */
+#define RES4328_RF_PLL_FILTBYP		18	/* 0x40000 */
+#define RES4328_BB_PLL_PU		19	/* 0x80000 */
+
+/* 4325 A0/A1 resources */
+#define RES4325_BUCK_BOOST_BURST	0	/* 0x00000001 */
+#define RES4325_CBUCK_BURST		1	/* 0x00000002 */
+#define RES4325_CBUCK_PWM		2	/* 0x00000004 */
+#define RES4325_CLDO_CBUCK_BURST	3	/* 0x00000008 */
+#define RES4325_CLDO_CBUCK_PWM		4	/* 0x00000010 */
+#define RES4325_BUCK_BOOST_PWM		5	/* 0x00000020 */
+#define RES4325_ILP_REQUEST		6	/* 0x00000040 */
+#define RES4325_ABUCK_BURST		7	/* 0x00000080 */
+#define RES4325_ABUCK_PWM		8	/* 0x00000100 */
+#define RES4325_LNLDO1_PU		9	/* 0x00000200 */
+#define RES4325_OTP_PU			10	/* 0x00000400 */
+#define RES4325_LNLDO3_PU		11	/* 0x00000800 */
+#define RES4325_LNLDO4_PU		12	/* 0x00001000 */
+#define RES4325_XTAL_PU			13	/* 0x00002000 */
+#define RES4325_ALP_AVAIL		14	/* 0x00004000 */
+#define RES4325_RX_PWRSW_PU		15	/* 0x00008000 */
+#define RES4325_TX_PWRSW_PU		16	/* 0x00010000 */
+#define RES4325_RFPLL_PWRSW_PU		17	/* 0x00020000 */
+#define RES4325_LOGEN_PWRSW_PU		18	/* 0x00040000 */
+#define RES4325_AFE_PWRSW_PU		19	/* 0x00080000 */
+#define RES4325_BBPLL_PWRSW_PU		20	/* 0x00100000 */
+#define RES4325_HT_AVAIL		21	/* 0x00200000 */
+
+/* 4325 B0/C0 resources */
+#define RES4325B0_CBUCK_LPOM		1	/* 0x00000002 */
+#define RES4325B0_CBUCK_BURST		2	/* 0x00000004 */
+#define RES4325B0_CBUCK_PWM		3	/* 0x00000008 */
+#define RES4325B0_CLDO_PU		4	/* 0x00000010 */
+
+/* 4325 C1 resources */
+#define RES4325C1_LNLDO2_PU		12	/* 0x00001000 */
+
+/* 4325 chip-specific ChipStatus register bits */
+#define CST4325_SPROM_OTP_SEL_MASK	0x00000003
+#define CST4325_DEFCIS_SEL		0	/* OTP is powered up, use def. CIS, no SPROM */
+#define CST4325_SPROM_SEL		1	/* OTP is powered up, SPROM is present */
+#define CST4325_OTP_SEL			2	/* OTP is powered up, no SPROM */
+#define CST4325_OTP_PWRDN		3	/* OTP is powered down, SPROM is present */
+#define CST4325_SDIO_USB_MODE_MASK	0x00000004
+#define CST4325_SDIO_USB_MODE_SHIFT	2
+#define CST4325_RCAL_VALID_MASK		0x00000008
+#define CST4325_RCAL_VALID_SHIFT	3
+#define CST4325_RCAL_VALUE_MASK		0x000001f0
+#define CST4325_RCAL_VALUE_SHIFT	4
+#define CST4325_PMUTOP_2B_MASK 		0x00000200	/* 1 for 2b, 0 for to 2a */
+#define CST4325_PMUTOP_2B_SHIFT   	9
+
+#define RES4329_RESERVED0		0	/* 0x00000001 */
+#define RES4329_CBUCK_LPOM		1	/* 0x00000002 */
+#define RES4329_CBUCK_BURST		2	/* 0x00000004 */
+#define RES4329_CBUCK_PWM		3	/* 0x00000008 */
+#define RES4329_CLDO_PU			4	/* 0x00000010 */
+#define RES4329_PALDO_PU		5	/* 0x00000020 */
+#define RES4329_ILP_REQUEST		6	/* 0x00000040 */
+#define RES4329_RESERVED7		7	/* 0x00000080 */
+#define RES4329_RESERVED8		8	/* 0x00000100 */
+#define RES4329_LNLDO1_PU		9	/* 0x00000200 */
+#define RES4329_OTP_PU			10	/* 0x00000400 */
+#define RES4329_RESERVED11		11	/* 0x00000800 */
+#define RES4329_LNLDO2_PU		12	/* 0x00001000 */
+#define RES4329_XTAL_PU			13	/* 0x00002000 */
+#define RES4329_ALP_AVAIL		14	/* 0x00004000 */
+#define RES4329_RX_PWRSW_PU		15	/* 0x00008000 */
+#define RES4329_TX_PWRSW_PU		16	/* 0x00010000 */
+#define RES4329_RFPLL_PWRSW_PU		17	/* 0x00020000 */
+#define RES4329_LOGEN_PWRSW_PU		18	/* 0x00040000 */
+#define RES4329_AFE_PWRSW_PU		19	/* 0x00080000 */
+#define RES4329_BBPLL_PWRSW_PU		20	/* 0x00100000 */
+#define RES4329_HT_AVAIL		21	/* 0x00200000 */
+
+#define CST4329_SPROM_OTP_SEL_MASK	0x00000003
+#define CST4329_DEFCIS_SEL		0	/* OTP is powered up, use def. CIS, no SPROM */
+#define CST4329_SPROM_SEL		1	/* OTP is powered up, SPROM is present */
+#define CST4329_OTP_SEL			2	/* OTP is powered up, no SPROM */
+#define CST4329_OTP_PWRDN		3	/* OTP is powered down, SPROM is present */
+#define CST4329_SPI_SDIO_MODE_MASK	0x00000004
+#define CST4329_SPI_SDIO_MODE_SHIFT	2
+
+/* 4312 chip-specific ChipStatus register bits */
+#define CST4312_SPROM_OTP_SEL_MASK	0x00000003
+#define CST4312_DEFCIS_SEL		0	/* OTP is powered up, use def. CIS, no SPROM */
+#define CST4312_SPROM_SEL		1	/* OTP is powered up, SPROM is present */
+#define CST4312_OTP_SEL			2	/* OTP is powered up, no SPROM */
+#define CST4312_OTP_BAD			3	/* OTP is broken, SPROM is present */
+
+/* 4312 resources (all PMU chips with little memory constraint) */
+#define RES4312_SWITCHER_BURST		0	/* 0x00000001 */
+#define RES4312_SWITCHER_PWM    	1	/* 0x00000002 */
+#define RES4312_PA_REF_LDO		2	/* 0x00000004 */
+#define RES4312_CORE_LDO_BURST		3	/* 0x00000008 */
+#define RES4312_CORE_LDO_PWM		4	/* 0x00000010 */
+#define RES4312_RADIO_LDO		5	/* 0x00000020 */
+#define RES4312_ILP_REQUEST		6	/* 0x00000040 */
+#define RES4312_BG_FILTBYP		7	/* 0x00000080 */
+#define RES4312_TX_FILTBYP		8	/* 0x00000100 */
+#define RES4312_RX_FILTBYP		9	/* 0x00000200 */
+#define RES4312_XTAL_PU			10	/* 0x00000400 */
+#define RES4312_ALP_AVAIL		11	/* 0x00000800 */
+#define RES4312_BB_PLL_FILTBYP		12	/* 0x00001000 */
+#define RES4312_RF_PLL_FILTBYP		13	/* 0x00002000 */
+#define RES4312_HT_AVAIL		14	/* 0x00004000 */
+
+/* 4322 resources */
+#define RES4322_RF_LDO			0
+#define RES4322_ILP_REQUEST		1
+#define RES4322_XTAL_PU			2
+#define RES4322_ALP_AVAIL		3
+#define RES4322_SI_PLL_ON		4
+#define RES4322_HT_SI_AVAIL		5
+#define RES4322_PHY_PLL_ON		6
+#define RES4322_HT_PHY_AVAIL		7
+#define RES4322_OTP_PU			8
+
+/* 4322 chip-specific ChipStatus register bits */
+#define CST4322_XTAL_FREQ_20_40MHZ	0x00000020
+#define CST4322_SPROM_OTP_SEL_MASK	0x000000c0
+#define CST4322_SPROM_OTP_SEL_SHIFT	6
+#define CST4322_NO_SPROM_OTP		0	/* no OTP, no SPROM */
+#define CST4322_SPROM_PRESENT		1	/* SPROM is present */
+#define CST4322_OTP_PRESENT		2	/* OTP is present */
+#define CST4322_PCI_OR_USB		0x00000100
+#define CST4322_BOOT_MASK		0x00000600
+#define CST4322_BOOT_SHIFT		9
+#define CST4322_BOOT_FROM_SRAM		0	/* boot from SRAM, ARM in reset */
+#define CST4322_BOOT_FROM_ROM		1	/* boot from ROM */
+#define CST4322_BOOT_FROM_FLASH		2	/* boot from FLASH */
+#define CST4322_BOOT_FROM_INVALID	3
+#define CST4322_ILP_DIV_EN		0x00000800
+#define CST4322_FLASH_TYPE_MASK		0x00001000
+#define CST4322_FLASH_TYPE_SHIFT	12
+#define CST4322_FLASH_TYPE_SHIFT_ST	0	/* ST serial FLASH */
+#define CST4322_FLASH_TYPE_SHIFT_ATMEL	1	/* ATMEL flash */
+#define CST4322_ARM_TAP_SEL		0x00002000
+#define CST4322_RES_INIT_MODE_MASK	0x0000c000
+#define CST4322_RES_INIT_MODE_SHIFT	14
+#define CST4322_RES_INIT_MODE_ILPAVAIL	0	/* resinitmode: ILP available */
+#define CST4322_RES_INIT_MODE_ILPREQ	1	/* resinitmode: ILP request */
+#define CST4322_RES_INIT_MODE_ALPAVAIL	2	/* resinitmode: ALP available */
+#define CST4322_RES_INIT_MODE_HTAVAIL	3	/* resinitmode: HT available */
+#define CST4322_PCIPLLCLK_GATING	0x00010000
+#define CST4322_CLK_SWITCH_PCI_TO_ALP	0x00020000
+#define CST4322_PCI_CARDBUS_MODE	0x00040000
+
+/* 43224 chip-specific ChipControl register bits */
+#define CCTRL43224_GPIO_TOGGLE          0x8000 /* gpio[3:0] pins as btcoex or s/w gpio */
+#define CCTRL_43224A0_12MA_LED_DRIVE    0x00F000F0 /* 12 mA drive strength */
+#define CCTRL_43224B0_12MA_LED_DRIVE    0xF0    /* 12 mA drive strength for later 43224s */
+
+/* 43236 resources */
+#define RES43236_REGULATOR		0
+#define RES43236_ILP_REQUEST		1
+#define RES43236_XTAL_PU		2
+#define RES43236_ALP_AVAIL		3
+#define RES43236_SI_PLL_ON		4
+#define RES43236_HT_SI_AVAIL		5
+
+/* 43236 chip-specific ChipControl register bits */
+#define CCTRL43236_BT_COEXIST		(1<<0)	/* 0 disable */
+#define CCTRL43236_SECI			(1<<1)	/* 0 SECI is disabled (JATG functional) */
+#define CCTRL43236_EXT_LNA		(1<<2)	/* 0 disable */
+#define CCTRL43236_ANT_MUX_2o3          (1<<3)	/* 2o3 mux, chipcontrol bit 3 */
+#define CCTRL43236_GSIO			(1<<4)	/* 0 disable */
+
+/* 43236 Chip specific ChipStatus register bits */
+#define CST43236_SFLASH_MASK		0x00000040
+#define CST43236_OTP_SEL_MASK		0x00000080
+#define CST43236_OTP_SEL_SHIFT		7
+#define CST43236_HSIC_MASK		0x00000100	/* USB/HSIC */
+#define CST43236_BP_CLK			0x00000200	/* 120/96Mbps */
+#define CST43236_BOOT_MASK		0x00001800
+#define CST43236_BOOT_SHIFT		11
+#define CST43236_BOOT_FROM_SRAM		0	/* boot from SRAM, ARM in reset */
+#define CST43236_BOOT_FROM_ROM		1	/* boot from ROM */
+#define CST43236_BOOT_FROM_FLASH	2	/* boot from FLASH */
+#define CST43236_BOOT_FROM_INVALID	3
+
+/* 43237 resources */
+#define RES43237_REGULATOR		0
+#define RES43237_ILP_REQUEST		1
+#define RES43237_XTAL_PU		2
+#define RES43237_ALP_AVAIL		3
+#define RES43237_SI_PLL_ON		4
+#define RES43237_HT_SI_AVAIL		5
+
+/* 43237 chip-specific ChipControl register bits */
+#define CCTRL43237_BT_COEXIST		(1<<0)	/* 0 disable */
+#define CCTRL43237_SECI			(1<<1)	/* 0 SECI is disabled (JATG functional) */
+#define CCTRL43237_EXT_LNA		(1<<2)	/* 0 disable */
+#define CCTRL43237_ANT_MUX_2o3          (1<<3)	/* 2o3 mux, chipcontrol bit 3 */
+#define CCTRL43237_GSIO			(1<<4)	/* 0 disable */
+
+/* 43237 Chip specific ChipStatus register bits */
+#define CST43237_SFLASH_MASK		0x00000040
+#define CST43237_OTP_SEL_MASK		0x00000080
+#define CST43237_OTP_SEL_SHIFT		7
+#define CST43237_HSIC_MASK		0x00000100	/* USB/HSIC */
+#define CST43237_BP_CLK			0x00000200	/* 120/96Mbps */
+#define CST43237_BOOT_MASK		0x00001800
+#define CST43237_BOOT_SHIFT		11
+#define CST43237_BOOT_FROM_SRAM		0	/* boot from SRAM, ARM in reset */
+#define CST43237_BOOT_FROM_ROM		1	/* boot from ROM */
+#define CST43237_BOOT_FROM_FLASH	2	/* boot from FLASH */
+#define CST43237_BOOT_FROM_INVALID	3
+
+/* 43239 resources */
+#define RES43239_OTP_PU			9
+#define RES43239_MACPHY_CLKAVAIL	23
+#define RES43239_HT_AVAIL		24
+
+/* 43239 Chip specific ChipStatus register bits */
+#define CST43239_SPROM_MASK			0x00000002
+#define CST43239_SFLASH_MASK		0x00000004
+#define	CST43239_RES_INIT_MODE_SHIFT	7
+#define	CST43239_RES_INIT_MODE_MASK		0x000001f0
+#define CST43239_CHIPMODE_SDIOD(cs)	((cs) & (1 << 15))	/* SDIO || gSPI */
+#define CST43239_CHIPMODE_USB20D(cs)	(~(cs) & (1 << 15))	/* USB || USBDA */
+#define CST43239_CHIPMODE_SDIO(cs)	(((cs) & (1 << 0)) == 0)	/* SDIO */
+#define CST43239_CHIPMODE_GSPI(cs)	(((cs) & (1 << 0)) == (1 << 0))	/* gSPI */
+
+/* 4324 resources */
+#define RES4324_OTP_PU				10
+#define RES4324_HT_AVAIL			29
+#define RES4324_MACPHY_CLKAVAIL		30
+
+/* 4324 Chip specific ChipStatus register bits */
+#define CST4324_SPROM_MASK			0x00000080
+#define CST4324_SFLASH_MASK			0x00400000
+#define	CST4324_RES_INIT_MODE_SHIFT	10
+#define	CST4324_RES_INIT_MODE_MASK	0x00000c00
+#define CST4324_CHIPMODE_MASK		0x7
+#define CST4324_CHIPMODE_SDIOD(cs)	((~(cs)) & (1 << 2))	/* SDIO || gSPI */
+#define CST4324_CHIPMODE_USB20D(cs)	(((cs) & CST4324_CHIPMODE_MASK) == 0x6)	/* USB || USBDA */
+
+/* 4331 resources */
+#define RES4331_REGULATOR		0
+#define RES4331_ILP_REQUEST		1
+#define RES4331_XTAL_PU			2
+#define RES4331_ALP_AVAIL		3
+#define RES4331_SI_PLL_ON		4
+#define RES4331_HT_SI_AVAIL		5
+
+/* 4331 chip-specific ChipControl register bits */
+#define CCTRL4331_BT_COEXIST		(1<<0)	/* 0 disable */
+#define CCTRL4331_SECI			(1<<1)	/* 0 SECI is disabled (JATG functional) */
+#define CCTRL4331_EXT_LNA_G		(1<<2)	/* 0 disable */
+#define CCTRL4331_SPROM_GPIO13_15       (1<<3)  /* sprom/gpio13-15 mux */
+#define CCTRL4331_EXTPA_EN		(1<<4)	/* 0 ext pa disable, 1 ext pa enabled */
+#define CCTRL4331_GPIOCLK_ON_SPROMCS	(1<<5)	/* set drive out GPIO_CLK on sprom_cs pin */
+#define CCTRL4331_PCIE_MDIO_ON_SPROMCS	(1<<6)	/* use sprom_cs pin as PCIE mdio interface */
+#define CCTRL4331_EXTPA_ON_GPIO2_5	(1<<7)	/* aband extpa will be at gpio2/5 and sprom_dout */
+#define CCTRL4331_OVR_PIPEAUXCLKEN	(1<<8)	/* override core control on pipe_AuxClkEnable */
+#define CCTRL4331_OVR_PIPEAUXPWRDOWN	(1<<9)	/* override core control on pipe_AuxPowerDown */
+#define CCTRL4331_PCIE_AUXCLKEN		(1<<10)	/* pcie_auxclkenable */
+#define CCTRL4331_PCIE_PIPE_PLLDOWN	(1<<11)	/* pcie_pipe_pllpowerdown */
+#define CCTRL4331_EXTPA_EN2		(1<<12)	/* 0 ext pa disable, 1 ext pa enabled */
+#define CCTRL4331_EXT_LNA_A		(1<<13)	/* 0 disable */
+#define CCTRL4331_BT_SHD0_ON_GPIO4	(1<<16)	/* enable bt_shd0 at gpio4 */
+#define CCTRL4331_BT_SHD1_ON_GPIO5	(1<<17)	/* enable bt_shd1 at gpio5 */
+#define CCTRL4331_EXTPA_ANA_EN		(1<<24)	/* 0 ext pa disable, 1 ext pa enabled */
+
+/* 4331 Chip specific ChipStatus register bits */
+#define	CST4331_XTAL_FREQ		0x00000001	/* crystal frequency 20/40Mhz */
+#define	CST4331_SPROM_OTP_SEL_MASK	0x00000006
+#define	CST4331_SPROM_OTP_SEL_SHIFT	1
+#define	CST4331_SPROM_PRESENT		0x00000002
+#define	CST4331_OTP_PRESENT		0x00000004
+#define	CST4331_LDO_RF			0x00000008
+#define	CST4331_LDO_PAR			0x00000010
+
+/* 4315 resource */
+#define RES4315_CBUCK_LPOM		1	/* 0x00000002 */
+#define RES4315_CBUCK_BURST		2	/* 0x00000004 */
+#define RES4315_CBUCK_PWM		3	/* 0x00000008 */
+#define RES4315_CLDO_PU			4	/* 0x00000010 */
+#define RES4315_PALDO_PU		5	/* 0x00000020 */
+#define RES4315_ILP_REQUEST		6	/* 0x00000040 */
+#define RES4315_LNLDO1_PU		9	/* 0x00000200 */
+#define RES4315_OTP_PU			10	/* 0x00000400 */
+#define RES4315_LNLDO2_PU		12	/* 0x00001000 */
+#define RES4315_XTAL_PU			13	/* 0x00002000 */
+#define RES4315_ALP_AVAIL		14	/* 0x00004000 */
+#define RES4315_RX_PWRSW_PU		15	/* 0x00008000 */
+#define RES4315_TX_PWRSW_PU		16	/* 0x00010000 */
+#define RES4315_RFPLL_PWRSW_PU		17	/* 0x00020000 */
+#define RES4315_LOGEN_PWRSW_PU		18	/* 0x00040000 */
+#define RES4315_AFE_PWRSW_PU		19	/* 0x00080000 */
+#define RES4315_BBPLL_PWRSW_PU		20	/* 0x00100000 */
+#define RES4315_HT_AVAIL		21	/* 0x00200000 */
+
+/* 4315 chip-specific ChipStatus register bits */
+#define CST4315_SPROM_OTP_SEL_MASK	0x00000003	/* gpio [7:6], SDIO CIS selection */
+#define CST4315_DEFCIS_SEL		0x00000000	/* use default CIS, OTP is powered up */
+#define CST4315_SPROM_SEL		0x00000001	/* use SPROM, OTP is powered up */
+#define CST4315_OTP_SEL			0x00000002	/* use OTP, OTP is powered up */
+#define CST4315_OTP_PWRDN		0x00000003	/* use SPROM, OTP is powered down */
+#define CST4315_SDIO_MODE		0x00000004	/* gpio [8], sdio/usb mode */
+#define CST4315_RCAL_VALID		0x00000008
+#define CST4315_RCAL_VALUE_MASK		0x000001f0
+#define CST4315_RCAL_VALUE_SHIFT	4
+#define CST4315_PALDO_EXTPNP		0x00000200	/* PALDO is configured with external PNP */
+#define CST4315_CBUCK_MODE_MASK		0x00000c00
+#define CST4315_CBUCK_MODE_BURST	0x00000400
+#define CST4315_CBUCK_MODE_LPBURST	0x00000c00
+
+/* 4319 resources */
+#define RES4319_CBUCK_LPOM		1	/* 0x00000002 */
+#define RES4319_CBUCK_BURST		2	/* 0x00000004 */
+#define RES4319_CBUCK_PWM		3	/* 0x00000008 */
+#define RES4319_CLDO_PU			4	/* 0x00000010 */
+#define RES4319_PALDO_PU		5	/* 0x00000020 */
+#define RES4319_ILP_REQUEST		6	/* 0x00000040 */
+#define RES4319_LNLDO1_PU		9	/* 0x00000200 */
+#define RES4319_OTP_PU			10	/* 0x00000400 */
+#define RES4319_LNLDO2_PU		12	/* 0x00001000 */
+#define RES4319_XTAL_PU			13	/* 0x00002000 */
+#define RES4319_ALP_AVAIL		14	/* 0x00004000 */
+#define RES4319_RX_PWRSW_PU		15	/* 0x00008000 */
+#define RES4319_TX_PWRSW_PU		16	/* 0x00010000 */
+#define RES4319_RFPLL_PWRSW_PU		17	/* 0x00020000 */
+#define RES4319_LOGEN_PWRSW_PU		18	/* 0x00040000 */
+#define RES4319_AFE_PWRSW_PU		19	/* 0x00080000 */
+#define RES4319_BBPLL_PWRSW_PU		20	/* 0x00100000 */
+#define RES4319_HT_AVAIL		21	/* 0x00200000 */
+
+/* 4319 chip-specific ChipStatus register bits */
+#define	CST4319_SPI_CPULESSUSB		0x00000001
+#define	CST4319_SPI_CLK_POL		0x00000002
+#define	CST4319_SPI_CLK_PH		0x00000008
+#define	CST4319_SPROM_OTP_SEL_MASK	0x000000c0	/* gpio [7:6], SDIO CIS selection */
+#define	CST4319_SPROM_OTP_SEL_SHIFT	6
+#define	CST4319_DEFCIS_SEL		0x00000000	/* use default CIS, OTP is powered up */
+#define	CST4319_SPROM_SEL		0x00000040	/* use SPROM, OTP is powered up */
+#define	CST4319_OTP_SEL			0x00000080      /* use OTP, OTP is powered up */
+#define	CST4319_OTP_PWRDN		0x000000c0      /* use SPROM, OTP is powered down */
+#define	CST4319_SDIO_USB_MODE		0x00000100	/* gpio [8], sdio/usb mode */
+#define	CST4319_REMAP_SEL_MASK		0x00000600
+#define	CST4319_ILPDIV_EN		0x00000800
+#define	CST4319_XTAL_PD_POL		0x00001000
+#define	CST4319_LPO_SEL			0x00002000
+#define	CST4319_RES_INIT_MODE		0x0000c000
+#define	CST4319_PALDO_EXTPNP		0x00010000	/* PALDO is configured with external PNP */
+#define	CST4319_CBUCK_MODE_MASK		0x00060000
+#define CST4319_CBUCK_MODE_BURST	0x00020000
+#define CST4319_CBUCK_MODE_LPBURST	0x00060000
+#define	CST4319_RCAL_VALID		0x01000000
+#define	CST4319_RCAL_VALUE_MASK		0x3e000000
+#define	CST4319_RCAL_VALUE_SHIFT	25
+
+#define PMU1_PLL0_CHIPCTL0		0
+#define PMU1_PLL0_CHIPCTL1		1
+#define PMU1_PLL0_CHIPCTL2		2
+#define CCTL_4319USB_XTAL_SEL_MASK	0x00180000
+#define CCTL_4319USB_XTAL_SEL_SHIFT	19
+#define CCTL_4319USB_48MHZ_PLL_SEL	1
+#define CCTL_4319USB_24MHZ_PLL_SEL	2
+
+/* PMU resources for 4336 */
+#define	RES4336_CBUCK_LPOM		0
+#define	RES4336_CBUCK_BURST		1
+#define	RES4336_CBUCK_LP_PWM		2
+#define	RES4336_CBUCK_PWM		3
+#define	RES4336_CLDO_PU			4
+#define	RES4336_DIS_INT_RESET_PD	5
+#define	RES4336_ILP_REQUEST		6
+#define	RES4336_LNLDO_PU		7
+#define	RES4336_LDO3P3_PU		8
+#define	RES4336_OTP_PU			9
+#define	RES4336_XTAL_PU			10
+#define	RES4336_ALP_AVAIL		11
+#define	RES4336_RADIO_PU		12
+#define	RES4336_BG_PU			13
+#define	RES4336_VREG1p4_PU_PU		14
+#define	RES4336_AFE_PWRSW_PU		15
+#define	RES4336_RX_PWRSW_PU		16
+#define	RES4336_TX_PWRSW_PU		17
+#define	RES4336_BB_PWRSW_PU		18
+#define	RES4336_SYNTH_PWRSW_PU		19
+#define	RES4336_MISC_PWRSW_PU		20
+#define	RES4336_LOGEN_PWRSW_PU		21
+#define	RES4336_BBPLL_PWRSW_PU		22
+#define	RES4336_MACPHY_CLKAVAIL		23
+#define	RES4336_HT_AVAIL		24
+#define	RES4336_RSVD			25
+
+/* 4336 chip-specific ChipStatus register bits */
+#define	CST4336_SPI_MODE_MASK		0x00000001
+#define	CST4336_SPROM_PRESENT		0x00000002
+#define	CST4336_OTP_PRESENT		0x00000004
+#define	CST4336_ARMREMAP_0		0x00000008
+#define	CST4336_ILPDIV_EN_MASK		0x00000010
+#define	CST4336_ILPDIV_EN_SHIFT		4
+#define	CST4336_XTAL_PD_POL_MASK	0x00000020
+#define	CST4336_XTAL_PD_POL_SHIFT	5
+#define	CST4336_LPO_SEL_MASK		0x00000040
+#define	CST4336_LPO_SEL_SHIFT		6
+#define	CST4336_RES_INIT_MODE_MASK	0x00000180
+#define	CST4336_RES_INIT_MODE_SHIFT	7
+#define	CST4336_CBUCK_MODE_MASK		0x00000600
+#define	CST4336_CBUCK_MODE_SHIFT	9
+
+/* 4336 Chip specific PMU ChipControl register bits */
+#define PCTL_4336_SERIAL_ENAB	(1  << 24)
+
+/* 4330 resources */
+#define	RES4330_CBUCK_LPOM		0
+#define	RES4330_CBUCK_BURST		1
+#define	RES4330_CBUCK_LP_PWM		2
+#define	RES4330_CBUCK_PWM		3
+#define	RES4330_CLDO_PU			4
+#define	RES4330_DIS_INT_RESET_PD	5
+#define	RES4330_ILP_REQUEST		6
+#define	RES4330_LNLDO_PU		7
+#define	RES4330_LDO3P3_PU		8
+#define	RES4330_OTP_PU			9
+#define	RES4330_XTAL_PU			10
+#define	RES4330_ALP_AVAIL		11
+#define	RES4330_RADIO_PU		12
+#define	RES4330_BG_PU			13
+#define	RES4330_VREG1p4_PU_PU		14
+#define	RES4330_AFE_PWRSW_PU		15
+#define	RES4330_RX_PWRSW_PU		16
+#define	RES4330_TX_PWRSW_PU		17
+#define	RES4330_BB_PWRSW_PU		18
+#define	RES4330_SYNTH_PWRSW_PU		19
+#define	RES4330_MISC_PWRSW_PU		20
+#define	RES4330_LOGEN_PWRSW_PU		21
+#define	RES4330_BBPLL_PWRSW_PU		22
+#define	RES4330_MACPHY_CLKAVAIL		23
+#define	RES4330_HT_AVAIL		24
+#define	RES4330_5gRX_PWRSW_PU		25
+#define	RES4330_5gTX_PWRSW_PU		26
+#define	RES4330_5g_LOGEN_PWRSW_PU	27
+
+/* 4330 chip-specific ChipStatus register bits */
+#define CST4330_CHIPMODE_SDIOD(cs)	(((cs) & 0x7) < 6)	/* SDIO || gSPI */
+#define CST4330_CHIPMODE_USB20D(cs)	(((cs) & 0x7) >= 6)	/* USB || USBDA */
+#define CST4330_CHIPMODE_SDIO(cs)	(((cs) & 0x4) == 0)	/* SDIO */
+#define CST4330_CHIPMODE_GSPI(cs)	(((cs) & 0x6) == 4)	/* gSPI */
+#define CST4330_CHIPMODE_USB(cs)	(((cs) & 0x7) == 6)	/* USB packet-oriented */
+#define CST4330_CHIPMODE_USBDA(cs)	(((cs) & 0x7) == 7)	/* USB Direct Access */
+#define	CST4330_OTP_PRESENT		0x00000010
+#define	CST4330_LPO_AUTODET_EN		0x00000020
+#define	CST4330_ARMREMAP_0		0x00000040
+#define	CST4330_SPROM_PRESENT		0x00000080	/* takes priority over OTP if both set */
+#define	CST4330_ILPDIV_EN		0x00000100
+#define	CST4330_LPO_SEL			0x00000200
+#define	CST4330_RES_INIT_MODE_SHIFT	10
+#define	CST4330_RES_INIT_MODE_MASK	0x00000c00
+#define CST4330_CBUCK_MODE_SHIFT	12
+#define CST4330_CBUCK_MODE_MASK		0x00003000
+#define	CST4330_CBUCK_POWER_OK		0x00004000
+#define	CST4330_BB_PLL_LOCKED		0x00008000
+#define SOCDEVRAM_BP_ADDR		0x1E000000
+#define SOCDEVRAM_ARM_ADDR		0x00800000
+
+/* 4330 Chip specific PMU ChipControl register bits */
+#define PCTL_4330_SERIAL_ENAB	(1  << 24)
+
+/* 4330 Chip specific ChipControl register bits */
+#define CCTRL_4330_GPIO_SEL		0x00000001    /* 1=select GPIOs to be muxed out */
+#define CCTRL_4330_ERCX_SEL		0x00000002    /* 1=select ERCX BT coex to be muxed out */
+#define CCTRL_4330_SDIO_HOST_WAKE	0x00000004    /* SDIO: 1=configure GPIO0 for host wake */
+#define CCTRL_4330_JTAG_DISABLE	0x00000008    /* 1=disable JTAG interface on mux'd pins */
+
+/* 4334 resources */
+#define RES4334_LPLDO_PU		0
+#define RES4334_RESET_PULLDN_DIS	1
+#define RES4334_PMU_BG_PU		2
+#define RES4334_HSIC_LDO_PU		3
+#define RES4334_CBUCK_LPOM_PU		4
+#define RES4334_CBUCK_PFM_PU		5
+#define RES4334_CLDO_PU			6
+#define RES4334_LPLDO2_LVM		7
+#define RES4334_LNLDO_PU		8
+#define RES4334_LDO3P3_PU		9
+#define RES4334_OTP_PU			10
+#define RES4334_XTAL_PU			11
+#define RES4334_WL_PWRSW_PU		12
+#define RES4334_LQ_AVAIL		13
+#define RES4334_LOGIC_RET		14
+#define RES4334_MEM_SLEEP		15
+#define RES4334_MACPHY_RET		16
+#define RES4334_WL_CORE_READY		17
+#define RES4334_ILP_REQ			18
+#define RES4334_ALP_AVAIL		19
+#define RES4334_MISC_PWRSW_PU		20
+#define RES4334_SYNTH_PWRSW_PU		21
+#define RES4334_RX_PWRSW_PU		22
+#define RES4334_RADIO_PU		23
+#define RES4334_WL_PMU_PU		24
+#define RES4334_VCO_LDO_PU		25
+#define RES4334_AFE_LDO_PU		26
+#define RES4334_RX_LDO_PU		27
+#define RES4334_TX_LDO_PU		28
+#define RES4334_HT_AVAIL		29
+#define RES4334_MACPHY_CLK_AVAIL	30
+
+/* 4334 chip-specific ChipStatus register bits */
+#define CST4334_CHIPMODE_MASK		7
+#define CST4334_SDIO_MODE		0x00000000
+#define CST4334_SPI_MODE		0x00000004
+#define CST4334_HSIC_MODE		0x00000006
+#define CST4334_BLUSB_MODE		0x00000007
+#define CST4334_CHIPMODE_HSIC(cs)	(((cs) & CST4334_CHIPMODE_MASK) == CST4334_HSIC_MODE)
+#define CST4334_OTP_PRESENT		0x00000010
+#define CST4334_LPO_AUTODET_EN		0x00000020
+#define CST4334_ARMREMAP_0		0x00000040
+#define CST4334_SPROM_PRESENT		0x00000080
+#define CST4334_ILPDIV_EN_MASK		0x00000100
+#define CST4334_ILPDIV_EN_SHIFT		8
+#define CST4334_LPO_SEL_MASK		0x00000200
+#define CST4334_LPO_SEL_SHIFT		9
+#define CST4334_RES_INIT_MODE_MASK	0x00000C00
+#define CST4334_RES_INIT_MODE_SHIFT	10
+
+/* 4334 Chip specific PMU ChipControl register bits */
+#define PCTL_4334_GPIO3_ENAB    (1  << 3)
+
+/* 4334 Chip control */
+#define CCTRL4334_HSIC_LDO_PU		(1  << 23)
+
+/* 4324 Chip specific ChipControl1 register bits */
+#define CCTRL1_4324_GPIO_SEL            (1 << 0)    /* 1=select GPIOs to be muxed out */
+#define CCTRL1_4324_SDIO_HOST_WAKE (1 << 2)  /* SDIO: 1=configure GPIO0 for host wake */
+
+
+/* 4313 resources */
+#define	RES4313_BB_PU_RSRC		0
+#define	RES4313_ILP_REQ_RSRC		1
+#define	RES4313_XTAL_PU_RSRC		2
+#define	RES4313_ALP_AVAIL_RSRC		3
+#define	RES4313_RADIO_PU_RSRC		4
+#define	RES4313_BG_PU_RSRC		5
+#define	RES4313_VREG1P4_PU_RSRC		6
+#define	RES4313_AFE_PWRSW_RSRC		7
+#define	RES4313_RX_PWRSW_RSRC		8
+#define	RES4313_TX_PWRSW_RSRC		9
+#define	RES4313_BB_PWRSW_RSRC		10
+#define	RES4313_SYNTH_PWRSW_RSRC	11
+#define	RES4313_MISC_PWRSW_RSRC		12
+#define	RES4313_BB_PLL_PWRSW_RSRC	13
+#define	RES4313_HT_AVAIL_RSRC		14
+#define	RES4313_MACPHY_CLK_AVAIL_RSRC	15
+
+/* 4313 chip-specific ChipStatus register bits */
+#define	CST4313_SPROM_PRESENT			1
+#define	CST4313_OTP_PRESENT			2
+#define	CST4313_SPROM_OTP_SEL_MASK		0x00000002
+#define	CST4313_SPROM_OTP_SEL_SHIFT		0
+
+/* 4313 Chip specific ChipControl register bits */
+#define CCTRL_4313_12MA_LED_DRIVE    0x00000007    /* 12 mA drive strengh for later 4313 */
+
+/* PMU respources for 4314 */
+#define RES4314_LPLDO_PU		0
+#define RES4314_PMU_SLEEP_DIS		1
+#define RES4314_PMU_BG_PU		2
+#define RES4314_CBUCK_LPOM_PU		3
+#define RES4314_CBUCK_PFM_PU		4
+#define RES4314_CLDO_PU			5
+#define RES4314_LPLDO2_LVM		6
+#define RES4314_WL_PMU_PU		7
+#define RES4314_LNLDO_PU		8
+#define RES4314_LDO3P3_PU		9
+#define RES4314_OTP_PU			10
+#define RES4314_XTAL_PU			11
+#define RES4314_WL_PWRSW_PU		12
+#define RES4314_LQ_AVAIL		13
+#define RES4314_LOGIC_RET		14
+#define RES4314_MEM_SLEEP		15
+#define RES4314_MACPHY_RET		16
+#define RES4314_WL_CORE_READY		17
+#define RES4314_ILP_REQ			18
+#define RES4314_ALP_AVAIL		19
+#define RES4314_MISC_PWRSW_PU		20
+#define RES4314_SYNTH_PWRSW_PU		21
+#define RES4314_RX_PWRSW_PU		22
+#define RES4314_RADIO_PU		23
+#define RES4314_VCO_LDO_PU		24
+#define RES4314_AFE_LDO_PU		25
+#define RES4314_RX_LDO_PU		26
+#define RES4314_TX_LDO_PU		27
+#define RES4314_HT_AVAIL		28
+#define RES4314_MACPHY_CLK_AVAIL	29
+
+/* 4314 chip-specific ChipStatus register bits */
+#define CST4314_OTP_ENABLED		0x00200000
+
+/* 43228 resources */
+#define RES43228_NOT_USED		0
+#define RES43228_ILP_REQUEST		1
+#define RES43228_XTAL_PU		2
+#define RES43228_ALP_AVAIL		3
+#define RES43228_PLL_EN			4
+#define RES43228_HT_PHY_AVAIL		5
+
+/* 43228 chipstatus  reg bits */
+#define CST43228_ILP_DIV_EN		0x1
+#define	CST43228_OTP_PRESENT		0x2
+#define	CST43228_SERDES_REFCLK_PADSEL	0x4
+#define	CST43228_SDIO_MODE		0x8
+#define	CST43228_SDIO_OTP_PRESENT	0x10
+#define	CST43228_SDIO_RESET		0x20
+
+/* 4706 chipstatus reg bits */
+#define	CST4706_PKG_OPTION		(1<<0) /* 0: full-featured package 1: low-cost package */
+#define	CST4706_SFLASH_PRESENT	(1<<1) /* 0: parallel, 1: serial flash is present */
+#define	CST4706_SFLASH_TYPE		(1<<2) /* 0: 8b-p/ST-s flash, 1: 16b-p/Atmal-s flash */
+#define	CST4706_MIPS_BENDIAN	(1<<3) /* 0: little,  1: big endian */
+#define	CST4706_PCIE1_DISABLE	(1<<5) /* PCIE1 enable strap pin */
+
+/* 4706 flashstrconfig reg bits */
+#define FLSTRCF4706_MASK		0x000000ff
+#define FLSTRCF4706_SF1			0x00000001	/* 2nd serial flash present */
+#define FLSTRCF4706_PF1			0x00000002	/* 2nd parallel flash present */
+#define FLSTRCF4706_SF1_TYPE	0x00000004	/* 2nd serial flash type : 0 : ST, 1 : Atmel */
+#define FLSTRCF4706_NF1			0x00000008	/* 2nd NAND flash present */
+#define FLSTRCF4706_1ST_MADDR_SEG_MASK		0x000000f0	/* Valid value mask */
+#define FLSTRCF4706_1ST_MADDR_SEG_4MB		0x00000010	/* 4MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_8MB		0x00000020	/* 8MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_16MB		0x00000030	/* 16MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_32MB		0x00000040	/* 32MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_64MB		0x00000050	/* 64MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_128MB		0x00000060	/* 128MB */
+#define FLSTRCF4706_1ST_MADDR_SEG_256MB		0x00000070	/* 256MB */
+
+/* 4360 Chip specific ChipControl register bits */
+#define CCTRL4360_SECI_MODE			(1 << 2)
+#define CCTRL4360_BTSWCTRL_MODE			(1 << 3)
+#define CCTRL4360_EXTRA_FEMCTRL_MODE		(1 << 8)
+#define CCTRL4360_BT_LGCY_MODE			(1 << 9)
+#define CCTRL4360_CORE2FEMCTRL4_ON		(1 << 21)
+
+/* 4360 PMU resources and chip status bits */
+#define RES4360_REGULATOR          0
+#define RES4360_ILP_AVAIL          1
+#define RES4360_ILP_REQ            2
+#define RES4360_XTAL_PU            3
+#define RES4360_ALP_AVAIL          4
+#define RES4360_BBPLLPWRSW_PU      5
+#define RES4360_HT_AVAIL           6
+#define RES4360_OTP_PU             7
+#define RES4360_USBLDO_PU          8
+#define RES4360_USBPLL_PWRSW_PU    9
+#define RES4360_LQ_AVAIL           10
+
+#define CST4360_XTAL_40MZ                  0x00000001
+#define CST4360_SFLASH                     0x00000002
+#define CST4360_SPROM_PRESENT              0x00000004
+#define CST4360_SFLASH_TYPE                0x00000004
+#define CST4360_OTP_ENABLED                0x00000008
+#define CST4360_REMAP_ROM                  0x00000010
+#define CST4360_RSRC_INIT_MODE_MASK        0x00000060
+#define CST4360_RSRC_INIT_MODE_SHIFT       5
+#define CST4360_ILP_DIVEN                  0x00000080
+#define CST4360_MODE_USB                   0x00000100
+#define CST4360_SPROM_SIZE_MASK            0x00000600
+#define CST4360_SPROM_SIZE_SHIFT           9
+#define CST4360_BBPLL_LOCK                 0x00000800
+#define CST4360_AVBBPLL_LOCK               0x00001000
+#define CST4360_USBBBPLL_LOCK              0x00002000
+
+#define CCTL_4360_UART_SEL	2
+
+/* 4335 resources */
+#define RES4335_LPLDO_PO           0
+#define RES4335_PMU_BG_PU          1
+#define RES4335_PMU_SLEEP          2
+#define RES4335_RSVD_3             3
+#define RES4335_CBUCK_LPOM_PU		4
+#define RES4335_CBUCK_PFM_PU		5
+#define RES4335_RSVD_6             6
+#define RES4335_RSVD_7             7
+#define RES4335_LNLDO_PU           8
+#define RES4335_XTALLDO_PU         9
+#define RES4335_LDO3P3_PU			10
+#define RES4335_OTP_PU				11
+#define RES4335_XTAL_PU				12
+#define RES4335_SR_CLK_START       13
+#define RES4335_LQ_AVAIL			14
+#define RES4335_LQ_START           15
+#define RES4335_RSVD_16            16
+#define RES4335_WL_CORE_RDY        17
+#define RES4335_ILP_REQ				18
+#define RES4335_ALP_AVAIL			19
+#define RES4335_MINI_PMU           20
+#define RES4335_RADIO_PU			21
+#define RES4335_SR_CLK_STABLE		22
+#define RES4335_SR_SAVE_RESTORE		23
+#define RES4335_SR_PHY_PWRSW		24
+#define RES4335_SR_VDDM_PWRSW      25
+#define RES4335_SR_SUBCORE_PWRSW	26
+#define RES4335_SR_SLEEP           27
+#define RES4335_HT_START           28
+#define RES4335_HT_AVAIL			29
+#define RES4335_MACPHY_CLKAVAIL		30
+
+/* 4335 Chip specific ChipStatus register bits */
+#define CST4335_SPROM_MASK			0x00000020
+#define CST4335_SFLASH_MASK			0x00000040
+#define	CST4335_RES_INIT_MODE_SHIFT	7
+#define	CST4335_RES_INIT_MODE_MASK	0x00000180
+#define CST4335_CHIPMODE_MASK		0xF
+#define CST4335_CHIPMODE_SDIOD(cs)	(((cs) & (1 << 0)) != 0)	/* SDIO */
+#define CST4335_CHIPMODE_GSPI(cs)	(((cs) & (1 << 1)) != 0)	/* gSPI */
+#define CST4335_CHIPMODE_USB20D(cs)	(((cs) & (1 << 2)) != 0)	/* USB || USBDA */
+#define CST4335_CHIPMODE_PCIE(cs)	(((cs) & (1 << 3)) != 0)	/* PCIE */
+
+/* 4335 Chip specific ChipControl1 register bits */
+#define CCTRL1_4335_GPIO_SEL		(1 << 0)    /* 1=select GPIOs to be muxed out */
+#define CCTRL1_4335_SDIO_HOST_WAKE (1 << 2)  /* SDIO: 1=configure GPIO0 for host wake */
+
+
+#define CR4_RAM_BASE                    (0x180000)
+#define PATCHTBL_SIZE			(0x800)
+
+
+/* 4335 resources--END */
+
+/* GCI chipcontrol register indices */
+#define CC_GCI_CHIPCTRL_00	(0)
+#define CC_GCI_CHIPCTRL_01	(1)
+#define CC_GCI_CHIPCTRL_02	(2)
+#define CC_GCI_CHIPCTRL_03	(3)
+#define CC_GCI_CHIPCTRL_04	(4)
+#define CC_GCI_CHIPCTRL_05	(5)
+#define CC_GCI_CHIPCTRL_06	(6)
+#define CC_GCI_CHIPCTRL_07	(7)
+#define CC_GCI_CHIPCTRL_08	(8)
+
+#define CC_GCI_NUMCHIPCTRLREGS(cap1)	((cap1 & 0xF00) >> 8)
+
+/* 4335 pins
+* note: only the values set as default/used are added here.
+*/
+#define CC4335_PIN_GPIO_00		(0)
+#define CC4335_PIN_GPIO_01		(1)
+#define CC4335_PIN_GPIO_02		(2)
+#define CC4335_PIN_GPIO_03		(3)
+#define CC4335_PIN_GPIO_04		(4)
+#define CC4335_PIN_GPIO_05		(5)
+#define CC4335_PIN_GPIO_06		(6)
+#define CC4335_PIN_GPIO_07		(7)
+#define CC4335_PIN_GPIO_08		(8)
+#define CC4335_PIN_GPIO_09		(9)
+#define CC4335_PIN_GPIO_10		(10)
+#define CC4335_PIN_GPIO_11		(11)
+#define CC4335_PIN_GPIO_12		(12)
+#define CC4335_PIN_GPIO_13		(13)
+#define CC4335_PIN_GPIO_14		(14)
+#define CC4335_PIN_GPIO_15		(15)
+#define CC4335_PIN_SDIO_CLK		(16)
+#define CC4335_PIN_SDIO_CMD		(17)
+#define CC4335_PIN_SDIO_DATA0	(18)
+#define CC4335_PIN_SDIO_DATA1	(19)
+#define CC4335_PIN_SDIO_DATA2	(20)
+#define CC4335_PIN_SDIO_DATA3	(21)
+#define CC4335_PIN_RF_SW_CTRL_0	(22)
+#define CC4335_PIN_RF_SW_CTRL_1	(23)
+#define CC4335_PIN_RF_SW_CTRL_2	(24)
+#define CC4335_PIN_RF_SW_CTRL_3	(25)
+#define CC4335_PIN_RF_SW_CTRL_4	(26)
+#define CC4335_PIN_RF_SW_CTRL_5	(27)
+#define CC4335_PIN_RF_SW_CTRL_6	(28)
+#define CC4335_PIN_RF_SW_CTRL_7	(29)
+#define CC4335_PIN_RF_SW_CTRL_8	(30)
+#define CC4335_PIN_RF_SW_CTRL_9	(31)
+
+/* 4335 GCI function sel values
+*/
+#define CC4335_FNSEL_HWDEF		(0)
+#define CC4335_FNSEL_SAMEASPIN	(1)
+#define CC4335_FNSEL_GPIO0		(2)
+#define CC4335_FNSEL_GPIO1		(3)
+#define CC4335_FNSEL_GCI0		(4)
+#define CC4335_FNSEL_GCI1		(5)
+#define CC4335_FNSEL_UART		(6)
+#define CC4335_FNSEL_SFLASH		(7)
+#define CC4335_FNSEL_SPROM		(8)
+#define CC4335_FNSEL_MISC0		(9)
+#define CC4335_FNSEL_MISC1		(10)
+#define CC4335_FNSEL_MISC2		(11)
+#define CC4335_FNSEL_IND		(12)
+#define CC4335_FNSEL_PDN		(13)
+#define CC4335_FNSEL_PUP		(14)
+#define CC4335_FNSEL_TRI		(15)
+
+/* find the 4 bit mask given the bit position */
+#define GCIMASK(pos)  (((uint32)0xF) << pos)
+
+/* get the value which can be used to directly OR with chipcontrol reg */
+#define GCIPOSVAL(val, pos)  ((((uint32)val) << pos) & GCIMASK(pos))
+
+/* 4335 MUX options. each nibble belongs to a setting. Non-zero value specifies a logic
+* for now only UART for bootloader.
+*/
+#define MUXENAB4335_UART_MASK		(0x0000000f)
+
+
+/* defines to detect active host interface in use */
+#define CHIP_HOSTIF_USB(sih)	(si_chip_hostif(sih) & CST4360_MODE_USB)
+
+/*
+* Maximum delay for the PMU state transition in us.
+* This is an upper bound intended for spinwaits etc.
+*/
+#define PMU_MAX_TRANSITION_DLY	20000
+
+/* PMU resource up transition time in ILP cycles */
+#define PMURES_UP_TRANSITION	2
+
+/*
+* Information from BT to WLAN over eci_inputlo, eci_inputmi &
+* eci_inputhi register.  Rev >=21
+*/
+/* Fields in eci_inputlo register - [0:31] */
+#define	ECI_INLO_TASKTYPE_MASK	0x0000000f /* [3:0] - 4 bits */
+#define ECI_INLO_TASKTYPE_SHIFT 0
+#define	ECI_INLO_PKTDUR_MASK	0x000000f0 /* [7:4] - 4 bits */
+#define ECI_INLO_PKTDUR_SHIFT	4
+#define	ECI_INLO_ROLE_MASK	0x00000100 /* [8] - 1 bits */
+#define ECI_INLO_ROLE_SHIFT	8
+#define	ECI_INLO_MLP_MASK	0x00000e00 /* [11:9] - 3 bits */
+#define ECI_INLO_MLP_SHIFT	9
+#define	ECI_INLO_TXPWR_MASK	0x000ff000 /* [19:12] - 8 bits */
+#define ECI_INLO_TXPWR_SHIFT	12
+#define	ECI_INLO_RSSI_MASK	0x0ff00000 /* [27:20] - 8 bits */
+#define ECI_INLO_RSSI_SHIFT	20
+#define	ECI_INLO_VAD_MASK	0x10000000 /* [28] - 1 bits */
+#define ECI_INLO_VAD_SHIFT	28
+
+/*
+* Register eci_inputlo bitfield values.
+* - BT packet type information bits [7:0]
+*/
+/*  [3:0] - Task (link) type */
+#define BT_ACL				0x00
+#define BT_SCO				0x01
+#define BT_eSCO				0x02
+#define BT_A2DP				0x03
+#define BT_SNIFF			0x04
+#define BT_PAGE_SCAN			0x05
+#define BT_INQUIRY_SCAN			0x06
+#define BT_PAGE				0x07
+#define BT_INQUIRY			0x08
+#define BT_MSS				0x09
+#define BT_PARK				0x0a
+#define BT_RSSISCAN			0x0b
+#define BT_MD_ACL			0x0c
+#define BT_MD_eSCO			0x0d
+#define BT_SCAN_WITH_SCO_LINK		0x0e
+#define BT_SCAN_WITHOUT_SCO_LINK	0x0f
+/* [7:4] = packet duration code */
+/* [8] - Master / Slave */
+#define BT_MASTER			0
+#define BT_SLAVE			1
+/* [11:9] - multi-level priority */
+#define BT_LOWEST_PRIO			0x0
+#define BT_HIGHEST_PRIO			0x3
+/* [19:12] - BT transmit power */
+/* [27:20] - BT RSSI */
+/* [28] - VAD silence */
+/* [31:29] - Undefined */
+/* Register eci_inputmi values - [32:63] - none defined */
+/* [63:32] - Undefined */
+
+/* Information from WLAN to BT over eci_output register. */
+/* Fields in eci_output register - [0:31] */
+#define ECI48_OUT_MASKMAGIC_HIWORD 0x55550000
+#define ECI_OUT_CHANNEL_MASK(ccrev) ((ccrev) < 35 ? 0xf : (ECI48_OUT_MASKMAGIC_HIWORD | 0xf000))
+#define ECI_OUT_CHANNEL_SHIFT(ccrev) ((ccrev) < 35 ? 0 : 12)
+#define ECI_OUT_BW_MASK(ccrev) ((ccrev) < 35 ? 0x70 : (ECI48_OUT_MASKMAGIC_HIWORD | 0xe00))
+#define ECI_OUT_BW_SHIFT(ccrev) ((ccrev) < 35 ? 4 : 9)
+#define ECI_OUT_ANTENNA_MASK(ccrev) ((ccrev) < 35 ? 0x80 : (ECI48_OUT_MASKMAGIC_HIWORD | 0x100))
+#define ECI_OUT_ANTENNA_SHIFT(ccrev) ((ccrev) < 35 ? 7 : 8)
+#define ECI_OUT_SIMUL_TXRX_MASK(ccrev) \
+	((ccrev) < 35 ? 0x10000 : (ECI48_OUT_MASKMAGIC_HIWORD | 0x80))
+#define ECI_OUT_SIMUL_TXRX_SHIFT(ccrev) ((ccrev) < 35 ? 16 : 7)
+#define ECI_OUT_FM_DISABLE_MASK(ccrev) \
+	((ccrev) < 35 ? 0x40000 : (ECI48_OUT_MASKMAGIC_HIWORD | 0x40))
+#define ECI_OUT_FM_DISABLE_SHIFT(ccrev) ((ccrev) < 35 ? 18 : 6)
+
+/* Indicate control of ECI bits between s/w and dot11mac.
+ * 0 => FW control, 1=> MAC/ucode control
+
+ * Current assignment (ccrev >= 35):
+ *  0 - TxConf (ucode)
+ * 38 - FM disable (wl)
+ * 39 - Allow sim rx (ucode)
+ * 40 - Num antennas (wl)
+ * 43:41 - WLAN channel exclusion BW (wl)
+ * 47:44 - WLAN channel (wl)
+ *
+ * (ccrev < 35)
+ * 15:0 - wl
+ * 16 -
+ * 18 - FM disable
+ * 30 - wl interrupt
+ * 31 - ucode interrupt
+ * others - unassigned (presumed to be with dot11mac/ucode)
+ */
+#define ECI_MACCTRL_BITS	0xbffb0000
+#define ECI_MACCTRLLO_BITS	0x1
+#define ECI_MACCTRLHI_BITS	0xFF
+
+
+/* SECI configuration */
+#define SECI_MODE_UART			0x0
+#define SECI_MODE_SECI			0x1
+#define SECI_MODE_LEGACY_3WIRE_BT	0x2
+#define SECI_MODE_LEGACY_3WIRE_WLAN	0x3
+#define SECI_MODE_HALF_SECI		0x4
+
+#define SECI_RESET		(1 << 0)
+#define SECI_RESET_BAR_UART	(1 << 1)
+#define SECI_ENAB_SECI_ECI	(1 << 2)
+#define SECI_ENAB_SECIOUT_DIS	(1 << 3)
+#define SECI_MODE_MASK		0x7
+#define SECI_MODE_SHIFT		4 /* (bits 5, 6, 7) */
+#define SECI_UPD_SECI		(1 << 7)
+
+#define SECI_SIGNOFF_0     0xDB
+#define SECI_SIGNOFF_1     0
+
+/* seci clk_ctl_st bits */
+#define CLKCTL_STS_SECI_CLK_REQ		(1 << 8)
+#define CLKCTL_STS_SECI_CLK_AVAIL	(1 << 24)
+
+#define SECI_UART_MSR_CTS_STATE		(1 << 0)
+#define SECI_UART_MSR_RTS_STATE		(1 << 1)
+#define SECI_UART_SECI_IN_STATE		(1 << 2)
+#define SECI_UART_SECI_IN2_STATE	(1 << 3)
+
+/* SECI UART LCR/MCR register bits */
+#define SECI_UART_LCR_STOP_BITS		(1 << 0) /* 0 - 1bit, 1 - 2bits */
+#define SECI_UART_LCR_PARITY_EN		(1 << 1)
+#define SECI_UART_LCR_PARITY		(1 << 2) /* 0 - odd, 1 - even */
+#define SECI_UART_LCR_RX_EN		(1 << 3)
+#define SECI_UART_LCR_LBRK_CTRL		(1 << 4) /* 1 => SECI_OUT held low */
+#define SECI_UART_LCR_TXO_EN		(1 << 5)
+#define SECI_UART_LCR_RTSO_EN		(1 << 6)
+#define SECI_UART_LCR_SLIPMODE_EN	(1 << 7)
+#define SECI_UART_LCR_RXCRC_CHK		(1 << 8)
+#define SECI_UART_LCR_TXCRC_INV		(1 << 9)
+#define SECI_UART_LCR_TXCRC_LSBF	(1 << 10)
+#define SECI_UART_LCR_TXCRC_EN		(1 << 11)
+
+#define SECI_UART_MCR_TX_EN		(1 << 0)
+#define SECI_UART_MCR_PRTS		(1 << 1)
+#define SECI_UART_MCR_SWFLCTRL_EN	(1 << 2)
+#define SECI_UART_MCR_HIGHRATE_EN	(1 << 3)
+#define SECI_UART_MCR_LOOPBK_EN		(1 << 4)
+#define SECI_UART_MCR_AUTO_RTS		(1 << 5)
+#define SECI_UART_MCR_AUTO_TX_DIS	(1 << 6)
+#define SECI_UART_MCR_BAUD_ADJ_EN	(1 << 7)
+#define SECI_UART_MCR_XONOFF_RPT	(1 << 9)
+
+/* WLAN channel numbers - used from wifi.h */
+
+/* WLAN BW */
+#define ECI_BW_20   0x0
+#define ECI_BW_25   0x1
+#define ECI_BW_30   0x2
+#define ECI_BW_35   0x3
+#define ECI_BW_40   0x4
+#define ECI_BW_45   0x5
+#define ECI_BW_50   0x6
+#define ECI_BW_ALL  0x7
+
+/* WLAN - number of antenna */
+#define WLAN_NUM_ANT1 TXANT_0
+#define WLAN_NUM_ANT2 TXANT_1
+
+#endif	/* _SBCHIPC_H */
diff --git a/drivers/bcmdrivers/gmac/src/include/sbconfig.h b/drivers/bcmdrivers/gmac/src/include/sbconfig.h
new file mode 100755
index 0000000..cd13ce6
