--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/aidmp.h
@@ -0,0 +1,383 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Broadcom AMBA Interconnect definitions.
+ *
+ * $Id: aidmp.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef	_AIDMP_H
+#define	_AIDMP_H
+
+/* Manufacturer Ids */
+#define	MFGID_ARM		0x43b
+#define	MFGID_BRCM		0x4bf
+#define	MFGID_MIPS		0x4a7
+
+/* Component Classes */
+#define	CC_SIM			0
+#define	CC_EROM			1
+#define	CC_CORESIGHT		9
+#define	CC_VERIF		0xb
+#define	CC_OPTIMO		0xd
+#define	CC_GEN			0xe
+#define	CC_PRIMECELL		0xf
+
+/* Enumeration ROM registers */
+#define	ER_EROMENTRY		0x000
+#define	ER_REMAPCONTROL		0xe00
+#define	ER_REMAPSELECT		0xe04
+#define	ER_MASTERSELECT		0xe10
+#define	ER_ITCR			0xf00
+#define	ER_ITIP			0xf04
+
+/* Erom entries */
+#define	ER_TAG			0xe
+#define	ER_TAG1			0x6
+#define	ER_VALID		1
+#define	ER_CI			0
+#define	ER_MP			2
+#define	ER_ADD			4
+#define	ER_END			0xe
+#define	ER_BAD			0xffffffff
+
+/* EROM CompIdentA */
+#define	CIA_MFG_MASK		0xfff00000
+#define	CIA_MFG_SHIFT		20
+#define	CIA_CID_MASK		0x000fff00
+#define	CIA_CID_SHIFT		8
+#define	CIA_CCL_MASK		0x000000f0
+#define	CIA_CCL_SHIFT		4
+
+/* EROM CompIdentB */
+#define	CIB_REV_MASK		0xff000000
+#define	CIB_REV_SHIFT		24
+#define	CIB_NSW_MASK		0x00f80000
+#define	CIB_NSW_SHIFT		19
+#define	CIB_NMW_MASK		0x0007c000
+#define	CIB_NMW_SHIFT		14
+#define	CIB_NSP_MASK		0x00003e00
+#define	CIB_NSP_SHIFT		9
+#define	CIB_NMP_MASK		0x000001f0
+#define	CIB_NMP_SHIFT		4
+
+/* EROM MasterPortDesc */
+#define	MPD_MUI_MASK		0x0000ff00
+#define	MPD_MUI_SHIFT		8
+#define	MPD_MP_MASK		0x000000f0
+#define	MPD_MP_SHIFT		4
+
+/* EROM AddrDesc */
+#define	AD_ADDR_MASK		0xfffff000
+#define	AD_SP_MASK		0x00000f00
+#define	AD_SP_SHIFT		8
+#define	AD_ST_MASK		0x000000c0
+#define	AD_ST_SHIFT		6
+#define	AD_ST_SLAVE		0x00000000
+#define	AD_ST_BRIDGE		0x00000040
+#define	AD_ST_SWRAP		0x00000080
+#define	AD_ST_MWRAP		0x000000c0
+#define	AD_SZ_MASK		0x00000030
+#define	AD_SZ_SHIFT		4
+#define	AD_SZ_4K		0x00000000
+#define	AD_SZ_8K		0x00000010
+#define	AD_SZ_16K		0x00000020
+#define	AD_SZ_SZD		0x00000030
+#define	AD_AG32			0x00000008
+#define	AD_ADDR_ALIGN		0x00000fff
+#define	AD_SZ_BASE		0x00001000	/* 4KB */
+
+/* EROM SizeDesc */
+#define	SD_SZ_MASK		0xfffff000
+#define	SD_SG32			0x00000008
+#define	SD_SZ_ALIGN		0x00000fff
+
+
+#ifndef _LANGUAGE_ASSEMBLY
+
+typedef volatile struct _aidmp {
+	uint32	oobselina30;	/* 0x000 */
+	uint32	oobselina74;	/* 0x004 */
+	uint32	PAD[6];
+	uint32	oobselinb30;	/* 0x020 */
+	uint32	oobselinb74;	/* 0x024 */
+	uint32	PAD[6];
+	uint32	oobselinc30;	/* 0x040 */
+	uint32	oobselinc74;	/* 0x044 */
+	uint32	PAD[6];
+	uint32	oobselind30;	/* 0x060 */
+	uint32	oobselind74;	/* 0x064 */
+	uint32	PAD[38];
+	uint32	oobselouta30;	/* 0x100 */
+	uint32	oobselouta74;	/* 0x104 */
+	uint32	PAD[6];
+	uint32	oobseloutb30;	/* 0x120 */
+	uint32	oobseloutb74;	/* 0x124 */
+	uint32	PAD[6];
+	uint32	oobseloutc30;	/* 0x140 */
+	uint32	oobseloutc74;	/* 0x144 */
+	uint32	PAD[6];
+	uint32	oobseloutd30;	/* 0x160 */
+	uint32	oobseloutd74;	/* 0x164 */
+	uint32	PAD[38];
+	uint32	oobsynca;	/* 0x200 */
+	uint32	oobseloutaen;	/* 0x204 */
+	uint32	PAD[6];
+	uint32	oobsyncb;	/* 0x220 */
+	uint32	oobseloutben;	/* 0x224 */
+	uint32	PAD[6];
+	uint32	oobsyncc;	/* 0x240 */
+	uint32	oobseloutcen;	/* 0x244 */
+	uint32	PAD[6];
+	uint32	oobsyncd;	/* 0x260 */
+	uint32	oobseloutden;	/* 0x264 */
+	uint32	PAD[38];
+	uint32	oobaextwidth;	/* 0x300 */
+	uint32	oobainwidth;	/* 0x304 */
+	uint32	oobaoutwidth;	/* 0x308 */
+	uint32	PAD[5];
+	uint32	oobbextwidth;	/* 0x320 */
+	uint32	oobbinwidth;	/* 0x324 */
+	uint32	oobboutwidth;	/* 0x328 */
+	uint32	PAD[5];
+	uint32	oobcextwidth;	/* 0x340 */
+	uint32	oobcinwidth;	/* 0x344 */
+	uint32	oobcoutwidth;	/* 0x348 */
+	uint32	PAD[5];
+	uint32	oobdextwidth;	/* 0x360 */
+	uint32	oobdinwidth;	/* 0x364 */
+	uint32	oobdoutwidth;	/* 0x368 */
+	uint32	PAD[37];
+	uint32	ioctrlset;	/* 0x400 */
+	uint32	ioctrlclear;	/* 0x404 */
+	uint32	ioctrl;		/* 0x408 */
+	uint32	PAD[61];
+	uint32	iostatus;	/* 0x500 */
+	uint32	PAD[127];
+	uint32	ioctrlwidth;	/* 0x700 */
+	uint32	iostatuswidth;	/* 0x704 */
+	uint32	PAD[62];
+	uint32	resetctrl;	/* 0x800 */
+	uint32	resetstatus;	/* 0x804 */
+	uint32	resetreadid;	/* 0x808 */
+	uint32	resetwriteid;	/* 0x80c */
+	uint32	PAD[60];
+	uint32	errlogctrl;	/* 0x900 */
+	uint32	errlogdone;	/* 0x904 */
+	uint32	errlogstatus;	/* 0x908 */
+	uint32	errlogaddrlo;	/* 0x90c */
+	uint32	errlogaddrhi;	/* 0x910 */
+	uint32	errlogid;	/* 0x914 */
+	uint32	errloguser;	/* 0x918 */
+	uint32	errlogflags;	/* 0x91c */
+	uint32	PAD[56];
+	uint32	intstatus;	/* 0xa00 */
+	uint32	PAD[255];
+	uint32	config;		/* 0xe00 */
+	uint32	PAD[63];
+	uint32	itcr;		/* 0xf00 */
+	uint32	PAD[3];
+	uint32	itipooba;	/* 0xf10 */
+	uint32	itipoobb;	/* 0xf14 */
+	uint32	itipoobc;	/* 0xf18 */
+	uint32	itipoobd;	/* 0xf1c */
+	uint32	PAD[4];
+	uint32	itipoobaout;	/* 0xf30 */
+	uint32	itipoobbout;	/* 0xf34 */
+	uint32	itipoobcout;	/* 0xf38 */
+	uint32	itipoobdout;	/* 0xf3c */
+	uint32	PAD[4];
+	uint32	itopooba;	/* 0xf50 */
+	uint32	itopoobb;	/* 0xf54 */
+	uint32	itopoobc;	/* 0xf58 */
+	uint32	itopoobd;	/* 0xf5c */
+	uint32	PAD[4];
+	uint32	itopoobain;	/* 0xf70 */
+	uint32	itopoobbin;	/* 0xf74 */
+	uint32	itopoobcin;	/* 0xf78 */
+	uint32	itopoobdin;	/* 0xf7c */
+	uint32	PAD[4];
+	uint32	itopreset;	/* 0xf90 */
+	uint32	PAD[15];
+	uint32	peripherialid4;	/* 0xfd0 */
+	uint32	peripherialid5;	/* 0xfd4 */
+	uint32	peripherialid6;	/* 0xfd8 */
+	uint32	peripherialid7;	/* 0xfdc */
+	uint32	peripherialid0;	/* 0xfe0 */
+	uint32	peripherialid1;	/* 0xfe4 */
+	uint32	peripherialid2;	/* 0xfe8 */
+	uint32	peripherialid3;	/* 0xfec */
+	uint32	componentid0;	/* 0xff0 */
+	uint32	componentid1;	/* 0xff4 */
+	uint32	componentid2;	/* 0xff8 */
+	uint32	componentid3;	/* 0xffc */
+} aidmp_t;
+
+#endif /* _LANGUAGE_ASSEMBLY */
+
+/* Out-of-band Router registers */
+#define	OOB_BUSCONFIG		0x020
+#define	OOB_STATUSA		0x100
+#define	OOB_STATUSB		0x104
+#define	OOB_STATUSC		0x108
+#define	OOB_STATUSD		0x10c
+#define	OOB_ENABLEA0		0x200
+#define	OOB_ENABLEA1		0x204
+#define	OOB_ENABLEA2		0x208
+#define	OOB_ENABLEA3		0x20c
+#define	OOB_ENABLEB0		0x280
+#define	OOB_ENABLEB1		0x284
+#define	OOB_ENABLEB2		0x288
+#define	OOB_ENABLEB3		0x28c
+#define	OOB_ENABLEC0		0x300
+#define	OOB_ENABLEC1		0x304
+#define	OOB_ENABLEC2		0x308
+#define	OOB_ENABLEC3		0x30c
+#define	OOB_ENABLED0		0x380
+#define	OOB_ENABLED1		0x384
+#define	OOB_ENABLED2		0x388
+#define	OOB_ENABLED3		0x38c
+#define	OOB_ITCR		0xf00
+#define	OOB_ITIPOOBA		0xf10
+#define	OOB_ITIPOOBB		0xf14
+#define	OOB_ITIPOOBC		0xf18
+#define	OOB_ITIPOOBD		0xf1c
+#define	OOB_ITOPOOBA		0xf30
+#define	OOB_ITOPOOBB		0xf34
+#define	OOB_ITOPOOBC		0xf38
+#define	OOB_ITOPOOBD		0xf3c
+
+/* DMP wrapper registers */
+#define	AI_OOBSELINA30		0x000
+#define	AI_OOBSELINA74		0x004
+#define	AI_OOBSELINB30		0x020
+#define	AI_OOBSELINB74		0x024
+#define	AI_OOBSELINC30		0x040
+#define	AI_OOBSELINC74		0x044
+#define	AI_OOBSELIND30		0x060
+#define	AI_OOBSELIND74		0x064
+#define	AI_OOBSELOUTA30		0x100
+#define	AI_OOBSELOUTA74		0x104
+#define	AI_OOBSELOUTB30		0x120
+#define	AI_OOBSELOUTB74		0x124
+#define	AI_OOBSELOUTC30		0x140
+#define	AI_OOBSELOUTC74		0x144
+#define	AI_OOBSELOUTD30		0x160
+#define	AI_OOBSELOUTD74		0x164
+#define	AI_OOBSYNCA		0x200
+#define	AI_OOBSELOUTAEN		0x204
+#define	AI_OOBSYNCB		0x220
+#define	AI_OOBSELOUTBEN		0x224
+#define	AI_OOBSYNCC		0x240
+#define	AI_OOBSELOUTCEN		0x244
+#define	AI_OOBSYNCD		0x260
+#define	AI_OOBSELOUTDEN		0x264
+#define	AI_OOBAEXTWIDTH		0x300
+#define	AI_OOBAINWIDTH		0x304
+#define	AI_OOBAOUTWIDTH		0x308
+#define	AI_OOBBEXTWIDTH		0x320
+#define	AI_OOBBINWIDTH		0x324
+#define	AI_OOBBOUTWIDTH		0x328
+#define	AI_OOBCEXTWIDTH		0x340
+#define	AI_OOBCINWIDTH		0x344
+#define	AI_OOBCOUTWIDTH		0x348
+#define	AI_OOBDEXTWIDTH		0x360
+#define	AI_OOBDINWIDTH		0x364
+#define	AI_OOBDOUTWIDTH		0x368
+
+#if	defined(IL_BIGENDIAN) && defined(BCMHND74K)
+/* Selective swapped defines for those registers we need in
+ * big-endian code.
+ */
+#define	AI_IOCTRLSET		0x404
+#define	AI_IOCTRLCLEAR		0x400
+#define	AI_IOCTRL		0x40c
+#define	AI_IOSTATUS		0x504
+#define	AI_RESETCTRL		0x804
+#define	AI_RESETSTATUS		0x800
+
+#else	/* !IL_BIGENDIAN || !BCMHND74K */
+
+#define	AI_IOCTRLSET		0x400
+#define	AI_IOCTRLCLEAR		0x404
+#define	AI_IOCTRL		0x408
+#define	AI_IOSTATUS		0x500
+#define	AI_RESETCTRL		0x800
+#define	AI_RESETSTATUS		0x804
+
+#endif	/* IL_BIGENDIAN && BCMHND74K */
+
+#define	AI_IOCTRLWIDTH		0x700
+#define	AI_IOSTATUSWIDTH	0x704
+
+#define	AI_RESETREADID		0x808
+#define	AI_RESETWRITEID		0x80c
+#define	AI_ERRLOGCTRL		0xa00
+#define	AI_ERRLOGDONE		0xa04
+#define	AI_ERRLOGSTATUS		0xa08
+#define	AI_ERRLOGADDRLO		0xa0c
+#define	AI_ERRLOGADDRHI		0xa10
+#define	AI_ERRLOGID		0xa14
+#define	AI_ERRLOGUSER		0xa18
+#define	AI_ERRLOGFLAGS		0xa1c
+#define	AI_INTSTATUS		0xa00
+#define	AI_CONFIG		0xe00
+#define	AI_ITCR			0xf00
+#define	AI_ITIPOOBA		0xf10
+#define	AI_ITIPOOBB		0xf14
+#define	AI_ITIPOOBC		0xf18
+#define	AI_ITIPOOBD		0xf1c
+#define	AI_ITIPOOBAOUT		0xf30
+#define	AI_ITIPOOBBOUT		0xf34
+#define	AI_ITIPOOBCOUT		0xf38
+#define	AI_ITIPOOBDOUT		0xf3c
+#define	AI_ITOPOOBA		0xf50
+#define	AI_ITOPOOBB		0xf54
+#define	AI_ITOPOOBC		0xf58
+#define	AI_ITOPOOBD		0xf5c
+#define	AI_ITOPOOBAIN		0xf70
+#define	AI_ITOPOOBBIN		0xf74
+#define	AI_ITOPOOBCIN		0xf78
+#define	AI_ITOPOOBDIN		0xf7c
+#define	AI_ITOPRESET		0xf90
+#define	AI_PERIPHERIALID4	0xfd0
+#define	AI_PERIPHERIALID5	0xfd4
+#define	AI_PERIPHERIALID6	0xfd8
+#define	AI_PERIPHERIALID7	0xfdc
+#define	AI_PERIPHERIALID0	0xfe0
+#define	AI_PERIPHERIALID1	0xfe4
+#define	AI_PERIPHERIALID2	0xfe8
+#define	AI_PERIPHERIALID3	0xfec
+#define	AI_COMPONENTID0		0xff0
+#define	AI_COMPONENTID1		0xff4
+#define	AI_COMPONENTID2		0xff8
+#define	AI_COMPONENTID3		0xffc
+
+/* resetctrl */
+#define	AIRC_RESET		1
+
+/* config */
+#define	AICFG_OOB		0x00000020
+#define	AICFG_IOS		0x00000010
+#define	AICFG_IOC		0x00000008
+#define	AICFG_TO		0x00000004
+#define	AICFG_ERRL		0x00000002
+#define	AICFG_RST		0x00000001
+
+/* bit defines for AI_OOBSELOUTB74 reg */
+#define OOB_SEL_OUTEN_B_5	15
+#define OOB_SEL_OUTEN_B_6	23
+
+#endif	/* _AIDMP_H */
diff --git a/drivers/bcmdrivers/gmac/src/include/arminc.h b/drivers/bcmdrivers/gmac/src/include/arminc.h
new file mode 100755
index 0000000..a0f2401
