--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmutils.h
@@ -0,0 +1,864 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Misc useful os-independent macros and functions.
+ *
+ * $Id: bcmutils.h 325951 2012-04-05 06:03:27Z $
+ */
+
+#ifndef	_bcmutils_h_
+#define	_bcmutils_h_
+
+#if defined(UNDER_CE)
+#include <bcmsafestr.h>
+#else
+#define bcm_strcpy_s(dst, noOfElements, src)            strcpy((dst), (src))
+#define bcm_strncpy_s(dst, noOfElements, src, count)    strncpy((dst), (src), (count))
+#define bcm_strcat_s(dst, noOfElements, src)            strcat((dst), (src))
+#endif
+
+#ifdef __cplusplus
+extern "C" {
+#endif
+
+#ifdef PKTQ_LOG
+#include <wlioctl.h>
+#endif
+
+/* ctype replacement */
+#define _BCM_U	0x01	/* upper */
+#define _BCM_L	0x02	/* lower */
+#define _BCM_D	0x04	/* digit */
+#define _BCM_C	0x08	/* cntrl */
+#define _BCM_P	0x10	/* punct */
+#define _BCM_S	0x20	/* white space (space/lf/tab) */
+#define _BCM_X	0x40	/* hex digit */
+#define _BCM_SP	0x80	/* hard space (0x20) */
+
+#if defined(BCMROMBUILD)
+extern const unsigned char BCMROMDATA(bcm_ctype)[];
+#else
+extern const unsigned char bcm_ctype[];
+#endif
+#define bcm_ismask(x)	(bcm_ctype[(int)(unsigned char)(x)])
+
+#define bcm_isalnum(c)	((bcm_ismask(c)&(_BCM_U|_BCM_L|_BCM_D)) != 0)
+#define bcm_isalpha(c)	((bcm_ismask(c)&(_BCM_U|_BCM_L)) != 0)
+#define bcm_iscntrl(c)	((bcm_ismask(c)&(_BCM_C)) != 0)
+#define bcm_isdigit(c)	((bcm_ismask(c)&(_BCM_D)) != 0)
+#define bcm_isgraph(c)	((bcm_ismask(c)&(_BCM_P|_BCM_U|_BCM_L|_BCM_D)) != 0)
+#define bcm_islower(c)	((bcm_ismask(c)&(_BCM_L)) != 0)
+#define bcm_isprint(c)	((bcm_ismask(c)&(_BCM_P|_BCM_U|_BCM_L|_BCM_D|_BCM_SP)) != 0)
+#define bcm_ispunct(c)	((bcm_ismask(c)&(_BCM_P)) != 0)
+#define bcm_isspace(c)	((bcm_ismask(c)&(_BCM_S)) != 0)
+#define bcm_isupper(c)	((bcm_ismask(c)&(_BCM_U)) != 0)
+#define bcm_isxdigit(c)	((bcm_ismask(c)&(_BCM_D|_BCM_X)) != 0)
+#define bcm_tolower(c)	(bcm_isupper((c)) ? ((c) + 'a' - 'A') : (c))
+#define bcm_toupper(c)	(bcm_islower((c)) ? ((c) + 'A' - 'a') : (c))
+
+/* Buffer structure for collecting string-formatted data
+* using bcm_bprintf() API.
+* Use bcm_binit() to initialize before use
+*/
+
+struct bcmstrbuf {
+	char *buf;	/* pointer to current position in origbuf */
+	unsigned int size;	/* current (residual) size in bytes */
+	char *origbuf;	/* unmodified pointer to orignal buffer */
+	unsigned int origsize;	/* unmodified orignal buffer size in bytes */
+};
+
+/* ** driver-only section ** */
+#ifdef BCMDRIVER
+#ifdef EFI
+/* forward declare structyre type */
+struct spktq;
+#endif
+#include <osl.h>
+
+#define GPIO_PIN_NOTDEFINED 	0x20	/* Pin not defined */
+
+/*
+ * Spin at most 'us' microseconds while 'exp' is true.
+ * Caller should explicitly test 'exp' when this completes
+ * and take appropriate error action if 'exp' is still true.
+ */
+#define SPINWAIT(exp, us) { \
+	uint countdown = (us) + 9; \
+	while ((exp) && (countdown >= 10)) {\
+		OSL_DELAY(10); \
+		countdown -= 10; \
+	} \
+}
+
+/* osl multi-precedence packet queue */
+#ifndef PKTQ_LEN_DEFAULT
+#define PKTQ_LEN_DEFAULT        128	/* Max 128 packets */
+#endif
+#ifndef PKTQ_MAX_PREC
+#define PKTQ_MAX_PREC           16	/* Maximum precedence levels */
+#endif
+
+typedef struct pktq_prec {
+	void *head;     /* first packet to dequeue */
+	void *tail;     /* last packet to dequeue */
+	uint16 len;     /* number of queued packets */
+	uint16 max;     /* maximum number of queued packets */
+} pktq_prec_t;
+
+#ifdef PKTQ_LOG
+typedef struct {
+	uint32 requested;    /* packets requested to be stored */
+	uint32 stored;	     /* packets stored */
+	uint32 saved;	     /* packets saved,
+	                            because a lowest priority queue has given away one packet
+	                      */
+	uint32 selfsaved;    /* packets saved,
+	                            because an older packet from the same queue has been dropped
+	                      */
+	uint32 full_dropped; /* packets dropped,
+	                            because pktq is full with higher precedence packets
+	                      */
+	uint32 dropped;      /* packets dropped because pktq per that precedence is full */
+	uint32 sacrificed;   /* packets dropped,
+	                            in order to save one from a queue of a highest priority
+	                      */
+	uint32 busy;         /* packets droped because of hardware/transmission error */
+	uint32 retry;        /* packets re-sent because they were not received */
+	uint32 ps_retry;     /* packets retried again prior to moving power save mode */
+	uint32 retry_drop;   /* packets finally dropped after retry limit */
+	uint32 max_avail;    /* the high-water mark of the queue capacity for packets -
+	                            goes to zero as queue fills
+	                      */
+	uint32 max_used;     /* the high-water mark of the queue utilisation for packets -
+						        increases with use ('inverse' of max_avail)
+				          */
+	uint32 queue_capacity; /* the maximum capacity of the queue */
+} pktq_counters_t;
+#endif /* PKTQ_LOG */
+
+
+#define PKTQ_COMMON	\
+	uint16 num_prec;        /* number of precedences in use */			\
+	uint16 hi_prec;         /* rapid dequeue hint (>= highest non-empty prec) */	\
+	uint16 max;             /* total max packets */					\
+	uint16 len;             /* total number of packets */
+
+/* multi-priority pkt queue */
+struct pktq {
+	PKTQ_COMMON
+	/* q array must be last since # of elements can be either PKTQ_MAX_PREC or 1 */
+	struct pktq_prec q[PKTQ_MAX_PREC];
+#ifdef PKTQ_LOG
+	pktq_counters_t	_prec_cnt[PKTQ_MAX_PREC];		/* Counters per queue  */
+#endif
+};
+
+/* simple, non-priority pkt queue */
+struct spktq {
+	PKTQ_COMMON
+	/* q array must be last since # of elements can be either PKTQ_MAX_PREC or 1 */
+	struct pktq_prec q[1];
+};
+
+#define PKTQ_PREC_ITER(pq, prec)        for (prec = (pq)->num_prec - 1; prec >= 0; prec--)
+
+/* fn(pkt, arg).  return true if pkt belongs to if */
+typedef bool (*ifpkt_cb_t)(void*, int);
+
+#ifdef BCMPKTPOOL
+#define POOL_ENAB(pool)		((pool) && (pool)->inited)
+#if defined(BCM4329C0)
+#define SHARED_POOL		(pktpool_shared_ptr)
+#else
+#define SHARED_POOL		(pktpool_shared)
+#endif /* BCM4329C0 */
+#else /* BCMPKTPOOL */
+#define POOL_ENAB(bus)		0
+#define SHARED_POOL		((struct pktpool *)NULL)
+#endif /* BCMPKTPOOL */
+
+#ifndef PKTPOOL_LEN_MAX
+#define PKTPOOL_LEN_MAX		40
+#endif /* PKTPOOL_LEN_MAX */
+#define PKTPOOL_CB_MAX		3
+
+struct pktpool;
+typedef void (*pktpool_cb_t)(struct pktpool *pool, void *arg);
+typedef struct {
+	pktpool_cb_t cb;
+	void *arg;
+} pktpool_cbinfo_t;
+
+#ifdef BCMDBG_POOL
+/* pkt pool debug states */
+#define POOL_IDLE	0
+#define POOL_RXFILL	1
+#define POOL_RXDH	2
+#define POOL_RXD11	3
+#define POOL_TXDH	4
+#define POOL_TXD11	5
+#define POOL_AMPDU	6
+#define POOL_TXENQ	7
+
+typedef struct {
+	void *p;
+	uint32 cycles;
+	uint32 dur;
+} pktpool_dbg_t;
+
+typedef struct {
+	uint8 txdh;	/* tx to host */
+	uint8 txd11;	/* tx to d11 */
+	uint8 enq;	/* waiting in q */
+	uint8 rxdh;	/* rx from host */
+	uint8 rxd11;	/* rx from d11 */
+	uint8 rxfill;	/* dma_rxfill */
+	uint8 idle;	/* avail in pool */
+} pktpool_stats_t;
+#endif /* BCMDBG_POOL */
+
+typedef struct pktpool {
+	bool inited;
+	uint16 r;
+	uint16 w;
+	uint16 len;
+	uint16 maxlen;
+	uint16 plen;
+	bool istx;
+	bool empty;
+	uint8 cbtoggle;
+	uint8 cbcnt;
+	uint8 ecbcnt;
+	bool emptycb_disable;
+	pktpool_cbinfo_t *availcb_excl;
+	pktpool_cbinfo_t cbs[PKTPOOL_CB_MAX];
+	pktpool_cbinfo_t ecbs[PKTPOOL_CB_MAX];
+	void *q[PKTPOOL_LEN_MAX + 1];
+
+#ifdef BCMDBG_POOL
+	uint8 dbg_cbcnt;
+	pktpool_cbinfo_t dbg_cbs[PKTPOOL_CB_MAX];
+	uint16 dbg_qlen;
+	pktpool_dbg_t dbg_q[PKTPOOL_LEN_MAX + 1];
+#endif
+} pktpool_t;
+
+#if defined(BCM4329C0)
+extern pktpool_t *pktpool_shared_ptr;
+#else
+extern pktpool_t *pktpool_shared;
+#endif /* BCM4329C0 */
+
+extern int pktpool_init(osl_t *osh, pktpool_t *pktp, int *pktplen, int plen, bool istx);
+extern int pktpool_deinit(osl_t *osh, pktpool_t *pktp);
+extern int pktpool_fill(osl_t *osh, pktpool_t *pktp, bool minimal);
+extern void* pktpool_get(pktpool_t *pktp);
+extern void pktpool_free(pktpool_t *pktp, void *p);
+extern int pktpool_add(pktpool_t *pktp, void *p);
+extern uint16 pktpool_avail(pktpool_t *pktp);
+extern int pktpool_avail_notify_normal(osl_t *osh, pktpool_t *pktp);
+extern int pktpool_avail_notify_exclusive(osl_t *osh, pktpool_t *pktp, pktpool_cb_t cb);
+extern int pktpool_avail_register(pktpool_t *pktp, pktpool_cb_t cb, void *arg);
+extern int pktpool_empty_register(pktpool_t *pktp, pktpool_cb_t cb, void *arg);
+extern int pktpool_setmaxlen(pktpool_t *pktp, uint16 maxlen);
+extern int pktpool_setmaxlen_strict(osl_t *osh, pktpool_t *pktp, uint16 maxlen);
+extern void pktpool_emptycb_disable(pktpool_t *pktp, bool disable);
+extern bool pktpool_emptycb_disabled(pktpool_t *pktp);
+
+#define POOLPTR(pp)			((pktpool_t *)(pp))
+#define pktpool_len(pp)			(POOLPTR(pp)->len - 1)
+#define pktpool_plen(pp)		(POOLPTR(pp)->plen)
+#define pktpool_maxlen(pp)		(POOLPTR(pp)->maxlen)
+
+#ifdef BCMDBG_POOL
+extern int pktpool_dbg_register(pktpool_t *pktp, pktpool_cb_t cb, void *arg);
+extern int pktpool_start_trigger(pktpool_t *pktp, void *p);
+extern int pktpool_dbg_dump(pktpool_t *pktp);
+extern int pktpool_dbg_notify(pktpool_t *pktp);
+extern int pktpool_stats_dump(pktpool_t *pktp, pktpool_stats_t *stats);
+#endif /* BCMDBG_POOL */
+
+/* forward definition of ether_addr structure used by some function prototypes */
+
+struct ether_addr;
+
+extern int ether_isbcast(const void *ea);
+extern int ether_isnulladdr(const void *ea);
+
+/* operations on a specific precedence in packet queue */
+
+#define pktq_psetmax(pq, prec, _max)	((pq)->q[prec].max = (_max))
+#define pktq_pmax(pq, prec)		((pq)->q[prec].max)
+#define pktq_plen(pq, prec)		((pq)->q[prec].len)
+#define pktq_pavail(pq, prec)		((pq)->q[prec].max - (pq)->q[prec].len)
+#define pktq_pfull(pq, prec)		((pq)->q[prec].len >= (pq)->q[prec].max)
+#define pktq_pempty(pq, prec)		((pq)->q[prec].len == 0)
+
+#define pktq_ppeek(pq, prec)		((pq)->q[prec].head)
+#define pktq_ppeek_tail(pq, prec)	((pq)->q[prec].tail)
+
+extern void *pktq_penq(struct pktq *pq, int prec, void *p);
+extern void *pktq_penq_head(struct pktq *pq, int prec, void *p);
+extern void *pktq_pdeq(struct pktq *pq, int prec);
+extern void *pktq_pdeq_prev(struct pktq *pq, int prec, void *prev_p);
+extern void *pktq_pdeq_tail(struct pktq *pq, int prec);
+/* Empty the queue at particular precedence level */
+extern void pktq_pflush(osl_t *osh, struct pktq *pq, int prec, bool dir,
+	ifpkt_cb_t fn, int arg);
+/* Remove a specified packet from its queue */
+extern bool pktq_pdel(struct pktq *pq, void *p, int prec);
+
+/* operations on a set of precedences in packet queue */
+
+extern int pktq_mlen(struct pktq *pq, uint prec_bmp);
+extern void *pktq_mdeq(struct pktq *pq, uint prec_bmp, int *prec_out);
+extern void *pktq_mpeek(struct pktq *pq, uint prec_bmp, int *prec_out);
+
+/* operations on packet queue as a whole */
+
+#define pktq_len(pq)		((int)(pq)->len)
+#define pktq_max(pq)		((int)(pq)->max)
+#define pktq_avail(pq)		((int)((pq)->max - (pq)->len))
+#define pktq_full(pq)		((pq)->len >= (pq)->max)
+#define pktq_empty(pq)		((pq)->len == 0)
+
+/* operations for single precedence queues */
+#define pktenq(pq, p)		pktq_penq(((struct pktq *)(void *)pq), 0, (p))
+#define pktenq_head(pq, p)	pktq_penq_head(((struct pktq *)(void *)pq), 0, (p))
+#define pktdeq(pq)		pktq_pdeq(((struct pktq *)(void *)pq), 0)
+#define pktdeq_tail(pq)		pktq_pdeq_tail(((struct pktq *)(void *)pq), 0)
+#define pktqinit(pq, len)	pktq_init(((struct pktq *)(void *)pq), 1, len)
+
+extern void pktq_init(struct pktq *pq, int num_prec, int max_len);
+extern void pktq_set_max_plen(struct pktq *pq, int prec, int max_len);
+
+/* prec_out may be NULL if caller is not interested in return value */
+extern void *pktq_deq(struct pktq *pq, int *prec_out);
+extern void *pktq_deq_tail(struct pktq *pq, int *prec_out);
+extern void *pktq_peek(struct pktq *pq, int *prec_out);
+extern void *pktq_peek_tail(struct pktq *pq, int *prec_out);
+extern void pktq_flush(osl_t *osh, struct pktq *pq, bool dir, ifpkt_cb_t fn, int arg);
+
+/* externs */
+/* packet */
+extern uint pktcopy(osl_t *osh, void *p, uint offset, int len, uchar *buf);
+extern uint pktfrombuf(osl_t *osh, void *p, uint offset, int len, uchar *buf);
+extern uint pkttotlen(osl_t *osh, void *p);
+extern void *pktlast(osl_t *osh, void *p);
+extern uint pktsegcnt(osl_t *osh, void *p);
+extern uint pktsegcnt_war(osl_t *osh, void *p);
+extern uint8 *pktdataoffset(osl_t *osh, void *p,  uint offset);
+extern void *pktoffset(osl_t *osh, void *p,  uint offset);
+
+/* Get priority from a packet and pass it back in scb (or equiv) */
+#define	PKTPRIO_VDSCP	0x100		/* DSCP prio found after VLAN tag */
+#define	PKTPRIO_VLAN	0x200		/* VLAN prio found */
+#define	PKTPRIO_UPD	0x400		/* DSCP used to update VLAN prio */
+#define	PKTPRIO_DSCP	0x800		/* DSCP prio found */
+
+extern uint pktsetprio(void *pkt, bool update_vtag);
+
+/* string */
+extern int BCMROMFN(bcm_atoi)(const char *s);
+extern ulong BCMROMFN(bcm_strtoul)(const char *cp, char **endp, uint base);
+extern char *BCMROMFN(bcmstrstr)(const char *haystack, const char *needle);
+extern char *BCMROMFN(bcmstrcat)(char *dest, const char *src);
+extern char *BCMROMFN(bcmstrncat)(char *dest, const char *src, uint size);
+extern ulong wchar2ascii(char *abuf, ushort *wbuf, ushort wbuflen, ulong abuflen);
+char* bcmstrtok(char **string, const char *delimiters, char *tokdelim);
+int bcmstricmp(const char *s1, const char *s2);
+int bcmstrnicmp(const char* s1, const char* s2, int cnt);
+
+
+/* ethernet address */
+extern char *bcm_ether_ntoa(const struct ether_addr *ea, char *buf);
+extern int BCMROMFN(bcm_ether_atoe)(const char *p, struct ether_addr *ea);
+
+/* ip address */
+struct ipv4_addr;
+extern char *bcm_ip_ntoa(struct ipv4_addr *ia, char *buf);
+
+/* delay */
+extern void bcm_mdelay(uint ms);
+/* variable access */
+#if defined(DONGLEBUILD) && !defined(WLTEST)
+#ifdef BCMDBG
+#define NVRAM_RECLAIM_CHECK(name)							\
+	if (attach_part_reclaimed == TRUE) {						\
+		printf("%s: NVRAM already reclaimed, %s\n", __FUNCTION__, (name));	\
+		*(char*) 0 = 0; /* TRAP */						\
+		return NULL;								\
+	}
+#else /* BCMDBG */
+#define NVRAM_RECLAIM_CHECK(name)							\
+	if (attach_part_reclaimed == TRUE) {						\
+		*(char*) 0 = 0; /* TRAP */						\
+		return NULL;								\
+	}
+#endif /* BCMDBG */
+#else /* DONGLEBUILD && !WLTEST && !BCMINTERNAL && !BCMDBG_DUMP */
+#define NVRAM_RECLAIM_CHECK(name)
+#endif
+
+extern char *getvar(char *vars, const char *name);
+extern int getintvar(char *vars, const char *name);
+extern int getintvararray(char *vars, const char *name, int index);
+extern int getintvararraysize(char *vars, const char *name);
+extern uint getgpiopin(char *vars, char *pin_name, uint def_pin);
+extern int getwanport(void);
+extern int getbrcmtag(void);
+#ifdef BCMDBG
+extern void prpkt(const char *msg, osl_t *osh, void *p0);
+#endif /* BCMDBG */
+#ifdef BCMPERFSTATS
+extern void bcm_perf_enable(void);
+extern void bcmstats(char *fmt);
+extern void bcmlog(char *fmt, uint a1, uint a2);
+extern void bcmdumplog(char *buf, int size);
+extern int bcmdumplogent(char *buf, uint idx);
+#else
+#define bcm_perf_enable()
+#define bcmstats(fmt)
+#define	bcmlog(fmt, a1, a2)
+#define	bcmdumplog(buf, size)	*buf = '\0'
+#define	bcmdumplogent(buf, idx)	-1
+#endif /* BCMPERFSTATS */
+
+#if defined(BCMTSTAMPEDLOGS)
+#define TSF_TICKS_PER_MS	1024
+/* Store a TSF timestamp and a log line in the log buffer */
+extern void bcmtslog(uint32 tstamp, char *fmt, uint a1, uint a2);
+/* Print out the log buffer with timestamps */
+extern void bcmprinttslogs(void);
+/* Print out a microsecond timestamp as "sec.ms.us " */
+extern void bcmprinttstamp(uint32 us);
+/* Dump to buffer a microsecond timestamp as "sec.ms.us " */
+extern void bcmdumptslog(char *buf, int size);
+#else
+#define bcmtslog(tstamp, fmt, a1, a2)
+#define bcmprinttslogs()
+#define bcmprinttstamp(us)
+#define bcmdumptslog(buf, size)
+#endif /* BCMTSTAMPEDLOGS */
+
+extern char *bcm_nvram_vars(uint *length);
+extern int bcm_nvram_cache(void *sih);
+
+/* Support for sharing code across in-driver iovar implementations.
+ * The intent is that a driver use this structure to map iovar names
+ * to its (private) iovar identifiers, and the lookup function to
+ * find the entry.  Macros are provided to map ids and get/set actions
+ * into a single number space for a switch statement.
+ */
+
+/* iovar structure */
+typedef struct bcm_iovar {
+	const char *name;	/* name for lookup and display */
+	uint16 varid;		/* id for switch */
+	uint16 flags;		/* driver-specific flag bits */
+	uint16 type;		/* base type of argument */
+	uint16 minlen;		/* min length for buffer vars */
+} bcm_iovar_t;
+
+/* varid definitions are per-driver, may use these get/set bits */
+
+/* IOVar action bits for id mapping */
+#define IOV_GET 0 /* Get an iovar */
+#define IOV_SET 1 /* Set an iovar */
+
+/* Varid to actionid mapping */
+#define IOV_GVAL(id)		((id) * 2)
+#define IOV_SVAL(id)		((id) * 2 + IOV_SET)
+#define IOV_ISSET(actionid)	((actionid & IOV_SET) == IOV_SET)
+#define IOV_ID(actionid)	(actionid >> 1)
+
+/* flags are per-driver based on driver attributes */
+
+extern const bcm_iovar_t *bcm_iovar_lookup(const bcm_iovar_t *table, const char *name);
+extern int bcm_iovar_lencheck(const bcm_iovar_t *table, void *arg, int len, bool set);
+#if defined(WLTINYDUMP) || defined(BCMDBG) || defined(WLMSG_INFORM) || \
+	defined(WLMSG_ASSOC) || defined(WLMSG_PRPKT) || defined(WLMSG_WSEC)
+extern int bcm_format_ssid(char* buf, const uchar ssid[], uint ssid_len);
+#endif /* WLTINYDUMP || BCMDBG || WLMSG_INFORM || WLMSG_ASSOC || WLMSG_PRPKT */
+#endif	/* BCMDRIVER */
+
+/* Base type definitions */
+#define IOVT_VOID	0	/* no value (implictly set only) */
+#define IOVT_BOOL	1	/* any value ok (zero/nonzero) */
+#define IOVT_INT8	2	/* integer values are range-checked */
+#define IOVT_UINT8	3	/* unsigned int 8 bits */
+#define IOVT_INT16	4	/* int 16 bits */
+#define IOVT_UINT16	5	/* unsigned int 16 bits */
+#define IOVT_INT32	6	/* int 32 bits */
+#define IOVT_UINT32	7	/* unsigned int 32 bits */
+#define IOVT_BUFFER	8	/* buffer is size-checked as per minlen */
+#define BCM_IOVT_VALID(type) (((unsigned int)(type)) <= IOVT_BUFFER)
+
+/* Initializer for IOV type strings */
+#define BCM_IOV_TYPE_INIT { \
+	"void", \
+	"bool", \
+	"int8", \
+	"uint8", \
+	"int16", \
+	"uint16", \
+	"int32", \
+	"uint32", \
+	"buffer", \
+	"" }
+
+#define BCM_IOVT_IS_INT(type) (\
+	(type == IOVT_BOOL) || \
+	(type == IOVT_INT8) || \
+	(type == IOVT_UINT8) || \
+	(type == IOVT_INT16) || \
+	(type == IOVT_UINT16) || \
+	(type == IOVT_INT32) || \
+	(type == IOVT_UINT32))
+
+/* ** driver/apps-shared section ** */
+
+#define BCME_STRLEN 		64	/* Max string length for BCM errors */
+#define VALID_BCMERROR(e)  ((e <= 0) && (e >= BCME_LAST))
+
+
+/*
+ * error codes could be added but the defined ones shouldn't be changed/deleted
+ * these error codes are exposed to the user code
+ * when ever a new error code is added to this list
+ * please update errorstring table with the related error string and
+ * update osl files with os specific errorcode map
+*/
+
+#define BCME_OK				0	/* Success */
+#define BCME_ERROR			-1	/* Error generic */
+#define BCME_BADARG			-2	/* Bad Argument */
+#define BCME_BADOPTION			-3	/* Bad option */
+#define BCME_NOTUP			-4	/* Not up */
+#define BCME_NOTDOWN			-5	/* Not down */
+#define BCME_NOTAP			-6	/* Not AP */
+#define BCME_NOTSTA			-7	/* Not STA  */
+#define BCME_BADKEYIDX			-8	/* BAD Key Index */
+#define BCME_RADIOOFF 			-9	/* Radio Off */
+#define BCME_NOTBANDLOCKED		-10	/* Not  band locked */
+#define BCME_NOCLK			-11	/* No Clock */
+#define BCME_BADRATESET			-12	/* BAD Rate valueset */
+#define BCME_BADBAND			-13	/* BAD Band */
+#define BCME_BUFTOOSHORT		-14	/* Buffer too short */
+#define BCME_BUFTOOLONG			-15	/* Buffer too long */
+#define BCME_BUSY			-16	/* Busy */
+#define BCME_NOTASSOCIATED		-17	/* Not Associated */
+#define BCME_BADSSIDLEN			-18	/* Bad SSID len */
+#define BCME_OUTOFRANGECHAN		-19	/* Out of Range Channel */
+#define BCME_BADCHAN			-20	/* Bad Channel */
+#define BCME_BADADDR			-21	/* Bad Address */
+#define BCME_NORESOURCE			-22	/* Not Enough Resources */
+#define BCME_UNSUPPORTED		-23	/* Unsupported */
+#define BCME_BADLEN			-24	/* Bad length */
+#define BCME_NOTREADY			-25	/* Not Ready */
+#define BCME_EPERM			-26	/* Not Permitted */
+#define BCME_NOMEM			-27	/* No Memory */
+#define BCME_ASSOCIATED			-28	/* Associated */
+#define BCME_RANGE			-29	/* Not In Range */
+#define BCME_NOTFOUND			-30	/* Not Found */
+#define BCME_WME_NOT_ENABLED		-31	/* WME Not Enabled */
+#define BCME_TSPEC_NOTFOUND		-32	/* TSPEC Not Found */
+#define BCME_ACM_NOTSUPPORTED		-33	/* ACM Not Supported */
+#define BCME_NOT_WME_ASSOCIATION	-34	/* Not WME Association */
+#define BCME_SDIO_ERROR			-35	/* SDIO Bus Error */
+#define BCME_DONGLE_DOWN		-36	/* Dongle Not Accessible */
+#define BCME_VERSION			-37 	/* Incorrect version */
+#define BCME_TXFAIL			-38 	/* TX failure */
+#define BCME_RXFAIL			-39	/* RX failure */
+#define BCME_NODEVICE			-40 	/* Device not present */
+#define BCME_NMODE_DISABLED		-41 	/* NMODE disabled */
+#define BCME_NONRESIDENT		-42 /* access to nonresident overlay */
+#define BCME_LAST			BCME_NONRESIDENT
+
+/* These are collection of BCME Error strings */
+#define BCMERRSTRINGTABLE {		\
+	"OK",				\
+	"Undefined error",		\
+	"Bad Argument",			\
+	"Bad Option",			\
+	"Not up",			\
+	"Not down",			\
+	"Not AP",			\
+	"Not STA",			\
+	"Bad Key Index",		\
+	"Radio Off",			\
+	"Not band locked",		\
+	"No clock",			\
+	"Bad Rate valueset",		\
+	"Bad Band",			\
+	"Buffer too short",		\
+	"Buffer too long",		\
+	"Busy",				\
+	"Not Associated",		\
+	"Bad SSID len",			\
+	"Out of Range Channel",		\
+	"Bad Channel",			\
+	"Bad Address",			\
+	"Not Enough Resources",		\
+	"Unsupported",			\
+	"Bad length",			\
+	"Not Ready",			\
+	"Not Permitted",		\
+	"No Memory",			\
+	"Associated",			\
+	"Not In Range",			\
+	"Not Found",			\
+	"WME Not Enabled",		\
+	"TSPEC Not Found",		\
+	"ACM Not Supported",		\
+	"Not WME Association",		\
+	"SDIO Bus Error",		\
+	"Dongle Not Accessible",	\
+	"Incorrect version",		\
+	"TX Failure",			\
+	"RX Failure",			\
+	"Device Not Present",		\
+	"NMODE Disabled",		\
+	"Nonresident overlay access", \
+}
+
+#ifndef ABS
+#define	ABS(a)			(((a) < 0) ? -(a) : (a))
+#endif /* ABS */
+
+#ifndef MIN
+#define	MIN(a, b)		(((a) < (b)) ? (a) : (b))
+#endif /* MIN */
+
+#ifndef MAX
+#define	MAX(a, b)		(((a) > (b)) ? (a) : (b))
+#endif /* MAX */
+
+#define CEIL(x, y)		(((x) + ((y) - 1)) / (y))
+#define	ROUNDUP(x, y)		((((x) + ((y) - 1)) / (y)) * (y))
+#define	ISALIGNED(a, x)		(((uintptr)(a) & ((x) - 1)) == 0)
+#define ALIGN_ADDR(addr, boundary) (void *)(((uintptr)(addr) + (boundary) - 1) \
+	                                         & ~((boundary) - 1))
+#define ALIGN_SIZE(size, boundary) (((size) + (boundary) - 1) \
+	                                         & ~((boundary) - 1))
+#define	ISPOWEROF2(x)		((((x) - 1) & (x)) == 0)
+#define VALID_MASK(mask)	!((mask) & ((mask) + 1))
+
+#ifndef OFFSETOF
+#ifdef __ARMCC_VERSION
+/*
+ * The ARM RVCT compiler complains when using OFFSETOF where a constant
+ * expression is expected, such as an initializer for a static object.
+ * offsetof from the runtime library doesn't have that problem.
+ */
+#include <stddef.h>
+#define	OFFSETOF(type, member)	offsetof(type, member)
+#else
+#define	OFFSETOF(type, member)	((uint)(uintptr)&((type *)0)->member)
+#endif /* __ARMCC_VERSION */
+#endif /* OFFSETOF */
+
+#ifndef ARRAYSIZE
+#define ARRAYSIZE(a)		(sizeof(a) / sizeof(a[0]))
+#endif
+
+/* Reference a function; used to prevent a static function from being optimized out */
+extern void *_bcmutils_dummy_fn;
+#define REFERENCE_FUNCTION(f)	(_bcmutils_dummy_fn = (void *)(f))
+
+/* bit map related macros */
+#ifndef setbit
+#ifndef NBBY		  /* the BSD family defines NBBY */
+#define	NBBY	8	/* 8 bits per byte */
+#endif /* #ifndef NBBY */
+#define	setbit(a, i)	(((uint8 *)a)[(i) / NBBY] |= 1 << ((i) % NBBY))
+#define	clrbit(a, i)	(((uint8 *)a)[(i) / NBBY] &= ~(1 << ((i) % NBBY)))
+#define	isset(a, i)	(((const uint8 *)a)[(i) / NBBY] & (1 << ((i) % NBBY)))
+#define	isclr(a, i)	((((const uint8 *)a)[(i) / NBBY] & (1 << ((i) % NBBY))) == 0)
+#endif /* setbit */
+
+#define	NBITS(type)	(sizeof(type) * 8)
+#define NBITVAL(nbits)	(1 << (nbits))
+#define MAXBITVAL(nbits)	((1 << (nbits)) - 1)
+#define	NBITMASK(nbits)	MAXBITVAL(nbits)
+#define MAXNBVAL(nbyte)	MAXBITVAL((nbyte) * 8)
+
+/* basic mux operation - can be optimized on several architectures */
+#define MUX(pred, true, false) ((pred) ? (true) : (false))
+
+/* modulo inc/dec - assumes x E [0, bound - 1] */
+#define MODDEC(x, bound) MUX((x) == 0, (bound) - 1, (x) - 1)
+#define MODINC(x, bound) MUX((x) == (bound) - 1, 0, (x) + 1)
+
+/* modulo inc/dec, bound = 2^k */
+#define MODDEC_POW2(x, bound) (((x) - 1) & ((bound) - 1))
+#define MODINC_POW2(x, bound) (((x) + 1) & ((bound) - 1))
+
+/* modulo add/sub - assumes x, y E [0, bound - 1] */
+#define MODADD(x, y, bound) \
+    MUX((x) + (y) >= (bound), (x) + (y) - (bound), (x) + (y))
+#define MODSUB(x, y, bound) \
+    MUX(((int)(x)) - ((int)(y)) < 0, (x) - (y) + (bound), (x) - (y))
+
+/* module add/sub, bound = 2^k */
+#define MODADD_POW2(x, y, bound) (((x) + (y)) & ((bound) - 1))
+#define MODSUB_POW2(x, y, bound) (((x) - (y)) & ((bound) - 1))
+
+/* crc defines */
+#define CRC8_INIT_VALUE  0xff		/* Initial CRC8 checksum value */
+#define CRC8_GOOD_VALUE  0x9f		/* Good final CRC8 checksum value */
+#define CRC16_INIT_VALUE 0xffff		/* Initial CRC16 checksum value */
+#define CRC16_GOOD_VALUE 0xf0b8		/* Good final CRC16 checksum value */
+#define CRC32_INIT_VALUE 0xffffffff	/* Initial CRC32 checksum value */
+#define CRC32_GOOD_VALUE 0xdebb20e3	/* Good final CRC32 checksum value */
+
+/* use for direct output of MAC address in printf etc */
+#define MACF				"%02x:%02x:%02x:%02x:%02x:%02x"
+#define ETHERP_TO_MACF(ea)	((struct ether_addr *) (ea))->octet[0], \
+							((struct ether_addr *) (ea))->octet[1], \
+							((struct ether_addr *) (ea))->octet[2], \
+							((struct ether_addr *) (ea))->octet[3], \
+							((struct ether_addr *) (ea))->octet[4], \
+							((struct ether_addr *) (ea))->octet[5]
+
+#define ETHER_TO_MACF(ea) 	(ea).octet[0], \
+							(ea).octet[1], \
+							(ea).octet[2], \
+							(ea).octet[3], \
+							(ea).octet[4], \
+							(ea).octet[5]
+
+/* bcm_format_flags() bit description structure */
+typedef struct bcm_bit_desc {
+	uint32	bit;
+	const char* name;
+} bcm_bit_desc_t;
+
+/* tag_ID/length/value_buffer tuple */
+typedef struct bcm_tlv {
+	uint8	id;
+	uint8	len;
+	uint8	data[1];
+} bcm_tlv_t;
+
+/* Check that bcm_tlv_t fits into the given buflen */
+#define bcm_valid_tlv(elt, buflen) ((buflen) >= 2 && (int)(buflen) >= (int)(2 + (elt)->len))
+
+/* buffer length for ethernet address from bcm_ether_ntoa() */
+#define ETHER_ADDR_STR_LEN	18	/* 18-bytes of Ethernet address buffer length */
+
+/* crypto utility function */
+/* 128-bit xor: *dst = *src1 xor *src2. dst1, src1 and src2 may have any alignment */
+static INLINE void
+xor_128bit_block(const uint8 *src1, const uint8 *src2, uint8 *dst)
+{
+	if (
+#ifdef __i386__
+	    1 ||
+#endif
+	    (((uintptr)src1 | (uintptr)src2 | (uintptr)dst) & 3) == 0) {
+		/* ARM CM3 rel time: 1229 (727 if alignment check could be omitted) */
+		/* x86 supports unaligned.  This version runs 6x-9x faster on x86. */
+		((uint32 *)dst)[0] = ((const uint32 *)src1)[0] ^ ((const uint32 *)src2)[0];
+		((uint32 *)dst)[1] = ((const uint32 *)src1)[1] ^ ((const uint32 *)src2)[1];
+		((uint32 *)dst)[2] = ((const uint32 *)src1)[2] ^ ((const uint32 *)src2)[2];
+		((uint32 *)dst)[3] = ((const uint32 *)src1)[3] ^ ((const uint32 *)src2)[3];
+	} else {
+		/* ARM CM3 rel time: 4668 (4191 if alignment check could be omitted) */
+		int k;
+		for (k = 0; k < 16; k++)
+			dst[k] = src1[k] ^ src2[k];
+	}
+}
+
+/* externs */
+/* crc */
+extern uint8 BCMROMFN(hndcrc8)(uint8 *p, uint nbytes, uint8 crc);
+extern uint16 BCMROMFN(hndcrc16)(uint8 *p, uint nbytes, uint16 crc);
+extern uint32 BCMROMFN(hndcrc32)(uint8 *p, uint nbytes, uint32 crc);
+
+/* format/print */
+#if defined(BCMDBG) || defined(DHD_DEBUG) || defined(BCMDBG_ERR) || \
+	defined(WLMSG_PRHDRS) || defined(WLMSG_PRPKT) || defined(WLMSG_ASSOC)
+extern int bcm_format_flags(const bcm_bit_desc_t *bd, uint32 flags, char* buf, int len);
+#endif
+
+#if defined(BCMDBG) || defined(DHD_DEBUG) || defined(BCMDBG_ERR) || \
+	defined(WLMSG_PRHDRS) || defined(WLMSG_PRPKT) || defined(WLMSG_ASSOC) || \
+	defined(WLMEDIA_PEAKRATE)
+extern int bcm_format_hex(char *str, const void *bytes, int len);
+#endif
+
+#ifdef BCMDBG
+extern void deadbeef(void *p, size_t len);
+#endif
+extern const char *bcm_crypto_algo_name(uint algo);
+extern char *bcm_chipname(uint chipid, char *buf, uint len);
+extern char *bcm_brev_str(uint32 brev, char *buf);
+extern void printbig(char *buf);
+extern void prhex(const char *msg, uchar *buf, uint len);
+
+/* IE parsing */
+extern bcm_tlv_t *BCMROMFN(bcm_next_tlv)(bcm_tlv_t *elt, int *buflen);
+extern bcm_tlv_t *BCMROMFN(bcm_parse_tlvs)(void *buf, int buflen, uint key);
+extern bcm_tlv_t *BCMROMFN(bcm_parse_ordered_tlvs)(void *buf, int buflen, uint key);
+
+/* bcmerror */
+extern const char *bcmerrorstr(int bcmerror);
+extern bcm_tlv_t *BCMROMFN(bcm_parse_tlvs)(void *buf, int buflen, uint key);
+
+/* multi-bool data type: set of bools, mbool is true if any is set */
+typedef uint32 mbool;
+#define mboolset(mb, bit)		((mb) |= (bit))		/* set one bool */
+#define mboolclr(mb, bit)		((mb) &= ~(bit))	/* clear one bool */
+#define mboolisset(mb, bit)		(((mb) & (bit)) != 0)	/* TRUE if one bool is set */
+#define	mboolmaskset(mb, mask, val)	((mb) = (((mb) & ~(mask)) | (val)))
+
+/* generic datastruct to help dump routines */
+struct fielddesc {
+	const char *nameandfmt;
+	uint32 	offset;
+	uint32 	len;
+};
+
+extern void bcm_binit(struct bcmstrbuf *b, char *buf, uint size);
+extern void bcm_bprhex(struct bcmstrbuf *b, const char *msg, bool newline, uint8 *buf, int len);
+
+extern void bcm_inc_bytes(uchar *num, int num_bytes, uint8 amount);
+extern int bcm_cmp_bytes(const uchar *arg1, const uchar *arg2, uint8 nbytes);
+extern void bcm_print_bytes(const char *name, const uchar *cdata, int len);
+
+typedef  uint32 (*bcmutl_rdreg_rtn)(void *arg0, uint arg1, uint32 offset);
+extern uint bcmdumpfields(bcmutl_rdreg_rtn func_ptr, void *arg0, uint arg1, struct fielddesc *str,
+                          char *buf, uint32 bufsize);
+extern uint BCMROMFN(bcm_bitcount)(uint8 *bitmap, uint bytelength);
+
+extern int bcm_bprintf(struct bcmstrbuf *b, const char *fmt, ...);
+
+/* power conversion */
+extern uint16 BCMROMFN(bcm_qdbm_to_mw)(uint8 qdbm);
+extern uint8 BCMROMFN(bcm_mw_to_qdbm)(uint16 mw);
+
+extern int32 exthdr_validate(char *ptr, uint size);
+extern uint bcm_mkiovar(char *name, char *data, uint datalen, char *buf, uint len);
+
+unsigned int process_nvram_vars(char *varbuf, unsigned int len);
+
+#ifdef __cplusplus
+	}
+#endif
+
+#endif	/* _bcmutils_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmwifi.h b/drivers/bcmdrivers/gmac/src/include/bcmwifi.h
new file mode 100755
index 0000000..1470332
