--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmenetrxh.h
@@ -0,0 +1,50 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Hardware-specific Receive Data Header for the
+ * Broadcom Home Networking Division
+ * BCM44XX and BCM47XX 10/100 Mbps Ethernet cores.
+ *
+ * $Id: bcmenetrxh.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef _bcmenetrxh_h_
+#define	_bcmenetrxh_h_
+
+/*
+ * The Ethernet MAC core returns an 8-byte Receive Frame Data Header
+ * with every frame consisting of
+ * 16bits of frame length, followed by
+ * 16bits of EMAC rx descriptor info, followed by 32bits of undefined.
+ */
+typedef volatile struct {
+	uint16	len;
+	uint16	flags;
+	uint16	pad[12];
+} bcmenetrxh_t;
+
+#define	RXHDR_LEN	28	/* Header length */
+
+#define	RXF_L		((uint16)1 << 11)	/* last buffer in a frame */
+#define	RXF_MISS	((uint16)1 << 7)	/* received due to promisc mode */
+#define	RXF_BRDCAST	((uint16)1 << 6)	/* dest is broadcast address */
+#define	RXF_MULT	((uint16)1 << 5)	/* dest is multicast address */
+#define	RXF_LG		((uint16)1 << 4)	/* frame length > rxmaxlength */
+#define	RXF_NO		((uint16)1 << 3)	/* odd number of nibbles */
+#define	RXF_RXER	((uint16)1 << 2)	/* receive symbol error */
+#define	RXF_CRC		((uint16)1 << 1)	/* crc error */
+#define	RXF_OV		((uint16)1 << 0)	/* fifo overflow */
+
+#endif	/* _bcmenetrxh_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmgmacmib.h b/drivers/bcmdrivers/gmac/src/include/bcmgmacmib.h
new file mode 100755
index 0000000..6f0cf09
