/*
 * P2020 RDB Device Tree Source
 *
 * Copyright 2009-2010 Freescale Semiconductor Inc.
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/dts-v1/;
/ {
	model = "powerpc-as5610-52x";
	compatible = "fsl,P2020RDB";
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		ethernet0 = &enet0;
		/* ethernet1 = &enet1;
		ethernet2 = &enet2; */
		serial0 = &serial0;
		serial1 = &serial1;
		pci0 = &pci0;
		pci1 = &pci1;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		PowerPC,P2020@0 {
			device_type = "cpu";
			reg = <0x0>;
			next-level-cache = <&L2>;
		};

		PowerPC,P2020@1 {
			device_type = "cpu";
			reg = <0x1>;
			next-level-cache = <&L2>;
		};
	};

	memory {
		device_type = "memory";
	};

	localbus@ff705000 {
		#address-cells = <2>;
		#size-cells = <1>;
		compatible = "fsl,p2020-elbc", "fsl,elbc", "simple-bus";
		reg = <0 0xff705000 0 0x1000>;
		interrupts = <19 2>;
		interrupt-parent = <&mpic>;

		/* NOR and CPLD, nvram, FPGA */
		ranges = <0x0 0x0 0x0 0xefc00000 0x00400000>;
		nor@0,0 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "cfi-flash";
			reg = <0x0 0x0 0x400000>;
			bank-width = <1>;       /* 1 = 64KB on each erase block */
			device-width = <1>;

			partition@0 {
				/* 3.3 MB for Linux Kernel Image */
				reg = <0x0 0x00360000>;
				label = "onie";
			};

			partition@360000 {
				/* 64 KB for u-boot environment */
				reg = <0x360000 0x00010000>;
				label = "u-boot environment";
			};

			partition@370000 {
				/* 64 KB for VPD */
				reg = <0x00370000 0x00010000>;
				label = "board_eeprom";
				read-only;
			};

			partition@380000 {
				/* 512 KB for bootloader */
				reg = <0x00380000 0x00080000>;
				label = "uboot";
				read-only;
			};
		};


	};

	soc@ff700000 {
		#address-cells = <1>;
		#size-cells = <1>;
		device_type = "soc";
		compatible = "fsl,p2020-immr", "simple-bus";
		ranges = <0x0  0x0 0xff700000 0x100000>;
		bus-frequency = <0>;		// Filled out by uboot.

		ecm-law@0 {
			compatible = "fsl,ecm-law";
			reg = <0x0 0x1000>;
			fsl,num-laws = <12>;
		};

		ecm@1000 {
			compatible = "fsl,p2020-ecm", "fsl,ecm";
			reg = <0x1000 0x1000>;
			interrupts = <17 2>;
			interrupt-parent = <&mpic>;
		};

		memory-controller@2000 {
			compatible = "fsl,p2020-memory-controller";
			reg = <0x2000 0x1000>;
			interrupt-parent = <&mpic>;
			interrupts = <18 2>;
		};

		i2c@3000 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <0>;
			compatible = "fsl-i2c";
			reg = <0x3000 0x100>;
			interrupts = <43 2>;
			interrupt-parent = <&mpic>;
			dfsrr;

            mux@70 {
                compatible = "nxp,pca9548";
                reg = <0x70>;
                #address-cells = <1>;
                #size-cells = <0>;

                i2c@0 {
                    #address-cells = <1>;
                    #size-cells = <0>;
                    reg = <0>;

                    rtc@51 {
                        compatible = "nxp,pcf8563";
                        reg = <0x51>;
                    };
                };
			};
		};

		i2c@3100 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <1>;
			compatible = "fsl-i2c";
			reg = <0x3100 0x100>;
			interrupts = <43 2>;
			interrupt-parent = <&mpic>;
			dfsrr;
		};

		serial0: serial@4500 {
			cell-index = <0>;
			device_type = "serial";
			compatible = "ns16550";
			reg = <0x4500 0x100>;
			clock-frequency = <0>;
			interrupts = <42 2>;
			interrupt-parent = <&mpic>;
		};

		serial1: serial@4600 {
			cell-index = <1>;
			device_type = "serial";
			compatible = "ns16550";
			reg = <0x4600 0x100>;
			clock-frequency = <0>;
			interrupts = <42 2>;
			interrupt-parent = <&mpic>;
		};

		spi@7000 {
			cell-index = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "fsl,espi";
			reg = <0x7000 0x1000>;
			interrupts = <59 0x2>;
			interrupt-parent = <&mpic>;
			mode = "cpu";

			fsl_m25p80@0 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "fsl,espi-flash";
				reg = <0>;
				linux,modalias = "fsl_m25p80";
				modal = "s25sl128b";
				spi-max-frequency = <32000000>;
				mode = <0>;

				partition@0 {
					/* 512KB for u-boot Bootloader Image */
					reg = <0x0 0x00080000>;
					label = "SPI (RO) U-Boot Image";
					read-only;
				};

				partition@80000 {
					/* 512KB for DTB Image */
					reg = <0x00080000 0x00080000>;
					label = "SPI (RO) DTB Image";
					read-only;
				};

				partition@100000 {
					/* 4MB for Linux Kernel Image */
					reg = <0x00100000 0x00400000>;
					label = "SPI (RO) Linux Kernel Image";
					read-only;
				};

				partition@500000 {
					/* 4MB for Compressed RFS Image */
					reg = <0x00500000 0x00400000>;
					label = "SPI (RO) Compressed RFS Image";
					read-only;
				};

				partition@900000 {
					/* 7MB for JFFS2 based RFS */
					reg = <0x00900000 0x00700000>;
					label = "SPI (RW) JFFS2 RFS";
				};
			};
		};

		dma@c300 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,eloplus-dma";
			reg = <0xc300 0x4>;
			ranges = <0x0 0xc100 0x200>;
			cell-index = <1>;
			dma-channel@0 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x0 0x80>;
				cell-index = <0>;
				interrupt-parent = <&mpic>;
				interrupts = <76 2>;
			};
			dma-channel@80 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x80 0x80>;
				cell-index = <1>;
				interrupt-parent = <&mpic>;
				interrupts = <77 2>;
			};
			dma-channel@100 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x100 0x80>;
				cell-index = <2>;
				interrupt-parent = <&mpic>;
				interrupts = <78 2>;
			};
			dma-channel@180 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x180 0x80>;
				cell-index = <3>;
				interrupt-parent = <&mpic>;
				interrupts = <79 2>;
			};
		};

		gpio: gpio-controller@f000 {
			#gpio-cells = <2>;
			compatible = "fsl,mpc8572-gpio";
			reg = <0xf000 0x100>;
			interrupts = <47 0x2>;
			interrupt-parent = <&mpic>;
			gpio-controller;
		};

		L2: l2-cache-controller@20000 {
			compatible = "fsl,p2020-l2-cache-controller";
			reg = <0x20000 0x1000>;
			cache-line-size = <32>;	// 32 bytes
			cache-size = <0x80000>; // L2,512K
			interrupt-parent = <&mpic>;
			interrupts = <16 2>;
		};

		dma@21300 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,eloplus-dma";
			reg = <0x21300 0x4>;
			ranges = <0x0 0x21100 0x200>;
			cell-index = <0>;
			dma-channel@0 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x0 0x80>;
				cell-index = <0>;
				interrupt-parent = <&mpic>;
				interrupts = <20 2>;
			};
			dma-channel@80 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x80 0x80>;
				cell-index = <1>;
				interrupt-parent = <&mpic>;
				interrupts = <21 2>;
			};
			dma-channel@100 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x100 0x80>;
				cell-index = <2>;
				interrupt-parent = <&mpic>;
				interrupts = <22 2>;
			};
			dma-channel@180 {
				compatible = "fsl,eloplus-dma-channel";
				reg = <0x180 0x80>;
				cell-index = <3>;
				interrupt-parent = <&mpic>;
				interrupts = <23 2>;
			};
		};

		usb@22000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "fsl-usb2-dr";
			reg = <0x22000 0x1000>;
			interrupt-parent = <&mpic>;
			interrupts = <28 0x2>;
			phy_type = "ulpi";
		};
/* No ptp_timer
		ptp_timer: ptimer@24e00 {
			compatible = "fsl,gianfar-ptp-timer";
			reg = <0x24e00 0xb0>;
		};
*/
		enet0: ethernet@24000 {
			#address-cells = <1>;
			#size-cells = <1>;
			cell-index = <0>;
			device_type = "network";
			model = "eTSEC";
			compatible = "gianfar";
			reg = <0x24000 0x1000>;
			ranges = <0x0 0x24000 0x1000>;
			local-mac-address = [ 00 00 00 00 00 00 ];
			interrupts = <29 2 30 2 34 2>;
			interrupt-parent = <&mpic>;
			fixed-link = <1 1 1000 0 0>;
			phy-handle = <&phy1>;
			phy-connection-type = "rgmii-id";
			/* ptimer-handle = <&ptp_timer>; */

			mdio@520 {
				#address-cells = <1>;
				#size-cells = <0>;
				device_type = "mdio";
				compatible = "fsl,gianfar-mdio";
				reg = <0x520 0x20>;
/*
				phy0: ethernet-phy@0 {
					interrupt-parent = <&mpic>;
					interrupts = <3 1>;
					reg = <0x0>;
				};
*/
				phy1: ethernet-phy@1 {
					reg = <0x1>;
					device_type = "ethernet-phy";
					linux,phandle = <0x4>;
				};
			};
		};
/* not used !
		enet1: ethernet@25000 {
			#address-cells = <1>;
			#size-cells = <1>;
			cell-index = <1>;
			device_type = "network";
			model = "eTSEC";
			compatible = "gianfar";
			reg = <0x25000 0x1000>;
			ranges = <0x0 0x25000 0x1000>;
			local-mac-address = [ 00 00 00 00 00 00 ];
			interrupts = <35 2 36 2 40 2>;
			interrupt-parent = <&mpic>;
			tbi-handle = <&tbi0>;
			phy-handle = <&phy0>;
			phy-connection-type = "sgmii";
			ptimer-handle = <&ptp_timer>;

			mdio@520 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,gianfar-tbi";
				reg = <0x520 0x20>;

				tbi0: tbi-phy@11 {
					reg = <0x11>;
					device_type = "tbi-phy";
				};
			};
		};

		enet2: ethernet@26000 {
			#address-cells = <1>;
			#size-cells = <1>;
			cell-index = <2>;
			device_type = "network";
			model = "eTSEC";
			compatible = "gianfar";
			reg = <0x26000 0x1000>;
			ranges = <0x0 0x26000 0x1000>;
			local-mac-address = [ 00 00 00 00 00 00 ];
			interrupts = <31 2 32 2 33 2>;
			interrupt-parent = <&mpic>;
			phy-handle = <&phy1>;
			phy-connection-type = "rgmii-id";
			ptimer-handle = <&ptp_timer>;
		};
*/

		sdhci@2e000 {
			compatible = "fsl,p2020-esdhc", "fsl,esdhc";
			reg = <0x2e000 0x1000>;
			interrupts = <72 0x2>;
			interrupt-parent = <&mpic>;
			fsl,sdhci-adjust-timeout;
			/* Filled in by U-Boot */
			clock-frequency = <0>;
		};

		crypto@30000 {
			compatible = "fsl,sec3.1", "fsl,sec3.0", "fsl,sec2.4",
				     "fsl,sec2.2", "fsl,sec2.1", "fsl,sec2.0";
			reg = <0x30000 0x10000>;
			interrupts = <45 2 58 2>;
			interrupt-parent = <&mpic>;
			fsl,num-channels = <4>;
			fsl,channel-fifo-len = <24>;
			fsl,exec-units-mask = <0xbfe>;
			fsl,descriptor-types-mask = <0x3ab0ebf>;
			fsl,multi-host-mode = "dual";
			fsl,channel-remap = <0x3>;
		};

		mpic: pic@40000 {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <2>;
			reg = <0x40000 0x40000>;
			compatible = "chrp,open-pic";
			device_type = "open-pic";
		};

		message@41400 {
			compatible = "fsl,p2020-msg", "fsl,mpic-msg";
			reg = <0x41400 0x200>;
			interrupts = <
				0xb0 2
				0xb1 2
				0xb2 2
				0xb3 2>;
			interrupt-parent = <&mpic>;
		};

		message@42400 {
			compatible = "fsl,p2020-msg", "fsl,mpic-msg";
			reg = <0x42400 0x200>;
			interrupts = <
				0xb4 2
				0xb5 2
				0xb6 2
				0xb7 2>;
			interrupt-parent = <&mpic>;
		};

		msi@41600 {
			compatible = "fsl,p2020-msi", "fsl,mpic-msi";
			reg = <0x41600 0x80>;
			msi-available-ranges = <0 0x100>;
			interrupts = <
				0xe0 0
				0xe1 0
				0xe2 0
				0xe3 0
				0xe4 0
				0xe5 0
				0xe6 0
				0xe7 0>;
			interrupt-parent = <&mpic>;
		};

		global-utilities@e0000 {	//global utilities block
			compatible = "fsl,p2020-guts";
			reg = <0xe0000 0x1000>;
			fsl,has-rstcr;
		};
	};

	pci0: pcie@ff709000 {
		cell-index = <1>;
		compatible = "fsl,mpc8548-pcie";
		device_type = "pci";
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		reg = <0 0xff709000 0 0x1000>;
		bus-range = <0 255>;
		ranges = <0x2000000 0x0 0xc0000000 0 0xc0000000 0x0 0x20000000
			  0x1000000 0x0 0x00000000 0 0xffc30000 0x0 0x10000>;
		clock-frequency = <33333333>;
		interrupt-parent = <&mpic>;
		interrupts = <25 2>;
		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
		interrupt-map = <
			/* IDSEL 0x0 */
			0000 0x0 0x0 0x1 &mpic 0x4 0x1
			0000 0x0 0x0 0x2 &mpic 0x5 0x1
			0000 0x0 0x0 0x3 &mpic 0x6 0x1
			0000 0x0 0x0 0x4 &mpic 0x7 0x1
			>;
		pcie@0 {
			reg = <0x0 0x0 0x0 0x0 0x0>;
			#size-cells = <2>;
			#address-cells = <3>;
			device_type = "pci";
			ranges = <0x2000000 0x0 0xc0000000
				  0x2000000 0x0 0xc0000000
				  0x0 0x20000000
				  0x1000000 0x0 0x0
				  0x1000000 0x0 0x0
				  0x0 0x100000>;
		};
	};
	pci1: pcie@ff70a000 {
		cell-index = <2>;
		compatible = "fsl,mpc8548-pcie";
		device_type = "pci";
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		reg = <0 0xff70a000 0 0x1000>;
		bus-range = <0 255>;
		ranges = <0x2000000 0x0 0xa0000000 0 0xa0000000 0x0 0x20000000
			  0x1000000 0x0 0x00000000 0 0xffc20000 0x0 0x10000>;
		clock-frequency = <33333333>;
		interrupt-parent = <&mpic>;
		interrupts = <26 2>;
		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
		interrupt-map = <
			/* IDSEL 0x0 */
			0000 0x0 0x0 0x1 &mpic 0x0 0x1
			0000 0x0 0x0 0x2 &mpic 0x1 0x1
			0000 0x0 0x0 0x3 &mpic 0x2 0x1
			0000 0x0 0x0 0x4 &mpic 0x3 0x1
			>;
		pcie@0 {
			reg = <0x0 0x0 0x0 0x0 0x0>;
			#size-cells = <2>;
			#address-cells = <3>;
			device_type = "pci";
			ranges = <0x2000000 0x0 0xc0000000
				  0x2000000 0x0 0xc0000000
				  0x0 0x20000000
				  0x1000000 0x0 0x0
				  0x1000000 0x0 0x0
				  0x0 0x100000>;
		};
	};

};
