--- /dev/null
+++ b/arch/arm/net/bpf_jit_32.c
@@ -0,0 +1,915 @@
+/*
+ * Just-In-Time compiler for BPF filters on 32bit ARM
+ *
+ * Copyright (c) 2011 Mircea Gherzan <mgherzan@gmail.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; version 2 of the License.
+ */
+
+#include <linux/bitops.h>
+#include <linux/compiler.h>
+#include <linux/errno.h>
+#include <linux/filter.h>
+#include <linux/moduleloader.h>
+#include <linux/netdevice.h>
+#include <linux/string.h>
+#include <linux/slab.h>
+#include <asm/cacheflush.h>
+#include <asm/hwcap.h>
+
+#include "bpf_jit_32.h"
+
+/*
+ * ABI:
+ *
+ * r0	scratch register
+ * r4	BPF register A
+ * r5	BPF register X
+ * r6	pointer to the skb
+ * r7	skb->data
+ * r8	skb_headlen(skb)
+ */
+
+#define r_scratch	ARM_R0
+/* r1-r3 are (also) used for the unaligned loads on the non-ARMv7 slowpath */
+#define r_off		ARM_R1
+#define r_A		ARM_R4
+#define r_X		ARM_R5
+#define r_skb		ARM_R6
+#define r_skb_data	ARM_R7
+#define r_skb_hl	ARM_R8
+
+#define SCRATCH_SP_OFFSET	0
+#define SCRATCH_OFF(k)		(SCRATCH_SP_OFFSET + (k))
+
+#define SEEN_MEM		((1 << BPF_MEMWORDS) - 1)
+#define SEEN_MEM_WORD(k)	(1 << (k))
+#define SEEN_X			(1 << BPF_MEMWORDS)
+#define SEEN_CALL		(1 << (BPF_MEMWORDS + 1))
+#define SEEN_SKB		(1 << (BPF_MEMWORDS + 2))
+#define SEEN_DATA		(1 << (BPF_MEMWORDS + 3))
+
+#define FLAG_NEED_X_RESET	(1 << 0)
+
+struct jit_ctx {
+	const struct sk_filter *skf;
+	unsigned idx;
+	unsigned prologue_bytes;
+	int ret0_fp_idx;
+	u32 seen;
+	u32 flags;
+	u32 *offsets;
+	u32 *target;
+#if __LINUX_ARM_ARCH__ < 7
+	u16 epilogue_bytes;
+	u16 imm_count;
+	u32 *imms;
+#endif
+};
+
+int bpf_jit_enable __read_mostly;
+
+static u64 jit_get_skb_b(struct sk_buff *skb, unsigned offset)
+{
+	u8 ret;
+	int err;
+
+	err = skb_copy_bits(skb, offset, &ret, 1);
+
+	return (u64)err << 32 | ret;
+}
+
+static u64 jit_get_skb_h(struct sk_buff *skb, unsigned offset)
+{
+	u16 ret;
+	int err;
+
+	err = skb_copy_bits(skb, offset, &ret, 2);
+
+	return (u64)err << 32 | ntohs(ret);
+}
+
+static u64 jit_get_skb_w(struct sk_buff *skb, unsigned offset)
+{
+	u32 ret;
+	int err;
+
+	err = skb_copy_bits(skb, offset, &ret, 4);
+
+	return (u64)err << 32 | ntohl(ret);
+}
+
+/*
+ * Wrapper that handles both OABI and EABI and assures Thumb2 interworking
+ * (where the assembly routines like __aeabi_uidiv could cause problems).
+ */
+static u32 jit_udiv(u32 dividend, u32 divisor)
+{
+	return dividend / divisor;
+}
+
+static inline void _emit(int cond, u32 inst, struct jit_ctx *ctx)
+{
+	if (ctx->target != NULL)
+		ctx->target[ctx->idx] = inst | (cond << 28);
+
+	ctx->idx++;
+}
+
+/*
+ * Emit an instruction that will be executed unconditionally.
+ */
+static inline void emit(u32 inst, struct jit_ctx *ctx)
+{
+	_emit(ARM_COND_AL, inst, ctx);
+}
+
+static u16 saved_regs(struct jit_ctx *ctx)
+{
+	u16 ret = 0;
+
+	if ((ctx->skf->len > 1) ||
+	    (ctx->skf->insns[0].code == BPF_S_RET_A))
+		ret |= 1 << r_A;
+
+#ifdef CONFIG_FRAME_POINTER
+	ret |= (1 << ARM_FP) | (1 << ARM_IP) | (1 << ARM_LR) | (1 << ARM_PC);
+#else
+	if (ctx->seen & SEEN_CALL)
+		ret |= 1 << ARM_LR;
+#endif
+	if (ctx->seen & (SEEN_DATA | SEEN_SKB))
+		ret |= 1 << r_skb;
+	if (ctx->seen & SEEN_DATA)
+		ret |= (1 << r_skb_data) | (1 << r_skb_hl);
+	if (ctx->seen & SEEN_X)
+		ret |= 1 << r_X;
+
+	return ret;
+}
+
+static inline int mem_words_used(struct jit_ctx *ctx)
+{
+	/* yes, we do waste some stack space IF there are "holes" in the set" */
+	return fls(ctx->seen & SEEN_MEM);
+}
+
+static inline bool is_load_to_a(u16 inst)
+{
+	switch (inst) {
+	case BPF_S_LD_W_LEN:
+	case BPF_S_LD_W_ABS:
+	case BPF_S_LD_H_ABS:
+	case BPF_S_LD_B_ABS:
+	case BPF_S_ANC_CPU:
+	case BPF_S_ANC_IFINDEX:
+	case BPF_S_ANC_MARK:
+	case BPF_S_ANC_PROTOCOL:
+	case BPF_S_ANC_RXHASH:
+	case BPF_S_ANC_QUEUE:
+		return true;
+	default:
+		return false;
+	}
+}
+
+static void build_prologue(struct jit_ctx *ctx)
+{
+	u16 reg_set = saved_regs(ctx);
+	u16 first_inst = ctx->skf->insns[0].code;
+	u16 off;
+
+#ifdef CONFIG_FRAME_POINTER
+	emit(ARM_MOV_R(ARM_IP, ARM_SP), ctx);
+	emit(ARM_PUSH(reg_set), ctx);
+	emit(ARM_SUB_I(ARM_FP, ARM_IP, 4), ctx);
+#else
+	if (reg_set)
+		emit(ARM_PUSH(reg_set), ctx);
+#endif
+
+	if (ctx->seen & (SEEN_DATA | SEEN_SKB))
+		emit(ARM_MOV_R(r_skb, ARM_R0), ctx);
+
+	if (ctx->seen & SEEN_DATA) {
+		off = offsetof(struct sk_buff, data);
+		emit(ARM_LDR_I(r_skb_data, r_skb, off), ctx);
+		/* headlen = len - data_len */
+		off = offsetof(struct sk_buff, len);
+		emit(ARM_LDR_I(r_skb_hl, r_skb, off), ctx);
+		off = offsetof(struct sk_buff, data_len);
+		emit(ARM_LDR_I(r_scratch, r_skb, off), ctx);
+		emit(ARM_SUB_R(r_skb_hl, r_skb_hl, r_scratch), ctx);
+	}
+
+	if (ctx->flags & FLAG_NEED_X_RESET)
+		emit(ARM_MOV_I(r_X, 0), ctx);
+
+	/* do not leak kernel data to userspace */
+	if ((first_inst != BPF_S_RET_K) && !(is_load_to_a(first_inst)))
+		emit(ARM_MOV_I(r_A, 0), ctx);
+
+	/* stack space for the BPF_MEM words */
+	if (ctx->seen & SEEN_MEM)
+		emit(ARM_SUB_I(ARM_SP, ARM_SP, mem_words_used(ctx) * 4), ctx);
+}
+
+static void build_epilogue(struct jit_ctx *ctx)
+{
+	u16 reg_set = saved_regs(ctx);
+
+	if (ctx->seen & SEEN_MEM)
+		emit(ARM_ADD_I(ARM_SP, ARM_SP, mem_words_used(ctx) * 4), ctx);
+
+	reg_set &= ~(1 << ARM_LR);
+
+#ifdef CONFIG_FRAME_POINTER
+	/* the first instruction of the prologue was: mov ip, sp */
+	reg_set &= ~(1 << ARM_IP);
+	reg_set |= (1 << ARM_SP);
+	emit(ARM_LDM(ARM_SP, reg_set), ctx);
+#else
+	if (reg_set) {
+		if (ctx->seen & SEEN_CALL)
+			reg_set |= 1 << ARM_PC;
+		emit(ARM_POP(reg_set), ctx);
+	}
+
+	if (!(ctx->seen & SEEN_CALL))
+		emit(ARM_BX(ARM_LR), ctx);
+#endif
+}
+
+static int16_t imm8m(u32 x)
+{
+	u32 rot;
+
+	for (rot = 0; rot < 16; rot++)
+		if ((x & ~ror32(0xff, 2 * rot)) == 0)
+			return rol32(x, 2 * rot) | (rot << 8);
+
+	return -1;
+}
+
+#if __LINUX_ARM_ARCH__ < 7
+
+static u16 imm_offset(u32 k, struct jit_ctx *ctx)
+{
+	unsigned i = 0, offset;
+	u16 imm;
+
+	/* on the "fake" run we just count them (duplicates included) */
+	if (ctx->target == NULL) {
+		ctx->imm_count++;
+		return 0;
+	}
+
+	while ((i < ctx->imm_count) && ctx->imms[i]) {
+		if (ctx->imms[i] == k)
+			break;
+		i++;
+	}
+
+	if (ctx->imms[i] == 0)
+		ctx->imms[i] = k;
+
+	/* constants go just after the epilogue */
+	offset =  ctx->offsets[ctx->skf->len];
+	offset += ctx->prologue_bytes;
+	offset += ctx->epilogue_bytes;
+	offset += i * 4;
+
+	ctx->target[offset / 4] = k;
+
+	/* PC in ARM mode == address of the instruction + 8 */
+	imm = offset - (8 + ctx->idx * 4);
+
+	return imm;
+}
+
+#endif /* __LINUX_ARM_ARCH__ */
+
+/*
+ * Move an immediate that's not an imm8m to a core register.
+ */
+static inline void emit_mov_i_no8m(int rd, u32 val, struct jit_ctx *ctx)
+{
+#if __LINUX_ARM_ARCH__ < 7
+	emit(ARM_LDR_I(rd, ARM_PC, imm_offset(val, ctx)), ctx);
+#else
+	emit(ARM_MOVW(rd, val & 0xffff), ctx);
+	if (val > 0xffff)
+		emit(ARM_MOVT(rd, val >> 16), ctx);
+#endif
+}
+
+static inline void emit_mov_i(int rd, u32 val, struct jit_ctx *ctx)
+{
+	int imm12 = imm8m(val);
+
+	if (imm12 >= 0)
+		emit(ARM_MOV_I(rd, imm12), ctx);
+	else
+		emit_mov_i_no8m(rd, val, ctx);
+}
+
+#if __LINUX_ARM_ARCH__ < 6
+
+static void emit_load_be32(u8 cond, u8 r_res, u8 r_addr, struct jit_ctx *ctx)
+{
+	_emit(cond, ARM_LDRB_I(ARM_R3, r_addr, 1), ctx);
+	_emit(cond, ARM_LDRB_I(ARM_R1, r_addr, 0), ctx);
+	_emit(cond, ARM_LDRB_I(ARM_R2, r_addr, 3), ctx);
+	_emit(cond, ARM_LSL_I(ARM_R3, ARM_R3, 16), ctx);
+	_emit(cond, ARM_LDRB_I(ARM_R0, r_addr, 2), ctx);
+	_emit(cond, ARM_ORR_S(ARM_R3, ARM_R3, ARM_R1, SRTYPE_LSL, 24), ctx);
+	_emit(cond, ARM_ORR_R(ARM_R3, ARM_R3, ARM_R2), ctx);
+	_emit(cond, ARM_ORR_S(r_res, ARM_R3, ARM_R0, SRTYPE_LSL, 8), ctx);
+}
+
+static void emit_load_be16(u8 cond, u8 r_res, u8 r_addr, struct jit_ctx *ctx)
+{
+	_emit(cond, ARM_LDRB_I(ARM_R1, r_addr, 0), ctx);
+	_emit(cond, ARM_LDRB_I(ARM_R2, r_addr, 1), ctx);
+	_emit(cond, ARM_ORR_S(r_res, ARM_R2, ARM_R1, SRTYPE_LSL, 8), ctx);
+}
+
+static inline void emit_swap16(u8 r_dst, u8 r_src, struct jit_ctx *ctx)
+{
+	emit(ARM_LSL_R(ARM_R1, r_src, 8), ctx);
+	emit(ARM_ORR_S(r_dst, ARM_R1, r_src, SRTYPE_LSL, 8), ctx);
+	emit(ARM_LSL_I(r_dst, r_dst, 8), ctx);
+	emit(ARM_LSL_R(r_dst, r_dst, 8), ctx);
+}
+
+#else  /* ARMv6+ */
+
+static void emit_load_be32(u8 cond, u8 r_res, u8 r_addr, struct jit_ctx *ctx)
+{
+	_emit(cond, ARM_LDR_I(r_res, r_addr, 0), ctx);
+#ifdef __LITTLE_ENDIAN
+	_emit(cond, ARM_REV(r_res, r_res), ctx);
+#endif
+}
+
+static void emit_load_be16(u8 cond, u8 r_res, u8 r_addr, struct jit_ctx *ctx)
+{
+	_emit(cond, ARM_LDRH_I(r_res, r_addr, 0), ctx);
+#ifdef __LITTLE_ENDIAN
+	_emit(cond, ARM_REV16(r_res, r_res), ctx);
+#endif
+}
+
+static inline void emit_swap16(u8 r_dst __maybe_unused,
+			       u8 r_src __maybe_unused,
+			       struct jit_ctx *ctx __maybe_unused)
+{
+#ifdef __LITTLE_ENDIAN
+	emit(ARM_REV16(r_dst, r_src), ctx);
+#endif
+}
+
+#endif /* __LINUX_ARM_ARCH__ < 6 */
+
+
+/* Compute the immediate value for a PC-relative branch. */
+static inline u32 b_imm(unsigned tgt, struct jit_ctx *ctx)
+{
+	u32 imm;
+
+	if (ctx->target == NULL)
+		return 0;
+	/*
+	 * BPF allows only forward jumps and the offset of the target is
+	 * still the one computed during the first pass.
+	 */
+	imm  = ctx->offsets[tgt] + ctx->prologue_bytes - (ctx->idx * 4 + 8);
+
+	return imm >> 2;
+}
+
+#define OP_IMM3(op, r1, r2, imm_val, ctx)				\
+	do {								\
+		imm12 = imm8m(imm_val);					\
+		if (imm12 < 0) {					\
+			emit_mov_i_no8m(r_scratch, imm_val, ctx);	\
+			emit(op ## _R((r1), (r2), r_scratch), ctx);	\
+		} else {						\
+			emit(op ## _I((r1), (r2), imm12), ctx);		\
+		}							\
+	} while (0)
+
+static inline void emit_err_ret(u8 cond, struct jit_ctx *ctx)
+{
+	if (ctx->ret0_fp_idx >= 0) {
+		_emit(cond, ARM_B(b_imm(ctx->ret0_fp_idx, ctx)), ctx);
+		/* NOP to keep the size constant between passes */
+		emit(ARM_MOV_R(ARM_R0, ARM_R0), ctx);
+	} else {
+		_emit(cond, ARM_MOV_I(ARM_R0, 0), ctx);
+		_emit(cond, ARM_B(b_imm(ctx->skf->len, ctx)), ctx);
+	}
+}
+
+static inline void emit_blx_r(u8 tgt_reg, struct jit_ctx *ctx)
+{
+#if __LINUX_ARM_ARCH__ < 5
+	emit(ARM_MOV_R(ARM_LR, ARM_PC), ctx);
+
+	if (elf_hwcap & HWCAP_THUMB)
+		emit(ARM_BX(tgt_reg), ctx);
+	else
+		emit(ARM_MOV_R(ARM_PC, tgt_reg), ctx);
+#else
+	emit(ARM_BLX_R(tgt_reg), ctx);
+#endif
+}
+
+static inline void emit_udiv(u8 rd, u8 rm, u8 rn, struct jit_ctx *ctx)
+{
+#if __LINUX_ARM_ARCH__ == 7
+	if (elf_hwcap & HWCAP_IDIVA) {
+		emit(ARM_UDIV(rd, rm, rn), ctx);
+		return;
+	}
+#endif
+	if (rm != ARM_R0)
+		emit(ARM_MOV_R(ARM_R0, rm), ctx);
+	if (rn != ARM_R1)
+		emit(ARM_MOV_R(ARM_R1, rn), ctx);
+
+	ctx->seen |= SEEN_CALL;
+	emit_mov_i(ARM_R3, (u32)jit_udiv, ctx);
+	emit_blx_r(ARM_R3, ctx);
+
+	if (rd != ARM_R0)
+		emit(ARM_MOV_R(rd, ARM_R0), ctx);
+}
+
+static inline void update_on_xread(struct jit_ctx *ctx)
+{
+	if (!(ctx->seen & SEEN_X))
+		ctx->flags |= FLAG_NEED_X_RESET;
+
+	ctx->seen |= SEEN_X;
+}
+
+static int build_body(struct jit_ctx *ctx)
+{
+	void *load_func[] = {jit_get_skb_b, jit_get_skb_h, jit_get_skb_w};
+	const struct sk_filter *prog = ctx->skf;
+	const struct sock_filter *inst;
+	unsigned i, load_order, off, condt;
+	int imm12;
+	u32 k;
+
+	for (i = 0; i < prog->len; i++) {
+		inst = &(prog->insns[i]);
+		/* K as an immediate value operand */
+		k = inst->k;
+
+		/* compute offsets only in the fake pass */
+		if (ctx->target == NULL)
+			ctx->offsets[i] = ctx->idx * 4;
+
+		switch (inst->code) {
+		case BPF_S_LD_IMM:
+			emit_mov_i(r_A, k, ctx);
+			break;
+		case BPF_S_LD_W_LEN:
+			ctx->seen |= SEEN_SKB;
+			BUILD_BUG_ON(FIELD_SIZEOF(struct sk_buff, len) != 4);
+			emit(ARM_LDR_I(r_A, r_skb,
+				       offsetof(struct sk_buff, len)), ctx);
+			break;
+		case BPF_S_LD_MEM:
+			/* A = scratch[k] */
+			ctx->seen |= SEEN_MEM_WORD(k);
+			emit(ARM_LDR_I(r_A, ARM_SP, SCRATCH_OFF(k)), ctx);
+			break;
+		case BPF_S_LD_W_ABS:
+			load_order = 2;
+			goto load;
+		case BPF_S_LD_H_ABS:
+			load_order = 1;
+			goto load;
+		case BPF_S_LD_B_ABS:
+			load_order = 0;
+load:
+			/* the interpreter will deal with the negative K */
+			if ((int)k < 0)
+				return -ENOTSUPP;
+			emit_mov_i(r_off, k, ctx);
+load_common:
+			ctx->seen |= SEEN_DATA | SEEN_CALL;
+
+			if (load_order > 0) {
+				emit(ARM_SUB_I(r_scratch, r_skb_hl,
+					       1 << load_order), ctx);
+				emit(ARM_CMP_R(r_scratch, r_off), ctx);
+				condt = ARM_COND_HS;
+			} else {
+				emit(ARM_CMP_R(r_skb_hl, r_off), ctx);
+				condt = ARM_COND_HI;
+			}
+
+			_emit(condt, ARM_ADD_R(r_scratch, r_off, r_skb_data),
+			      ctx);
+
+			if (load_order == 0)
+				_emit(condt, ARM_LDRB_I(r_A, r_scratch, 0),
+				      ctx);
+			else if (load_order == 1)
+				emit_load_be16(condt, r_A, r_scratch, ctx);
+			else if (load_order == 2)
+				emit_load_be32(condt, r_A, r_scratch, ctx);
+
+			_emit(condt, ARM_B(b_imm(i + 1, ctx)), ctx);
+
+			/* the slowpath */
+			emit_mov_i(ARM_R3, (u32)load_func[load_order], ctx);
+			emit(ARM_MOV_R(ARM_R0, r_skb), ctx);
+			/* the offset is already in R1 */
+			emit_blx_r(ARM_R3, ctx);
+			/* check the result of skb_copy_bits */
+			emit(ARM_CMP_I(ARM_R1, 0), ctx);
+			emit_err_ret(ARM_COND_NE, ctx);
+			emit(ARM_MOV_R(r_A, ARM_R0), ctx);
+			break;
+		case BPF_S_LD_W_IND:
+			load_order = 2;
+			goto load_ind;
+		case BPF_S_LD_H_IND:
+			load_order = 1;
+			goto load_ind;
+		case BPF_S_LD_B_IND:
+			load_order = 0;
+load_ind:
+			OP_IMM3(ARM_ADD, r_off, r_X, k, ctx);
+			goto load_common;
+		case BPF_S_LDX_IMM:
+			ctx->seen |= SEEN_X;
+			emit_mov_i(r_X, k, ctx);
+			break;
+		case BPF_S_LDX_W_LEN:
+			ctx->seen |= SEEN_X | SEEN_SKB;
+			emit(ARM_LDR_I(r_X, r_skb,
+				       offsetof(struct sk_buff, len)), ctx);
+			break;
+		case BPF_S_LDX_MEM:
+			ctx->seen |= SEEN_X | SEEN_MEM_WORD(k);
+			emit(ARM_LDR_I(r_X, ARM_SP, SCRATCH_OFF(k)), ctx);
+			break;
+		case BPF_S_LDX_B_MSH:
+			/* x = ((*(frame + k)) & 0xf) << 2; */
+			ctx->seen |= SEEN_X | SEEN_DATA | SEEN_CALL;
+			/* the interpreter should deal with the negative K */
+			if (k < 0)
+				return -1;
+			/* offset in r1: we might have to take the slow path */
+			emit_mov_i(r_off, k, ctx);
+			emit(ARM_CMP_R(r_skb_hl, r_off), ctx);
+
+			/* load in r0: common with the slowpath */
+			_emit(ARM_COND_HI, ARM_LDRB_R(ARM_R0, r_skb_data,
+						      ARM_R1), ctx);
+			/*
+			 * emit_mov_i() might generate one or two instructions,
+			 * the same holds for emit_blx_r()
+			 */
+			_emit(ARM_COND_HI, ARM_B(b_imm(i + 1, ctx) - 2), ctx);
+
+			emit(ARM_MOV_R(ARM_R0, r_skb), ctx);
+			/* r_off is r1 */
+			emit_mov_i(ARM_R3, (u32)jit_get_skb_b, ctx);
+			emit_blx_r(ARM_R3, ctx);
+			/* check the return value of skb_copy_bits */
+			emit(ARM_CMP_I(ARM_R1, 0), ctx);
+			emit_err_ret(ARM_COND_NE, ctx);
+
+			emit(ARM_AND_I(r_X, ARM_R0, 0x00f), ctx);
+			emit(ARM_LSL_I(r_X, r_X, 2), ctx);
+			break;
+		case BPF_S_ST:
+			ctx->seen |= SEEN_MEM_WORD(k);
+			emit(ARM_STR_I(r_A, ARM_SP, SCRATCH_OFF(k)), ctx);
+			break;
+		case BPF_S_STX:
+			update_on_xread(ctx);
+			ctx->seen |= SEEN_MEM_WORD(k);
+			emit(ARM_STR_I(r_X, ARM_SP, SCRATCH_OFF(k)), ctx);
+			break;
+		case BPF_S_ALU_ADD_K:
+			/* A += K */
+			OP_IMM3(ARM_ADD, r_A, r_A, k, ctx);
+			break;
+		case BPF_S_ALU_ADD_X:
+			update_on_xread(ctx);
+			emit(ARM_ADD_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_SUB_K:
+			/* A -= K */
+			OP_IMM3(ARM_SUB, r_A, r_A, k, ctx);
+			break;
+		case BPF_S_ALU_SUB_X:
+			update_on_xread(ctx);
+			emit(ARM_SUB_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_MUL_K:
+			/* A *= K */
+			emit_mov_i(r_scratch, k, ctx);
+			emit(ARM_MUL(r_A, r_A, r_scratch), ctx);
+			break;
+		case BPF_S_ALU_MUL_X:
+			update_on_xread(ctx);
+			emit(ARM_MUL(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_DIV_K:
+			/* current k == reciprocal_value(userspace k) */
+			emit_mov_i(r_scratch, k, ctx);
+			/* A = top 32 bits of the product */
+			emit(ARM_UMULL(r_scratch, r_A, r_A, r_scratch), ctx);
+			break;
+		case BPF_S_ALU_DIV_X:
+			update_on_xread(ctx);
+			emit(ARM_CMP_I(r_X, 0), ctx);
+			emit_err_ret(ARM_COND_EQ, ctx);
+			emit_udiv(r_A, r_A, r_X, ctx);
+			break;
+		case BPF_S_ALU_OR_K:
+			/* A |= K */
+			OP_IMM3(ARM_ORR, r_A, r_A, k, ctx);
+			break;
+		case BPF_S_ALU_OR_X:
+			update_on_xread(ctx);
+			emit(ARM_ORR_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_AND_K:
+			/* A &= K */
+			OP_IMM3(ARM_AND, r_A, r_A, k, ctx);
+			break;
+		case BPF_S_ALU_AND_X:
+			update_on_xread(ctx);
+			emit(ARM_AND_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_LSH_K:
+			if (unlikely(k > 31))
+				return -1;
+			emit(ARM_LSL_I(r_A, r_A, k), ctx);
+			break;
+		case BPF_S_ALU_LSH_X:
+			update_on_xread(ctx);
+			emit(ARM_LSL_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_RSH_K:
+			if (unlikely(k > 31))
+				return -1;
+			emit(ARM_LSR_I(r_A, r_A, k), ctx);
+			break;
+		case BPF_S_ALU_RSH_X:
+			update_on_xread(ctx);
+			emit(ARM_LSR_R(r_A, r_A, r_X), ctx);
+			break;
+		case BPF_S_ALU_NEG:
+			/* A = -A */
+			emit(ARM_RSB_I(r_A, r_A, 0), ctx);
+			break;
+		case BPF_S_JMP_JA:
+			/* pc += K */
+			emit(ARM_B(b_imm(i + k + 1, ctx)), ctx);
+			break;
+		case BPF_S_JMP_JEQ_K:
+			/* pc += (A == K) ? pc->jt : pc->jf */
+			condt  = ARM_COND_EQ;
+			goto cmp_imm;
+		case BPF_S_JMP_JGT_K:
+			/* pc += (A > K) ? pc->jt : pc->jf */
+			condt  = ARM_COND_HI;
+			goto cmp_imm;
+		case BPF_S_JMP_JGE_K:
+			/* pc += (A >= K) ? pc->jt : pc->jf */
+			condt  = ARM_COND_HS;
+cmp_imm:
+			imm12 = imm8m(k);
+			if (imm12 < 0) {
+				emit_mov_i_no8m(r_scratch, k, ctx);
+				emit(ARM_CMP_R(r_A, r_scratch), ctx);
+			} else {
+				emit(ARM_CMP_I(r_A, imm12), ctx);
+			}
+cond_jump:
+			if (inst->jt)
+				_emit(condt, ARM_B(b_imm(i + inst->jt + 1,
+						   ctx)), ctx);
+			if (inst->jf)
+				_emit(condt ^ 1, ARM_B(b_imm(i + inst->jf + 1,
+							     ctx)), ctx);
+			break;
+		case BPF_S_JMP_JEQ_X:
+			/* pc += (A == X) ? pc->jt : pc->jf */
+			condt   = ARM_COND_EQ;
+			goto cmp_x;
+		case BPF_S_JMP_JGT_X:
+			/* pc += (A > X) ? pc->jt : pc->jf */
+			condt   = ARM_COND_HI;
+			goto cmp_x;
+		case BPF_S_JMP_JGE_X:
+			/* pc += (A >= X) ? pc->jt : pc->jf */
+			condt   = ARM_COND_CS;
+cmp_x:
+			update_on_xread(ctx);
+			emit(ARM_CMP_R(r_A, r_X), ctx);
+			goto cond_jump;
+		case BPF_S_JMP_JSET_K:
+			/* pc += (A & K) ? pc->jt : pc->jf */
+			condt  = ARM_COND_NE;
+			/* not set iff all zeroes iff Z==1 iff EQ */
+
+			imm12 = imm8m(k);
+			if (imm12 < 0) {
+				emit_mov_i_no8m(r_scratch, k, ctx);
+				emit(ARM_TST_R(r_A, r_scratch), ctx);
+			} else {
+				emit(ARM_TST_I(r_A, imm12), ctx);
+			}
+			goto cond_jump;
+		case BPF_S_JMP_JSET_X:
+			/* pc += (A & X) ? pc->jt : pc->jf */
+			update_on_xread(ctx);
+			condt  = ARM_COND_NE;
+			emit(ARM_TST_R(r_A, r_X), ctx);
+			goto cond_jump;
+		case BPF_S_RET_A:
+			emit(ARM_MOV_R(ARM_R0, r_A), ctx);
+			goto b_epilogue;
+		case BPF_S_RET_K:
+			if ((k == 0) && (ctx->ret0_fp_idx < 0))
+				ctx->ret0_fp_idx = i;
+			emit_mov_i(ARM_R0, k, ctx);
+b_epilogue:
+			if (i != ctx->skf->len - 1)
+				emit(ARM_B(b_imm(prog->len, ctx)), ctx);
+			break;
+		case BPF_S_MISC_TAX:
+			/* X = A */
+			ctx->seen |= SEEN_X;
+			emit(ARM_MOV_R(r_X, r_A), ctx);
+			break;
+		case BPF_S_MISC_TXA:
+			/* A = X */
+			update_on_xread(ctx);
+			emit(ARM_MOV_R(r_A, r_X), ctx);
+			break;
+		case BPF_S_ANC_PROTOCOL:
+			/* A = ntohs(skb->protocol) */
+			ctx->seen |= SEEN_SKB;
+			BUILD_BUG_ON(FIELD_SIZEOF(struct sk_buff,
+						  protocol) != 2);
+			off = offsetof(struct sk_buff, protocol);
+			emit(ARM_LDRH_I(r_scratch, r_skb, off), ctx);
+			emit_swap16(r_A, r_scratch, ctx);
+			break;
+		case BPF_S_ANC_CPU:
+			/* r_scratch = current_thread_info() */
+			OP_IMM3(ARM_BIC, r_scratch, ARM_SP, THREAD_SIZE - 1, ctx);
+			/* A = current_thread_info()->cpu */
+			BUILD_BUG_ON(FIELD_SIZEOF(struct thread_info, cpu) != 4);
+			off = offsetof(struct thread_info, cpu);
+			emit(ARM_LDR_I(r_A, r_scratch, off), ctx);
+			break;
+		case BPF_S_ANC_IFINDEX:
+			/* A = skb->dev->ifindex */
+			ctx->seen |= SEEN_SKB;
+			off = offsetof(struct sk_buff, dev);
+			emit(ARM_LDR_I(r_scratch, r_skb, off), ctx);
+
+			emit(ARM_CMP_I(r_scratch, 0), ctx);
+			emit_err_ret(ARM_COND_EQ, ctx);
+
+			BUILD_BUG_ON(FIELD_SIZEOF(struct net_device,
+						  ifindex) != 4);
+			off = offsetof(struct net_device, ifindex);
+			emit(ARM_LDR_I(r_A, r_scratch, off), ctx);
+			break;
+		case BPF_S_ANC_MARK:
+			ctx->seen |= SEEN_SKB;
+			BUILD_BUG_ON(FIELD_SIZEOF(struct sk_buff, mark) != 4);
+			off = offsetof(struct sk_buff, mark);
+			emit(ARM_LDR_I(r_A, r_skb, off), ctx);
+			break;
+		case BPF_S_ANC_RXHASH:
+			ctx->seen |= SEEN_SKB;
+			BUILD_BUG_ON(FIELD_SIZEOF(struct sk_buff, rxhash) != 4);
+			off = offsetof(struct sk_buff, rxhash);
+			emit(ARM_LDR_I(r_A, r_skb, off), ctx);
+			break;
+		case BPF_S_ANC_QUEUE:
+			ctx->seen |= SEEN_SKB;
+			BUILD_BUG_ON(FIELD_SIZEOF(struct sk_buff,
+						  queue_mapping) != 2);
+			BUILD_BUG_ON(offsetof(struct sk_buff,
+					      queue_mapping) > 0xff);
+			off = offsetof(struct sk_buff, queue_mapping);
+			emit(ARM_LDRH_I(r_A, r_skb, off), ctx);
+			break;
+		default:
+			return -1;
+		}
+	}
+
+	/* compute offsets only during the first pass */
+	if (ctx->target == NULL)
+		ctx->offsets[i] = ctx->idx * 4;
+
+	return 0;
+}
+
+
+void bpf_jit_compile(struct sk_filter *fp)
+{
+	struct jit_ctx ctx;
+	unsigned tmp_idx;
+	unsigned alloc_size;
+
+	if (!bpf_jit_enable)
+		return;
+
+	memset(&ctx, 0, sizeof(ctx));
+	ctx.skf		= fp;
+	ctx.ret0_fp_idx = -1;
+
+	ctx.offsets = kzalloc(GFP_KERNEL, 4 * (ctx.skf->len + 1));
+	if (ctx.offsets == NULL)
+		return;
+
+	/* fake pass to fill in the ctx->seen */
+	if (unlikely(build_body(&ctx)))
+		goto out;
+
+	tmp_idx = ctx.idx;
+	build_prologue(&ctx);
+	ctx.prologue_bytes = (ctx.idx - tmp_idx) * 4;
+
+#if __LINUX_ARM_ARCH__ < 7
+	tmp_idx = ctx.idx;
+	build_epilogue(&ctx);
+	ctx.epilogue_bytes = (ctx.idx - tmp_idx) * 4;
+
+	ctx.idx += ctx.imm_count;
+	if (ctx.imm_count) {
+		ctx.imms = kzalloc(GFP_KERNEL, 4 * ctx.imm_count);
+		if (ctx.imms == NULL)
+			goto out;
+	}
+#else
+	/* there's nothing after the epilogue on ARMv7 */
+	build_epilogue(&ctx);
+#endif
+
+	alloc_size = 4 * ctx.idx;
+	ctx.target = module_alloc(max(sizeof(struct work_struct),
+				      alloc_size));
+	if (unlikely(ctx.target == NULL))
+		goto out;
+
+	ctx.idx = 0;
+	build_prologue(&ctx);
+	build_body(&ctx);
+	build_epilogue(&ctx);
+
+	flush_icache_range((u32)ctx.target, (u32)(ctx.target + ctx.idx));
+
+#if __LINUX_ARM_ARCH__ < 7
+	if (ctx.imm_count)
+		kfree(ctx.imms);
+#endif
+
+	if (bpf_jit_enable > 1)
+		print_hex_dump(KERN_INFO, "BPF JIT code: ",
+			       DUMP_PREFIX_ADDRESS, 16, 4, ctx.target,
+			       alloc_size, false);
+
+	fp->bpf_func = (void *)ctx.target;
+out:
+	kfree(ctx.offsets);
+	return;
+}
+
+static void bpf_jit_free_worker(struct work_struct *work)
+{
+	module_free(NULL, work);
+}
+
+void bpf_jit_free(struct sk_filter *fp)
+{
+	struct work_struct *work;
+
+	if (fp->bpf_func != sk_run_filter) {
+		work = (struct work_struct *)fp->bpf_func;
+
+		INIT_WORK(work, bpf_jit_free_worker);
+		schedule_work(work);
+	}
+}
diff --git a/arch/arm/net/bpf_jit_32.h b/arch/arm/net/bpf_jit_32.h
new file mode 100644
index 0000000..99ae5e3
