diff -Nur a/drivers/watchdog/Kconfig b/drivers/watchdog/Kconfig
--- a/drivers/watchdog/Kconfig	2019-08-20 14:26:04.438449328 +0300
+++ b/drivers/watchdog/Kconfig	2019-08-20 14:22:54.744883819 +0300
@@ -241,6 +241,22 @@
 	help
 	  Support for the watchdog on RAVE SP device.
 
+config MLX_WDT
+	tristate "Mellanox Watchdog"
+	depends on MELLANOX_PLATFORM
+	select WATCHDOG_CORE
+	select REGMAP
+	help
+	  This is the driver for the hardware watchdog on Mellanox systems.
+	  If you are going to use it, say Y here, otherwise N.
+	  This driver can be used together with the watchdog daemon.
+	  It can also watch your kernel to make sure it doesn't freeze,
+	  and if it does, it reboots your system after a certain amount of
+	  time.
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called mlx-wdt.
+
 # ALPHA Architecture
 
 # ARM Architecture
diff -Nur a/drivers/watchdog/Makefile b/drivers/watchdog/Makefile
--- a/drivers/watchdog/Makefile	2019-08-20 14:26:04.438449328 +0300
+++ b/drivers/watchdog/Makefile	2019-08-20 14:23:27.893157429 +0300
@@ -139,6 +139,7 @@
 obj-$(CONFIG_INTEL_MEI_WDT) += mei_wdt.o
 obj-$(CONFIG_NI903X_WDT) += ni903x_wdt.o
 obj-$(CONFIG_NIC7018_WDT) += nic7018_wdt.o
+obj-$(CONFIG_MLX_WDT) += mlx_wdt.o
 
 # M68K Architecture
 obj-$(CONFIG_M54xx_WATCHDOG) += m54xx_wdt.o
diff -Nur a/drivers/watchdog/mlx_wdt.c b/drivers/watchdog/mlx_wdt.c
--- a/drivers/watchdog/mlx_wdt.c	1970-01-01 02:00:00.000000000 +0200
+++ b/drivers/watchdog/mlx_wdt.c	2019-08-20 14:21:55.748396514 +0300
@@ -0,0 +1,289 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Mellanox watchdog driver
+ *
+ * Copyright (C) 2019 Mellanox Technologies
+ * Copyright (C) 2019 Michael Shych <mshych@mellanox.com>
+ */
+
+#include <linux/bitops.h>
+#include <linux/device.h>
+#include <linux/errno.h>
+#include <linux/log2.h>
+#include <linux/module.h>
+#include <linux/platform_data/mlxreg.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+#include <linux/spinlock.h>
+#include <linux/types.h>
+#include <linux/watchdog.h>
+
+#define MLXREG_WDT_CLOCK_SCALE		1000
+#define MLXREG_WDT_MAX_TIMEOUT_TYPE1	32
+#define MLXREG_WDT_MAX_TIMEOUT_TYPE2	255
+#define MLXREG_WDT_MIN_TIMEOUT		1
+#define MLXREG_WDT_OPTIONS_BASE (WDIOF_KEEPALIVEPING | WDIOF_MAGICCLOSE | \
+				 WDIOF_SETTIMEOUT)
+
+/**
+ * struct mlxreg_wdt - wd private data:
+ *
+ * @wdd:	watchdog device;
+ * @device:	basic device;
+ * @pdata:	data received from platform driver;
+ * @regmap:	register map of parent device;
+ * @timeout:	defined timeout in sec.;
+ * @action_idx:	index for direct access to action register;
+ * @timeout_idx:index for direct access to TO register;
+ * @tleft_idx:	index for direct access to time left register;
+ * @ping_idx:	index for direct access to ping register;
+ * @reset_idx:	index for direct access to reset cause register;
+ * @wd_type:	watchdog HW type;
+ */
+struct mlxreg_wdt {
+	struct watchdog_device wdd;
+	struct mlxreg_core_platform_data *pdata;
+	void *regmap;
+	int action_idx;
+	int timeout_idx;
+	int tleft_idx;
+	int ping_idx;
+	int reset_idx;
+	enum mlxreg_wdt_type wdt_type;
+};
+
+static void mlxreg_wdt_check_card_reset(struct mlxreg_wdt *wdt)
+{
+	struct mlxreg_core_data *reg_data;
+	u32 regval;
+	int rc;
+
+	if (wdt->reset_idx == -EINVAL)
+		return;
+
+	if (!(wdt->wdd.info->options & WDIOF_CARDRESET))
+		return;
+
+	reg_data = &wdt->pdata->data[wdt->reset_idx];
+	rc = regmap_read(wdt->regmap, reg_data->reg, &regval);
+	if (!rc) {
+		if (regval & ~reg_data->mask) {
+			wdt->wdd.bootstatus = WDIOF_CARDRESET;
+			dev_info(wdt->wdd.parent,
+				 "watchdog previously reset the CPU\n");
+		}
+	}
+}
+
+static int mlxreg_wdt_start(struct watchdog_device *wdd)
+{
+	struct mlxreg_wdt *wdt = watchdog_get_drvdata(wdd);
+	struct mlxreg_core_data *reg_data = &wdt->pdata->data[wdt->action_idx];
+
+	return regmap_update_bits(wdt->regmap, reg_data->reg, ~reg_data->mask,
+				  BIT(reg_data->bit));
+}
+
+static int mlxreg_wdt_stop(struct watchdog_device *wdd)
+{
+	struct mlxreg_wdt *wdt = watchdog_get_drvdata(wdd);
+	struct mlxreg_core_data *reg_data = &wdt->pdata->data[wdt->action_idx];
+
+	return regmap_update_bits(wdt->regmap, reg_data->reg, ~reg_data->mask,
+				  ~BIT(reg_data->bit));
+}
+
+static int mlxreg_wdt_ping(struct watchdog_device *wdd)
+{
+	struct mlxreg_wdt *wdt = watchdog_get_drvdata(wdd);
+	struct mlxreg_core_data *reg_data = &wdt->pdata->data[wdt->ping_idx];
+
+	return regmap_update_bits_base(wdt->regmap, reg_data->reg,
+				       ~reg_data->mask, BIT(reg_data->bit),
+				       NULL, false, true);
+}
+
+static int mlxreg_wdt_set_timeout(struct watchdog_device *wdd,
+				  unsigned int timeout)
+{
+	struct mlxreg_wdt *wdt = watchdog_get_drvdata(wdd);
+	struct mlxreg_core_data *reg_data = &wdt->pdata->data[wdt->timeout_idx];
+	u32 regval, set_time, hw_timeout;
+	int rc;
+
+	if (wdt->wdt_type == MLX_WDT_TYPE1) {
+		rc = regmap_read(wdt->regmap, reg_data->reg, &regval);
+		if (rc)
+			return rc;
+
+		hw_timeout = order_base_2(timeout * MLXREG_WDT_CLOCK_SCALE);
+		regval = (regval & reg_data->mask) | hw_timeout;
+		/* Rowndown to actual closest number of sec. */
+		set_time = BIT(hw_timeout) / MLXREG_WDT_CLOCK_SCALE;
+	} else {
+		set_time = timeout;
+		regval = timeout;
+	}
+
+	wdd->timeout = set_time;
+	rc = regmap_write(wdt->regmap, reg_data->reg, regval);
+
+	if (!rc) {
+		/*
+		 * Restart watchdog with new timeout period
+		 * if watchdog is already started.
+		 */
+		if (watchdog_active(wdd)) {
+			rc = mlxreg_wdt_stop(wdd);
+			if (!rc)
+				rc = mlxreg_wdt_start(wdd);
+		}
+	}
+
+	return rc;
+}
+
+static unsigned int mlxreg_wdt_get_timeleft(struct watchdog_device *wdd)
+{
+	struct mlxreg_wdt *wdt = watchdog_get_drvdata(wdd);
+	struct mlxreg_core_data *reg_data = &wdt->pdata->data[wdt->tleft_idx];
+	u32 regval;
+	int rc;
+
+	rc = regmap_read(wdt->regmap, reg_data->reg, &regval);
+	/* Return 0 timeleft in case of failure register read. */
+	return rc == 0 ? regval : 0;
+}
+
+static const struct watchdog_ops mlxreg_wdt_ops_type1 = {
+	.start		= mlxreg_wdt_start,
+	.stop		= mlxreg_wdt_stop,
+	.ping		= mlxreg_wdt_ping,
+	.set_timeout	= mlxreg_wdt_set_timeout,
+	.owner		= THIS_MODULE,
+};
+
+static const struct watchdog_ops mlxreg_wdt_ops_type2 = {
+	.start		= mlxreg_wdt_start,
+	.stop		= mlxreg_wdt_stop,
+	.ping		= mlxreg_wdt_ping,
+	.set_timeout	= mlxreg_wdt_set_timeout,
+	.get_timeleft	= mlxreg_wdt_get_timeleft,
+	.owner		= THIS_MODULE,
+};
+
+static const struct watchdog_info mlxreg_wdt_main_info = {
+	.options	= MLXREG_WDT_OPTIONS_BASE
+			| WDIOF_CARDRESET,
+	.identity	= "mlx-wdt-main",
+};
+
+static const struct watchdog_info mlxreg_wdt_aux_info = {
+	.options	= MLXREG_WDT_OPTIONS_BASE
+			| WDIOF_ALARMONLY,
+	.identity	= "mlx-wdt-aux",
+};
+
+static void mlxreg_wdt_config(struct mlxreg_wdt *wdt,
+			      struct mlxreg_core_platform_data *pdata)
+{
+	struct mlxreg_core_data *data = pdata->data;
+	int i;
+
+	wdt->reset_idx = -EINVAL;
+	for (i = 0; i < pdata->counter; i++, data++) {
+		if (strnstr(data->label, "action", sizeof(data->label)))
+			wdt->action_idx = i;
+		else if (strnstr(data->label, "timeout", sizeof(data->label)))
+			wdt->timeout_idx = i;
+		else if (strnstr(data->label, "timeleft", sizeof(data->label)))
+			wdt->tleft_idx = i;
+		else if (strnstr(data->label, "ping", sizeof(data->label)))
+			wdt->ping_idx = i;
+		else if (strnstr(data->label, "reset", sizeof(data->label)))
+			wdt->reset_idx = i;
+	}
+
+	wdt->pdata = pdata;
+	if (strnstr(pdata->identity, mlxreg_wdt_main_info.identity,
+		    sizeof(mlxreg_wdt_main_info.identity)))
+		wdt->wdd.info = &mlxreg_wdt_main_info;
+	else
+		wdt->wdd.info = &mlxreg_wdt_aux_info;
+
+	wdt->wdt_type = pdata->version;
+	if (wdt->wdt_type == MLX_WDT_TYPE2) {
+		wdt->wdd.ops = &mlxreg_wdt_ops_type2;
+		wdt->wdd.max_timeout = MLXREG_WDT_MAX_TIMEOUT_TYPE2;
+	} else {
+		wdt->wdd.ops = &mlxreg_wdt_ops_type1;
+		wdt->wdd.max_timeout = MLXREG_WDT_MAX_TIMEOUT_TYPE1;
+	}
+	wdt->wdd.min_timeout = MLXREG_WDT_MIN_TIMEOUT;
+}
+
+static int mlxreg_wdt_init_timeout(struct mlxreg_wdt *wdt,
+				   struct mlxreg_core_platform_data *pdata)
+{
+	u32 timeout;
+
+	timeout = pdata->data[wdt->timeout_idx].health_cntr;
+	return mlxreg_wdt_set_timeout(&wdt->wdd, timeout);
+}
+
+static int mlxreg_wdt_probe(struct platform_device *pdev)
+{
+	struct mlxreg_core_platform_data *pdata;
+	struct mlxreg_wdt *wdt;
+	int rc;
+
+	pdata = dev_get_platdata(&pdev->dev);
+	if (!pdata) {
+		dev_err(&pdev->dev, "Failed to get platform data.\n");
+		return -EINVAL;
+	}
+	wdt = devm_kzalloc(&pdev->dev, sizeof(*wdt), GFP_KERNEL);
+	if (!wdt)
+		return -ENOMEM;
+
+	wdt->wdd.parent = &pdev->dev;
+	wdt->regmap = pdata->regmap;
+	mlxreg_wdt_config(wdt, pdata);
+
+	if ((pdata->features & MLXREG_CORE_WD_FEATURE_NOWAYOUT))
+		watchdog_set_nowayout(&wdt->wdd, WATCHDOG_NOWAYOUT);
+	watchdog_stop_on_reboot(&wdt->wdd);
+	watchdog_set_drvdata(&wdt->wdd, wdt);
+	rc = mlxreg_wdt_init_timeout(wdt, pdata);
+	if (rc)
+		goto register_error;
+
+	if ((pdata->features & MLXREG_CORE_WD_FEATURE_START_AT_BOOT)) {
+		rc = mlxreg_wdt_start(&wdt->wdd);
+		if (rc)
+			goto register_error;
+		set_bit(WDOG_HW_RUNNING, &wdt->wdd.status);
+	}
+	mlxreg_wdt_check_card_reset(wdt);
+	rc = devm_watchdog_register_device(&pdev->dev, &wdt->wdd);
+
+register_error:
+	if (rc)
+		dev_err(&pdev->dev,
+			"Cannot register watchdog device (err=%d)\n", rc);
+	return rc;
+}
+
+static struct platform_driver mlxreg_wdt_driver = {
+	.probe	= mlxreg_wdt_probe,
+	.driver	= {
+			.name = "mlx-wdt",
+	},
+};
+
+module_platform_driver(mlxreg_wdt_driver);
+
+MODULE_AUTHOR("Michael Shych <michaelsh@mellanox.com>");
+MODULE_DESCRIPTION("Mellanox watchdog driver");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:mlx-wdt");
