--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmgmacrxh.h
@@ -0,0 +1,53 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Hardware-specific Receive Data Header for the
+ * Broadcom Home Networking Division
+ * BCM47XX GbE cores.
+ *
+ * $Id: bcmgmacrxh.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef _bcmgmacrxh_h_
+#define	_bcmgmacrxh_h_
+
+/*
+ * The Ethernet GMAC core returns an 8-byte Receive Frame Data Header
+ * with every frame consisting of
+ * 16 bits of frame length, followed by
+ * 16 bits of GMAC rx descriptor info, followed by 32bits of undefined.
+ */
+typedef volatile struct {
+	uint16	len;
+	uint16	flags;
+	uint16	pad[12];
+} bcmgmacrxh_t;
+
+#define	RXHDR_LEN	28	/* Header length */
+
+#define	GRXF_DT_MASK	((uint16)0xf)		/* data type */
+#define	GRXF_DT_SHIFT	12
+#define	GRXF_DC_MASK	((uint16)0xf)		/* (num descr to xfer the frame) - 1 */
+#define	GRXF_DC_SHIFT	8
+#define	GRXF_OVF	((uint16)1 << 7)	/* overflow error occured */
+#define	GRXF_CTFERR	((uint16)1 << 6)	/* overflow error occured */
+#define	GRXF_OVERSIZE	((uint16)1 << 4)	/* frame size > rxmaxlength */
+#define	GRXF_CRC	((uint16)1 << 3)	/* crc error */
+#define	GRXF_VLAN	((uint16)1 << 2)	/* vlan tag detected */
+#define	GRXF_PT_MASK	((uint16)3)		/* packet type 0 - Unicast,
+						 * 1 - Multicast, 2 - Broadcast
+						 */
+
+#endif	/* _bcmgmacrxh_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmiproc_phy.h b/drivers/bcmdrivers/gmac/src/include/bcmiproc_phy.h
new file mode 100755
index 0000000..3698729
