--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/proto/bcmevent.h
@@ -0,0 +1,313 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Broadcom Event  protocol definitions
+ *
+ * Dependencies: proto/bcmeth.h
+ *
+ * $Id: bcmevent.h 315348 2012-02-16 07:32:51Z $
+ *
+ */
+
+/*
+ * Broadcom Ethernet Events protocol defines
+ *
+ */
+
+#ifndef _BCMEVENT_H_
+#define _BCMEVENT_H_
+
+#ifndef _TYPEDEFS_H_
+#include <typedefs.h>
+#endif
+
+/* This marks the start of a packed structure section. */
+#include <packed_section_start.h>
+
+#define BCM_EVENT_MSG_VERSION		2	/* wl_event_msg_t struct version */
+#define BCM_MSG_IFNAME_MAX		16	/* max length of interface name */
+
+/* flags */
+#define WLC_EVENT_MSG_LINK		0x01	/* link is up */
+#define WLC_EVENT_MSG_FLUSHTXQ		0x02	/* flush tx queue on MIC error */
+#define WLC_EVENT_MSG_GROUP		0x04	/* group MIC error */
+#define WLC_EVENT_MSG_UNKBSS		0x08	/* unknown source bsscfg */
+#define WLC_EVENT_MSG_UNKIF		0x10	/* unknown source OS i/f */
+
+/* these fields are stored in network order */
+
+/* version 1 */
+typedef BWL_PRE_PACKED_STRUCT struct
+{
+	uint16	version;
+	uint16	flags;			/* see flags below */
+	uint32	event_type;		/* Message (see below) */
+	uint32	status;			/* Status code (see below) */
+	uint32	reason;			/* Reason code (if applicable) */
+	uint32	auth_type;		/* WLC_E_AUTH */
+	uint32	datalen;		/* data buf */
+	struct ether_addr	addr;	/* Station address (if applicable) */
+	char	ifname[BCM_MSG_IFNAME_MAX]; /* name of the packet incoming interface */
+} BWL_POST_PACKED_STRUCT wl_event_msg_v1_t;
+
+/* the current version */
+typedef BWL_PRE_PACKED_STRUCT struct
+{
+	uint16	version;
+	uint16	flags;			/* see flags below */
+	uint32	event_type;		/* Message (see below) */
+	uint32	status;			/* Status code (see below) */
+	uint32	reason;			/* Reason code (if applicable) */
+	uint32	auth_type;		/* WLC_E_AUTH */
+	uint32	datalen;		/* data buf */
+	struct ether_addr	addr;	/* Station address (if applicable) */
+	char	ifname[BCM_MSG_IFNAME_MAX]; /* name of the packet incoming interface */
+	uint8	ifidx;			/* destination OS i/f index */
+	uint8	bsscfgidx;		/* source bsscfg index */
+} BWL_POST_PACKED_STRUCT wl_event_msg_t;
+
+/* used by driver msgs */
+typedef BWL_PRE_PACKED_STRUCT struct bcm_event {
+	struct ether_header eth;
+	bcmeth_hdr_t		bcm_hdr;
+	wl_event_msg_t		event;
+	/* data portion follows */
+} BWL_POST_PACKED_STRUCT bcm_event_t;
+
+#define BCM_MSG_LEN	(sizeof(bcm_event_t) - sizeof(bcmeth_hdr_t) - sizeof(struct ether_header))
+
+/* Event messages */
+#define WLC_E_SET_SSID		0	/* indicates status of set SSID */
+#define WLC_E_JOIN		1	/* differentiates join IBSS from found (WLC_E_START) IBSS */
+#define WLC_E_START		2	/* STA founded an IBSS or AP started a BSS */
+#define WLC_E_AUTH		3	/* 802.11 AUTH request */
+#define WLC_E_AUTH_IND		4	/* 802.11 AUTH indication */
+#define WLC_E_DEAUTH		5	/* 802.11 DEAUTH request */
+#define WLC_E_DEAUTH_IND	6	/* 802.11 DEAUTH indication */
+#define WLC_E_ASSOC		7	/* 802.11 ASSOC request */
+#define WLC_E_ASSOC_IND		8	/* 802.11 ASSOC indication */
+#define WLC_E_REASSOC		9	/* 802.11 REASSOC request */
+#define WLC_E_REASSOC_IND	10	/* 802.11 REASSOC indication */
+#define WLC_E_DISASSOC		11	/* 802.11 DISASSOC request */
+#define WLC_E_DISASSOC_IND	12	/* 802.11 DISASSOC indication */
+#define WLC_E_QUIET_START	13	/* 802.11h Quiet period started */
+#define WLC_E_QUIET_END		14	/* 802.11h Quiet period ended */
+#define WLC_E_BEACON_RX		15	/* BEACONS received/lost indication */
+#define WLC_E_LINK		16	/* generic link indication */
+#define WLC_E_MIC_ERROR		17	/* TKIP MIC error occurred */
+#define WLC_E_NDIS_LINK		18	/* NDIS style link indication */
+#define WLC_E_ROAM		19	/* roam attempt occurred: indicate status & reason */
+#define WLC_E_TXFAIL		20	/* change in dot11FailedCount (txfail) */
+#define WLC_E_PMKID_CACHE	21	/* WPA2 pmkid cache indication */
+#define WLC_E_RETROGRADE_TSF	22	/* current AP's TSF value went backward */
+#define WLC_E_PRUNE		23	/* AP was pruned from join list for reason */
+#define WLC_E_AUTOAUTH		24	/* report AutoAuth table entry match for join attempt */
+#define WLC_E_EAPOL_MSG		25	/* Event encapsulating an EAPOL message */
+#define WLC_E_SCAN_COMPLETE	26	/* Scan results are ready or scan was aborted */
+#define WLC_E_ADDTS_IND		27	/* indicate to host addts fail/success */
+#define WLC_E_DELTS_IND		28	/* indicate to host delts fail/success */
+#define WLC_E_BCNSENT_IND	29	/* indicate to host of beacon transmit */
+#define WLC_E_BCNRX_MSG		30	/* Send the received beacon up to the host */
+#define WLC_E_BCNLOST_MSG	31	/* indicate to host loss of beacon */
+#define WLC_E_ROAM_PREP		32	/* before attempting to roam */
+#define WLC_E_PFN_NET_FOUND	33	/* PFN network found event */
+#define WLC_E_PFN_NET_LOST	34	/* PFN network lost event */
+#define WLC_E_RESET_COMPLETE	35
+#define WLC_E_JOIN_START	36
+#define WLC_E_ROAM_START	37
+#define WLC_E_ASSOC_START	38
+#define WLC_E_IBSS_ASSOC	39
+#define WLC_E_RADIO		40
+#define WLC_E_PSM_WATCHDOG	41	/* PSM microcode watchdog fired */
+#define WLC_E_PROBREQ_MSG       44      /* probe request received */
+#define WLC_E_SCAN_CONFIRM_IND  45
+#define WLC_E_PSK_SUP		46	/* WPA Handshake fail */
+#define WLC_E_COUNTRY_CODE_CHANGED	47
+#define	WLC_E_EXCEEDED_MEDIUM_TIME	48	/* WMMAC excedded medium time */
+#define WLC_E_ICV_ERROR		49	/* WEP ICV error occurred */
+#define WLC_E_UNICAST_DECODE_ERROR	50	/* Unsupported unicast encrypted frame */
+#define WLC_E_MULTICAST_DECODE_ERROR	51 /* Unsupported multicast encrypted frame */
+#define WLC_E_TRACE		52
+#define WLC_E_IF		54	/* I/F change (for dongle host notification) */
+#define WLC_E_P2P_DISC_LISTEN_COMPLETE	55	/* listen state expires */
+#define WLC_E_RSSI		56	/* indicate RSSI change based on configured levels */
+#define WLC_E_PFN_SCAN_COMPLETE	57	/* PFN completed scan of network list */
+#define WLC_E_EXTLOG_MSG	58
+#define WLC_E_ACTION_FRAME      59 	/* Action frame Rx */
+#define WLC_E_ACTION_FRAME_COMPLETE	60	/* Action frame Tx complete */
+#define WLC_E_PRE_ASSOC_IND	61	/* assoc request received */
+#define WLC_E_PRE_REASSOC_IND	62	/* re-assoc request received */
+#define WLC_E_CHANNEL_ADOPTED	63
+#define WLC_E_AP_STARTED	64	/* AP started */
+#define WLC_E_DFS_AP_STOP	65	/* AP stopped due to DFS */
+#define WLC_E_DFS_AP_RESUME	66	/* AP resumed due to DFS */
+#define WLC_E_WAI_STA_EVENT	67	/* WAI stations event */
+#define WLC_E_WAI_MSG 		68	/* event encapsulating an WAI message */
+#define WLC_E_ESCAN_RESULT 	69	/* escan result event */
+#define WLC_E_ACTION_FRAME_OFF_CHAN_COMPLETE 	70	/* action frame off channel complete */
+#define WLC_E_PROBRESP_MSG	71	/* probe response received */
+#define WLC_E_P2P_PROBREQ_MSG	72	/* P2P Probe request received */
+#define WLC_E_DCS_REQUEST	73
+
+#define WLC_E_FIFO_CREDIT_MAP	74	/* credits for D11 FIFOs. [AC0,AC1,AC2,AC3,BC_MC,ATIM] */
+
+#define WLC_E_ACTION_FRAME_RX	75	/* Received action frame event WITH
+					 * wl_event_rx_frame_data_t header
+					 */
+#define WLC_E_WAKE_EVENT	76	/* Wake Event timer fired, used for wake WLAN test mode */
+#define WLC_E_RM_COMPLETE	77	/* Radio measurement complete */
+#define WLC_E_HTSFSYNC		78	/* Synchronize TSF with the host */
+#define WLC_E_OVERLAY_REQ	79	/* request an overlay IOCTL/iovar from the host */
+#define WLC_E_CSA_COMPLETE_IND		80	/* 802.11 CHANNEL SWITCH ACTION completed */
+#define WLC_E_EXCESS_PM_WAKE_EVENT	81	/* excess PM Wake Event to inform host  */
+#define WLC_E_PFN_SCAN_NONE		82	/* no PFN networks around */
+#define WLC_E_PFN_SCAN_ALLGONE		83	/* last found PFN network gets lost */
+#define WLC_E_GTK_PLUMBED 		84
+#define WLC_E_ASSOC_IND_NDIS		85	/* 802.11 ASSOC indication for NDIS only */
+#define WLC_E_REASSOC_IND_NDIS		86	/* 802.11 REASSOC indication for NDIS only */
+#define WLC_E_ASSOC_REQ_IE 		87
+#define WLC_E_ASSOC_RESP_IE 		88
+
+#define WLC_E_LAST			89	/* highest val + 1 for range checking */
+
+/* Table of event name strings for UIs and debugging dumps */
+typedef struct {
+	uint event;
+	const char *name;
+} bcmevent_name_t;
+
+extern const bcmevent_name_t	bcmevent_names[];
+extern const int		bcmevent_names_size;
+
+/* Event status codes */
+#define WLC_E_STATUS_SUCCESS		0	/* operation was successful */
+#define WLC_E_STATUS_FAIL		1	/* operation failed */
+#define WLC_E_STATUS_TIMEOUT		2	/* operation timed out */
+#define WLC_E_STATUS_NO_NETWORKS	3	/* failed due to no matching network found */
+#define WLC_E_STATUS_ABORT		4	/* operation was aborted */
+#define WLC_E_STATUS_NO_ACK		5	/* protocol failure: packet not ack'd */
+#define WLC_E_STATUS_UNSOLICITED	6	/* AUTH or ASSOC packet was unsolicited */
+#define WLC_E_STATUS_ATTEMPT		7	/* attempt to assoc to an auto auth configuration */
+#define WLC_E_STATUS_PARTIAL		8	/* scan results are incomplete */
+#define WLC_E_STATUS_NEWSCAN		9	/* scan aborted by another scan */
+#define WLC_E_STATUS_NEWASSOC		10	/* scan aborted due to assoc in progress */
+#define WLC_E_STATUS_11HQUIET		11	/* 802.11h quiet period started */
+#define WLC_E_STATUS_SUPPRESS		12	/* user disabled scanning (WLC_SET_SCANSUPPRESS) */
+#define WLC_E_STATUS_NOCHANS		13	/* no allowable channels to scan */
+#define WLC_E_STATUS_CS_ABORT		15	/* abort channel select */
+#define WLC_E_STATUS_ERROR		16	/* request failed due to error */
+
+/* roam reason codes */
+#define WLC_E_REASON_INITIAL_ASSOC	0	/* initial assoc */
+#define WLC_E_REASON_LOW_RSSI		1	/* roamed due to low RSSI */
+#define WLC_E_REASON_DEAUTH		2	/* roamed due to DEAUTH indication */
+#define WLC_E_REASON_DISASSOC		3	/* roamed due to DISASSOC indication */
+#define WLC_E_REASON_BCNS_LOST		4	/* roamed due to lost beacons */
+#define WLC_E_REASON_MINTXRATE		9	/* roamed because at mintxrate for too long */
+#define WLC_E_REASON_TXFAIL		10	/* We can hear AP, but AP can't hear us */
+
+/* Roam codes used primarily by CCX */
+#define WLC_E_REASON_FAST_ROAM_FAILED	5	/* roamed due to fast roam failure */
+#define WLC_E_REASON_DIRECTED_ROAM	6	/* roamed due to request by AP */
+#define WLC_E_REASON_TSPEC_REJECTED	7	/* roamed due to TSPEC rejection */
+#define WLC_E_REASON_BETTER_AP		8	/* roamed due to finding better AP */
+
+#define WLC_E_REASON_REQUESTED_ROAM 11	/* roamed due to BSS Mgmt Transition request by AP */
+
+/* prune reason codes */
+#define WLC_E_PRUNE_ENCR_MISMATCH	1	/* encryption mismatch */
+#define WLC_E_PRUNE_BCAST_BSSID		2	/* AP uses a broadcast BSSID */
+#define WLC_E_PRUNE_MAC_DENY		3	/* STA's MAC addr is in AP's MAC deny list */
+#define WLC_E_PRUNE_MAC_NA		4	/* STA's MAC addr is not in AP's MAC allow list */
+#define WLC_E_PRUNE_REG_PASSV		5	/* AP not allowed due to regulatory restriction */
+#define WLC_E_PRUNE_SPCT_MGMT		6	/* AP does not support STA locale spectrum mgmt */
+#define WLC_E_PRUNE_RADAR		7	/* AP is on a radar channel of STA locale */
+#define WLC_E_RSN_MISMATCH		8	/* STA does not support AP's RSN */
+#define WLC_E_PRUNE_NO_COMMON_RATES	9	/* No rates in common with AP */
+#define WLC_E_PRUNE_BASIC_RATES		10	/* STA does not support all basic rates of BSS */
+#define WLC_E_PRUNE_CIPHER_NA		12	/* BSS's cipher not supported */
+#define WLC_E_PRUNE_KNOWN_STA		13	/* AP is already known to us as a STA */
+#define WLC_E_PRUNE_WDS_PEER		15	/* AP is already known to us as a WDS peer */
+#define WLC_E_PRUNE_QBSS_LOAD		16	/* QBSS LOAD - AAC is too low */
+#define WLC_E_PRUNE_HOME_AP		17	/* prune home AP */
+
+/* WPA failure reason codes carried in the WLC_E_PSK_SUP event */
+#define WLC_E_SUP_OTHER			0	/* Other reason */
+#define WLC_E_SUP_DECRYPT_KEY_DATA	1	/* Decryption of key data failed */
+#define WLC_E_SUP_BAD_UCAST_WEP128	2	/* Illegal use of ucast WEP128 */
+#define WLC_E_SUP_BAD_UCAST_WEP40	3	/* Illegal use of ucast WEP40 */
+#define WLC_E_SUP_UNSUP_KEY_LEN		4	/* Unsupported key length */
+#define WLC_E_SUP_PW_KEY_CIPHER		5	/* Unicast cipher mismatch in pairwise key */
+#define WLC_E_SUP_MSG3_TOO_MANY_IE	6	/* WPA IE contains > 1 RSN IE in key msg 3 */
+#define WLC_E_SUP_MSG3_IE_MISMATCH	7	/* WPA IE mismatch in key message 3 */
+#define WLC_E_SUP_NO_INSTALL_FLAG	8	/* INSTALL flag unset in 4-way msg */
+#define WLC_E_SUP_MSG3_NO_GTK		9	/* encapsulated GTK missing from msg 3 */
+#define WLC_E_SUP_GRP_KEY_CIPHER	10	/* Multicast cipher mismatch in group key */
+#define WLC_E_SUP_GRP_MSG1_NO_GTK	11	/* encapsulated GTK missing from group msg 1 */
+#define WLC_E_SUP_GTK_DECRYPT_FAIL	12	/* GTK decrypt failure */
+#define WLC_E_SUP_SEND_FAIL		13	/* message send failure */
+#define WLC_E_SUP_DEAUTH		14	/* received FC_DEAUTH */
+#define WLC_E_SUP_WPA_PSK_TMO		15	/* WPA PSK 4-way handshake timeout */
+
+/* Event data for events that include frames received over the air */
+/* WLC_E_PROBRESP_MSG
+ * WLC_E_P2P_PROBREQ_MSG
+ * WLC_E_ACTION_FRAME_RX
+ */
+typedef BWL_PRE_PACKED_STRUCT struct wl_event_rx_frame_data {
+	uint16	version;
+	uint16	channel;	/* Matches chanspec_t format from bcmwifi_channels.h */
+	int32	rssi;
+	uint32	mactime;
+	uint32	rate;
+} BWL_POST_PACKED_STRUCT wl_event_rx_frame_data_t;
+
+#define BCM_RX_FRAME_DATA_VERSION 1
+
+/* WLC_E_IF event data */
+typedef struct wl_event_data_if {
+	uint8 ifidx;		/* RTE virtual device index (for dongle) */
+	uint8 opcode;		/* see I/F opcode */
+	uint8 reserved;
+	uint8 bssidx;		/* bsscfg index */
+	uint8 role;		/* see I/F role */
+} wl_event_data_if_t;
+
+/* opcode in WLC_E_IF event */
+#define WLC_E_IF_ADD		1	/* bsscfg add */
+#define WLC_E_IF_DEL		2	/* bsscfg delete */
+#define WLC_E_IF_CHANGE		3	/* bsscfg role change */
+
+/* I/F role code in WLC_E_IF event */
+#define WLC_E_IF_ROLE_STA		0	/* Infra STA */
+#define WLC_E_IF_ROLE_AP		1	/* Access Point */
+#define WLC_E_IF_ROLE_WDS		2	/* WDS link */
+#define WLC_E_IF_ROLE_P2P_GO		3	/* P2P Group Owner */
+#define WLC_E_IF_ROLE_P2P_CLIENT	4	/* P2P Client */
+
+/* Reason codes for LINK */
+#define WLC_E_LINK_BCN_LOSS	1	/* Link down because of beacon loss */
+#define WLC_E_LINK_DISASSOC	2	/* Link down because of disassoc */
+#define WLC_E_LINK_ASSOC_REC	3	/* Link down because assoc recreate failed */
+#define WLC_E_LINK_BSSCFG_DIS	4	/* Link down due to bsscfg down */
+
+/* reason codes for WLC_E_OVERLAY_REQ event */
+#define WLC_E_OVL_DOWNLOAD		0	/* overlay download request */
+#define WLC_E_OVL_UPDATE_IND	1	/* device indication of host overlay update */
+
+/* This marks the end of a packed structure section. */
+#include <packed_section_end.h>
+
+#endif /* _BCMEVENT_H_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/proto/bcmip.h b/drivers/bcmdrivers/gmac/src/include/proto/bcmip.h
new file mode 100755
index 0000000..4f01aee
