--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmwifi.h
@@ -0,0 +1,456 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Misc utility routines for WL and Apps
+ * This header file housing the define and function prototype use by
+ * both the wl driver, tools & Apps.
+ *
+ * $Id: bcmwifi.h 293848 2011-11-03 12:31:04Z $
+ */
+
+#ifndef	_bcmwifi_h_
+#define	_bcmwifi_h_
+
+
+/* A chanspec holds the channel number, band, bandwidth and control sideband */
+typedef uint16 chanspec_t;
+
+/* channel defines */
+#define CH_UPPER_SB			0x01
+#define CH_LOWER_SB			0x02
+#define CH_EWA_VALID			0x04
+#define CH_80MHZ_APART			16
+#define CH_40MHZ_APART			8
+#define CH_20MHZ_APART			4
+#define CH_10MHZ_APART			2
+#define CH_5MHZ_APART			1	/* 2G band channels are 5 Mhz apart */
+#define CH_MAX_2G_CHANNEL		14	/* Max channel in 2G band */
+#define	MAXCHANNEL		224	/* max # supported channels. The max channel no is 216,
+					 * this is that + 1 rounded up to a multiple of NBBY (8).
+					 * DO NOT MAKE it > 255: channels are uint8's all over
+					 */
+#define CHSPEC_CTLOVLP(sp1, sp2, sep)	ABS(wf_chspec_ctlchan(sp1) - wf_chspec_ctlchan(sp2)) < (sep)
+
+#ifndef D11AC_IOTYPES
+
+#define WL_CHANSPEC_CHAN_MASK		0x00ff
+#define WL_CHANSPEC_CHAN_SHIFT		0
+
+#define WL_CHANSPEC_CTL_SB_MASK		0x0300
+#define WL_CHANSPEC_CTL_SB_SHIFT	     8
+#define WL_CHANSPEC_CTL_SB_LOWER	0x0100
+#define WL_CHANSPEC_CTL_SB_UPPER	0x0200
+#define WL_CHANSPEC_CTL_SB_NONE		0x0300
+
+#define WL_CHANSPEC_BW_MASK		0x0C00
+#define WL_CHANSPEC_BW_SHIFT		    10
+#define WL_CHANSPEC_BW_10		0x0400
+#define WL_CHANSPEC_BW_20		0x0800
+#define WL_CHANSPEC_BW_40		0x0C00
+
+#define WL_CHANSPEC_BAND_MASK		0xf000
+#define WL_CHANSPEC_BAND_SHIFT		12
+#define WL_CHANSPEC_BAND_5G		0x1000
+#define WL_CHANSPEC_BAND_2G		0x2000
+#define INVCHANSPEC			255
+
+/* channel defines */
+#define LOWER_20_SB(channel)	(((channel) > CH_10MHZ_APART) ? ((channel) - CH_10MHZ_APART) : 0)
+#define UPPER_20_SB(channel)	(((channel) < (MAXCHANNEL - CH_10MHZ_APART)) ? \
+				((channel) + CH_10MHZ_APART) : 0)
+#define CHSPEC_WLCBANDUNIT(chspec)	(CHSPEC_IS5G(chspec) ? BAND_5G_INDEX : BAND_2G_INDEX)
+#define CH20MHZ_CHSPEC(channel)	(chanspec_t)((chanspec_t)(channel) | WL_CHANSPEC_BW_20 | \
+				WL_CHANSPEC_CTL_SB_NONE | (((channel) <= CH_MAX_2G_CHANNEL) ? \
+				WL_CHANSPEC_BAND_2G : WL_CHANSPEC_BAND_5G))
+#define NEXT_20MHZ_CHAN(channel)	(((channel) < (MAXCHANNEL - CH_20MHZ_APART)) ? \
+					((channel) + CH_20MHZ_APART) : 0)
+#define CH40MHZ_CHSPEC(channel, ctlsb)	(chanspec_t) \
+					((channel) | (ctlsb) | WL_CHANSPEC_BW_40 | \
+					((channel) <= CH_MAX_2G_CHANNEL ? WL_CHANSPEC_BAND_2G : \
+					WL_CHANSPEC_BAND_5G))
+#define CHSPEC_CHANNEL(chspec)	((uint8)((chspec) & WL_CHANSPEC_CHAN_MASK))
+#define CHSPEC_BAND(chspec)	((chspec) & WL_CHANSPEC_BAND_MASK)
+
+/* chanspec stores radio channel & flags to indicate control channel location, i.e. upper/lower */
+#define CHSPEC_CTL_SB(chspec)	((chspec) & WL_CHANSPEC_CTL_SB_MASK)
+#define CHSPEC_BW(chspec)	((chspec) & WL_CHANSPEC_BW_MASK)
+
+#ifdef WL11N_20MHZONLY
+
+#define CHSPEC_IS10(chspec)	0
+#define CHSPEC_IS20(chspec)	1
+#ifndef CHSPEC_IS40
+#define CHSPEC_IS40(chspec)	0
+#endif
+
+#else /* !WL11N_20MHZONLY */
+
+#define CHSPEC_IS10(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_10)
+#define CHSPEC_IS20(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_20)
+#ifndef CHSPEC_IS40
+#define CHSPEC_IS40(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_40)
+#endif
+
+#endif /* !WL11N_20MHZONLY */
+
+#define CHSPEC_IS5G(chspec)	(((chspec) & WL_CHANSPEC_BAND_MASK) == WL_CHANSPEC_BAND_5G)
+#define CHSPEC_IS2G(chspec)	(((chspec) & WL_CHANSPEC_BAND_MASK) == WL_CHANSPEC_BAND_2G)
+#define CHSPEC_SB_NONE(chspec)	(((chspec) & WL_CHANSPEC_CTL_SB_MASK) == WL_CHANSPEC_CTL_SB_NONE)
+#define CHSPEC_SB_UPPER(chspec)	(((chspec) & WL_CHANSPEC_CTL_SB_MASK) == WL_CHANSPEC_CTL_SB_UPPER)
+#define CHSPEC_SB_LOWER(chspec)	(((chspec) & WL_CHANSPEC_CTL_SB_MASK) == WL_CHANSPEC_CTL_SB_LOWER)
+#define CHSPEC_CTL_CHAN(chspec)  ((CHSPEC_SB_LOWER(chspec)) ? \
+				  (LOWER_20_SB(((chspec) & WL_CHANSPEC_CHAN_MASK))) : \
+				  (UPPER_20_SB(((chspec) & WL_CHANSPEC_CHAN_MASK))))
+#define CHSPEC2WLC_BAND(chspec) (CHSPEC_IS5G(chspec) ? WLC_BAND_5G : WLC_BAND_2G)
+
+#define CHANSPEC_STR_LEN    8
+
+#else /* D11AC_IOTYPES */
+
+#define WL_CHANSPEC_CHAN_MASK		0x00ff
+#define WL_CHANSPEC_CHAN_SHIFT		0
+#define WL_CHANSPEC_CHAN1_MASK		0x000f
+#define WL_CHANSPEC_CHAN1_SHIFT		0
+#define WL_CHANSPEC_CHAN2_MASK		0x00f0
+#define WL_CHANSPEC_CHAN2_SHIFT		4
+
+#define WL_CHANSPEC_CTL_SB_MASK		0x0700
+#define WL_CHANSPEC_CTL_SB_SHIFT	8
+#define WL_CHANSPEC_CTL_SB_LLL		0x0000
+#define WL_CHANSPEC_CTL_SB_LLU		0x0100
+#define WL_CHANSPEC_CTL_SB_LUL		0x0200
+#define WL_CHANSPEC_CTL_SB_LUU		0x0300
+#define WL_CHANSPEC_CTL_SB_ULL		0x0400
+#define WL_CHANSPEC_CTL_SB_ULU		0x0500
+#define WL_CHANSPEC_CTL_SB_UUL		0x0600
+#define WL_CHANSPEC_CTL_SB_UUU		0x0700
+#define WL_CHANSPEC_CTL_SB_LL		WL_CHANSPEC_CTL_SB_LLL
+#define WL_CHANSPEC_CTL_SB_LU		WL_CHANSPEC_CTL_SB_LLU
+#define WL_CHANSPEC_CTL_SB_UL		WL_CHANSPEC_CTL_SB_LUL
+#define WL_CHANSPEC_CTL_SB_UU		WL_CHANSPEC_CTL_SB_LUU
+#define WL_CHANSPEC_CTL_SB_L		WL_CHANSPEC_CTL_SB_LLL
+#define WL_CHANSPEC_CTL_SB_U		WL_CHANSPEC_CTL_SB_LLU
+#define WL_CHANSPEC_CTL_SB_LOWER 	WL_CHANSPEC_CTL_SB_LLL
+#define WL_CHANSPEC_CTL_SB_UPPER	WL_CHANSPEC_CTL_SB_LLU
+
+#define WL_CHANSPEC_BW_MASK		0x3800
+#define WL_CHANSPEC_BW_SHIFT		11
+#define WL_CHANSPEC_BW_5		0x0000
+#define WL_CHANSPEC_BW_10		0x0800
+#define WL_CHANSPEC_BW_20		0x1000
+#define WL_CHANSPEC_BW_40		0x1800
+#define WL_CHANSPEC_BW_80		0x2000
+#define WL_CHANSPEC_BW_160		0x2800
+#define WL_CHANSPEC_BW_8080		0x3000
+
+#define WL_CHANSPEC_BAND_MASK		0xc000
+#define WL_CHANSPEC_BAND_SHIFT		14
+#define WL_CHANSPEC_BAND_2G		0x0000
+#define WL_CHANSPEC_BAND_3G		0x4000
+#define WL_CHANSPEC_BAND_4G		0x8000
+#define WL_CHANSPEC_BAND_5G		0xc000
+#define INVCHANSPEC			255
+
+/* channel defines */
+#define LOWER_20_SB(channel)		(((channel) > CH_10MHZ_APART) ? \
+					((channel) - CH_10MHZ_APART) : 0)
+#define UPPER_20_SB(channel)		(((channel) < (MAXCHANNEL - CH_10MHZ_APART)) ? \
+					((channel) + CH_10MHZ_APART) : 0)
+#define CHSPEC_WLCBANDUNIT(chspec)	(CHSPEC_IS5G(chspec) ? BAND_5G_INDEX : BAND_2G_INDEX)
+#define CH20MHZ_CHSPEC(channel)		(chanspec_t)((chanspec_t)(channel) | WL_CHANSPEC_BW_20 | \
+					(((channel) <= CH_MAX_2G_CHANNEL) ? \
+					WL_CHANSPEC_BAND_2G : WL_CHANSPEC_BAND_5G))
+#define NEXT_20MHZ_CHAN(channel)	(((channel) < (MAXCHANNEL - CH_20MHZ_APART)) ? \
+					((channel) + CH_20MHZ_APART) : 0)
+#define CH40MHZ_CHSPEC(channel, ctlsb)	(chanspec_t) \
+					((channel) | (ctlsb) | WL_CHANSPEC_BW_40 | \
+					((channel) <= CH_MAX_2G_CHANNEL ? WL_CHANSPEC_BAND_2G : \
+					WL_CHANSPEC_BAND_5G))
+#define CH80MHZ_CHSPEC(channel, ctlsb)	(chanspec_t) \
+					((channel) | (ctlsb) | WL_CHANSPEC_BW_80 | \
+					((channel) <= CH_MAX_2G_CHANNEL ? WL_CHANSPEC_BAND_2G : \
+					WL_CHANSPEC_BAND_5G))
+#define CH160MHZ_CHSPEC(channel, ctlsb)	(chanspec_t) \
+					((channel) | (ctlsb) | WL_CHANSPEC_BW_160 | \
+					((channel) <= CH_MAX_2G_CHANNEL ? WL_CHANSPEC_BAND_2G : \
+					WL_CHANSPEC_BAND_5G))
+
+/* simple MACROs to get different fields of chanspec */
+#define CHSPEC_CHANNEL(chspec)		((uint8)((chspec) & WL_CHANSPEC_CHAN_MASK))
+#define CHSPEC_CHAN1(chspec)		((chspec) & WL_CHANSPEC_CHAN1_MASK)
+#define CHSPEC_CHAN2(chspec)		((chspec) & WL_CHANSPEC_CHAN2_MASK)
+#define CHSPEC_BAND(chspec)		((chspec) & WL_CHANSPEC_BAND_MASK)
+#define CHSPEC_CTL_SB(chspec)		((chspec) & WL_CHANSPEC_CTL_SB_MASK)
+#define CHSPEC_BW(chspec)		((chspec) & WL_CHANSPEC_BW_MASK)
+
+#ifdef WL11N_20MHZONLY
+
+#define CHSPEC_IS10(chspec)	0
+#define CHSPEC_IS20(chspec)	1
+#ifndef CHSPEC_IS40
+#define CHSPEC_IS40(chspec)	0
+#endif
+#ifndef CHSPEC_IS80
+#define CHSPEC_IS160(chspec)	0
+#endif
+#ifndef CHSPEC_IS160
+#define CHSPEC_IS160(chspec)	0
+#endif
+#ifndef CHSPEC_IS8080
+#define CHSPEC_IS8080(chspec)	0
+#endif
+
+#else /* !WL11N_20MHZONLY */
+
+#define CHSPEC_IS10(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_10)
+#define CHSPEC_IS20(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_20)
+#ifndef CHSPEC_IS40
+#define CHSPEC_IS40(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_40)
+#endif
+#ifndef CHSPEC_IS80
+#define CHSPEC_IS80(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_80)
+#endif
+#ifndef CHSPEC_IS160
+#define CHSPEC_IS160(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_160)
+#endif
+#ifndef CHSPEC_IS8080
+#define CHSPEC_IS8080(chspec)	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_8080)
+#endif
+
+#endif /* !WL11N_20MHZONLY */
+
+#define CHSPEC_IS5G(chspec)	(((chspec) & WL_CHANSPEC_BAND_MASK) == WL_CHANSPEC_BAND_5G)
+#define CHSPEC_IS2G(chspec)	(((chspec) & WL_CHANSPEC_BAND_MASK) == WL_CHANSPEC_BAND_2G)
+#define CHSPEC_SB_UPPER(chspec)	\
+	((((chspec) & WL_CHANSPEC_CTL_SB_MASK) == WL_CHANSPEC_CTL_SB_UPPER) && \
+	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_40))
+#define CHSPEC_SB_LOWER(chspec)	\
+	((((chspec) & WL_CHANSPEC_CTL_SB_MASK) == WL_CHANSPEC_CTL_SB_LOWER) && \
+	(((chspec) & WL_CHANSPEC_BW_MASK) == WL_CHANSPEC_BW_40))
+#define CHSPEC2WLC_BAND(chspec) (CHSPEC_IS5G(chspec) ? WLC_BAND_5G : WLC_BAND_2G)
+
+/**
+ * Number of chars needed for wf_chspec_ntoa() destination character buffer.
+ */
+#define CHANSPEC_STR_LEN    20
+
+
+/* Legacy Chanspec defines
+ * These are the defines for the previous format of the chanspec_t
+ */
+#define WL_LCHANSPEC_CHAN_MASK		0x00ff
+#define WL_LCHANSPEC_CHAN_SHIFT		     0
+
+#define WL_LCHANSPEC_CTL_SB_MASK	0x0300
+#define WL_LCHANSPEC_CTL_SB_SHIFT	     8
+#define WL_LCHANSPEC_CTL_SB_LOWER	0x0100
+#define WL_LCHANSPEC_CTL_SB_UPPER	0x0200
+#define WL_LCHANSPEC_CTL_SB_NONE	0x0300
+
+#define WL_LCHANSPEC_BW_MASK		0x0C00
+#define WL_LCHANSPEC_BW_SHIFT		    10
+#define WL_LCHANSPEC_BW_10		0x0400
+#define WL_LCHANSPEC_BW_20		0x0800
+#define WL_LCHANSPEC_BW_40		0x0C00
+
+#define WL_LCHANSPEC_BAND_MASK		0xf000
+#define WL_LCHANSPEC_BAND_SHIFT		    12
+#define WL_LCHANSPEC_BAND_5G		0x1000
+#define WL_LCHANSPEC_BAND_2G		0x2000
+
+#define LCHSPEC_CHANNEL(chspec)	((uint8)((chspec) & WL_LCHANSPEC_CHAN_MASK))
+#define LCHSPEC_BAND(chspec)	((chspec) & WL_LCHANSPEC_BAND_MASK)
+#define LCHSPEC_CTL_SB(chspec)	((chspec) & WL_LCHANSPEC_CTL_SB_MASK)
+#define LCHSPEC_BW(chspec)	((chspec) & WL_LCHANSPEC_BW_MASK)
+#define LCHSPEC_IS10(chspec)	(((chspec) & WL_LCHANSPEC_BW_MASK) == WL_LCHANSPEC_BW_10)
+#define LCHSPEC_IS20(chspec)	(((chspec) & WL_LCHANSPEC_BW_MASK) == WL_LCHANSPEC_BW_20)
+#define LCHSPEC_IS40(chspec)	(((chspec) & WL_LCHANSPEC_BW_MASK) == WL_LCHANSPEC_BW_40)
+#define LCHSPEC_IS5G(chspec)	(((chspec) & WL_LCHANSPEC_BAND_MASK) == WL_LCHANSPEC_BAND_5G)
+#define LCHSPEC_IS2G(chspec)	(((chspec) & WL_LCHANSPEC_BAND_MASK) == WL_LCHANSPEC_BAND_2G)
+
+#define LCHSPEC_CREATE(chan, band, bw, sb)  ((uint16)((chan) | (sb) | (bw) | (band)))
+
+#endif /* D11AC_IOTYPES */
+
+/*
+ * WF_CHAN_FACTOR_* constants are used to calculate channel frequency
+ * given a channel number.
+ * chan_freq = chan_factor * 500Mhz + chan_number * 5
+ */
+
+/**
+ * Channel Factor for the starting frequence of 2.4 GHz channels.
+ * The value corresponds to 2407 MHz.
+ */
+#define WF_CHAN_FACTOR_2_4_G		4814	/* 2.4 GHz band, 2407 MHz */
+
+/**
+ * Channel Factor for the starting frequence of 5 GHz channels.
+ * The value corresponds to 5000 MHz.
+ */
+#define WF_CHAN_FACTOR_5_G		10000	/* 5   GHz band, 5000 MHz */
+
+/**
+ * Channel Factor for the starting frequence of 4.9 GHz channels.
+ * The value corresponds to 4000 MHz.
+ */
+#define WF_CHAN_FACTOR_4_G		8000	/* 4.9 GHz band for Japan */
+
+/* defined rate in 500kbps */
+#define WLC_MAXRATE	108	/* in 500kbps units */
+#define WLC_RATE_1M	2	/* in 500kbps units */
+#define WLC_RATE_2M	4	/* in 500kbps units */
+#define WLC_RATE_5M5	11	/* in 500kbps units */
+#define WLC_RATE_11M	22	/* in 500kbps units */
+#define WLC_RATE_6M	12	/* in 500kbps units */
+#define WLC_RATE_9M	18	/* in 500kbps units */
+#define WLC_RATE_12M	24	/* in 500kbps units */
+#define WLC_RATE_18M	36	/* in 500kbps units */
+#define WLC_RATE_24M	48	/* in 500kbps units */
+#define WLC_RATE_36M	72	/* in 500kbps units */
+#define WLC_RATE_48M	96	/* in 500kbps units */
+#define WLC_RATE_54M	108	/* in 500kbps units */
+
+#define WLC_2G_25MHZ_OFFSET		5	/* 2.4GHz band channel offset */
+
+/**
+ * Convert chanspec to ascii string
+ *
+ * @param	chspec		chanspec format
+ * @param	buf		ascii string of chanspec
+ *
+ * @return	pointer to buf with room for at least CHANSPEC_STR_LEN bytes
+ *
+ * @see		CHANSPEC_STR_LEN
+ */
+extern char * wf_chspec_ntoa(chanspec_t chspec, char *buf);
+
+/**
+ * Convert ascii string to chanspec
+ *
+ * @param	a     pointer to input string
+ *
+ * @return	>= 0 if successful or 0 otherwise
+ */
+extern chanspec_t wf_chspec_aton(const char *a);
+
+/**
+ * Verify the chanspec fields are valid.
+ *
+ * Verify the chanspec is using a legal set field values, i.e. that the chanspec
+ * specified a band, bw, ctl_sb and channel and that the combination could be
+ * legal given some set of circumstances.
+ *
+ * @param	chanspec   input chanspec to verify
+ *
+ * @return TRUE if the chanspec is malformed, FALSE if it looks good.
+ */
+extern bool wf_chspec_malformed(chanspec_t chanspec);
+
+/**
+ * Verify the chanspec specifies a valid channel according to 802.11.
+ *
+ * @param	chanspec   input chanspec to verify
+ *
+ * @return TRUE if the chanspec is a valid 802.11 channel
+ */
+extern bool wf_chspec_valid(chanspec_t chanspec);
+
+/**
+ * Return the primary (control) channel.
+ *
+ * This function returns the channel number of the primary 20MHz channel. For
+ * 20MHz channels this is just the channel number. For 40MHz or wider channels
+ * it is the primary 20MHz channel specified by the chanspec.
+ *
+ * @param	chspec    input chanspec
+ *
+ * @return Returns the channel number of the primary 20MHz channel
+ */
+extern uint8 wf_chspec_ctlchan(chanspec_t chspec);
+
+/**
+ * Return the primary (control) chanspec.
+ *
+ * This function returns the chanspec of the primary 20MHz channel. For 20MHz
+ * channels this is just the chanspec. For 40MHz or wider channels it is the
+ * chanspec of the primary 20MHZ channel specified by the chanspec.
+ *
+ * @param	chspec    input chanspec
+ *
+ * @return Returns the chanspec of the primary 20MHz channel
+ */
+extern chanspec_t wf_chspec_ctlchspec(chanspec_t chspec);
+
+/**
+ * Return a channel number corresponding to a frequency.
+ *
+ * Return the channel number for a given frequency and base frequency.
+ * The returned channel number is relative to the given base frequency.
+ * If the given base frequency is zero, a base frequency of 5 GHz is assumed for
+ * frequencies from 5 - 6 GHz, and 2.407 GHz is assumed for 2.4 - 2.5 GHz.
+ *
+ * Frequency is specified in MHz.
+ * The base frequency is specified as (start_factor * 500 kHz).
+ * Constants WF_CHAN_FACTOR_2_4_G, WF_CHAN_FACTOR_5_G are defined for
+ * 2.4 GHz and 5 GHz bands.
+ *
+ * The returned channel will be in the range [1, 14] in the 2.4 GHz band
+ * and [0, 200] otherwise.
+ * -1 is returned if the start_factor is WF_CHAN_FACTOR_2_4_G and the
+ * frequency is not a 2.4 GHz channel, or if the frequency is not and even
+ * multiple of 5 MHz from the base frequency to the base plus 1 GHz.
+ *
+ * Reference 802.11 REVma, section 17.3.8.3, and 802.11B section 18.4.6.2
+ *
+ * @param	freq          frequency in MHz
+ * @param	start_factor  base frequency in 500 kHz units, e.g. 10000 for 5 GHz
+ *
+ * @return Returns a channel number
+ *
+ * @see  WF_CHAN_FACTOR_2_4_G
+ * @see  WF_CHAN_FACTOR_5_G
+ */
+extern int wf_mhz2channel(uint freq, uint start_factor);
+
+/**
+ * Return the center frequency in MHz of the given channel and base frequency.
+ *
+ * Return the center frequency in MHz of the given channel and base frequency.
+ * The channel number is interpreted relative to the given base frequency.
+ *
+ * The valid channel range is [1, 14] in the 2.4 GHz band and [0, 200] otherwise.
+ * The base frequency is specified as (start_factor * 500 kHz).
+ * Constants WF_CHAN_FACTOR_2_4_G, WF_CHAN_FACTOR_5_G are defined for
+ * 2.4 GHz and 5 GHz bands.
+ * The channel range of [1, 14] is only checked for a start_factor of
+ * WF_CHAN_FACTOR_2_4_G (4814).
+ * Odd start_factors produce channels on .5 MHz boundaries, in which case
+ * the answer is rounded down to an integral MHz.
+ * -1 is returned for an out of range channel.
+ *
+ * Reference 802.11 REVma, section 17.3.8.3, and 802.11B section 18.4.6.2
+ *
+ * @param	channel       input channel number
+ * @param	start_factor  base frequency in 500 kHz units, e.g. 10000 for 5 GHz
+ *
+ * @return Returns a frequency in MHz
+ *
+ * @see  WF_CHAN_FACTOR_2_4_G
+ * @see  WF_CHAN_FACTOR_5_G
+ */
+extern int wf_channel2mhz(uint channel, uint start_factor);
+
+#endif	/* _bcmwifi_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/compvers.sh b/drivers/bcmdrivers/gmac/src/include/compvers.sh
new file mode 100755
index 0000000..3f6fd6a
