--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/sbsocram.h
@@ -0,0 +1,193 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * BCM47XX Sonics SiliconBackplane embedded ram core
+ *
+ * $Id: sbsocram.h 271781 2011-07-13 20:00:06Z $
+ */
+
+#ifndef	_SBSOCRAM_H
+#define	_SBSOCRAM_H
+
+#ifndef _LANGUAGE_ASSEMBLY
+
+/* cpp contortions to concatenate w/arg prescan */
+#ifndef PAD
+#define	_PADLINE(line)	pad ## line
+#define	_XSTR(line)	_PADLINE(line)
+#define	PAD		_XSTR(__LINE__)
+#endif	/* PAD */
+
+/* Memcsocram core registers */
+typedef volatile struct sbsocramregs {
+	uint32	coreinfo;
+	uint32	bwalloc;
+	uint32	extracoreinfo;
+	uint32	biststat;
+	uint32	bankidx;
+	uint32	standbyctrl;
+
+	uint32	errlogstatus;	/* rev 6 */
+	uint32	errlogaddr;	/* rev 6 */
+	/* used for patching rev 3 & 5 */
+	uint32	cambankidx;
+	uint32	cambankstandbyctrl;
+	uint32	cambankpatchctrl;
+	uint32	cambankpatchtblbaseaddr;
+	uint32	cambankcmdreg;
+	uint32	cambankdatareg;
+	uint32	cambankmaskreg;
+	uint32	PAD[1];
+	uint32	bankinfo;	/* corev 8 */
+	uint32	PAD[15];
+	uint32	extmemconfig;
+	uint32	extmemparitycsr;
+	uint32	extmemparityerrdata;
+	uint32	extmemparityerrcnt;
+	uint32	extmemwrctrlandsize;
+	uint32	PAD[84];
+	uint32	workaround;
+	uint32	pwrctl;		/* corerev >= 2 */
+	uint32	PAD[133];
+	uint32  sr_control;     /* corerev >= 15 */
+	uint32  sr_status;      /* corerev >= 15 */
+	uint32  sr_address;     /* corerev >= 15 */
+	uint32  sr_data;        /* corerev >= 15 */
+} sbsocramregs_t;
+
+#endif	/* _LANGUAGE_ASSEMBLY */
+
+/* Register offsets */
+#define	SR_COREINFO		0x00
+#define	SR_BWALLOC		0x04
+#define	SR_BISTSTAT		0x0c
+#define	SR_BANKINDEX		0x10
+#define	SR_BANKSTBYCTL		0x14
+#define SR_PWRCTL		0x1e8
+
+/* Coreinfo register */
+#define	SRCI_PT_MASK		0x00070000	/* corerev >= 6; port type[18:16] */
+#define	SRCI_PT_SHIFT		16
+/* port types : SRCI_PT_<processorPT>_<backplanePT> */
+#define SRCI_PT_OCP_OCP		0
+#define SRCI_PT_AXI_OCP		1
+#define SRCI_PT_ARM7AHB_OCP	2
+#define SRCI_PT_CM3AHB_OCP	3
+#define SRCI_PT_AXI_AXI		4
+#define SRCI_PT_AHB_AXI		5
+/* corerev >= 3 */
+#define SRCI_LSS_MASK		0x00f00000
+#define SRCI_LSS_SHIFT		20
+#define SRCI_LRS_MASK		0x0f000000
+#define SRCI_LRS_SHIFT		24
+
+/* In corerev 0, the memory size is 2 to the power of the
+ * base plus 16 plus to the contents of the memsize field plus 1.
+ */
+#define	SRCI_MS0_MASK		0xf
+#define SR_MS0_BASE		16
+
+/*
+ * In corerev 1 the bank size is 2 ^ the bank size field plus 14,
+ * the memory size is number of banks times bank size.
+ * The same applies to rom size.
+ */
+#define	SRCI_ROMNB_MASK		0xf000
+#define	SRCI_ROMNB_SHIFT	12
+#define	SRCI_ROMBSZ_MASK	0xf00
+#define	SRCI_ROMBSZ_SHIFT	8
+#define	SRCI_SRNB_MASK		0xf0
+#define	SRCI_SRNB_SHIFT		4
+#define	SRCI_SRBSZ_MASK		0xf
+#define	SRCI_SRBSZ_SHIFT	0
+
+#define SR_BSZ_BASE		14
+
+/* Standby control register */
+#define	SRSC_SBYOVR_MASK	0x80000000
+#define	SRSC_SBYOVR_SHIFT	31
+#define	SRSC_SBYOVRVAL_MASK	0x60000000
+#define	SRSC_SBYOVRVAL_SHIFT	29
+#define	SRSC_SBYEN_MASK		0x01000000	/* rev >= 3 */
+#define	SRSC_SBYEN_SHIFT	24
+
+/* Power control register */
+#define SRPC_PMU_STBYDIS_MASK	0x00000010	/* rev >= 3 */
+#define SRPC_PMU_STBYDIS_SHIFT	4
+#define SRPC_STBYOVRVAL_MASK	0x00000008
+#define SRPC_STBYOVRVAL_SHIFT	3
+#define SRPC_STBYOVR_MASK	0x00000007
+#define SRPC_STBYOVR_SHIFT	0
+
+/* Extra core capability register */
+#define SRECC_NUM_BANKS_MASK   0x000000F0
+#define SRECC_NUM_BANKS_SHIFT  4
+#define SRECC_BANKSIZE_MASK    0x0000000F
+#define SRECC_BANKSIZE_SHIFT   0
+
+#define SRECC_BANKSIZE(value)	 (1 << (value))
+
+/* CAM bank patch control */
+#define SRCBPC_PATCHENABLE 0x80000000
+
+#define SRP_ADDRESS   0x0001FFFC
+#define SRP_VALID     0x8000
+
+/* CAM bank command reg */
+#define SRCMD_WRITE  0x00020000
+#define SRCMD_READ   0x00010000
+#define SRCMD_DONE   0x80000000
+
+#define SRCMD_DONE_DLY	1000
+
+/* bankidx and bankinfo reg defines corerev >= 8 */
+#define SOCRAM_BANKINFO_SZMASK		0x7f
+#define SOCRAM_BANKIDX_ROM_MASK		0x100
+
+#define SOCRAM_BANKIDX_MEMTYPE_SHIFT	8
+/* socram bankinfo memtype */
+#define SOCRAM_MEMTYPE_RAM		0
+#define SOCRAM_MEMTYPE_R0M		1
+#define SOCRAM_MEMTYPE_DEVRAM		2
+
+#define	SOCRAM_BANKINFO_REG		0x40
+#define	SOCRAM_BANKIDX_REG		0x10
+#define	SOCRAM_BANKINFO_STDBY_MASK	0x400
+#define	SOCRAM_BANKINFO_STDBY_TIMER	0x800
+
+/* bankinfo rev >= 10 */
+#define SOCRAM_BANKINFO_DEVRAMSEL_SHIFT		13
+#define SOCRAM_BANKINFO_DEVRAMSEL_MASK		0x2000
+#define SOCRAM_BANKINFO_DEVRAMPRO_SHIFT		14
+#define SOCRAM_BANKINFO_DEVRAMPRO_MASK		0x4000
+#define SOCRAM_BANKINFO_SLPSUPP_SHIFT		15
+#define SOCRAM_BANKINFO_SLPSUPP_MASK		0x8000
+#define SOCRAM_BANKINFO_RETNTRAM_SHIFT		16
+#define SOCRAM_BANKINFO_RETNTRAM_MASK		0x00010000
+#define SOCRAM_BANKINFO_PDASZ_SHIFT		17
+#define SOCRAM_BANKINFO_PDASZ_MASK		0x003E0000
+#define SOCRAM_BANKINFO_DEVRAMREMAP_SHIFT	24
+#define SOCRAM_BANKINFO_DEVRAMREMAP_MASK	0x01000000
+
+/* extracoreinfo register */
+#define SOCRAM_DEVRAMBANK_MASK		0xF000
+#define SOCRAM_DEVRAMBANK_SHIFT		12
+
+/* bank info to calculate bank size */
+#define   SOCRAM_BANKINFO_SZBASE          8192
+#define SOCRAM_BANKSIZE_SHIFT         13      /* SOCRAM_BANKINFO_SZBASE */
+
+
+#endif	/* _SBSOCRAM_H */
diff --git a/drivers/bcmdrivers/gmac/src/include/siutils.h b/drivers/bcmdrivers/gmac/src/include/siutils.h
new file mode 100755
index 0000000..5e4ce7d
