--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/hndsoc.h
@@ -0,0 +1,269 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Broadcom HND chip & on-chip-interconnect-related definitions.
+ *
+ * $Id: hndsoc.h 325951 2012-04-05 06:03:27Z $
+ */
+
+#ifndef	_HNDSOC_H
+#define	_HNDSOC_H
+
+/* Include the soci specific files */
+#include <sbconfig.h>
+#include <aidmp.h>
+
+/*
+ * SOC Interconnect Address Map.
+ * All regions may not exist on all chips.
+ */
+#define SI_SDRAM_BASE		0x00000000	/* Physical SDRAM */
+#define SI_PCI_MEM		0x08000000	/* Host Mode sb2pcitranslation0 (64 MB) */
+#define SI_PCI_MEM_SZ		(64 * 1024 * 1024)
+#define SI_PCI_CFG		0x0c000000	/* Host Mode sb2pcitranslation1 (64 MB) */
+#define	SI_SDRAM_SWAPPED	0x10000000	/* Byteswapped Physical SDRAM */
+#define SI_SDRAM_R2		0x80000000	/* Region 2 for sdram (512 MB) */
+
+#ifdef SI_ENUM_BASE_VARIABLE
+#define SI_ENUM_BASE		(sii->pub.si_enum_base)
+#else
+#define SI_ENUM_BASE    	0x18000000	/* Enumeration space base */
+#endif /* SI_ENUM_BASE_VARIABLE */
+
+#define SI_WRAP_BASE    	0x18100000	/* Wrapper space base */
+#define SI_CORE_SIZE    	0x1000		/* each core gets 4Kbytes for registers */
+#define	SI_MAXCORES		20		/* Max cores (this is arbitrary, for software
+						 * convenience and could be changed if we
+						 * make any larger chips
+						 */
+
+#define	SI_FASTRAM		0x19000000	/* On-chip RAM on chips that also have DDR */
+#define	SI_FASTRAM_SWAPPED	0x19800000
+
+#define	SI_FLASH2		0x1c000000	/* Flash Region 2 (region 1 shadowed here) */
+#define	SI_FLASH2_SZ		0x02000000	/* Size of Flash Region 2 */
+#define	SI_ARMCM3_ROM		0x1e000000	/* ARM Cortex-M3 ROM */
+#define	SI_FLASH1		0x1fc00000	/* MIPS Flash Region 1 */
+#define	SI_FLASH1_SZ		0x00400000	/* MIPS Size of Flash Region 1 */
+
+#define SI_NS_NANDFLASH		0x1c000000	/* NorthStar NAND flash base */
+#define SI_NS_NORFLASH		0x1e000000	/* NorthStar NOR flash base */
+#define	SI_NS_NORFLASH_SZ	0x02000000	/* Size of NorthStar NOR flash region */
+#define SI_NS_ROM		0xfffd0000	/* NorthStar ROM */
+
+#define	SI_ARM7S_ROM		0x20000000	/* ARM7TDMI-S ROM */
+#define	SI_ARMCR4_ROM		0x000f0000	/* ARM Cortex-R4 ROM */
+#define	SI_ARMCM3_SRAM2		0x60000000	/* ARM Cortex-M3 SRAM Region 2 */
+#define	SI_ARM7S_SRAM2		0x80000000	/* ARM7TDMI-S SRAM Region 2 */
+#define	SI_ARM_FLASH1		0xffff0000	/* ARM Flash Region 1 */
+#define	SI_ARM_FLASH1_SZ	0x00010000	/* ARM Size of Flash Region 1 */
+
+#define SI_PCI_DMA		0x40000000	/* Client Mode sb2pcitranslation2 (1 GB) */
+#define SI_PCI_DMA2		0x80000000	/* Client Mode sb2pcitranslation2 (1 GB) */
+#define SI_PCI_DMA_SZ		0x40000000	/* Client Mode sb2pcitranslation2 size in bytes */
+#define SI_PCIE_DMA_L32		0x00000000	/* PCIE Client Mode sb2pcitranslation2
+						 * (2 ZettaBytes), low 32 bits
+						 */
+#define SI_PCIE_DMA_H32		0x80000000	/* PCIE Client Mode sb2pcitranslation2
+						 * (2 ZettaBytes), high 32 bits
+						 */
+#define SI_NS_CUR		0x1800B000	/* NorthStar CUR base */
+
+#if defined(CONFIG_MACH_NS)
+#define SI_NS_CHIPCB_SRAB	0x18007000	/* NorthStar Chip Common B SRAB base */
+#else
+#define SI_NS_CHIPCB_SRAB	0x18036000	/* NorthStar+ Chip Common B SRAB base */
+#endif
+
+/* core codes */
+#define	NODEV_CORE_ID		0x700		/* Invalid coreid */
+#define	CC_CORE_ID		0x800		/* chipcommon core */
+#define	ILINE20_CORE_ID		0x801		/* iline20 core */
+#define	SRAM_CORE_ID		0x802		/* sram core */
+#define	SDRAM_CORE_ID		0x803		/* sdram core */
+#define	PCI_CORE_ID		0x804		/* pci core */
+#define	MIPS_CORE_ID		0x805		/* mips core */
+#define	ENET_CORE_ID		0x806		/* enet mac core */
+#define	CODEC_CORE_ID		0x807		/* v90 codec core */
+#define	USB_CORE_ID		0x808		/* usb 1.1 host/device core */
+#define	ADSL_CORE_ID		0x809		/* ADSL core */
+#define	ILINE100_CORE_ID	0x80a		/* iline100 core */
+#define	IPSEC_CORE_ID		0x80b		/* ipsec core */
+#define	UTOPIA_CORE_ID		0x80c		/* utopia core */
+#define	PCMCIA_CORE_ID		0x80d		/* pcmcia core */
+#define	SOCRAM_CORE_ID		0x80e		/* internal memory core */
+#define	MEMC_CORE_ID		0x80f		/* memc sdram core */
+#define	OFDM_CORE_ID		0x810		/* OFDM phy core */
+#define	EXTIF_CORE_ID		0x811		/* external interface core */
+#define	D11_CORE_ID		0x812		/* 802.11 MAC core */
+#define	APHY_CORE_ID		0x813		/* 802.11a phy core */
+#define	BPHY_CORE_ID		0x814		/* 802.11b phy core */
+#define	GPHY_CORE_ID		0x815		/* 802.11g phy core */
+#define	MIPS33_CORE_ID		0x816		/* mips3302 core */
+#define	USB11H_CORE_ID		0x817		/* usb 1.1 host core */
+#define	USB11D_CORE_ID		0x818		/* usb 1.1 device core */
+#define	USB20H_CORE_ID		0x819		/* usb 2.0 host core */
+#define	USB20D_CORE_ID		0x81a		/* usb 2.0 device core */
+#define	SDIOH_CORE_ID		0x81b		/* sdio host core */
+#define	ROBO_CORE_ID		0x81c		/* roboswitch core */
+#define	ATA100_CORE_ID		0x81d		/* parallel ATA core */
+#define	SATAXOR_CORE_ID		0x81e		/* serial ATA & XOR DMA core */
+#define	GIGETH_CORE_ID		0x81f		/* gigabit ethernet core */
+#define	PCIE_CORE_ID		0x820		/* pci express core */
+#define	NPHY_CORE_ID		0x821		/* 802.11n 2x2 phy core */
+#define	SRAMC_CORE_ID		0x822		/* SRAM controller core */
+#define	MINIMAC_CORE_ID		0x823		/* MINI MAC/phy core */
+#define	ARM11_CORE_ID		0x824		/* ARM 1176 core */
+#define	ARM7S_CORE_ID		0x825		/* ARM7tdmi-s core */
+#define	LPPHY_CORE_ID		0x826		/* 802.11a/b/g phy core */
+#define	PMU_CORE_ID		0x827		/* PMU core */
+#define	SSNPHY_CORE_ID		0x828		/* 802.11n single-stream phy core */
+#define	SDIOD_CORE_ID		0x829		/* SDIO device core */
+#define	ARMCM3_CORE_ID		0x82a		/* ARM Cortex M3 core */
+#define	HTPHY_CORE_ID		0x82b		/* 802.11n 4x4 phy core */
+#define	MIPS74K_CORE_ID		0x82c		/* mips 74k core */
+#define	GMAC_CORE_ID		0x82d		/* Gigabit MAC core */
+#define	DMEMC_CORE_ID		0x82e		/* DDR1/2 memory controller core */
+#define	PCIERC_CORE_ID		0x82f		/* PCIE Root Complex core */
+#define	OCP_CORE_ID		0x830		/* OCP2OCP bridge core */
+#define	SC_CORE_ID		0x831		/* shared common core */
+#define	AHB_CORE_ID		0x832		/* OCP2AHB bridge core */
+#define	SPIH_CORE_ID		0x833		/* SPI host core */
+#define	I2S_CORE_ID		0x834		/* I2S core */
+#define	DMEMS_CORE_ID		0x835		/* SDR/DDR1 memory controller core */
+#define	DEF_SHIM_COMP		0x837		/* SHIM component in ubus/6362 */
+
+#define ACPHY_CORE_ID		0x83b		/* Dot11 ACPHY */
+#define PCIE2_CORE_ID		0x83c		/* pci express Gen2 core */
+#define USB30D_CORE_ID		0x83d		/* usb 3.0 device core */
+#define ARMCR4_CORE_ID		0x83e		/* ARM CR4 CPU */
+#define APB_BRIDGE_CORE_ID	0x135		/* APB bridge core ID */
+#define AXI_CORE_ID		0x301		/* AXI/GPV core ID */
+#define EROM_CORE_ID		0x366		/* EROM core ID */
+#define OOB_ROUTER_CORE_ID	0x367		/* OOB router core ID */
+#define DEF_AI_COMP		0xfff		/* Default component, in ai chips it maps all
+						 * unused address ranges
+						 */
+
+#define CC_4706_CORE_ID		0x500		/* chipcommon core */
+#define NS_PCIEG2_CORE_ID	0x501		/* PCIE Gen 2 core */
+#define NS_DMA_CORE_ID		0x502		/* DMA core */
+#define NS_SDIO3_CORE_ID	0x503		/* SDIO3 core */
+#define NS_USB20_CORE_ID	0x504		/* USB2.0 core */
+#define NS_USB30_CORE_ID	0x505		/* USB3.0 core */
+#define NS_A9JTAG_CORE_ID	0x506		/* ARM Cortex A9 JTAG core */
+#define NS_DDR23_CORE_ID	0x507		/* Denali DDR2/DDR3 memory controller */
+#define NS_ROM_CORE_ID		0x508		/* ROM core */
+#define NS_NAND_CORE_ID		0x509		/* NAND flash controller core */
+#define NS_QSPI_CORE_ID		0x50a		/* SPI flash controller core */
+#define NS_CCB_CORE_ID		0x50b		/* ChipcommonB core */
+#define SOCRAM_4706_CORE_ID	0x50e		/* internal memory core */
+#define NS_SOCRAM_CORE_ID	SOCRAM_4706_CORE_ID
+#define	ARMCA9_CORE_ID		0x510		/* ARM Cortex A9 core (ihost) */
+#define	NS_IHOST_CORE_ID	ARMCA9_CORE_ID	/* ARM Cortex A9 core (ihost) */
+#define GMAC_COMMON_4706_CORE_ID	0x5dc		/* Gigabit MAC core */
+#define GMAC_4706_CORE_ID	0x52d		/* Gigabit MAC core */
+#define AMEMC_CORE_ID		0x52e		/* DDR1/2 memory controller core */
+#define ALTA_CORE_ID		0x534		/* I2S core */
+#define DDR23_PHY_CORE_ID	0x5dd
+
+#define SI_PCI1_MEM     0x40000000  /* Host Mode sb2pcitranslation0 (64 MB) */
+#define SI_PCI1_CFG     0x44000000  /* Host Mode sb2pcitranslation1 (64 MB) */
+#define SI_PCIE1_DMA_H32		0xc0000000	/* PCIE Client Mode sb2pcitranslation2
+						 * (2 ZettaBytes), high 32 bits
+						 */
+#define CC_4706B0_CORE_REV	0x8000001f		/* chipcommon core */
+#define SOCRAM_4706B0_CORE_REV	0x80000005		/* internal memory core */
+#define GMAC_4706B0_CORE_REV	0x80000000		/* Gigabit MAC core */
+
+/* There are TWO constants on all HND chips: SI_ENUM_BASE above,
+ * and chipcommon being the first core:
+ */
+#define	SI_CC_IDX		0
+
+/* SOC Interconnect types (aka chip types) */
+#define	SOCI_SB			0
+#define	SOCI_AI			1
+#define	SOCI_UBUS		2
+#define	SOCI_NS			3
+
+/* Common core control flags */
+#define	SICF_BIST_EN		0x8000
+#define	SICF_PME_EN		0x4000
+#define	SICF_CORE_BITS		0x3ffc
+#define	SICF_FGC		0x0002
+#define	SICF_CLOCK_EN		0x0001
+
+/* Common core status flags */
+#define	SISF_BIST_DONE		0x8000
+#define	SISF_BIST_ERROR		0x4000
+#define	SISF_GATED_CLK		0x2000
+#define	SISF_DMA64		0x1000
+#define	SISF_CORE_BITS		0x0fff
+
+/* Norstar core status flags */
+#define SISF_NS_BOOTDEV_MASK	0x0003	/* ROM core */
+#define SISF_NS_BOOTDEV_NOR	0x0000	/* ROM core */
+#define SISF_NS_BOOTDEV_NAND	0x0001	/* ROM core */
+#define SISF_NS_BOOTDEV_ROM	0x0002	/* ROM core */
+#define SISF_NS_BOOTDEV_OFFLOAD	0x0003	/* ROM core */
+#define SISF_NS_SKUVEC_MASK	0x000c	/* ROM core */
+
+/* A register that is common to all cores to
+ * communicate w/PMU regarding clock control.
+ */
+#define SI_CLK_CTL_ST		0x1e0		/* clock control and status */
+
+/* clk_ctl_st register */
+#define	CCS_FORCEALP		0x00000001	/* force ALP request */
+#define	CCS_FORCEHT		0x00000002	/* force HT request */
+#define	CCS_FORCEILP		0x00000004	/* force ILP request */
+#define	CCS_ALPAREQ		0x00000008	/* ALP Avail Request */
+#define	CCS_HTAREQ		0x00000010	/* HT Avail Request */
+#define	CCS_FORCEHWREQOFF	0x00000020	/* Force HW Clock Request Off */
+#define CCS_HQCLKREQ		0x00000040	/* HQ Clock Required */
+#define CCS_USBCLKREQ		0x00000100	/* USB Clock Req */
+#define CCS_ERSRC_REQ_MASK	0x00000700	/* external resource requests */
+#define CCS_ERSRC_REQ_SHIFT	8
+#define	CCS_ALPAVAIL		0x00010000	/* ALP is available */
+#define	CCS_HTAVAIL		0x00020000	/* HT is available */
+#define CCS_BP_ON_APL		0x00040000	/* RO: Backplane is running on ALP clock */
+#define CCS_BP_ON_HT		0x00080000	/* RO: Backplane is running on HT clock */
+#define CCS_ERSRC_STS_MASK	0x07000000	/* external resource status */
+#define CCS_ERSRC_STS_SHIFT	24
+
+#define	CCS0_HTAVAIL		0x00010000	/* HT avail in chipc and pcmcia on 4328a0 */
+#define	CCS0_ALPAVAIL		0x00020000	/* ALP avail in chipc and pcmcia on 4328a0 */
+
+/* Not really related to SOC Interconnect, but a couple of software
+ * conventions for the use the flash space:
+ */
+
+/* Minumum amount of flash we support */
+#define FLASH_MIN		0x00020000	/* Minimum flash size */
+
+/* A boot/binary may have an embedded block that describes its size  */
+#define	BISZ_OFFSET		0x3e0		/* At this offset into the binary */
+#define	BISZ_MAGIC		0x4249535a	/* Marked with this value: 'BISZ' */
+#define	BISZ_MAGIC_IDX		0		/* Word 0: magic */
+#define	BISZ_TXTST_IDX		1		/*	1: text start */
+#define	BISZ_TXTEND_IDX		2		/*	2: text end */
+#define	BISZ_DATAST_IDX		3		/*	3: data start */
+#define	BISZ_DATAEND_IDX	4		/*	4: data end */
+#define	BISZ_BSSST_IDX		5		/*	5: bss start */
+#define	BISZ_BSSEND_IDX		6		/*	6: bss end */
+#define BISZ_SIZE		7		/* descriptor size in 32-bit integers */
+
+#endif /* _HNDSOC_H */
diff --git a/drivers/bcmdrivers/gmac/src/include/hndtcam.h b/drivers/bcmdrivers/gmac/src/include/hndtcam.h
new file mode 100755
index 0000000..da7acf8
