--- /dev/null
+++ b/arch/arm/plat-iproc/include/mach/gpio.h
@@ -0,0 +1,30 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+#ifndef __PLAT_GPIO_H
+#define __PLAT_GPIO_H
+
+#include <mach/iproc_regs.h>
+#include <mach/irqs.h>
+
+#include <asm-generic/gpio.h>
+
+
+#define gpio_to_irq(gpio)           __gpio_to_irq(gpio)
+//#define gpio_get_value(gpio)		__gpio_get_value(gpio)
+//#define gpio_set_value(gpio,value)  __gpio_set_value(gpio,value)
+//#define gpio_cansleep(gpio)		   __gpio_cansleep(gpio)
+
+#endif
diff --git a/arch/arm/plat-iproc/include/mach/hardware.h b/arch/arm/plat-iproc/include/mach/hardware.h
new file mode 100644
index 0000000..b373b58
