--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/proto/bcmeth.h
@@ -0,0 +1,106 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Broadcom Ethernettype  protocol definitions
+ *
+ * $Id: bcmeth.h 294352 2011-11-06 19:23:00Z $
+ */
+
+/*
+ * Broadcom Ethernet protocol defines
+ */
+
+#ifndef _BCMETH_H_
+#define _BCMETH_H_
+
+#ifndef _TYPEDEFS_H_
+#include <typedefs.h>
+#endif
+
+/* This marks the start of a packed structure section. */
+#include <packed_section_start.h>
+
+/* ETHER_TYPE_BRCM is defined in ethernet.h */
+
+/*
+ * Following the 2byte BRCM ether_type is a 16bit BRCM subtype field
+ * in one of two formats: (only subtypes 32768-65535 are in use now)
+ *
+ * subtypes 0-32767:
+ *     8 bit subtype (0-127)
+ *     8 bit length in bytes (0-255)
+ *
+ * subtypes 32768-65535:
+ *     16 bit big-endian subtype
+ *     16 bit big-endian length in bytes (0-65535)
+ *
+ * length is the number of additional bytes beyond the 4 or 6 byte header
+ *
+ * Reserved values:
+ * 0 reserved
+ * 5-15 reserved for iLine protocol assignments
+ * 17-126 reserved, assignable
+ * 127 reserved
+ * 32768 reserved
+ * 32769-65534 reserved, assignable
+ * 65535 reserved
+ */
+
+/*
+ * While adding the subtypes and their specific processing code make sure
+ * bcmeth_bcm_hdr_t is the first data structure in the user specific data structure definition
+ */
+
+#define	BCMILCP_SUBTYPE_RATE		1
+#define	BCMILCP_SUBTYPE_LINK		2
+#define	BCMILCP_SUBTYPE_CSA		3
+#define	BCMILCP_SUBTYPE_LARQ		4
+#define BCMILCP_SUBTYPE_VENDOR		5
+#define	BCMILCP_SUBTYPE_FLH		17
+
+#define BCMILCP_SUBTYPE_VENDOR_LONG	32769
+#define BCMILCP_SUBTYPE_CERT		32770
+#define BCMILCP_SUBTYPE_SES		32771
+
+
+#define BCMILCP_BCM_SUBTYPE_RESERVED		0
+#define BCMILCP_BCM_SUBTYPE_EVENT		1
+#define BCMILCP_BCM_SUBTYPE_SES			2
+/*
+ * The EAPOL type is not used anymore. Instead EAPOL messages are now embedded
+ * within BCMILCP_BCM_SUBTYPE_EVENT type messages
+ */
+/* #define BCMILCP_BCM_SUBTYPE_EAPOL		3 */
+#define BCMILCP_BCM_SUBTYPE_DPT			4
+
+#define BCMILCP_BCM_SUBTYPEHDR_MINLENGTH	8
+#define BCMILCP_BCM_SUBTYPEHDR_VERSION		0
+
+/* These fields are stored in network order */
+typedef BWL_PRE_PACKED_STRUCT struct bcmeth_hdr
+{
+	uint16	subtype;	/* Vendor specific..32769 */
+	uint16	length;
+	uint8	version;	/* Version is 0 */
+	uint8	oui[3];		/* Broadcom OUI */
+	/* user specific Data */
+	uint16	usr_subtype;
+} BWL_POST_PACKED_STRUCT bcmeth_hdr_t;
+
+
+/* This marks the end of a packed structure section. */
+#include <packed_section_end.h>
+
+#endif	/*  _BCMETH_H_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/proto/bcmevent.h b/drivers/bcmdrivers/gmac/src/include/proto/bcmevent.h
new file mode 100755
index 0000000..57776ae
