--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/sbconfig.h
@@ -0,0 +1,276 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Broadcom SiliconBackplane hardware register definitions.
+ *
+ * $Id: sbconfig.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef	_SBCONFIG_H
+#define	_SBCONFIG_H
+
+/* cpp contortions to concatenate w/arg prescan */
+#ifndef PAD
+#define	_PADLINE(line)	pad ## line
+#define	_XSTR(line)	_PADLINE(line)
+#define	PAD		_XSTR(__LINE__)
+#endif
+
+/* enumeration in SB is based on the premise that cores are contiguos in the
+ * enumeration space.
+ */
+#define SB_BUS_SIZE		0x10000		/* Each bus gets 64Kbytes for cores */
+#define SB_BUS_BASE(b)		(SI_ENUM_BASE + (b) * SB_BUS_SIZE)
+#define	SB_BUS_MAXCORES		(SB_BUS_SIZE / SI_CORE_SIZE)	/* Max cores per bus */
+
+/*
+ * Sonics Configuration Space Registers.
+ */
+#define	SBCONFIGOFF		0xf00		/* core sbconfig regs are top 256bytes of regs */
+#define	SBCONFIGSIZE		256		/* sizeof (sbconfig_t) */
+
+#define SBIPSFLAG		0x08
+#define SBTPSFLAG		0x18
+#define	SBTMERRLOGA		0x48		/* sonics >= 2.3 */
+#define	SBTMERRLOG		0x50		/* sonics >= 2.3 */
+#define SBADMATCH3		0x60
+#define SBADMATCH2		0x68
+#define SBADMATCH1		0x70
+#define SBIMSTATE		0x90
+#define SBINTVEC		0x94
+#define SBTMSTATELOW		0x98
+#define SBTMSTATEHIGH		0x9c
+#define SBBWA0			0xa0
+#define SBIMCONFIGLOW		0xa8
+#define SBIMCONFIGHIGH		0xac
+#define SBADMATCH0		0xb0
+#define SBTMCONFIGLOW		0xb8
+#define SBTMCONFIGHIGH		0xbc
+#define SBBCONFIG		0xc0
+#define SBBSTATE		0xc8
+#define SBACTCNFG		0xd8
+#define	SBFLAGST		0xe8
+#define SBIDLOW			0xf8
+#define SBIDHIGH		0xfc
+
+/* All the previous registers are above SBCONFIGOFF, but with Sonics 2.3, we have
+ * a few registers *below* that line. I think it would be very confusing to try
+ * and change the value of SBCONFIGOFF, so I'm definig them as absolute offsets here,
+ */
+
+#define SBIMERRLOGA		0xea8
+#define SBIMERRLOG		0xeb0
+#define SBTMPORTCONNID0		0xed8
+#define SBTMPORTLOCK0		0xef8
+
+#ifndef _LANGUAGE_ASSEMBLY
+
+typedef volatile struct _sbconfig {
+	uint32	PAD[2];
+	uint32	sbipsflag;		/* initiator port ocp slave flag */
+	uint32	PAD[3];
+	uint32	sbtpsflag;		/* target port ocp slave flag */
+	uint32	PAD[11];
+	uint32	sbtmerrloga;		/* (sonics >= 2.3) */
+	uint32	PAD;
+	uint32	sbtmerrlog;		/* (sonics >= 2.3) */
+	uint32	PAD[3];
+	uint32	sbadmatch3;		/* address match3 */
+	uint32	PAD;
+	uint32	sbadmatch2;		/* address match2 */
+	uint32	PAD;
+	uint32	sbadmatch1;		/* address match1 */
+	uint32	PAD[7];
+	uint32	sbimstate;		/* initiator agent state */
+	uint32	sbintvec;		/* interrupt mask */
+	uint32	sbtmstatelow;		/* target state */
+	uint32	sbtmstatehigh;		/* target state */
+	uint32	sbbwa0;			/* bandwidth allocation table0 */
+	uint32	PAD;
+	uint32	sbimconfiglow;		/* initiator configuration */
+	uint32	sbimconfighigh;		/* initiator configuration */
+	uint32	sbadmatch0;		/* address match0 */
+	uint32	PAD;
+	uint32	sbtmconfiglow;		/* target configuration */
+	uint32	sbtmconfighigh;		/* target configuration */
+	uint32	sbbconfig;		/* broadcast configuration */
+	uint32	PAD;
+	uint32	sbbstate;		/* broadcast state */
+	uint32	PAD[3];
+	uint32	sbactcnfg;		/* activate configuration */
+	uint32	PAD[3];
+	uint32	sbflagst;		/* current sbflags */
+	uint32	PAD[3];
+	uint32	sbidlow;		/* identification */
+	uint32	sbidhigh;		/* identification */
+} sbconfig_t;
+
+#endif /* _LANGUAGE_ASSEMBLY */
+
+/* sbipsflag */
+#define	SBIPS_INT1_MASK		0x3f		/* which sbflags get routed to mips interrupt 1 */
+#define	SBIPS_INT1_SHIFT	0
+#define	SBIPS_INT2_MASK		0x3f00		/* which sbflags get routed to mips interrupt 2 */
+#define	SBIPS_INT2_SHIFT	8
+#define	SBIPS_INT3_MASK		0x3f0000	/* which sbflags get routed to mips interrupt 3 */
+#define	SBIPS_INT3_SHIFT	16
+#define	SBIPS_INT4_MASK		0x3f000000	/* which sbflags get routed to mips interrupt 4 */
+#define	SBIPS_INT4_SHIFT	24
+
+/* sbtpsflag */
+#define	SBTPS_NUM0_MASK		0x3f		/* interrupt sbFlag # generated by this core */
+#define	SBTPS_F0EN0		0x40		/* interrupt is always sent on the backplane */
+
+/* sbtmerrlog */
+#define	SBTMEL_CM		0x00000007	/* command */
+#define	SBTMEL_CI		0x0000ff00	/* connection id */
+#define	SBTMEL_EC		0x0f000000	/* error code */
+#define	SBTMEL_ME		0x80000000	/* multiple error */
+
+/* sbimstate */
+#define	SBIM_PC			0xf		/* pipecount */
+#define	SBIM_AP_MASK		0x30		/* arbitration policy */
+#define	SBIM_AP_BOTH		0x00		/* use both timeslaces and token */
+#define	SBIM_AP_TS		0x10		/* use timesliaces only */
+#define	SBIM_AP_TK		0x20		/* use token only */
+#define	SBIM_AP_RSV		0x30		/* reserved */
+#define	SBIM_IBE		0x20000		/* inbanderror */
+#define	SBIM_TO			0x40000		/* timeout */
+#define	SBIM_BY			0x01800000	/* busy (sonics >= 2.3) */
+#define	SBIM_RJ			0x02000000	/* reject (sonics >= 2.3) */
+
+/* sbtmstatelow */
+#define	SBTML_RESET		0x0001		/* reset */
+#define	SBTML_REJ_MASK		0x0006		/* reject field */
+#define	SBTML_REJ		0x0002		/* reject */
+#define	SBTML_TMPREJ		0x0004		/* temporary reject, for error recovery */
+
+#define	SBTML_SICF_SHIFT	16		/* Shift to locate the SI control flags in sbtml */
+
+/* sbtmstatehigh */
+#define	SBTMH_SERR		0x0001		/* serror */
+#define	SBTMH_INT		0x0002		/* interrupt */
+#define	SBTMH_BUSY		0x0004		/* busy */
+#define	SBTMH_TO		0x0020		/* timeout (sonics >= 2.3) */
+
+#define	SBTMH_SISF_SHIFT	16		/* Shift to locate the SI status flags in sbtmh */
+
+/* sbbwa0 */
+#define	SBBWA_TAB0_MASK		0xffff		/* lookup table 0 */
+#define	SBBWA_TAB1_MASK		0xffff		/* lookup table 1 */
+#define	SBBWA_TAB1_SHIFT	16
+
+/* sbimconfiglow */
+#define	SBIMCL_STO_MASK		0x7		/* service timeout */
+#define	SBIMCL_RTO_MASK		0x70		/* request timeout */
+#define	SBIMCL_RTO_SHIFT	4
+#define	SBIMCL_CID_MASK		0xff0000	/* connection id */
+#define	SBIMCL_CID_SHIFT	16
+
+/* sbimconfighigh */
+#define	SBIMCH_IEM_MASK		0xc		/* inband error mode */
+#define	SBIMCH_TEM_MASK		0x30		/* timeout error mode */
+#define	SBIMCH_TEM_SHIFT	4
+#define	SBIMCH_BEM_MASK		0xc0		/* bus error mode */
+#define	SBIMCH_BEM_SHIFT	6
+
+/* sbadmatch0 */
+#define	SBAM_TYPE_MASK		0x3		/* address type */
+#define	SBAM_AD64		0x4		/* reserved */
+#define	SBAM_ADINT0_MASK	0xf8		/* type0 size */
+#define	SBAM_ADINT0_SHIFT	3
+#define	SBAM_ADINT1_MASK	0x1f8		/* type1 size */
+#define	SBAM_ADINT1_SHIFT	3
+#define	SBAM_ADINT2_MASK	0x1f8		/* type2 size */
+#define	SBAM_ADINT2_SHIFT	3
+#define	SBAM_ADEN		0x400		/* enable */
+#define	SBAM_ADNEG		0x800		/* negative decode */
+#define	SBAM_BASE0_MASK		0xffffff00	/* type0 base address */
+#define	SBAM_BASE0_SHIFT	8
+#define	SBAM_BASE1_MASK		0xfffff000	/* type1 base address for the core */
+#define	SBAM_BASE1_SHIFT	12
+#define	SBAM_BASE2_MASK		0xffff0000	/* type2 base address for the core */
+#define	SBAM_BASE2_SHIFT	16
+
+/* sbtmconfiglow */
+#define	SBTMCL_CD_MASK		0xff		/* clock divide */
+#define	SBTMCL_CO_MASK		0xf800		/* clock offset */
+#define	SBTMCL_CO_SHIFT		11
+#define	SBTMCL_IF_MASK		0xfc0000	/* interrupt flags */
+#define	SBTMCL_IF_SHIFT		18
+#define	SBTMCL_IM_MASK		0x3000000	/* interrupt mode */
+#define	SBTMCL_IM_SHIFT		24
+
+/* sbtmconfighigh */
+#define	SBTMCH_BM_MASK		0x3		/* busy mode */
+#define	SBTMCH_RM_MASK		0x3		/* retry mode */
+#define	SBTMCH_RM_SHIFT		2
+#define	SBTMCH_SM_MASK		0x30		/* stop mode */
+#define	SBTMCH_SM_SHIFT		4
+#define	SBTMCH_EM_MASK		0x300		/* sb error mode */
+#define	SBTMCH_EM_SHIFT		8
+#define	SBTMCH_IM_MASK		0xc00		/* int mode */
+#define	SBTMCH_IM_SHIFT		10
+
+/* sbbconfig */
+#define	SBBC_LAT_MASK		0x3		/* sb latency */
+#define	SBBC_MAX0_MASK		0xf0000		/* maxccntr0 */
+#define	SBBC_MAX0_SHIFT		16
+#define	SBBC_MAX1_MASK		0xf00000	/* maxccntr1 */
+#define	SBBC_MAX1_SHIFT		20
+
+/* sbbstate */
+#define	SBBS_SRD		0x1		/* st reg disable */
+#define	SBBS_HRD		0x2		/* hold reg disable */
+
+/* sbidlow */
+#define	SBIDL_CS_MASK		0x3		/* config space */
+#define	SBIDL_AR_MASK		0x38		/* # address ranges supported */
+#define	SBIDL_AR_SHIFT		3
+#define	SBIDL_SYNCH		0x40		/* sync */
+#define	SBIDL_INIT		0x80		/* initiator */
+#define	SBIDL_MINLAT_MASK	0xf00		/* minimum backplane latency */
+#define	SBIDL_MINLAT_SHIFT	8
+#define	SBIDL_MAXLAT		0xf000		/* maximum backplane latency */
+#define	SBIDL_MAXLAT_SHIFT	12
+#define	SBIDL_FIRST		0x10000		/* this initiator is first */
+#define	SBIDL_CW_MASK		0xc0000		/* cycle counter width */
+#define	SBIDL_CW_SHIFT		18
+#define	SBIDL_TP_MASK		0xf00000	/* target ports */
+#define	SBIDL_TP_SHIFT		20
+#define	SBIDL_IP_MASK		0xf000000	/* initiator ports */
+#define	SBIDL_IP_SHIFT		24
+#define	SBIDL_RV_MASK		0xf0000000	/* sonics backplane revision code */
+#define	SBIDL_RV_SHIFT		28
+#define	SBIDL_RV_2_2		0x00000000	/* version 2.2 or earlier */
+#define	SBIDL_RV_2_3		0x10000000	/* version 2.3 */
+
+/* sbidhigh */
+#define	SBIDH_RC_MASK		0x000f		/* revision code */
+#define	SBIDH_RCE_MASK		0x7000		/* revision code extension field */
+#define	SBIDH_RCE_SHIFT		8
+#define	SBCOREREV(sbidh) \
+	((((sbidh) & SBIDH_RCE_MASK) >> SBIDH_RCE_SHIFT) | ((sbidh) & SBIDH_RC_MASK))
+#define	SBIDH_CC_MASK		0x8ff0		/* core code */
+#define	SBIDH_CC_SHIFT		4
+#define	SBIDH_VC_MASK		0xffff0000	/* vendor code */
+#define	SBIDH_VC_SHIFT		16
+
+#define	SB_COMMIT		0xfd8		/* update buffered registers value */
+
+/* vendor codes */
+#define	SB_VEND_BCM		0x4243		/* Broadcom's SB vendor code */
+
+#endif	/* _SBCONFIG_H */
diff --git a/drivers/bcmdrivers/gmac/src/include/sbhndarm.h b/drivers/bcmdrivers/gmac/src/include/sbhndarm.h
new file mode 100755
index 0000000..f925da3
