--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/proto/802.11.h
@@ -0,0 +1,2356 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Fundamental types and constants relating to 802.11
+ *
+ * $Id: 802.11.h 308961 2012-01-18 03:01:00Z $
+ */
+
+#ifndef _802_11_H_
+#define _802_11_H_
+
+#ifndef _TYPEDEFS_H_
+#include <typedefs.h>
+#endif
+
+#ifndef _NET_ETHERNET_H_
+#include <proto/ethernet.h>
+#endif
+
+#include <proto/wpa.h>
+
+/* This marks the start of a packed structure section. */
+#include <packed_section_start.h>
+
+
+#define DOT11_TU_TO_US			1024	/* 802.11 Time Unit is 1024 microseconds */
+
+/* Generic 802.11 frame constants */
+#define DOT11_A3_HDR_LEN		24	/* d11 header length with A3 */
+#define DOT11_A4_HDR_LEN		30	/* d11 header length with A4 */
+#define DOT11_MAC_HDR_LEN		DOT11_A3_HDR_LEN	/* MAC header length */
+#define DOT11_FCS_LEN			4	/* d11 FCS length */
+#define DOT11_ICV_LEN			4	/* d11 ICV length */
+#define DOT11_ICV_AES_LEN		8	/* d11 ICV/AES length */
+#define DOT11_QOS_LEN			2	/* d11 QoS length */
+#define DOT11_HTC_LEN			4	/* d11 HT Control field length */
+
+#define DOT11_KEY_INDEX_SHIFT		6	/* d11 key index shift */
+#define DOT11_IV_LEN			4	/* d11 IV length */
+#define DOT11_IV_TKIP_LEN		8	/* d11 IV TKIP length */
+#define DOT11_IV_AES_OCB_LEN		4	/* d11 IV/AES/OCB length */
+#define DOT11_IV_AES_CCM_LEN		8	/* d11 IV/AES/CCM length */
+#define DOT11_IV_MAX_LEN		8	/* maximum iv len for any encryption */
+
+/* Includes MIC */
+#define DOT11_MAX_MPDU_BODY_LEN		2304	/* max MPDU body length */
+/* A4 header + QoS + CCMP + PDU + ICV + FCS = 2352 */
+#define DOT11_MAX_MPDU_LEN		(DOT11_A4_HDR_LEN + \
+					 DOT11_QOS_LEN + \
+					 DOT11_IV_AES_CCM_LEN + \
+					 DOT11_MAX_MPDU_BODY_LEN + \
+					 DOT11_ICV_LEN + \
+					 DOT11_FCS_LEN)	/* d11 max MPDU length */
+
+#define DOT11_MAX_SSID_LEN		32	/* d11 max ssid length */
+
+/* dot11RTSThreshold */
+#define DOT11_DEFAULT_RTS_LEN		2347	/* d11 default RTS length */
+#define DOT11_MAX_RTS_LEN		2347	/* d11 max RTS length */
+
+/* dot11FragmentationThreshold */
+#define DOT11_MIN_FRAG_LEN		256	/* d11 min fragmentation length */
+#define DOT11_MAX_FRAG_LEN		2346	/* Max frag is also limited by aMPDUMaxLength
+						* of the attached PHY
+						*/
+#define DOT11_DEFAULT_FRAG_LEN		2346	/* d11 default fragmentation length */
+
+/* dot11BeaconPeriod */
+#define DOT11_MIN_BEACON_PERIOD		1	/* d11 min beacon period */
+#define DOT11_MAX_BEACON_PERIOD		0xFFFF	/* d11 max beacon period */
+
+/* dot11DTIMPeriod */
+#define DOT11_MIN_DTIM_PERIOD		1	/* d11 min DTIM period */
+#define DOT11_MAX_DTIM_PERIOD		0xFF	/* d11 max DTIM period */
+
+/* 802.2 LLC/SNAP header used by 802.11 per 802.1H */
+#define DOT11_LLC_SNAP_HDR_LEN		8	/* d11 LLC/SNAP header length */
+#define DOT11_OUI_LEN			3	/* d11 OUI length */
+BWL_PRE_PACKED_STRUCT struct dot11_llc_snap_header {
+	uint8	dsap;				/* always 0xAA */
+	uint8	ssap;				/* always 0xAA */
+	uint8	ctl;				/* always 0x03 */
+	uint8	oui[DOT11_OUI_LEN];		/* RFC1042: 0x00 0x00 0x00
+						 * Bridge-Tunnel: 0x00 0x00 0xF8
+						 */
+	uint16	type;				/* ethertype */
+} BWL_POST_PACKED_STRUCT;
+
+/* RFC1042 header used by 802.11 per 802.1H */
+#define RFC1042_HDR_LEN	(ETHER_HDR_LEN + DOT11_LLC_SNAP_HDR_LEN)	/* RCF1042 header length */
+
+/* Generic 802.11 MAC header */
+/*
+ * N.B.: This struct reflects the full 4 address 802.11 MAC header.
+ *		 The fields are defined such that the shorter 1, 2, and 3
+ *		 address headers just use the first k fields.
+ */
+BWL_PRE_PACKED_STRUCT struct dot11_header {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	a1;		/* address 1 */
+	struct ether_addr	a2;		/* address 2 */
+	struct ether_addr	a3;		/* address 3 */
+	uint16			seq;		/* sequence control */
+	struct ether_addr	a4;		/* address 4 */
+} BWL_POST_PACKED_STRUCT;
+
+/* Control frames */
+
+BWL_PRE_PACKED_STRUCT struct dot11_rts_frame {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	ra;		/* receiver address */
+	struct ether_addr	ta;		/* transmitter address */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_RTS_LEN		16		/* d11 RTS frame length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_cts_frame {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	ra;		/* receiver address */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_CTS_LEN		10		/* d11 CTS frame length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_ack_frame {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	ra;		/* receiver address */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_ACK_LEN		10		/* d11 ACK frame length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_ps_poll_frame {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* AID */
+	struct ether_addr	bssid;		/* receiver address, STA in AP */
+	struct ether_addr	ta;		/* transmitter address */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_PS_POLL_LEN	16		/* d11 PS poll frame length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_cf_end_frame {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	ra;		/* receiver address */
+	struct ether_addr	bssid;		/* transmitter address, STA in AP */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_CS_END_LEN	16		/* d11 CF-END frame length */
+
+/* RWL wifi protocol: The Vendor Specific Action frame is defined for vendor-specific signaling
+*  category+OUI+vendor specific content ( this can be variable)
+*/
+BWL_PRE_PACKED_STRUCT struct dot11_action_wifi_vendor_specific {
+	uint8	category;
+	uint8	OUI[3];
+	uint8	type;
+	uint8	subtype;
+	uint8	data[1040];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_action_wifi_vendor_specific dot11_action_wifi_vendor_specific_t;
+
+/* generic vender specific action frame with variable length */
+BWL_PRE_PACKED_STRUCT struct dot11_action_vs_frmhdr {
+	uint8	category;
+	uint8	OUI[3];
+	uint8	type;
+	uint8	subtype;
+	uint8	data[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_action_vs_frmhdr dot11_action_vs_frmhdr_t;
+#define DOT11_ACTION_VS_HDR_LEN	6
+
+#define BCM_ACTION_OUI_BYTE0	0x00
+#define BCM_ACTION_OUI_BYTE1	0x90
+#define BCM_ACTION_OUI_BYTE2	0x4c
+
+/* BA/BAR Control parameters */
+#define DOT11_BA_CTL_POLICY_NORMAL	0x0000	/* normal ack */
+#define DOT11_BA_CTL_POLICY_NOACK	0x0001	/* no ack */
+#define DOT11_BA_CTL_POLICY_MASK	0x0001	/* ack policy mask */
+
+#define DOT11_BA_CTL_MTID		0x0002	/* multi tid BA */
+#define DOT11_BA_CTL_COMPRESSED		0x0004	/* compressed bitmap */
+
+#define DOT11_BA_CTL_NUMMSDU_MASK	0x0FC0	/* num msdu in bitmap mask */
+#define DOT11_BA_CTL_NUMMSDU_SHIFT	6	/* num msdu in bitmap shift */
+
+#define DOT11_BA_CTL_TID_MASK		0xF000	/* tid mask */
+#define DOT11_BA_CTL_TID_SHIFT		12	/* tid shift */
+
+/* control frame header (BA/BAR) */
+BWL_PRE_PACKED_STRUCT struct dot11_ctl_header {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	ra;		/* receiver address */
+	struct ether_addr	ta;		/* transmitter address */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_CTL_HDR_LEN	16		/* control frame hdr len */
+
+/* BAR frame payload */
+BWL_PRE_PACKED_STRUCT struct dot11_bar {
+	uint16			bar_control;	/* BAR Control */
+	uint16			seqnum;		/* Starting Sequence control */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_BAR_LEN		4		/* BAR frame payload length */
+
+#define DOT11_BA_BITMAP_LEN	128		/* bitmap length */
+#define DOT11_BA_CMP_BITMAP_LEN	8		/* compressed bitmap length */
+/* BA frame payload */
+BWL_PRE_PACKED_STRUCT struct dot11_ba {
+	uint16			ba_control;	/* BA Control */
+	uint16			seqnum;		/* Starting Sequence control */
+	uint8			bitmap[DOT11_BA_BITMAP_LEN];	/* Block Ack Bitmap */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_BA_LEN		4		/* BA frame payload len (wo bitmap) */
+
+/* Management frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_management_header {
+	uint16			fc;		/* frame control */
+	uint16			durid;		/* duration/ID */
+	struct ether_addr	da;		/* receiver address */
+	struct ether_addr	sa;		/* transmitter address */
+	struct ether_addr	bssid;		/* BSS ID */
+	uint16			seq;		/* sequence control */
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_MGMT_HDR_LEN	24		/* d11 management header length */
+
+/* Management frame payloads */
+
+BWL_PRE_PACKED_STRUCT struct dot11_bcn_prb {
+	uint32			timestamp[2];
+	uint16			beacon_interval;
+	uint16			capability;
+} BWL_POST_PACKED_STRUCT;
+#define	DOT11_BCN_PRB_LEN	12		/* 802.11 beacon/probe frame fixed length */
+#define	DOT11_BCN_PRB_FIXED_LEN	12		/* 802.11 beacon/probe frame fixed length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_auth {
+	uint16			alg;		/* algorithm */
+	uint16			seq;		/* sequence control */
+	uint16			status;		/* status code */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_AUTH_FIXED_LEN	6		/* length of auth frame without challenge IE */
+
+BWL_PRE_PACKED_STRUCT struct dot11_assoc_req {
+	uint16			capability;	/* capability information */
+	uint16			listen;		/* listen interval */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_ASSOC_REQ_FIXED_LEN	4	/* length of assoc frame without info elts */
+
+BWL_PRE_PACKED_STRUCT struct dot11_reassoc_req {
+	uint16			capability;	/* capability information */
+	uint16			listen;		/* listen interval */
+	struct ether_addr	ap;		/* Current AP address */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_REASSOC_REQ_FIXED_LEN	10	/* length of assoc frame without info elts */
+
+BWL_PRE_PACKED_STRUCT struct dot11_assoc_resp {
+	uint16			capability;	/* capability information */
+	uint16			status;		/* status code */
+	uint16			aid;		/* association ID */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_ASSOC_RESP_FIXED_LEN	6	/* length of assoc resp frame without info elts */
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_measure {
+	uint8	category;
+	uint8	action;
+	uint8	token;
+	uint8	data[1];
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_ACTION_MEASURE_LEN	3	/* d11 action measurement header length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_ht_ch_width {
+	uint8	category;
+	uint8	action;
+	uint8	ch_width;
+} BWL_POST_PACKED_STRUCT;
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_ht_mimops {
+	uint8	category;
+	uint8	action;
+	uint8	control;
+} BWL_POST_PACKED_STRUCT;
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_sa_query {
+	uint8	category;
+	uint8	action;
+	uint16	id;
+} BWL_POST_PACKED_STRUCT;
+
+#define SM_PWRSAVE_ENABLE	1
+#define SM_PWRSAVE_MODE		2
+
+/* ************* 802.11h related definitions. ************* */
+BWL_PRE_PACKED_STRUCT struct dot11_power_cnst {
+	uint8 id;
+	uint8 len;
+	uint8 power;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_power_cnst dot11_power_cnst_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_power_cap {
+	uint8 min;
+	uint8 max;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_power_cap dot11_power_cap_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_tpc_rep {
+	uint8 id;
+	uint8 len;
+	uint8 tx_pwr;
+	uint8 margin;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_tpc_rep dot11_tpc_rep_t;
+#define DOT11_MNG_IE_TPC_REPORT_LEN	2 	/* length of IE data, not including 2 byte header */
+
+BWL_PRE_PACKED_STRUCT struct dot11_supp_channels {
+	uint8 id;
+	uint8 len;
+	uint8 first_channel;
+	uint8 num_channels;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_supp_channels dot11_supp_channels_t;
+
+/* Extension Channel Offset IE: 802.11n-D1.0 spec. added sideband
+ * offset for 40MHz operation.  The possible 3 values are:
+ * 1 = above control channel
+ * 3 = below control channel
+ * 0 = no extension channel
+ */
+BWL_PRE_PACKED_STRUCT struct dot11_extch {
+	uint8	id;		/* IE ID, 62, DOT11_MNG_EXT_CHANNEL_OFFSET */
+	uint8	len;		/* IE length */
+	uint8	extch;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_extch dot11_extch_ie_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_brcm_extch {
+	uint8	id;		/* IE ID, 221, DOT11_MNG_PROPR_ID */
+	uint8	len;		/* IE length */
+	uint8	oui[3];		/* Proprietary OUI, BRCM_PROP_OUI */
+	uint8	type;           /* type inidicates what follows */
+	uint8	extch;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_brcm_extch dot11_brcm_extch_ie_t;
+
+#define BRCM_EXTCH_IE_LEN	5
+#define BRCM_EXTCH_IE_TYPE	53	/* 802.11n ID not yet assigned */
+#define DOT11_EXTCH_IE_LEN	1
+#define DOT11_EXT_CH_MASK	0x03	/* extension channel mask */
+#define DOT11_EXT_CH_UPPER	0x01	/* ext. ch. on upper sb */
+#define DOT11_EXT_CH_LOWER	0x03	/* ext. ch. on lower sb */
+#define DOT11_EXT_CH_NONE	0x00	/* no extension ch.  */
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_frmhdr {
+	uint8	category;
+	uint8	action;
+	uint8	data[1];
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_ACTION_FRMHDR_LEN	2
+
+/* CSA IE data structure */
+BWL_PRE_PACKED_STRUCT struct dot11_channel_switch {
+	uint8 id;	/* id DOT11_MNG_CHANNEL_SWITCH_ID */
+	uint8 len;	/* length of IE */
+	uint8 mode;	/* mode 0 or 1 */
+	uint8 channel;	/* channel switch to */
+	uint8 count;	/* number of beacons before switching */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_channel_switch dot11_chan_switch_ie_t;
+
+#define DOT11_SWITCH_IE_LEN	3	/* length of IE data, not including 2 byte header */
+/* CSA mode - 802.11h-2003 $7.3.2.20 */
+#define DOT11_CSA_MODE_ADVISORY		0	/* no DOT11_CSA_MODE_NO_TX restriction imposed */
+#define DOT11_CSA_MODE_NO_TX		1	/* no transmission upon receiving CSA frame. */
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_switch_channel {
+	uint8	category;
+	uint8	action;
+	dot11_chan_switch_ie_t chan_switch_ie;	/* for switch IE */
+	dot11_brcm_extch_ie_t extch_ie;		/* extension channel offset */
+} BWL_POST_PACKED_STRUCT;
+
+BWL_PRE_PACKED_STRUCT struct dot11_csa_body {
+	uint8 mode;	/* mode 0 or 1 */
+	uint8 reg;	/* regulatory class */
+	uint8 channel;	/* channel switch to */
+	uint8 count;	/* number of beacons before switching */
+} BWL_POST_PACKED_STRUCT;
+
+/* 11n Extended Channel Switch IE data structure */
+BWL_PRE_PACKED_STRUCT struct dot11_ext_csa {
+	uint8 id;	/* id DOT11_MNG_EXT_CHANNEL_SWITCH_ID */
+	uint8 len;	/* length of IE */
+	struct dot11_csa_body b;	/* body of the ie */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_ext_csa dot11_ext_csa_ie_t;
+#define DOT11_EXT_CSA_IE_LEN	4	/* length of extended channel switch IE body */
+
+BWL_PRE_PACKED_STRUCT struct dot11_action_ext_csa {
+	uint8	category;
+	uint8	action;
+	dot11_ext_csa_ie_t chan_switch_ie;	/* for switch IE */
+} BWL_POST_PACKED_STRUCT;
+
+BWL_PRE_PACKED_STRUCT struct dot11y_action_ext_csa {
+	uint8	category;
+	uint8	action;
+	struct dot11_csa_body b;	/* body of the ie */
+} BWL_POST_PACKED_STRUCT;
+
+BWL_PRE_PACKED_STRUCT struct dot11_obss_coex {
+	uint8	id;
+	uint8	len;
+	uint8	info;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_obss_coex dot11_obss_coex_t;
+#define DOT11_OBSS_COEXINFO_LEN	1	/* length of OBSS Coexistence INFO IE */
+
+#define	DOT11_OBSS_COEX_INFO_REQ		0x01
+#define	DOT11_OBSS_COEX_40MHZ_INTOLERANT	0x02
+#define	DOT11_OBSS_COEX_20MHZ_WIDTH_REQ	0x04
+
+BWL_PRE_PACKED_STRUCT struct dot11_obss_chanlist {
+	uint8	id;
+	uint8	len;
+	uint8	regclass;
+	uint8	chanlist[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_obss_chanlist dot11_obss_chanlist_t;
+#define DOT11_OBSS_CHANLIST_FIXED_LEN	1	/* fixed length of regclass */
+
+BWL_PRE_PACKED_STRUCT struct dot11_extcap_ie {
+	uint8 id;
+	uint8 len;
+	uint8 cap[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_extcap_ie dot11_extcap_ie_t;
+
+#define DOT11_EXTCAP_LEN_MAX	7
+#define DOT11_EXTCAP_LEN_COEX	1
+#define DOT11_EXTCAP_LEN_BT	3
+#define DOT11_EXTCAP_LEN_IW	4
+#define DOT11_EXTCAP_LEN_SI	6
+
+#define DOT11_EXTCAP_LEN_TDLS	5
+BWL_PRE_PACKED_STRUCT struct dot11_extcap {
+	uint8 extcap[DOT11_EXTCAP_LEN_TDLS];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_extcap dot11_extcap_t;
+
+/* TDLS Capabilities */
+#define TDLS_CAP_TDLS			37		/* TDLS support */
+#define TDLS_CAP_PU_BUFFER_STA	28		/* TDLS Peer U-APSD buffer STA support */
+#define TDLS_CAP_PEER_PSM		20		/* TDLS Peer PSM support */
+#define TDLS_CAP_CH_SW			30		/* TDLS Channel switch */
+#define TDLS_CAP_PROH			38		/* TDLS prohibited */
+#define TDLS_CAP_CH_SW_PROH		39		/* TDLS Channel switch prohibited */
+
+#define TDLS_CAP_MAX_BIT		39		/* TDLS max bit defined in ext cap */
+
+/* 802.11h/802.11k Measurement Request/Report IEs */
+/* Measurement Type field */
+#define DOT11_MEASURE_TYPE_BASIC 	0	/* d11 measurement basic type */
+#define DOT11_MEASURE_TYPE_CCA 		1	/* d11 measurement CCA type */
+#define DOT11_MEASURE_TYPE_RPI		2	/* d11 measurement RPI type */
+#define DOT11_MEASURE_TYPE_CHLOAD		3	/* d11 measurement Channel Load type */
+#define DOT11_MEASURE_TYPE_NOISE		4	/* d11 measurement Noise Histogram type */
+#define DOT11_MEASURE_TYPE_BEACON		5	/* d11 measurement Beacon type */
+#define DOT11_MEASURE_TYPE_FRAME	6	/* d11 measurement Frame type */
+#define DOT11_MEASURE_TYPE_STATS		7	/* d11 measurement STA Statistics type */
+#define DOT11_MEASURE_TYPE_LCI		8	/* d11 measurement LCI type */
+#define DOT11_MEASURE_TYPE_TXSTREAM		9	/* d11 measurement TX Stream type */
+#define DOT11_MEASURE_TYPE_PAUSE		255	/* d11 measurement pause type */
+
+/* Measurement Request Modes */
+#define DOT11_MEASURE_MODE_PARALLEL 	(1<<0)	/* d11 measurement parallel */
+#define DOT11_MEASURE_MODE_ENABLE 	(1<<1)	/* d11 measurement enable */
+#define DOT11_MEASURE_MODE_REQUEST	(1<<2)	/* d11 measurement request */
+#define DOT11_MEASURE_MODE_REPORT 	(1<<3)	/* d11 measurement report */
+#define DOT11_MEASURE_MODE_DUR 	(1<<4)	/* d11 measurement dur mandatory */
+/* Measurement Report Modes */
+#define DOT11_MEASURE_MODE_LATE 	(1<<0)	/* d11 measurement late */
+#define DOT11_MEASURE_MODE_INCAPABLE	(1<<1)	/* d11 measurement incapable */
+#define DOT11_MEASURE_MODE_REFUSED	(1<<2)	/* d11 measurement refuse */
+/* Basic Measurement Map bits */
+#define DOT11_MEASURE_BASIC_MAP_BSS	((uint8)(1<<0))	/* d11 measurement basic map BSS */
+#define DOT11_MEASURE_BASIC_MAP_OFDM	((uint8)(1<<1))	/* d11 measurement map OFDM */
+#define DOT11_MEASURE_BASIC_MAP_UKNOWN	((uint8)(1<<2))	/* d11 measurement map unknown */
+#define DOT11_MEASURE_BASIC_MAP_RADAR	((uint8)(1<<3))	/* d11 measurement map radar */
+#define DOT11_MEASURE_BASIC_MAP_UNMEAS	((uint8)(1<<4))	/* d11 measurement map unmeasuremnt */
+
+BWL_PRE_PACKED_STRUCT struct dot11_meas_req {
+	uint8 id;
+	uint8 len;
+	uint8 token;
+	uint8 mode;
+	uint8 type;
+	uint8 channel;
+	uint8 start_time[8];
+	uint16 duration;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_meas_req dot11_meas_req_t;
+#define DOT11_MNG_IE_MREQ_LEN 14	/* d11 measurement request IE length */
+/* length of Measure Request IE data not including variable len */
+#define DOT11_MNG_IE_MREQ_FIXED_LEN 3	/* d11 measurement request IE fixed length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_meas_rep {
+	uint8 id;
+	uint8 len;
+	uint8 token;
+	uint8 mode;
+	uint8 type;
+	BWL_PRE_PACKED_STRUCT union
+	{
+		BWL_PRE_PACKED_STRUCT struct {
+			uint8 channel;
+			uint8 start_time[8];
+			uint16 duration;
+			uint8 map;
+		} BWL_POST_PACKED_STRUCT basic;
+		uint8 data[1];
+	} BWL_POST_PACKED_STRUCT rep;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_meas_rep dot11_meas_rep_t;
+
+/* length of Measure Report IE data not including variable len */
+#define DOT11_MNG_IE_MREP_FIXED_LEN	3	/* d11 measurement response IE fixed length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_meas_rep_basic {
+	uint8 channel;
+	uint8 start_time[8];
+	uint16 duration;
+	uint8 map;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_meas_rep_basic dot11_meas_rep_basic_t;
+#define DOT11_MEASURE_BASIC_REP_LEN	12	/* d11 measurement basic report length */
+
+BWL_PRE_PACKED_STRUCT struct dot11_quiet {
+	uint8 id;
+	uint8 len;
+	uint8 count;	/* TBTTs until beacon interval in quiet starts */
+	uint8 period;	/* Beacon intervals between periodic quiet periods ? */
+	uint16 duration;	/* Length of quiet period, in TU's */
+	uint16 offset;	/* TU's offset from TBTT in Count field */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_quiet dot11_quiet_t;
+
+BWL_PRE_PACKED_STRUCT struct chan_map_tuple {
+	uint8 channel;
+	uint8 map;
+} BWL_POST_PACKED_STRUCT;
+typedef struct chan_map_tuple chan_map_tuple_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_ibss_dfs {
+	uint8 id;
+	uint8 len;
+	uint8 eaddr[ETHER_ADDR_LEN];
+	uint8 interval;
+	chan_map_tuple_t map[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_ibss_dfs dot11_ibss_dfs_t;
+
+/* WME Elements */
+#define WME_OUI			"\x00\x50\xf2"	/* WME OUI */
+#define WME_OUI_LEN		3
+#define WME_OUI_TYPE		2	/* WME type */
+#define WME_TYPE		2	/* WME type, deprecated */
+#define WME_SUBTYPE_IE		0	/* Information Element */
+#define WME_SUBTYPE_PARAM_IE	1	/* Parameter Element */
+#define WME_SUBTYPE_TSPEC	2	/* Traffic Specification */
+#define WME_VER			1	/* WME version */
+
+/* WME Access Category Indices (ACIs) */
+#define AC_BE			0	/* Best Effort */
+#define AC_BK			1	/* Background */
+#define AC_VI			2	/* Video */
+#define AC_VO			3	/* Voice */
+#define AC_COUNT		4	/* number of ACs */
+
+typedef uint8 ac_bitmap_t;	/* AC bitmap of (1 << AC_xx) */
+
+#define AC_BITMAP_NONE		0x0	/* No ACs */
+#define AC_BITMAP_ALL		0xf	/* All ACs */
+#define AC_BITMAP_TST(ab, ac)	(((ab) & (1 << (ac))) != 0)
+#define AC_BITMAP_SET(ab, ac)	(((ab) |= (1 << (ac))))
+#define AC_BITMAP_RESET(ab, ac) (((ab) &= ~(1 << (ac))))
+
+/* WME Information Element (IE) */
+BWL_PRE_PACKED_STRUCT struct wme_ie {
+	uint8 oui[3];
+	uint8 type;
+	uint8 subtype;
+	uint8 version;
+	uint8 qosinfo;
+} BWL_POST_PACKED_STRUCT;
+typedef struct wme_ie wme_ie_t;
+#define WME_IE_LEN 7	/* WME IE length */
+
+BWL_PRE_PACKED_STRUCT struct edcf_acparam {
+	uint8	ACI;
+	uint8	ECW;
+	uint16  TXOP;		/* stored in network order (ls octet first) */
+} BWL_POST_PACKED_STRUCT;
+typedef struct edcf_acparam edcf_acparam_t;
+
+/* WME Parameter Element (PE) */
+BWL_PRE_PACKED_STRUCT struct wme_param_ie {
+	uint8 oui[3];
+	uint8 type;
+	uint8 subtype;
+	uint8 version;
+	uint8 qosinfo;
+	uint8 rsvd;
+	edcf_acparam_t acparam[AC_COUNT];
+} BWL_POST_PACKED_STRUCT;
+typedef struct wme_param_ie wme_param_ie_t;
+#define WME_PARAM_IE_LEN            24          /* WME Parameter IE length */
+
+/* QoS Info field for IE as sent from AP */
+#define WME_QI_AP_APSD_MASK         0x80        /* U-APSD Supported mask */
+#define WME_QI_AP_APSD_SHIFT        7           /* U-APSD Supported shift */
+#define WME_QI_AP_COUNT_MASK        0x0f        /* Parameter set count mask */
+#define WME_QI_AP_COUNT_SHIFT       0           /* Parameter set count shift */
+
+/* QoS Info field for IE as sent from STA */
+#define WME_QI_STA_MAXSPLEN_MASK    0x60        /* Max Service Period Length mask */
+#define WME_QI_STA_MAXSPLEN_SHIFT   5           /* Max Service Period Length shift */
+#define WME_QI_STA_APSD_ALL_MASK    0xf         /* APSD all AC bits mask */
+#define WME_QI_STA_APSD_ALL_SHIFT   0           /* APSD all AC bits shift */
+#define WME_QI_STA_APSD_BE_MASK     0x8         /* APSD AC_BE mask */
+#define WME_QI_STA_APSD_BE_SHIFT    3           /* APSD AC_BE shift */
+#define WME_QI_STA_APSD_BK_MASK     0x4         /* APSD AC_BK mask */
+#define WME_QI_STA_APSD_BK_SHIFT    2           /* APSD AC_BK shift */
+#define WME_QI_STA_APSD_VI_MASK     0x2         /* APSD AC_VI mask */
+#define WME_QI_STA_APSD_VI_SHIFT    1           /* APSD AC_VI shift */
+#define WME_QI_STA_APSD_VO_MASK     0x1         /* APSD AC_VO mask */
+#define WME_QI_STA_APSD_VO_SHIFT    0           /* APSD AC_VO shift */
+
+/* ACI */
+#define EDCF_AIFSN_MIN               1           /* AIFSN minimum value */
+#define EDCF_AIFSN_MAX               15          /* AIFSN maximum value */
+#define EDCF_AIFSN_MASK              0x0f        /* AIFSN mask */
+#define EDCF_ACM_MASK                0x10        /* ACM mask */
+#define EDCF_ACI_MASK                0x60        /* ACI mask */
+#define EDCF_ACI_SHIFT               5           /* ACI shift */
+#define EDCF_AIFSN_SHIFT             12          /* 4 MSB(0xFFF) in ifs_ctl for AC idx */
+
+/* ECW */
+#define EDCF_ECW_MIN                 0           /* cwmin/cwmax exponent minimum value */
+#define EDCF_ECW_MAX                 15          /* cwmin/cwmax exponent maximum value */
+#define EDCF_ECW2CW(exp)             ((1 << (exp)) - 1)
+#define EDCF_ECWMIN_MASK             0x0f        /* cwmin exponent form mask */
+#define EDCF_ECWMAX_MASK             0xf0        /* cwmax exponent form mask */
+#define EDCF_ECWMAX_SHIFT            4           /* cwmax exponent form shift */
+
+/* TXOP */
+#define EDCF_TXOP_MIN                0           /* TXOP minimum value */
+#define EDCF_TXOP_MAX                65535       /* TXOP maximum value */
+#define EDCF_TXOP2USEC(txop)         ((txop) << 5)
+
+/* Default BE ACI value for non-WME connection STA */
+#define NON_EDCF_AC_BE_ACI_STA          0x02
+
+/* Default EDCF parameters that AP advertises for STA to use; WMM draft Table 12 */
+#define EDCF_AC_BE_ACI_STA           0x03	/* STA ACI value for best effort AC */
+#define EDCF_AC_BE_ECW_STA           0xA4	/* STA ECW value for best effort AC */
+#define EDCF_AC_BE_TXOP_STA          0x0000	/* STA TXOP value for best effort AC */
+#define EDCF_AC_BK_ACI_STA           0x27	/* STA ACI value for background AC */
+#define EDCF_AC_BK_ECW_STA           0xA4	/* STA ECW value for background AC */
+#define EDCF_AC_BK_TXOP_STA          0x0000	/* STA TXOP value for background AC */
+#define EDCF_AC_VI_ACI_STA           0x42	/* STA ACI value for video AC */
+#define EDCF_AC_VI_ECW_STA           0x43	/* STA ECW value for video AC */
+#define EDCF_AC_VI_TXOP_STA          0x005e	/* STA TXOP value for video AC */
+#define EDCF_AC_VO_ACI_STA           0x62	/* STA ACI value for audio AC */
+#define EDCF_AC_VO_ECW_STA           0x32	/* STA ECW value for audio AC */
+#define EDCF_AC_VO_TXOP_STA          0x002f	/* STA TXOP value for audio AC */
+
+/* Default EDCF parameters that AP uses; WMM draft Table 14 */
+#define EDCF_AC_BE_ACI_AP            0x03	/* AP ACI value for best effort AC */
+#define EDCF_AC_BE_ECW_AP            0x64	/* AP ECW value for best effort AC */
+#define EDCF_AC_BE_TXOP_AP           0x0000	/* AP TXOP value for best effort AC */
+#define EDCF_AC_BK_ACI_AP            0x27	/* AP ACI value for background AC */
+#define EDCF_AC_BK_ECW_AP            0xA4	/* AP ECW value for background AC */
+#define EDCF_AC_BK_TXOP_AP           0x0000	/* AP TXOP value for background AC */
+#define EDCF_AC_VI_ACI_AP            0x41	/* AP ACI value for video AC */
+#define EDCF_AC_VI_ECW_AP            0x43	/* AP ECW value for video AC */
+#define EDCF_AC_VI_TXOP_AP           0x005e	/* AP TXOP value for video AC */
+#define EDCF_AC_VO_ACI_AP            0x61	/* AP ACI value for audio AC */
+#define EDCF_AC_VO_ECW_AP            0x32	/* AP ECW value for audio AC */
+#define EDCF_AC_VO_TXOP_AP           0x002f	/* AP TXOP value for audio AC */
+
+/* EDCA Parameter IE */
+BWL_PRE_PACKED_STRUCT struct edca_param_ie {
+	uint8 qosinfo;
+	uint8 rsvd;
+	edcf_acparam_t acparam[AC_COUNT];
+} BWL_POST_PACKED_STRUCT;
+typedef struct edca_param_ie edca_param_ie_t;
+#define EDCA_PARAM_IE_LEN            18          /* EDCA Parameter IE length */
+
+/* QoS Capability IE */
+BWL_PRE_PACKED_STRUCT struct qos_cap_ie {
+	uint8 qosinfo;
+} BWL_POST_PACKED_STRUCT;
+typedef struct qos_cap_ie qos_cap_ie_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_qbss_load_ie {
+	uint8 id; 			/* 11, DOT11_MNG_QBSS_LOAD_ID */
+	uint8 length;
+	uint16 station_count; 		/* total number of STAs associated */
+	uint8 channel_utilization;	/* % of time, normalized to 255, QAP sensed medium busy */
+	uint16 aac; 			/* available admission capacity */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_qbss_load_ie dot11_qbss_load_ie_t;
+#define BSS_LOAD_IE_SIZE 	7	/* BSS load IE size */
+
+/* nom_msdu_size */
+#define FIXED_MSDU_SIZE 0x8000		/* MSDU size is fixed */
+#define MSDU_SIZE_MASK	0x7fff		/* (Nominal or fixed) MSDU size */
+
+/* surplus_bandwidth */
+/* Represented as 3 bits of integer, binary point, 13 bits fraction */
+#define	INTEGER_SHIFT	13	/* integer shift */
+#define FRACTION_MASK	0x1FFF	/* fraction mask */
+
+/* Management Notification Frame */
+BWL_PRE_PACKED_STRUCT struct dot11_management_notification {
+	uint8 category;			/* DOT11_ACTION_NOTIFICATION */
+	uint8 action;
+	uint8 token;
+	uint8 status;
+	uint8 data[1];			/* Elements */
+} BWL_POST_PACKED_STRUCT;
+#define DOT11_MGMT_NOTIFICATION_LEN 4	/* Fixed length */
+
+/* Timeout Interval IE */
+BWL_PRE_PACKED_STRUCT struct ti_ie {
+	uint8 ti_type;
+	uint32 ti_val;
+} BWL_POST_PACKED_STRUCT;
+typedef struct ti_ie ti_ie_t;
+#define TI_TYPE_REASSOC_DEADLINE	1
+#define TI_TYPE_KEY_LIFETIME		2
+
+/* WME Action Codes */
+#define WME_ADDTS_REQUEST	0	/* WME ADDTS request */
+#define WME_ADDTS_RESPONSE	1	/* WME ADDTS response */
+#define WME_DELTS_REQUEST	2	/* WME DELTS request */
+
+/* WME Setup Response Status Codes */
+#define WME_ADMISSION_ACCEPTED		0	/* WME admission accepted */
+#define WME_INVALID_PARAMETERS		1	/* WME invalide parameters */
+#define WME_ADMISSION_REFUSED		3	/* WME admission refused */
+
+/* Macro to take a pointer to a beacon or probe response
+ * body and return the char* pointer to the SSID info element
+ */
+#define BCN_PRB_SSID(body) ((char*)(body) + DOT11_BCN_PRB_LEN)
+
+/* Authentication frame payload constants */
+#define DOT11_OPEN_SYSTEM	0	/* d11 open authentication */
+#define DOT11_SHARED_KEY	1	/* d11 shared authentication */
+#define DOT11_FAST_BSS		2	/* d11 fast bss authentication */
+#define DOT11_CHALLENGE_LEN	128	/* d11 challenge text length */
+
+/* Frame control macros */
+#define FC_PVER_MASK		0x3	/* PVER mask */
+#define FC_PVER_SHIFT		0	/* PVER shift */
+#define FC_TYPE_MASK		0xC	/* type mask */
+#define FC_TYPE_SHIFT		2	/* type shift */
+#define FC_SUBTYPE_MASK		0xF0	/* subtype mask */
+#define FC_SUBTYPE_SHIFT	4	/* subtype shift */
+#define FC_TODS			0x100	/* to DS */
+#define FC_TODS_SHIFT		8	/* to DS shift */
+#define FC_FROMDS		0x200	/* from DS */
+#define FC_FROMDS_SHIFT		9	/* from DS shift */
+#define FC_MOREFRAG		0x400	/* more frag. */
+#define FC_MOREFRAG_SHIFT	10	/* more frag. shift */
+#define FC_RETRY		0x800	/* retry */
+#define FC_RETRY_SHIFT		11	/* retry shift */
+#define FC_PM			0x1000	/* PM */
+#define FC_PM_SHIFT		12	/* PM shift */
+#define FC_MOREDATA		0x2000	/* more data */
+#define FC_MOREDATA_SHIFT	13	/* more data shift */
+#define FC_WEP			0x4000	/* WEP */
+#define FC_WEP_SHIFT		14	/* WEP shift */
+#define FC_ORDER		0x8000	/* order */
+#define FC_ORDER_SHIFT		15	/* order shift */
+
+/* sequence control macros */
+#define SEQNUM_SHIFT		4	/* seq. number shift */
+#define SEQNUM_MAX		0x1000	/* max seqnum + 1 */
+#define FRAGNUM_MASK		0xF	/* frag. number mask */
+
+/* Frame Control type/subtype defs */
+
+/* FC Types */
+#define FC_TYPE_MNG		0	/* management type */
+#define FC_TYPE_CTL		1	/* control type */
+#define FC_TYPE_DATA		2	/* data type */
+
+/* Management Subtypes */
+#define FC_SUBTYPE_ASSOC_REQ		0	/* assoc. request */
+#define FC_SUBTYPE_ASSOC_RESP		1	/* assoc. response */
+#define FC_SUBTYPE_REASSOC_REQ		2	/* reassoc. request */
+#define FC_SUBTYPE_REASSOC_RESP		3	/* reassoc. response */
+#define FC_SUBTYPE_PROBE_REQ		4	/* probe request */
+#define FC_SUBTYPE_PROBE_RESP		5	/* probe response */
+#define FC_SUBTYPE_BEACON		8	/* beacon */
+#define FC_SUBTYPE_ATIM			9	/* ATIM */
+#define FC_SUBTYPE_DISASSOC		10	/* disassoc. */
+#define FC_SUBTYPE_AUTH			11	/* authentication */
+#define FC_SUBTYPE_DEAUTH		12	/* de-authentication */
+#define FC_SUBTYPE_ACTION		13	/* action */
+#define FC_SUBTYPE_ACTION_NOACK		14	/* action no-ack */
+
+/* Control Subtypes */
+#define FC_SUBTYPE_CTL_WRAPPER		7	/* Control Wrapper */
+#define FC_SUBTYPE_BLOCKACK_REQ		8	/* Block Ack Req */
+#define FC_SUBTYPE_BLOCKACK		9	/* Block Ack */
+#define FC_SUBTYPE_PS_POLL		10	/* PS poll */
+#define FC_SUBTYPE_RTS			11	/* RTS */
+#define FC_SUBTYPE_CTS			12	/* CTS */
+#define FC_SUBTYPE_ACK			13	/* ACK */
+#define FC_SUBTYPE_CF_END		14	/* CF-END */
+#define FC_SUBTYPE_CF_END_ACK		15	/* CF-END ACK */
+
+/* Data Subtypes */
+#define FC_SUBTYPE_DATA			0	/* Data */
+#define FC_SUBTYPE_DATA_CF_ACK		1	/* Data + CF-ACK */
+#define FC_SUBTYPE_DATA_CF_POLL		2	/* Data + CF-Poll */
+#define FC_SUBTYPE_DATA_CF_ACK_POLL	3	/* Data + CF-Ack + CF-Poll */
+#define FC_SUBTYPE_NULL			4	/* Null */
+#define FC_SUBTYPE_CF_ACK		5	/* CF-Ack */
+#define FC_SUBTYPE_CF_POLL		6	/* CF-Poll */
+#define FC_SUBTYPE_CF_ACK_POLL		7	/* CF-Ack + CF-Poll */
+#define FC_SUBTYPE_QOS_DATA		8	/* QoS Data */
+#define FC_SUBTYPE_QOS_DATA_CF_ACK	9	/* QoS Data + CF-Ack */
+#define FC_SUBTYPE_QOS_DATA_CF_POLL	10	/* QoS Data + CF-Poll */
+#define FC_SUBTYPE_QOS_DATA_CF_ACK_POLL	11	/* QoS Data + CF-Ack + CF-Poll */
+#define FC_SUBTYPE_QOS_NULL		12	/* QoS Null */
+#define FC_SUBTYPE_QOS_CF_POLL		14	/* QoS CF-Poll */
+#define FC_SUBTYPE_QOS_CF_ACK_POLL	15	/* QoS CF-Ack + CF-Poll */
+
+/* Data Subtype Groups */
+#define FC_SUBTYPE_ANY_QOS(s)		(((s) & 8) != 0)
+#define FC_SUBTYPE_ANY_NULL(s)		(((s) & 4) != 0)
+#define FC_SUBTYPE_ANY_CF_POLL(s)	(((s) & 2) != 0)
+#define FC_SUBTYPE_ANY_CF_ACK(s)	(((s) & 1) != 0)
+
+/* Type/Subtype Combos */
+#define FC_KIND_MASK		(FC_TYPE_MASK | FC_SUBTYPE_MASK)	/* FC kind mask */
+
+#define FC_KIND(t, s)	(((t) << FC_TYPE_SHIFT) | ((s) << FC_SUBTYPE_SHIFT))	/* FC kind */
+
+#define FC_SUBTYPE(fc)	(((fc) & FC_SUBTYPE_MASK) >> FC_SUBTYPE_SHIFT)	/* Subtype from FC */
+#define FC_TYPE(fc)	(((fc) & FC_TYPE_MASK) >> FC_TYPE_SHIFT)	/* Type from FC */
+
+#define FC_ASSOC_REQ	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_ASSOC_REQ)	/* assoc. request */
+#define FC_ASSOC_RESP	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_ASSOC_RESP)	/* assoc. response */
+#define FC_REASSOC_REQ	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_REASSOC_REQ)	/* reassoc. request */
+#define FC_REASSOC_RESP	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_REASSOC_RESP)	/* reassoc. response */
+#define FC_PROBE_REQ	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_PROBE_REQ)	/* probe request */
+#define FC_PROBE_RESP	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_PROBE_RESP)	/* probe response */
+#define FC_BEACON	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_BEACON)		/* beacon */
+#define FC_DISASSOC	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_DISASSOC)	/* disassoc */
+#define FC_AUTH		FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_AUTH)		/* authentication */
+#define FC_DEAUTH	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_DEAUTH)		/* deauthentication */
+#define FC_ACTION	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_ACTION)		/* action */
+#define FC_ACTION_NOACK	FC_KIND(FC_TYPE_MNG, FC_SUBTYPE_ACTION_NOACK)	/* action no-ack */
+
+#define FC_CTL_WRAPPER	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_CTL_WRAPPER)	/* Control Wrapper */
+#define FC_BLOCKACK_REQ	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_BLOCKACK_REQ)	/* Block Ack Req */
+#define FC_BLOCKACK	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_BLOCKACK)	/* Block Ack */
+#define FC_PS_POLL	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_PS_POLL)	/* PS poll */
+#define FC_RTS		FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_RTS)		/* RTS */
+#define FC_CTS		FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_CTS)		/* CTS */
+#define FC_ACK		FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_ACK)		/* ACK */
+#define FC_CF_END	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_CF_END)		/* CF-END */
+#define FC_CF_END_ACK	FC_KIND(FC_TYPE_CTL, FC_SUBTYPE_CF_END_ACK)	/* CF-END ACK */
+
+#define FC_DATA		FC_KIND(FC_TYPE_DATA, FC_SUBTYPE_DATA)		/* data */
+#define FC_NULL_DATA	FC_KIND(FC_TYPE_DATA, FC_SUBTYPE_NULL)		/* null data */
+#define FC_DATA_CF_ACK	FC_KIND(FC_TYPE_DATA, FC_SUBTYPE_DATA_CF_ACK)	/* data CF ACK */
+#define FC_QOS_DATA	FC_KIND(FC_TYPE_DATA, FC_SUBTYPE_QOS_DATA)	/* QoS data */
+#define FC_QOS_NULL	FC_KIND(FC_TYPE_DATA, FC_SUBTYPE_QOS_NULL)	/* QoS null */
+
+/* QoS Control Field */
+
+/* 802.1D Priority */
+#define QOS_PRIO_SHIFT		0	/* QoS priority shift */
+#define QOS_PRIO_MASK		0x0007	/* QoS priority mask */
+#define QOS_PRIO(qos)		(((qos) & QOS_PRIO_MASK) >> QOS_PRIO_SHIFT)	/* QoS priority */
+
+/* Traffic Identifier */
+#define QOS_TID_SHIFT		0	/* QoS TID shift */
+#define QOS_TID_MASK		0x000f	/* QoS TID mask */
+#define QOS_TID(qos)		(((qos) & QOS_TID_MASK) >> QOS_TID_SHIFT)	/* QoS TID */
+
+/* End of Service Period (U-APSD) */
+#define QOS_EOSP_SHIFT		4	/* QoS End of Service Period shift */
+#define QOS_EOSP_MASK		0x0010	/* QoS End of Service Period mask */
+#define QOS_EOSP(qos)		(((qos) & QOS_EOSP_MASK) >> QOS_EOSP_SHIFT)	/* Qos EOSP */
+
+/* Ack Policy */
+#define QOS_ACK_NORMAL_ACK	0	/* Normal Ack */
+#define QOS_ACK_NO_ACK		1	/* No Ack (eg mcast) */
+#define QOS_ACK_NO_EXP_ACK	2	/* No Explicit Ack */
+#define QOS_ACK_BLOCK_ACK	3	/* Block Ack */
+#define QOS_ACK_SHIFT		5	/* QoS ACK shift */
+#define QOS_ACK_MASK		0x0060	/* QoS ACK mask */
+#define QOS_ACK(qos)		(((qos) & QOS_ACK_MASK) >> QOS_ACK_SHIFT)	/* QoS ACK */
+
+/* A-MSDU flag */
+#define QOS_AMSDU_SHIFT		7	/* AMSDU shift */
+#define QOS_AMSDU_MASK		0x0080	/* AMSDU mask */
+
+/* Management Frames */
+
+/* Management Frame Constants */
+
+/* Fixed fields */
+#define DOT11_MNG_AUTH_ALGO_LEN		2	/* d11 management auth. algo. length */
+#define DOT11_MNG_AUTH_SEQ_LEN		2	/* d11 management auth. seq. length */
+#define DOT11_MNG_BEACON_INT_LEN	2	/* d11 management beacon interval length */
+#define DOT11_MNG_CAP_LEN		2	/* d11 management cap. length */
+#define DOT11_MNG_AP_ADDR_LEN		6	/* d11 management AP address length */
+#define DOT11_MNG_LISTEN_INT_LEN	2	/* d11 management listen interval length */
+#define DOT11_MNG_REASON_LEN		2	/* d11 management reason length */
+#define DOT11_MNG_AID_LEN		2	/* d11 management AID length */
+#define DOT11_MNG_STATUS_LEN		2	/* d11 management status length */
+#define DOT11_MNG_TIMESTAMP_LEN		8	/* d11 management timestamp length */
+
+/* DUR/ID field in assoc resp is 0xc000 | AID */
+#define DOT11_AID_MASK			0x3fff	/* d11 AID mask */
+
+/* Reason Codes */
+#define DOT11_RC_RESERVED		0	/* d11 RC reserved */
+#define DOT11_RC_UNSPECIFIED		1	/* Unspecified reason */
+#define DOT11_RC_AUTH_INVAL		2	/* Previous authentication no longer valid */
+#define DOT11_RC_DEAUTH_LEAVING		3	/* Deauthenticated because sending station
+						 * is leaving (or has left) IBSS or ESS
+						 */
+#define DOT11_RC_INACTIVITY		4	/* Disassociated due to inactivity */
+#define DOT11_RC_BUSY			5	/* Disassociated because AP is unable to handle
+						 * all currently associated stations
+						 */
+#define DOT11_RC_INVAL_CLASS_2		6	/* Class 2 frame received from
+						 * nonauthenticated station
+						 */
+#define DOT11_RC_INVAL_CLASS_3		7	/* Class 3 frame received from
+						 *  nonassociated station
+						 */
+#define DOT11_RC_DISASSOC_LEAVING	8	/* Disassociated because sending station is
+						 * leaving (or has left) BSS
+						 */
+#define DOT11_RC_NOT_AUTH		9	/* Station requesting (re)association is not
+						 * authenticated with responding station
+						 */
+#define DOT11_RC_BAD_PC			10	/* Unacceptable power capability element */
+#define DOT11_RC_BAD_CHANNELS		11	/* Unacceptable supported channels element */
+/* 12 is unused */
+
+/* 32-39 are QSTA specific reasons added in 11e */
+#define DOT11_RC_UNSPECIFIED_QOS	32	/* unspecified QoS-related reason */
+#define DOT11_RC_INSUFFCIENT_BW		33	/* QAP lacks sufficient bandwidth */
+#define DOT11_RC_EXCESSIVE_FRAMES	34	/* excessive number of frames need ack */
+#define DOT11_RC_TX_OUTSIDE_TXOP	35	/* transmitting outside the limits of txop */
+#define DOT11_RC_LEAVING_QBSS		36	/* QSTA is leaving the QBSS (or restting) */
+#define DOT11_RC_BAD_MECHANISM		37	/* does not want to use the mechanism */
+#define DOT11_RC_SETUP_NEEDED		38	/* mechanism needs a setup */
+#define DOT11_RC_TIMEOUT		39	/* timeout */
+
+#define DOT11_RC_MAX			23	/* Reason codes > 23 are reserved */
+
+#define DOT11_RC_TDLS_PEER_UNREACH	25
+#define DOT11_RC_TDLS_DOWN_UNSPECIFIED	26
+
+/* Status Codes */
+#define DOT11_SC_SUCCESS		0	/* Successful */
+#define DOT11_SC_FAILURE		1	/* Unspecified failure */
+#define DOT11_SC_TDLS_WAKEUP_SCH_ALT 2	/* TDLS wakeup schedule rejected but alternative  */
+					/* schedule provided */
+#define DOT11_SC_TDLS_WAKEUP_SCH_REJ 3	/* TDLS wakeup schedule rejected */
+#define DOT11_SC_TDLS_SEC_DISABLED	5	/* TDLS Security disabled */
+#define DOT11_SC_LIFETIME_REJ		6	/* Unacceptable lifetime */
+#define DOT11_SC_NOT_SAME_BSS		7	/* Not in same BSS */
+#define DOT11_SC_CAP_MISMATCH		10	/* Cannot support all requested
+						 * capabilities in the Capability
+						 * Information field
+						 */
+#define DOT11_SC_REASSOC_FAIL		11	/* Reassociation denied due to inability
+						 * to confirm that association exists
+						 */
+#define DOT11_SC_ASSOC_FAIL		12	/* Association denied due to reason
+						 * outside the scope of this standard
+						 */
+#define DOT11_SC_AUTH_MISMATCH		13	/* Responding station does not support
+						 * the specified authentication
+						 * algorithm
+						 */
+#define DOT11_SC_AUTH_SEQ		14	/* Received an Authentication frame
+						 * with authentication transaction
+						 * sequence number out of expected
+						 * sequence
+						 */
+#define DOT11_SC_AUTH_CHALLENGE_FAIL	15	/* Authentication rejected because of
+						 * challenge failure
+						 */
+#define DOT11_SC_AUTH_TIMEOUT		16	/* Authentication rejected due to timeout
+						 * waiting for next frame in sequence
+						 */
+#define DOT11_SC_ASSOC_BUSY_FAIL	17	/* Association denied because AP is
+						 * unable to handle additional
+						 * associated stations
+						 */
+#define DOT11_SC_ASSOC_RATE_MISMATCH	18	/* Association denied due to requesting
+						 * station not supporting all of the
+						 * data rates in the BSSBasicRateSet
+						 * parameter
+						 */
+#define DOT11_SC_ASSOC_SHORT_REQUIRED	19	/* Association denied due to requesting
+						 * station not supporting the Short
+						 * Preamble option
+						 */
+#define DOT11_SC_ASSOC_PBCC_REQUIRED	20	/* Association denied due to requesting
+						 * station not supporting the PBCC
+						 * Modulation option
+						 */
+#define DOT11_SC_ASSOC_AGILITY_REQUIRED	21	/* Association denied due to requesting
+						 * station not supporting the Channel
+						 * Agility option
+						 */
+#define DOT11_SC_ASSOC_SPECTRUM_REQUIRED	22	/* Association denied because Spectrum
+							 * Management capability is required.
+							 */
+#define DOT11_SC_ASSOC_BAD_POWER_CAP	23	/* Association denied because the info
+						 * in the Power Cap element is
+						 * unacceptable.
+						 */
+#define DOT11_SC_ASSOC_BAD_SUP_CHANNELS	24	/* Association denied because the info
+						 * in the Supported Channel element is
+						 * unacceptable
+						 */
+#define DOT11_SC_ASSOC_SHORTSLOT_REQUIRED	25	/* Association denied due to requesting
+							 * station not supporting the Short Slot
+							 * Time option
+							 */
+#define DOT11_SC_ASSOC_ERPBCC_REQUIRED	26	/* Association denied due to requesting
+						 * station not supporting the ER-PBCC
+						 * Modulation option
+						 */
+#define DOT11_SC_ASSOC_DSSOFDM_REQUIRED	27	/* Association denied due to requesting
+						 * station not supporting the DSS-OFDM
+						 * option
+						 */
+#define DOT11_SC_ASSOC_R0KH_UNREACHABLE	28	/* Association denied due to AP
+						 * being unable to reach the R0 Key Holder
+						 */
+#define DOT11_SC_ASSOC_TRY_LATER	30	/* Association denied temporarily, try again later
+						 */
+#define DOT11_SC_ASSOC_MFP_VIOLATION	31	/* Association denied due to Robust Management
+						 * frame policy violation
+						 */
+
+#define	DOT11_SC_DECLINED		37	/* request declined */
+#define	DOT11_SC_INVALID_PARAMS		38	/* One or more params have invalid values */
+#define DOT11_SC_INVALID_PAIRWISE_CIPHER	42 /* invalid pairwise cipher */
+#define	DOT11_SC_INVALID_AKMP		43	/* Association denied due to invalid AKMP */
+#define DOT11_SC_INVALID_RSNIE_CAP	45	/* invalid RSN IE capabilities */
+#define DOT11_SC_DLS_NOT_ALLOWED	48	/* DLS is not allowed in the BSS by policy */
+#define	DOT11_SC_INVALID_PMKID		53	/* Association denied due to invalid PMKID */
+#define	DOT11_SC_INVALID_MDID		54	/* Association denied due to invalid MDID */
+#define	DOT11_SC_INVALID_FTIE		55	/* Association denied due to invalid FTIE */
+
+#define DOT11_SC_UNEXP_MSG			70	/* Unexpected message */
+#define DOT11_SC_INVALID_SNONCE		71	/* Invalid SNonce */
+#define DOT11_SC_INVALID_RSNIE		72	/* Invalid contents of RSNIE */
+
+/* Info Elts, length of INFORMATION portion of Info Elts */
+#define DOT11_MNG_DS_PARAM_LEN			1	/* d11 management DS parameter length */
+#define DOT11_MNG_IBSS_PARAM_LEN		2	/* d11 management IBSS parameter length */
+
+/* TIM Info element has 3 bytes fixed info in INFORMATION field,
+ * followed by 1 to 251 bytes of Partial Virtual Bitmap
+ */
+#define DOT11_MNG_TIM_FIXED_LEN			3	/* d11 management TIM fixed length */
+#define DOT11_MNG_TIM_DTIM_COUNT		0	/* d11 management DTIM count */
+#define DOT11_MNG_TIM_DTIM_PERIOD		1	/* d11 management DTIM period */
+#define DOT11_MNG_TIM_BITMAP_CTL		2	/* d11 management TIM BITMAP control  */
+#define DOT11_MNG_TIM_PVB			3	/* d11 management TIM PVB */
+
+/* TLV defines */
+#define TLV_TAG_OFF		0	/* tag offset */
+#define TLV_LEN_OFF		1	/* length offset */
+#define TLV_HDR_LEN		2	/* header length */
+#define TLV_BODY_OFF		2	/* body offset */
+
+/* Management Frame Information Element IDs */
+#define DOT11_MNG_SSID_ID			0	/* d11 management SSID id */
+#define DOT11_MNG_RATES_ID			1	/* d11 management rates id */
+#define DOT11_MNG_FH_PARMS_ID			2	/* d11 management FH parameter id */
+#define DOT11_MNG_DS_PARMS_ID			3	/* d11 management DS parameter id */
+#define DOT11_MNG_CF_PARMS_ID			4	/* d11 management CF parameter id */
+#define DOT11_MNG_TIM_ID			5	/* d11 management TIM id */
+#define DOT11_MNG_IBSS_PARMS_ID			6	/* d11 management IBSS parameter id */
+#define DOT11_MNG_COUNTRY_ID			7	/* d11 management country id */
+#define DOT11_MNG_HOPPING_PARMS_ID		8	/* d11 management hopping parameter id */
+#define DOT11_MNG_HOPPING_TABLE_ID		9	/* d11 management hopping table id */
+#define DOT11_MNG_REQUEST_ID			10	/* d11 management request id */
+#define DOT11_MNG_QBSS_LOAD_ID 			11	/* d11 management QBSS Load id */
+#define DOT11_MNG_EDCA_PARAM_ID			12	/* 11E EDCA Parameter id */
+#define DOT11_MNG_CHALLENGE_ID			16	/* d11 management chanllenge id */
+#define DOT11_MNG_PWR_CONSTRAINT_ID		32	/* 11H PowerConstraint */
+#define DOT11_MNG_PWR_CAP_ID			33	/* 11H PowerCapability */
+#define DOT11_MNG_TPC_REQUEST_ID 		34	/* 11H TPC Request */
+#define DOT11_MNG_TPC_REPORT_ID			35	/* 11H TPC Report */
+#define DOT11_MNG_SUPP_CHANNELS_ID		36	/* 11H Supported Channels */
+#define DOT11_MNG_CHANNEL_SWITCH_ID		37	/* 11H ChannelSwitch Announcement */
+#define DOT11_MNG_MEASURE_REQUEST_ID		38	/* 11H MeasurementRequest */
+#define DOT11_MNG_MEASURE_REPORT_ID		39	/* 11H MeasurementReport */
+#define DOT11_MNG_QUIET_ID			40	/* 11H Quiet */
+#define DOT11_MNG_IBSS_DFS_ID			41	/* 11H IBSS_DFS */
+#define DOT11_MNG_ERP_ID			42	/* d11 management ERP id */
+#define DOT11_MNG_TS_DELAY_ID			43	/* d11 management TS Delay id */
+#define	DOT11_MNG_HT_CAP			45	/* d11 mgmt HT cap id */
+#define DOT11_MNG_QOS_CAP_ID			46	/* 11E QoS Capability id */
+#define DOT11_MNG_NONERP_ID			47	/* d11 management NON-ERP id */
+#define DOT11_MNG_RSN_ID			48	/* d11 management RSN id */
+#define DOT11_MNG_EXT_RATES_ID			50	/* d11 management ext. rates id */
+#define DOT11_MNG_AP_CHREP_ID		51	/* 11k AP Channel report id */
+#define DOT11_MNG_NBR_REP_ID		52	/* 11k Neighbor report id */
+#define DOT11_MNG_MDIE_ID		54	/* 11r Mobility domain id */
+#define DOT11_MNG_FTIE_ID		55	/* 11r Fast Bss Transition id */
+#define DOT11_MNG_FT_TI_ID		56	/* 11r Timeout Interval id */
+#define	DOT11_MNG_REGCLASS_ID			59	/* d11 management regulatory class id */
+#define DOT11_MNG_EXT_CSA_ID			60	/* d11 Extended CSA */
+#define	DOT11_MNG_HT_ADD			61	/* d11 mgmt additional HT info */
+#define	DOT11_MNG_EXT_CHANNEL_OFFSET		62	/* d11 mgmt ext channel offset */
+#define DOT11_MNG_WAPI_ID			68	/* d11 management WAPI id */
+#define DOT11_MNG_TIME_ADVERTISE_ID	69	/* 11p time advertisement */
+#define DOT11_MNG_RRM_CAP_ID		70	/* 11k radio measurement capability */
+#define	DOT11_MNG_HT_BSS_COEXINFO_ID		72	/* d11 mgmt OBSS Coexistence INFO */
+#define	DOT11_MNG_HT_BSS_CHANNEL_REPORT_ID	73	/* d11 mgmt OBSS Intolerant Channel list */
+#define	DOT11_MNG_HT_OBSS_ID			74	/* d11 mgmt OBSS HT info */
+#define DOT11_MNG_CHANNEL_USAGE			97 /* 11v channel usage */
+#define DOT11_MNG_TIME_ZONE_ID			98	/* 11v time zone */
+#define DOT11_MNG_LINK_IDENTIFIER_ID	101	/* 11z TDLS Link Identifier IE */
+#define DOT11_MNG_WAKEUP_SCHEDULE_ID	102 /* 11z TDLS Wakeup Schedule IE */
+#define DOT11_MNG_CHANNEL_SWITCH_TIMING_ID	104 /* 11z TDLS Channel Switch Timing IE */
+#define DOT11_MNG_PTI_CONTROL_ID		105	/* 11z TDLS PTI Control IE */
+#define DOT11_MNG_PU_BUFFER_STATUS_ID	106	/* 11z TDLS PU Buffer Status IE */
+#define DOT11_MNG_INTERWORKING_ID		107	/* 11u interworking */
+#define DOT11_MNG_ADVERTISEMENT_ID		108	/* 11u advertisement protocol */
+#define DOT11_MNG_EXP_BW_REQ_ID			109	/* 11u expedited bandwith request */
+#define DOT11_MNG_QOS_MAP_ID			110	/* 11u QoS map set */
+#define DOT11_MNG_ROAM_CONSORT_ID		111	/* 11u roaming consortium */
+#define DOT11_MNG_EMERGCY_ALERT_ID		112	/* 11u emergency alert identifier */
+#define	DOT11_MNG_EXT_CAP_ID		127	/* d11 mgmt ext capability */
+#define	DOT11_MNG_VHT_CAP_ID		191	/* d11 mgmt VHT cap id */
+#define	DOT11_MNG_VHT_OPERATION_ID	192	/* d11 mgmt VHT op id */
+
+#define DOT11_MNG_WPA_ID			221	/* d11 management WPA id */
+#define DOT11_MNG_PROPR_ID			221	/* d11 management proprietary id */
+/* should start using this one instead of above two */
+#define DOT11_MNG_VS_ID				221	/* d11 management Vendor Specific IE */
+
+/* Rate element Basic flag and rate mask */
+#define DOT11_RATE_BASIC			0x80	/* flag for a Basic Rate */
+#define DOT11_RATE_MASK				0x7F	/* mask for numeric part of rate */
+
+/* ERP info element bit values */
+#define DOT11_MNG_ERP_LEN			1	/* ERP is currently 1 byte long */
+#define DOT11_MNG_NONERP_PRESENT		0x01	/* NonERP (802.11b) STAs are present
+							 *in the BSS
+							 */
+#define DOT11_MNG_USE_PROTECTION		0x02	/* Use protection mechanisms for
+							 *ERP-OFDM frames
+							 */
+#define DOT11_MNG_BARKER_PREAMBLE		0x04	/* Short Preambles: 0 == allowed,
+							 * 1 == not allowed
+							 */
+/* TS Delay element offset & size */
+#define DOT11_MGN_TS_DELAY_LEN		4	/* length of TS DELAY IE */
+#define TS_DELAY_FIELD_SIZE			4	/* TS DELAY field size */
+
+/* Capability Information Field */
+#define DOT11_CAP_ESS				0x0001	/* d11 cap. ESS */
+#define DOT11_CAP_IBSS				0x0002	/* d11 cap. IBSS */
+#define DOT11_CAP_POLLABLE			0x0004	/* d11 cap. pollable */
+#define DOT11_CAP_POLL_RQ			0x0008	/* d11 cap. poll request */
+#define DOT11_CAP_PRIVACY			0x0010	/* d11 cap. privacy */
+#define DOT11_CAP_SHORT				0x0020	/* d11 cap. short */
+#define DOT11_CAP_PBCC				0x0040	/* d11 cap. PBCC */
+#define DOT11_CAP_AGILITY			0x0080	/* d11 cap. agility */
+#define DOT11_CAP_SPECTRUM			0x0100	/* d11 cap. spectrum */
+#define DOT11_CAP_SHORTSLOT			0x0400	/* d11 cap. shortslot */
+#define DOT11_CAP_RRM			0x1000	/* d11 cap. 11k radio measurement */
+#define DOT11_CAP_CCK_OFDM			0x2000	/* d11 cap. CCK/OFDM */
+
+/* Extended capabilities IE bitfields */
+/* 20/40 BSS Coexistence Management support bit position */
+#define DOT11_EXT_CAP_OBSS_COEX_MGMT		0
+/* scheduled PSMP support bit position */
+#define DOT11_EXT_CAP_SPSMP					6
+/* BSS Transition Management support bit position */
+#define DOT11_EXT_CAP_BSS_TRANSITION_MGMT	19
+/* Interworking support bit position */
+#define DOT11_EXT_CAP_IW						31
+/* service Interval granularity bit position and mask */
+#define DOT11_EXT_CAP_SI						41
+#define DOT11_EXT_CAP_SI_MASK					0x0E
+
+/*
+ * Action Frame Constants
+ */
+#define DOT11_ACTION_HDR_LEN		2	/* action frame category + action field */
+#define DOT11_ACTION_CAT_OFF		0	/* category offset */
+#define DOT11_ACTION_ACT_OFF		1	/* action offset */
+
+/* Action Category field (sec 7.3.1.11) */
+#define DOT11_ACTION_CAT_ERR_MASK	0x80	/* category error mask */
+#define DOT11_ACTION_CAT_MASK		0x7F	/* category mask */
+#define DOT11_ACTION_CAT_SPECT_MNG	0	/* category spectrum management */
+#define DOT11_ACTION_CAT_QOS		1	/* category QoS */
+#define DOT11_ACTION_CAT_DLS		2	/* category DLS */
+#define DOT11_ACTION_CAT_BLOCKACK	3	/* category block ack */
+#define DOT11_ACTION_CAT_PUBLIC		4	/* category public */
+#define DOT11_ACTION_CAT_RRM		5	/* category radio measurements */
+#define DOT11_ACTION_CAT_FBT	6	/* category fast bss transition */
+#define DOT11_ACTION_CAT_HT		7	/* category for HT */
+#define	DOT11_ACTION_CAT_SA_QUERY	8	/* security association query */
+#define	DOT11_ACTION_CAT_PDPA		9	/* protected dual of public action */
+#define DOT11_ACTION_CAT_BSSMGMT	10	/* category for BSS transition management */
+#define DOT11_ACTION_NOTIFICATION	17
+#define DOT11_ACTION_CAT_VSP		126	/* protected vendor specific */
+#define DOT11_ACTION_CAT_VS		127	/* category Vendor Specific */
+
+/* Spectrum Management Action IDs (sec 7.4.1) */
+#define DOT11_SM_ACTION_M_REQ		0	/* d11 action measurement request */
+#define DOT11_SM_ACTION_M_REP		1	/* d11 action measurement response */
+#define DOT11_SM_ACTION_TPC_REQ		2	/* d11 action TPC request */
+#define DOT11_SM_ACTION_TPC_REP		3	/* d11 action TPC response */
+#define DOT11_SM_ACTION_CHANNEL_SWITCH	4	/* d11 action channel switch */
+#define DOT11_SM_ACTION_EXT_CSA		5	/* d11 extened CSA for 11n */
+
+/* HT action ids */
+#define DOT11_ACTION_ID_HT_CH_WIDTH	0	/* notify channel width action id */
+#define DOT11_ACTION_ID_HT_MIMO_PS	1	/* mimo ps action id */
+
+/* Public action ids */
+#define DOT11_PUB_ACTION_BSS_COEX_MNG	0	/* 20/40 Coexistence Management action id */
+#define DOT11_PUB_ACTION_CHANNEL_SWITCH	4	/* d11 action channel switch */
+
+/* Block Ack action types */
+#define DOT11_BA_ACTION_ADDBA_REQ	0	/* ADDBA Req action frame type */
+#define DOT11_BA_ACTION_ADDBA_RESP	1	/* ADDBA Resp action frame type */
+#define DOT11_BA_ACTION_DELBA		2	/* DELBA action frame type */
+
+/* ADDBA action parameters */
+#define DOT11_ADDBA_PARAM_AMSDU_SUP	0x0001	/* AMSDU supported under BA */
+#define DOT11_ADDBA_PARAM_POLICY_MASK	0x0002	/* policy mask(ack vs delayed) */
+#define DOT11_ADDBA_PARAM_POLICY_SHIFT	1	/* policy shift */
+#define DOT11_ADDBA_PARAM_TID_MASK	0x003c	/* tid mask */
+#define DOT11_ADDBA_PARAM_TID_SHIFT	2	/* tid shift */
+#define DOT11_ADDBA_PARAM_BSIZE_MASK	0xffc0	/* buffer size mask */
+#define DOT11_ADDBA_PARAM_BSIZE_SHIFT	6	/* buffer size shift */
+
+#define DOT11_ADDBA_POLICY_DELAYED	0	/* delayed BA policy */
+#define DOT11_ADDBA_POLICY_IMMEDIATE	1	/* immediate BA policy */
+
+/* Fast Transition action types */
+#define DOT11_FT_ACTION_FT_RESERVED		0
+#define DOT11_FT_ACTION_FT_REQ			1	/* FBT request - for over-the-DS FBT */
+#define DOT11_FT_ACTION_FT_RES			2	/* FBT response - for over-the-DS FBT */
+#define DOT11_FT_ACTION_FT_CON			3	/* FBT confirm - for OTDS with RRP */
+#define DOT11_FT_ACTION_FT_ACK			4	/* FBT ack */
+
+/* DLS action types */
+#define DOT11_DLS_ACTION_REQ				0	/* DLS Request */
+#define DOT11_DLS_ACTION_RESP				1	/* DLS Response */
+#define DOT11_DLS_ACTION_TD				2	/* DLS Teardown */
+
+/* Wireless Network Management (WNM) action types */
+#define DOT11_WNM_ACTION_EVENT_REQ			0
+#define DOT11_WNM_ACTION_EVENT_REP			1
+#define DOT11_WNM_ACTION_DIAG_REQ			2
+#define DOT11_WNM_ACTION_DIAG_REP			3
+#define DOT11_WNM_ACTION_LOC_CFG_REQ		4
+#define DOT11_WNM_ACTION_LOC_RFG_RESP		5
+#define DOT11_WNM_ACTION_BSS_TRANS_QURY		6
+#define DOT11_WNM_ACTION_BSS_TRANS_REQ		7
+#define DOT11_WNM_ACTION_BSS_TRANS_RESP		8
+#define DOT11_WNM_ACTION_FMS_REQ			9
+#define DOT11_WNM_ACTION_FMS_RESP			10
+#define DOT11_WNM_ACTION_COL_INTRFRNCE_REQ	11
+#define DOT11_WNM_ACTION_COL_INTRFRNCE_REP	12
+#define DOT11_WNM_ACTION_TFS_REQ			13
+#define DOT11_WNM_ACTION_TFS_RESP			14
+#define DOT11_WNM_ACTION_TFS_NOTIFY			15
+#define DOT11_WNM_ACTION_WNM_SLEEP_REQ		16
+#define DOT11_WNM_ACTION_WNM_SLEEP_RESP		17
+#define DOT11_WNM_ACTION_TIM_BCAST_REQ		18
+#define DOT11_WNM_ACTION_TIM_BCAST_RESP		19
+#define DOT11_WNM_ACTION_QOS_TRFC_CAP_UPD	20
+#define DOT11_WNM_ACTION_CHAN_USAGE_REQ		21
+#define DOT11_WNM_ACTION_CHAN_USAGE_RESP	22
+#define DOT11_WNM_ACTION_DMS_REQ			23
+#define DOT11_WNM_ACTION_DMS_RESP			24
+#define DOT11_WNM_ACTION_TMNG_MEASUR_REQ	25
+#define DOT11_WNM_ACTION_NOTFCTN_REQ		26
+#define DOT11_WNM_ACTION_NOTFCTN_RES		27
+
+#define DOT11_MNG_COUNTRY_ID_LEN 3
+
+/* DLS Request frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_dls_req {
+	uint8 category;			/* category of action frame (2) */
+	uint8 action;				/* DLS action: req (0) */
+	struct ether_addr	da;		/* destination address */
+	struct ether_addr	sa;		/* source address */
+	uint16 cap;				/* capability */
+	uint16 timeout;			/* timeout value */
+	uint8 data[1];				/* IE:support rate, extend support rate, HT cap */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_dls_req dot11_dls_req_t;
+#define DOT11_DLS_REQ_LEN 18	/* Fixed length */
+
+/* DLS response frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_dls_resp {
+	uint8 category;			/* category of action frame (2) */
+	uint8 action;				/* DLS action: req (0) */
+	uint16 status;				/* status code field */
+	struct ether_addr	da;		/* destination address */
+	struct ether_addr	sa;		/* source address */
+	uint8 data[1];				/* optional: capability, rate ... */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_dls_resp dot11_dls_resp_t;
+#define DOT11_DLS_RESP_LEN 16	/* Fixed length */
+
+
+/* BSS Management Transition Query frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_bss_trans_query {
+	uint8 category;				/* category of action frame (10) */
+	uint8 action;				/* WNM action: trans_query (6) */
+	uint8 token;				/* dialog token */
+	uint8 reason;				/* transition query reason */
+	uint8 data[1];				/* Elements */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_bss_trans_query dot11_bss_trans_query_t;
+#define DOT11_BSS_TRANS_QUERY_LEN 4	/* Fixed length */
+
+/* BSS Management Transition Request frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_bss_trans_req {
+	uint8 category;				/* category of action frame (10) */
+	uint8 action;				/* WNM action: trans_req (7) */
+	uint8 token;				/* dialog token */
+	uint8 reqmode;				/* transition request mode */
+	uint16 disassoc_tmr;		/* disassociation timer */
+	uint8 validity_intrvl;		/* validity interval */
+	uint8 data[1];				/* optional: BSS term duration, ... */
+								/* ...session info URL, list */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_bss_trans_req dot11_bss_trans_req_t;
+#define DOT11_BSS_TRANS_REQ_LEN 7	/* Fixed length */
+
+#define DOT11_BSS_TERM_DUR_LEN 12	/* Fixed length if present */
+
+
+/* BSS Mgmt Transition Request Mode Field - 802.11v */
+#define DOT11_BSS_TRNS_REQMODE_PREF_LIST_INCL		0x01
+#define DOT11_BSS_TRNS_REQMODE_ABRIDGED				0x02
+#define DOT11_BSS_TRNS_REQMODE_DISASSOC_IMMINENT	0x04
+#define DOT11_BSS_TRNS_REQMODE_BSS_TERM_INCL		0x08
+#define DOT11_BSS_TRNS_REQMODE_ESS_DISASSOC_IMNT	0x10
+
+
+/* BSS Management transition response frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_bss_trans_res {
+	uint8 category;				/* category of action frame (10) */
+	uint8 action;				/* WNM action: trans_res (8) */
+	uint8 token;				/* dialog token */
+	uint8 status;				/* transition status */
+	uint8 term_delay;			/* validity interval */
+	uint8 data[1];				/* optional: BSS term duration, ... */
+								/* ...session info URL, list */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_bss_trans_res dot11_bss_trans_res_t;
+#define DOT11_BSS_TRANS_RES_LEN 5	/* Fixed length */
+
+/* BSS Mgmt Transition Response Status Field */
+#define DOT11_BSS_TRNS_RES_STATUS_ACCEPT				0
+#define DOT11_BSS_TRNS_RES_STATUS_REJECT				1
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_INSUFF_BCN		2
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_INSUFF_CAP		3
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_TERM_UNDESIRED	4
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_TERM_DELAY_REQ	5
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_BSS_LIST_PROVIDED	6
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_NO_SUITABLE_BSS	7
+#define DOT11_BSS_TRNS_RES_STATUS_REJ_LEAVING_ESS		8
+
+
+/* Neighbor Report BSSID Information Field */
+#define DOT11_NBR_RPRT_BSSID_INFO_REACHABILTY		0x0003
+#define DOT11_NBR_RPRT_BSSID_INFO_SEC				0x0004
+#define DOT11_NBR_RPRT_BSSID_INFO_KEY_SCOPE			0x0008
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP				0x03f0
+
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_SPEC_MGMT		0x0010
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_QOS			0x0020
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_APSD			0x0040
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_RDIO_MSMT		0x0080
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_DEL_BA		0x0100
+#define DOT11_NBR_RPRT_BSSID_INFO_CAP_IMM_BA		0x0200
+
+/* Neighbor Report Subelements */
+#define DOT11_NBR_RPRT_SUBELEM_BSS_CANDDT_PREF_ID	3
+
+
+BWL_PRE_PACKED_STRUCT struct dot11_addba_req {
+	uint8 category;				/* category of action frame (3) */
+	uint8 action;				/* action: addba req */
+	uint8 token;				/* identifier */
+	uint16 addba_param_set;		/* parameter set */
+	uint16 timeout;				/* timeout in seconds */
+	uint16 start_seqnum;		/* starting sequence number */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_addba_req dot11_addba_req_t;
+#define DOT11_ADDBA_REQ_LEN		9	/* length of addba req frame */
+
+BWL_PRE_PACKED_STRUCT struct dot11_addba_resp {
+	uint8 category;				/* category of action frame (3) */
+	uint8 action;				/* action: addba resp */
+	uint8 token;				/* identifier */
+	uint16 status;				/* status of add request */
+	uint16 addba_param_set;			/* negotiated parameter set */
+	uint16 timeout;				/* negotiated timeout in seconds */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_addba_resp dot11_addba_resp_t;
+#define DOT11_ADDBA_RESP_LEN		9	/* length of addba resp frame */
+
+/* DELBA action parameters */
+#define DOT11_DELBA_PARAM_INIT_MASK	0x0800	/* initiator mask */
+#define DOT11_DELBA_PARAM_INIT_SHIFT	11	/* initiator shift */
+#define DOT11_DELBA_PARAM_TID_MASK	0xf000	/* tid mask */
+#define DOT11_DELBA_PARAM_TID_SHIFT	12	/* tid shift */
+
+BWL_PRE_PACKED_STRUCT struct dot11_delba {
+	uint8 category;				/* category of action frame (3) */
+	uint8 action;				/* action: addba req */
+	uint16 delba_param_set;			/* paarmeter set */
+	uint16 reason;				/* reason for dellba */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_delba dot11_delba_t;
+#define DOT11_DELBA_LEN			6	/* length of delba frame */
+
+/* SA Query action field value */
+#define SA_QUERY_REQUEST		0
+#define SA_QUERY_RESPONSE		1
+
+/* ************* 802.11r related definitions. ************* */
+
+/* Over-the-DS Fast Transition Request frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_ft_req {
+	uint8 category;			/* category of action frame (6) */
+	uint8 action;			/* action: ft req */
+	uint8 sta_addr[ETHER_ADDR_LEN];
+	uint8 tgt_ap_addr[ETHER_ADDR_LEN];
+	uint8 data[1];			/* Elements */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_ft_req dot11_ft_req_t;
+#define DOT11_FT_REQ_FIXED_LEN 14
+
+/* Over-the-DS Fast Transition Response frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_ft_res {
+	uint8 category;			/* category of action frame (6) */
+	uint8 action;			/* action: ft resp */
+	uint8 sta_addr[ETHER_ADDR_LEN];
+	uint8 tgt_ap_addr[ETHER_ADDR_LEN];
+	uint16 status;			/* status code */
+	uint8 data[1];			/* Elements */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_ft_res dot11_ft_res_t;
+#define DOT11_FT_RES_FIXED_LEN 16
+
+
+/* ************* 802.11k related definitions. ************* */
+
+/* Radio measurements enabled capability ie */
+
+#define DOT11_RRM_CAP_LEN		5	/* length of rrm cap bitmap */
+BWL_PRE_PACKED_STRUCT struct dot11_rrm_cap_ie {
+	uint8 cap[DOT11_RRM_CAP_LEN];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rrm_cap_ie dot11_rrm_cap_ie_t;
+
+/* Bitmap definitions for cap ie */
+#define DOT11_RRM_CAP_LINK			0
+#define DOT11_RRM_CAP_NEIGHBOR_REPORT	1
+#define DOT11_RRM_CAP_PARALLEL		2
+#define DOT11_RRM_CAP_REPEATED		3
+#define DOT11_RRM_CAP_BCN_PASSIVE	4
+#define DOT11_RRM_CAP_BCN_ACTIVE	5
+#define DOT11_RRM_CAP_BCN_TABLE		6
+#define DOT11_RRM_CAP_BCN_REP_COND	7
+#define DOT11_RRM_CAP_AP_CHANREP	16
+
+
+/* Operating Class (formerly "Regulatory Class") definitions */
+#define DOT11_OP_CLASS_NONE			255
+
+
+/* Radio Measurements action ids */
+#define DOT11_RM_ACTION_RM_REQ		0	/* Radio measurement request */
+#define DOT11_RM_ACTION_RM_REP		1	/* Radio measurement report */
+#define DOT11_RM_ACTION_LM_REQ		2	/* Link measurement request */
+#define DOT11_RM_ACTION_LM_REP		3	/* Link measurement report */
+#define DOT11_RM_ACTION_NR_REQ		4	/* Neighbor report request */
+#define DOT11_RM_ACTION_NR_REP		5	/* Neighbor report response */
+
+/* Generic radio measurement action frame header */
+BWL_PRE_PACKED_STRUCT struct dot11_rm_action {
+	uint8 category;				/* category of action frame (5) */
+	uint8 action;				/* radio measurement action */
+	uint8 token;				/* dialog token */
+	uint8 data[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rm_action dot11_rm_action_t;
+#define DOT11_RM_ACTION_LEN 3
+
+BWL_PRE_PACKED_STRUCT struct dot11_rmreq {
+	uint8 category;				/* category of action frame (5) */
+	uint8 action;				/* radio measurement action */
+	uint8 token;				/* dialog token */
+	uint16 reps;				/* no. of repetitions */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rmreq dot11_rmreq_t;
+#define DOT11_RMREQ_LEN	5
+
+BWL_PRE_PACKED_STRUCT struct dot11_rm_ie {
+	uint8 id;
+	uint8 len;
+	uint8 token;
+	uint8 mode;
+	uint8 type;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rm_ie dot11_rm_ie_t;
+#define DOT11_RM_IE_LEN	5
+
+/* Definitions for "mode" bits in rm req */
+#define DOT11_RMREQ_MODE_PARALLEL	1
+#define DOT11_RMREQ_MODE_ENABLE		2
+#define DOT11_RMREQ_MODE_REQUEST	4
+#define DOT11_RMREQ_MODE_REPORT		8
+#define DOT11_RMREQ_MODE_DURMAND	0x10	/* Duration Mandatory */
+
+/* Definitions for "mode" bits in rm rep */
+#define DOT11_RMREP_MODE_LATE		1
+#define DOT11_RMREP_MODE_INCAPABLE	2
+#define DOT11_RMREP_MODE_REFUSED	4
+
+BWL_PRE_PACKED_STRUCT struct dot11_rmreq_bcn {
+	uint8 id;
+	uint8 len;
+	uint8 token;
+	uint8 mode;
+	uint8 type;
+	uint8 reg;
+	uint8 channel;
+	uint16 interval;
+	uint16 duration;
+	uint8 bcn_mode;
+	struct ether_addr	bssid;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rmreq_bcn dot11_rmreq_bcn_t;
+#define DOT11_RMREQ_BCN_LEN	18
+
+BWL_PRE_PACKED_STRUCT struct dot11_rmrep_bcn {
+	uint8 reg;
+	uint8 channel;
+	uint32 starttime[2];
+	uint16 duration;
+	uint8 frame_info;
+	uint8 rcpi;
+	uint8 rsni;
+	struct ether_addr	bssid;
+	uint8 antenna_id;
+	uint32 parent_tsf;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rmrep_bcn dot11_rmrep_bcn_t;
+#define DOT11_RMREP_BCN_LEN	26
+
+/* Beacon request measurement mode */
+#define DOT11_RMREQ_BCN_PASSIVE	0
+#define DOT11_RMREQ_BCN_ACTIVE	1
+#define DOT11_RMREQ_BCN_TABLE	2
+
+/* Sub-element IDs for Beacon Request */
+#define DOT11_RMREQ_BCN_SSID_ID	0
+#define DOT11_RMREQ_BCN_REPINFO_ID	1
+#define DOT11_RMREQ_BCN_REPDET_ID	2
+#define DOT11_RMREQ_BCN_REQUEST_ID	10
+#define DOT11_RMREQ_BCN_APCHREP_ID	51
+
+/* Reporting Detail element definition */
+#define DOT11_RMREQ_BCN_REPDET_FIXED	0	/* Fixed length fields only */
+#define DOT11_RMREQ_BCN_REPDET_REQUEST	1	/* + requested information elems */
+#define DOT11_RMREQ_BCN_REPDET_ALL	2	/* All fields */
+
+/* Sub-element IDs for Beacon Report */
+#define DOT11_RMREP_BCN_FRM_BODY	1
+
+/* Neighbor measurement report */
+BWL_PRE_PACKED_STRUCT struct dot11_rmrep_nbr {
+	struct ether_addr	bssid;
+	uint32	bssid_info;
+	uint8 reg;
+	uint8 channel;
+	uint8 phytype;
+	uchar sub_elements[1]; 	/* Variable size data */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_rmrep_nbr dot11_rmrep_nbr_t;
+#define DOT11_RMREP_NBR_LEN	13
+
+/* MLME Enumerations */
+#define DOT11_BSSTYPE_INFRASTRUCTURE		0	/* d11 infrastructure */
+#define DOT11_BSSTYPE_INDEPENDENT		1	/* d11 independent */
+#define DOT11_BSSTYPE_ANY			2	/* d11 any BSS type */
+#define DOT11_SCANTYPE_ACTIVE			0	/* d11 scan active */
+#define DOT11_SCANTYPE_PASSIVE			1	/* d11 scan passive */
+
+/* Link Measurement */
+BWL_PRE_PACKED_STRUCT struct dot11_lmreq {
+	uint8 category;				/* category of action frame (5) */
+	uint8 action;				/* radio measurement action */
+	uint8 token;				/* dialog token */
+	uint8 txpwr;				/* Transmit Power Used */
+	uint8 maxtxpwr;				/* Max Transmit Power */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_lmreq dot11_lmreq_t;
+#define DOT11_LMREQ_LEN	5
+
+BWL_PRE_PACKED_STRUCT struct dot11_lmrep {
+	uint8 category;				/* category of action frame (5) */
+	uint8 action;				/* radio measurement action */
+	uint8 token;				/* dialog token */
+	dot11_tpc_rep_t tpc;			/* TPC element */
+	uint8 rxant;				/* Receive Antenna ID */
+	uint8 txant;				/* Transmit Antenna ID */
+	uint8 rcpi;				/* RCPI */
+	uint8 rsni;				/* RSNI */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_lmrep dot11_lmrep_t;
+#define DOT11_LMREP_LEN	11
+
+/* 802.11 BRCM "Compromise" Pre N constants */
+#define PREN_PREAMBLE		24	/* green field preamble time */
+#define PREN_MM_EXT		12	/* extra mixed mode preamble time */
+#define PREN_PREAMBLE_EXT	4	/* extra preamble (multiply by unique_streams-1) */
+
+/* 802.11N PHY constants */
+#define RIFS_11N_TIME		2	/* NPHY RIFS time */
+
+/* 802.11 HT PLCP format 802.11n-2009, sec 20.3.9.4.3
+ * HT-SIG is composed of two 24 bit parts, HT-SIG1 and HT-SIG2
+ */
+/* HT-SIG1 */
+#define HT_SIG1_MCS_MASK	0x00007F
+#define HT_SIG1_CBW		0x000080
+#define HT_SIG1_HT_LENGTH	0xFFFF00
+
+/* HT-SIG2 */
+#define HT_SIG2_SMOOTHING	0x000001
+#define HT_SIG2_NOT_SOUNDING	0x000002
+#define HT_SIG2_RESERVED	0x000004
+#define HT_SIG2_AGGREGATION	0x000008
+#define HT_SIG2_STBC_MASK	0x000030
+#define HT_SIG2_STBC_SHIFT	4
+#define HT_SIG2_FEC_CODING	0x000040
+#define HT_SIG2_SHORT_GI	0x000080
+#define HT_SIG2_ESS_MASK	0x000300
+#define HT_SIG2_ESS_SHIFT	8
+#define HT_SIG2_CRC		0x03FC00
+#define HT_SIG2_TAIL		0x1C0000
+
+/* 802.11 A PHY constants */
+#define APHY_SLOT_TIME		9	/* APHY slot time */
+#define APHY_SIFS_TIME		16	/* APHY SIFS time */
+#define APHY_DIFS_TIME		(APHY_SIFS_TIME + (2 * APHY_SLOT_TIME))	/* APHY DIFS time */
+#define APHY_PREAMBLE_TIME	16	/* APHY preamble time */
+#define APHY_SIGNAL_TIME	4	/* APHY signal time */
+#define APHY_SYMBOL_TIME	4	/* APHY symbol time */
+#define APHY_SERVICE_NBITS	16	/* APHY service nbits */
+#define APHY_TAIL_NBITS		6	/* APHY tail nbits */
+#define	APHY_CWMIN		15	/* APHY cwmin */
+
+/* 802.11 B PHY constants */
+#define BPHY_SLOT_TIME		20	/* BPHY slot time */
+#define BPHY_SIFS_TIME		10	/* BPHY SIFS time */
+#define BPHY_DIFS_TIME		50	/* BPHY DIFS time */
+#define BPHY_PLCP_TIME		192	/* BPHY PLCP time */
+#define BPHY_PLCP_SHORT_TIME	96	/* BPHY PLCP short time */
+#define	BPHY_CWMIN		31	/* BPHY cwmin */
+
+/* 802.11 G constants */
+#define DOT11_OFDM_SIGNAL_EXTENSION	6	/* d11 OFDM signal extension */
+
+#define PHY_CWMAX		1023	/* PHY cwmax */
+
+#define	DOT11_MAXNUMFRAGS	16	/* max # fragments per MSDU */
+
+/* 802.11 AC (VHT) constants */
+
+typedef int vht_group_id_t;
+
+/* for VHT-A1 */
+/* SIG-A1 reserved bits */
+#define VHT_SIGA1_CONST_MASK 		0x800004
+
+#define VHT_SIGA1_20MHZ_VAL 		0x000000
+#define VHT_SIGA1_40MHZ_VAL 		0x000001
+#define VHT_SIGA1_80MHZ_VAL 		0x000002
+#define VHT_SIGA1_160MHZ_VAL 		0x000003
+
+#define VHT_SIGA1_STBC 			0x000008
+
+#define VHT_SIGA1_GID_MAX_GID 		0x3f
+#define VHT_SIGA1_GID_SHIFT 		4
+#define VHT_SIGA1_GID_TO_AP 		0x00
+#define VHT_SIGA1_GID_NOT_TO_AP 	0x3f
+
+#define VHT_SIGA1_NSTS_SHIFT 		10
+#define VHT_SIGA1_NSTS_SHIFT_MASK_USER0 0x001C00
+
+#define VHT_SIGA1_PARTIAL_AID_SHIFT 13
+
+/* for VHT-A2 */
+#define VHT_SIGA2_GI_NONE               0x000000
+#define VHT_SIGA2_GI_SHORT              0x000001
+#define VHT_SIGA2_GI_W_MOD10            0x000002
+#define VHT_SIGA2_CODING_LDPC           0x000004
+#define VHT_SIGA2_BEAMFORM_ENABLE       0x000100
+#define VHT_SIGA2_MCS_SHIFT             4
+
+#define VHT_SIGA2_B9_RESERVED           0x000200
+#define VHT_SIGA2_TAIL_MASK             0xfc0000
+#define VHT_SIGA2_TAIL_VALUE            0x000000
+
+#define VHT_SIGA2_SVC_BITS              16
+#define VHT_SIGA2_TAIL_BITS             6
+
+
+/* dot11Counters Table - 802.11 spec., Annex D */
+typedef struct d11cnt {
+	uint32		txfrag;		/* dot11TransmittedFragmentCount */
+	uint32		txmulti;	/* dot11MulticastTransmittedFrameCount */
+	uint32		txfail;		/* dot11FailedCount */
+	uint32		txretry;	/* dot11RetryCount */
+	uint32		txretrie;	/* dot11MultipleRetryCount */
+	uint32		rxdup;		/* dot11FrameduplicateCount */
+	uint32		txrts;		/* dot11RTSSuccessCount */
+	uint32		txnocts;	/* dot11RTSFailureCount */
+	uint32		txnoack;	/* dot11ACKFailureCount */
+	uint32		rxfrag;		/* dot11ReceivedFragmentCount */
+	uint32		rxmulti;	/* dot11MulticastReceivedFrameCount */
+	uint32		rxcrc;		/* dot11FCSErrorCount */
+	uint32		txfrmsnt;	/* dot11TransmittedFrameCount */
+	uint32		rxundec;	/* dot11WEPUndecryptableCount */
+} d11cnt_t;
+
+/* OUI for BRCM proprietary IE */
+#define BRCM_PROP_OUI		"\x00\x90\x4C"	/* Broadcom proprietary OUI */
+
+#ifndef LINUX_POSTMOGRIFY_REMOVAL
+/* The following BRCM_PROP_OUI types are currently in use (defined in
+ * relevant subsections). Each of them will be in a separate proprietary(221) IE
+ * #define SES_VNDR_IE_TYPE	1   (defined in src/ses/shared/ses.h)
+ * #define DPT_IE_TYPE		2
+ * #define HT_CAP_IE_TYPE	51
+ * #define HT_ADD_IE_TYPE	52
+ * #define BRCM_EXTCH_IE_TYPE	53
+ */
+
+/* Following is the generic structure for brcm_prop_ie (uses BRCM_PROP_OUI).
+ * DPT uses this format with type set to DPT_IE_TYPE
+ */
+BWL_PRE_PACKED_STRUCT struct brcm_prop_ie_s {
+	uint8 id;		/* IE ID, 221, DOT11_MNG_PROPR_ID */
+	uint8 len;		/* IE length */
+	uint8 oui[3];		/* Proprietary OUI, BRCM_PROP_OUI */
+	uint8 type;		/* type of this IE */
+	uint16 cap;		/* DPT capabilities */
+} BWL_POST_PACKED_STRUCT;
+typedef struct brcm_prop_ie_s brcm_prop_ie_t;
+
+#define BRCM_PROP_IE_LEN	6	/* len of fixed part of brcm_prop ie */
+
+#define DPT_IE_TYPE		2
+#define WET_TUNNEL_IE_TYPE	3
+#endif /* LINUX_POSTMOGRIFY_REMOVAL */
+
+/* BRCM OUI: Used in the proprietary(221) IE in all broadcom devices */
+#define BRCM_OUI		"\x00\x10\x18"	/* Broadcom OUI */
+
+/* BRCM info element */
+BWL_PRE_PACKED_STRUCT struct brcm_ie {
+	uint8	id;		/* IE ID, 221, DOT11_MNG_PROPR_ID */
+	uint8	len;		/* IE length */
+	uint8	oui[3];		/* Proprietary OUI, BRCM_OUI */
+	uint8	ver;		/* type/ver of this IE */
+	uint8	assoc;		/* # of assoc STAs */
+	uint8	flags;		/* misc flags */
+	uint8	flags1;		/* misc flags */
+	uint16	amsdu_mtu_pref;	/* preferred A-MSDU MTU */
+} BWL_POST_PACKED_STRUCT;
+typedef	struct brcm_ie brcm_ie_t;
+#define BRCM_IE_LEN		11	/* BRCM IE length */
+#define BRCM_IE_VER		2	/* BRCM IE version */
+#define BRCM_IE_LEGACY_AES_VER	1	/* BRCM IE legacy AES version */
+
+/* brcm_ie flags */
+#define	BRF_LZWDS		0x4	/* lazy wds enabled */
+#define	BRF_BLOCKACK		0x8	/* BlockACK capable */
+
+/* brcm_ie flags1 */
+#define	BRF1_AMSDU		0x1	/* A-MSDU capable */
+#define BRF1_WMEPS		0x4	/* AP is capable of handling WME + PS w/o APSD */
+#define BRF1_PSOFIX		0x8	/* AP has fixed PS mode out-of-order packets */
+#define	BRF1_RX_LARGE_AGG	0x10	/* device can rx large aggregates */
+#define BRF1_RFAWARE_DCS	0x20    /* RFAWARE dynamic channel selection (DCS) */
+#define BRF1_SOFTAP		0x40    /* Configure as Broadcom SOFTAP */
+
+/* Vendor IE structure */
+BWL_PRE_PACKED_STRUCT struct vndr_ie {
+	uchar id;
+	uchar len;
+	uchar oui [3];
+	uchar data [1]; 	/* Variable size data */
+} BWL_POST_PACKED_STRUCT;
+typedef struct vndr_ie vndr_ie_t;
+
+#define VNDR_IE_HDR_LEN		2	/* id + len field */
+#define VNDR_IE_MIN_LEN		3	/* size of the oui field */
+#define VNDR_IE_MAX_LEN		256	/* verdor IE max length */
+
+/* ************* HT definitions. ************* */
+#define MCSSET_LEN	16	/* 16-bits per 8-bit set to give 128-bits bitmap of MCS Index */
+#define MAX_MCS_NUM	(128)	/* max mcs number = 128 */
+
+BWL_PRE_PACKED_STRUCT struct ht_cap_ie {
+	uint16	cap;
+	uint8	params;
+	uint8	supp_mcs[MCSSET_LEN];
+	uint16	ext_htcap;
+	uint32	txbf_cap;
+	uint8	as_cap;
+} BWL_POST_PACKED_STRUCT;
+typedef struct ht_cap_ie ht_cap_ie_t;
+
+/* CAP IE: HT 1.0 spec. simply stole a 802.11 IE, we use our prop. IE until this is resolved */
+/* the capability IE is primarily used to convey this nodes abilities */
+BWL_PRE_PACKED_STRUCT struct ht_prop_cap_ie {
+	uint8	id;		/* IE ID, 221, DOT11_MNG_PROPR_ID */
+	uint8	len;		/* IE length */
+	uint8	oui[3];		/* Proprietary OUI, BRCM_PROP_OUI */
+	uint8	type;           /* type inidicates what follows */
+	ht_cap_ie_t cap_ie;
+} BWL_POST_PACKED_STRUCT;
+typedef struct ht_prop_cap_ie ht_prop_cap_ie_t;
+
+#define HT_PROP_IE_OVERHEAD	4	/* overhead bytes for prop oui ie */
+#define HT_CAP_IE_LEN		26	/* HT capability len (based on .11n d2.0) */
+#define HT_CAP_IE_TYPE		51
+
+#define HT_CAP_LDPC_CODING	0x0001	/* Support for rx of LDPC coded pkts */
+#define HT_CAP_40MHZ		0x0002  /* FALSE:20Mhz, TRUE:20/40MHZ supported */
+#define HT_CAP_MIMO_PS_MASK	0x000C  /* Mimo PS mask */
+#define HT_CAP_MIMO_PS_SHIFT	0x0002	/* Mimo PS shift */
+#define HT_CAP_MIMO_PS_OFF	0x0003	/* Mimo PS, no restriction */
+#define HT_CAP_MIMO_PS_RTS	0x0001	/* Mimo PS, send RTS/CTS around MIMO frames */
+#define HT_CAP_MIMO_PS_ON	0x0000	/* Mimo PS, MIMO disallowed */
+#define HT_CAP_GF		0x0010	/* Greenfield preamble support */
+#define HT_CAP_SHORT_GI_20	0x0020	/* 20MHZ short guard interval support */
+#define HT_CAP_SHORT_GI_40	0x0040	/* 40Mhz short guard interval support */
+#define HT_CAP_TX_STBC		0x0080	/* Tx STBC support */
+#define HT_CAP_RX_STBC_MASK	0x0300	/* Rx STBC mask */
+#define HT_CAP_RX_STBC_SHIFT	8	/* Rx STBC shift */
+#define HT_CAP_DELAYED_BA	0x0400	/* delayed BA support */
+#define HT_CAP_MAX_AMSDU	0x0800	/* Max AMSDU size in bytes , 0=3839, 1=7935 */
+
+#define HT_CAP_DSSS_CCK	0x1000	/* DSSS/CCK supported by the BSS */
+#define HT_CAP_PSMP		0x2000	/* Power Save Multi Poll support */
+#define HT_CAP_40MHZ_INTOLERANT 0x4000	/* 40MHz Intolerant */
+#define HT_CAP_LSIG_TXOP	0x8000	/* L-SIG TXOP protection support */
+
+#define HT_CAP_RX_STBC_NO		0x0	/* no rx STBC support */
+#define HT_CAP_RX_STBC_ONE_STREAM	0x1	/* rx STBC support of 1 spatial stream */
+#define HT_CAP_RX_STBC_TWO_STREAM	0x2	/* rx STBC support of 1-2 spatial streams */
+#define HT_CAP_RX_STBC_THREE_STREAM	0x3	/* rx STBC support of 1-3 spatial streams */
+
+#define VHT_MAX_MPDU		11454	/* max mpdu size for now (bytes) */
+#define VHT_MPDU_MSDU_DELTA	56		/* Difference in spec - vht mpdu, amsdu len */
+/* Max AMSDU len - per spec */
+#define VHT_MAX_AMSDU		(VHT_MAX_MPDU - VHT_MPDU_MSDU_DELTA)
+
+#define HT_MAX_AMSDU		7935	/* max amsdu size (bytes) per the HT spec */
+#define HT_MIN_AMSDU		3835	/* min amsdu size (bytes) per the HT spec */
+
+#define HT_PARAMS_RX_FACTOR_MASK	0x03	/* ampdu rcv factor mask */
+#define HT_PARAMS_DENSITY_MASK		0x1C	/* ampdu density mask */
+#define HT_PARAMS_DENSITY_SHIFT	2	/* ampdu density shift */
+
+/* HT/AMPDU specific define */
+#define AMPDU_MAX_MPDU_DENSITY	7	/* max mpdu density; in 1/8 usec units */
+#define AMPDU_RX_FACTOR_8K	0	/* max rcv ampdu len (8kb) */
+#define AMPDU_RX_FACTOR_16K	1	/* max rcv ampdu len (16kb) */
+#define AMPDU_RX_FACTOR_32K	2	/* max rcv ampdu len (32kb) */
+#define AMPDU_RX_FACTOR_64K	3	/* max rcv ampdu len (64kb) */
+#define AMPDU_RX_FACTOR_BASE	8*1024	/* ampdu factor base for rx len */
+
+#define AMPDU_DELIMITER_LEN	4	/* length of ampdu delimiter */
+#define AMPDU_DELIMITER_LEN_MAX	63	/* max length of ampdu delimiter(enforced in HW) */
+
+#define HT_CAP_EXT_PCO			0x0001
+#define HT_CAP_EXT_PCO_TTIME_MASK	0x0006
+#define HT_CAP_EXT_PCO_TTIME_SHIFT	1
+#define HT_CAP_EXT_MCS_FEEDBACK_MASK	0x0300
+#define HT_CAP_EXT_MCS_FEEDBACK_SHIFT	8
+#define HT_CAP_EXT_HTC			0x0400
+#define HT_CAP_EXT_RD_RESP		0x0800
+
+BWL_PRE_PACKED_STRUCT struct ht_add_ie {
+	uint8	ctl_ch;			/* control channel number */
+	uint8	byte1;			/* ext ch,rec. ch. width, RIFS support */
+	uint16	opmode;			/* operation mode */
+	uint16	misc_bits;		/* misc bits */
+	uint8	basic_mcs[MCSSET_LEN];  /* required MCS set */
+} BWL_POST_PACKED_STRUCT;
+typedef struct ht_add_ie ht_add_ie_t;
+
+/* ADD IE: HT 1.0 spec. simply stole a 802.11 IE, we use our prop. IE until this is resolved */
+/* the additional IE is primarily used to convey the current BSS configuration */
+BWL_PRE_PACKED_STRUCT struct ht_prop_add_ie {
+	uint8	id;		/* IE ID, 221, DOT11_MNG_PROPR_ID */
+	uint8	len;		/* IE length */
+	uint8	oui[3];		/* Proprietary OUI, BRCM_PROP_OUI */
+	uint8	type;		/* indicates what follows */
+	ht_add_ie_t add_ie;
+} BWL_POST_PACKED_STRUCT;
+typedef struct ht_prop_add_ie ht_prop_add_ie_t;
+
+#define HT_ADD_IE_LEN	22
+#define HT_ADD_IE_TYPE	52
+
+/* byte1 defn's */
+#define HT_BW_ANY		0x04	/* set, STA can use 20 or 40MHz */
+#define HT_RIFS_PERMITTED     	0x08	/* RIFS allowed */
+
+/* opmode defn's */
+#define HT_OPMODE_MASK	        0x0003	/* protection mode mask */
+#define HT_OPMODE_SHIFT		0	/* protection mode shift */
+#define HT_OPMODE_PURE		0x0000	/* protection mode PURE */
+#define HT_OPMODE_OPTIONAL	0x0001	/* protection mode optional */
+#define HT_OPMODE_HT20IN40	0x0002	/* protection mode 20MHz HT in 40MHz BSS */
+#define HT_OPMODE_MIXED	0x0003	/* protection mode Mixed Mode */
+#define HT_OPMODE_NONGF	0x0004	/* protection mode non-GF */
+#define DOT11N_TXBURST		0x0008	/* Tx burst limit */
+#define DOT11N_OBSS_NONHT	0x0010	/* OBSS Non-HT STA present */
+
+/* misc_bites defn's */
+#define HT_BASIC_STBC_MCS	0x007f	/* basic STBC MCS */
+#define HT_DUAL_STBC_PROT	0x0080	/* Dual STBC Protection */
+#define HT_SECOND_BCN		0x0100	/* Secondary beacon support */
+#define HT_LSIG_TXOP		0x0200	/* L-SIG TXOP Protection full support */
+#define HT_PCO_ACTIVE		0x0400	/* PCO active */
+#define HT_PCO_PHASE		0x0800	/* PCO phase */
+#define HT_DUALCTS_PROTECTION	0x0080	/* DUAL CTS protection needed */
+
+/* Tx Burst Limits */
+#define DOT11N_2G_TXBURST_LIMIT	6160	/* 2G band Tx burst limit per 802.11n Draft 1.10 (usec) */
+#define DOT11N_5G_TXBURST_LIMIT	3080	/* 5G band Tx burst limit per 802.11n Draft 1.10 (usec) */
+
+/* Macros for opmode */
+#define GET_HT_OPMODE(add_ie)		((ltoh16_ua(&add_ie->opmode) & HT_OPMODE_MASK) \
+					>> HT_OPMODE_SHIFT)
+#define HT_MIXEDMODE_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & HT_OPMODE_MASK) \
+					== HT_OPMODE_MIXED)	/* mixed mode present */
+#define HT_HT20_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & HT_OPMODE_MASK) \
+					== HT_OPMODE_HT20IN40)	/* 20MHz HT present */
+#define HT_OPTIONAL_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & HT_OPMODE_MASK) \
+					== HT_OPMODE_OPTIONAL)	/* Optional protection present */
+#define HT_USE_PROTECTION(add_ie)	(HT_HT20_PRESENT((add_ie)) || \
+					HT_MIXEDMODE_PRESENT((add_ie))) /* use protection */
+#define HT_NONGF_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & HT_OPMODE_NONGF) \
+					== HT_OPMODE_NONGF)	/* non-GF present */
+#define DOT11N_TXBURST_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & DOT11N_TXBURST) \
+					== DOT11N_TXBURST)	/* Tx Burst present */
+#define DOT11N_OBSS_NONHT_PRESENT(add_ie)	((ltoh16_ua(&add_ie->opmode) & DOT11N_OBSS_NONHT) \
+					== DOT11N_OBSS_NONHT)	/* OBSS Non-HT present */
+
+BWL_PRE_PACKED_STRUCT struct obss_params {
+	uint16	passive_dwell;
+	uint16	active_dwell;
+	uint16	bss_widthscan_interval;
+	uint16	passive_total;
+	uint16	active_total;
+	uint16	chanwidth_transition_dly;
+	uint16	activity_threshold;
+} BWL_POST_PACKED_STRUCT;
+typedef struct obss_params obss_params_t;
+
+BWL_PRE_PACKED_STRUCT struct dot11_obss_ie {
+	uint8	id;
+	uint8	len;
+	obss_params_t obss_params;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_obss_ie dot11_obss_ie_t;
+#define DOT11_OBSS_SCAN_IE_LEN	sizeof(obss_params_t)	/* HT OBSS len (based on 802.11n d3.0) */
+
+/* HT control field */
+#define HT_CTRL_LA_TRQ		0x00000002	/* sounding request */
+#define HT_CTRL_LA_MAI		0x0000003C	/* MCS request or antenna selection indication */
+#define HT_CTRL_LA_MAI_SHIFT	2
+#define HT_CTRL_LA_MAI_MRQ	0x00000004	/* MCS request */
+#define HT_CTRL_LA_MAI_MSI	0x00000038	/* MCS request sequence identifier */
+#define HT_CTRL_LA_MFSI		0x000001C0	/* MFB sequence identifier */
+#define HT_CTRL_LA_MFSI_SHIFT	6
+#define HT_CTRL_LA_MFB_ASELC	0x0000FE00	/* MCS feedback, antenna selection command/data */
+#define HT_CTRL_LA_MFB_ASELC_SH	9
+#define HT_CTRL_LA_ASELC_CMD	0x00000C00	/* ASEL command */
+#define HT_CTRL_LA_ASELC_DATA	0x0000F000	/* ASEL data */
+#define HT_CTRL_CAL_POS		0x00030000	/* Calibration position */
+#define HT_CTRL_CAL_SEQ		0x000C0000	/* Calibration sequence */
+#define HT_CTRL_CSI_STEERING	0x00C00000	/* CSI/Steering */
+#define HT_CTRL_CSI_STEER_SHIFT	22
+#define HT_CTRL_CSI_STEER_NFB	0		/* no fedback required */
+#define HT_CTRL_CSI_STEER_CSI	1		/* CSI, H matrix */
+#define HT_CTRL_CSI_STEER_NCOM	2		/* non-compressed beamforming */
+#define HT_CTRL_CSI_STEER_COM	3		/* compressed beamforming */
+#define HT_CTRL_NDP_ANNOUNCE	0x01000000	/* NDP announcement */
+#define HT_CTRL_AC_CONSTRAINT	0x40000000	/* AC Constraint */
+#define HT_CTRL_RDG_MOREPPDU	0x80000000	/* RDG/More PPDU */
+
+#define HT_OPMODE_OPTIONAL	0x0001	/* protection mode optional */
+#define HT_OPMODE_HT20IN40	0x0002	/* protection mode 20MHz HT in 40MHz BSS */
+#define HT_OPMODE_MIXED	0x0003	/* protection mode Mixed Mode */
+#define HT_OPMODE_NONGF	0x0004	/* protection mode non-GF */
+#define DOT11N_TXBURST		0x0008	/* Tx burst limit */
+#define DOT11N_OBSS_NONHT	0x0010	/* OBSS Non-HT STA present */
+
+/* ************* VHT definitions. ************* */
+
+BWL_PRE_PACKED_STRUCT struct vht_cap_ie {
+	uint32  vht_cap_info;
+	/* supported MCS set - 64 bit field */
+	uint16	rx_mcs_map;
+	uint16  rx_max_rate;
+	uint16  tx_mcs_map;
+	uint16	tx_max_rate;
+} BWL_POST_PACKED_STRUCT;
+typedef struct vht_cap_ie vht_cap_ie_t;
+/* 4B cap_info + 8B supp_mcs */
+#define VHT_CAP_IE_LEN 12
+/* 32bit - cap info */
+#define VHT_CAP_INFO_MAX_MPDU_LEN_MASK			0x00000003
+#define VHT_CAP_INFO_SUPP_CHAN_WIDTH_MASK       0x0000000c
+#define VHT_CAP_INFO_LDPC                       0x00000010
+#define VHT_CAP_INFO_SGI_80MHZ                  0x00000020
+#define VHT_CAP_INFO_SGI_160MHZ                 0x00000040
+#define VHT_CAP_INFO_TX_STBC                    0x00000080
+#define VHT_CAP_INFO_RX_STBC                    0x00000700
+
+#define VHT_CAP_INFO_RX_STBC_MASK               0x00000700
+#define VHT_CAP_INFO_RX_STBC_SHIFT              8
+#define VHT_CAP_INFO_SU_BEAMFMR                 0x00000800
+#define VHT_CAP_INFO_SU_BEAMFMEE                0x00001000
+#define VHT_CAP_INFO_NUM_BMFMR_ANT_MASK         0x0000e000
+#define VHT_CAP_INFO_NUM_BMFMR_ANT_SHIFT        13
+
+#define VHT_CAP_INFO_NUM_SOUNDING_DIM_MASK      0x00070000
+#define VHT_CAP_INFO_NUM_SOUNDING_DIM_SHIFT     16
+#define VHT_CAP_INFO_MU_BEAMFMR                 0x00080000
+#define VHT_CAP_INFO_MU_BEAMFMEE                0x00100000
+#define VHT_CAP_INFO_TXOPPS                     0x00200000
+#define VHT_CAP_INFO_HTCVHT                     0x00400000
+#define VHT_CAP_INFO_AMPDU_MAXLEN_EXP_MASK      0x03800000
+#define VHT_CAP_INFO_AMPDU_MAXLEN_EXP_SHIFT     23
+
+#define VHT_CAP_INFO_LINK_ADAPT_CAP_MASK        0x0c000000
+#define VHT_CAP_INFO_LINK_ADAPT_CAP_SHIFT       26
+
+/* 64-bit Supp MCS. */
+#define VHT_CAP_SUPP_MCS_RX_HIGHEST_RATE_MASK	0x1fff
+#define VHT_CAP_SUPP_MCS_RX_HIGHEST_RATE_SHIFT	0
+
+#define VHT_CAP_SUPP_MCS_TX_HIGHEST_RATE_MASK	0x1fff
+#define VHT_CAP_SUPP_MCS_TX_HIGHEST_RATE_SHIFT	0
+
+#define VHT_CAP_MCS_MAP_0_7						0
+#define VHT_CAP_MCS_MAP_0_8						1
+#define VHT_CAP_MCS_MAP_0_9						2
+#define VHT_CAP_MCS_MAP_NONE					3
+
+#define VHT_CAP_MCS_MAP_NSS_MAX					8
+
+/* VHT Capabilities Supported Channel Width */
+typedef enum vht_cap_chan_width {
+	VHT_CAP_CHAN_WIDTH_20_40  = 0x00,
+	VHT_CAP_CHAN_WIDTH_80	  = 0x04,
+	VHT_CAP_CHAN_WIDTH_160	  = 0x08
+} vht_cap_chan_width_t;
+
+/* VHT Capabilities Supported max MPDU LEN */
+typedef enum vht_cap_max_mpdu_len {
+	VHT_CAP_MPDU_MAX_4K		= 0x00,
+	VHT_CAP_MPDU_MAX_8K		= 0x01,
+	VHT_CAP_MPDU_MAX_11K	= 0x02
+} vht_cap_max_mpdu_len_t;
+
+/* VHT Operation Element */
+BWL_PRE_PACKED_STRUCT struct vht_op_ie {
+	uint8	chan_width;
+	uint8	chan1;
+	uint8	chan2;
+	uint16	supp_mcs;  /*  same def as above in vht cap */
+} BWL_POST_PACKED_STRUCT;
+typedef struct vht_op_ie vht_op_ie_t;
+/* 3B VHT Op info + 2B Basic MCS */
+#define VHT_OP_IE_LEN 5
+
+typedef enum vht_op_chan_width {
+	VHT_OP_CHAN_WIDTH_20_40	= 0,
+	VHT_OP_CHAN_WIDTH_80	= 1,
+	VHT_OP_CHAN_WIDTH_160	= 2,
+	VHT_OP_CHAN_WIDTH_80_80	= 3
+} vht_op_chan_width_t;
+
+/* Def for rx & tx basic mcs maps - ea ss num has 2 bits of info */
+#define VHT_MCS_MAP_GET_SS_IDX(nss) (((nss)-1)*2)
+#define VHT_MCS_MAP_GET_MCS_PER_SS(nss, mcsMap) \
+	(((mcsMap) >> VHT_MCS_MAP_GET_SS_IDX(nss)) & 0x3)
+#define VHT_MCS_MAP_SET_MCS_PER_SS(nss, numMcs, mcsMap) \
+	((mcsMap) |= (((numMcs) & 0x3) << VHT_MCS_MAP_GET_SS_IDX(nss)))
+
+/* ************* WPA definitions. ************* */
+#define WPA_OUI			"\x00\x50\xF2"	/* WPA OUI */
+#define WPA_OUI_LEN		3		/* WPA OUI length */
+#define WPA_OUI_TYPE		1
+#define WPA_VERSION		1		/* WPA version */
+#define WPA2_OUI		"\x00\x0F\xAC"	/* WPA2 OUI */
+#define WPA2_OUI_LEN		3		/* WPA2 OUI length */
+#define WPA2_VERSION		1		/* WPA2 version */
+#define WPA2_VERSION_LEN	2		/* WAP2 version length */
+
+/* ************* WPS definitions. ************* */
+#define WPS_OUI			"\x00\x50\xF2"	/* WPS OUI */
+#define WPS_OUI_LEN		3		/* WPS OUI length */
+#define WPS_OUI_TYPE		4
+
+/* ************* WFA definitions. ************* */
+#if defined(MACOSX)
+#define MAC_OUI			"\x00\x17\xF2"	/* MACOSX OUI */
+#define MAC_OUI_TYPE_P2P	5
+#endif /* MACOSX */
+
+#if defined(MACOSX) && !defined(WLP2P_NEW_WFA_OUI)
+#define WFA_OUI			WPS_OUI		/* WFA OUI */
+#else
+#ifdef P2P_IE_OVRD
+#define WFA_OUI			MAC_OUI
+#else
+#define WFA_OUI			"\x50\x6F\x9A"	/* WFA OUI */
+#endif /* P2P_IE_OVRD */
+#endif /* MACOSX && !WLP2P_NEW_WFA_OUI */
+#define WFA_OUI_LEN		3		/* WFA OUI length */
+#ifdef P2P_IE_OVRD
+#define WFA_OUI_TYPE_P2P	MAC_OUI_TYPE_P2P
+#else
+#define WFA_OUI_TYPE_P2P	9
+#endif
+
+#define WFA_OUI_TYPE_TPC	8
+
+/* RSN authenticated key managment suite */
+#define RSN_AKM_NONE		0	/* None (IBSS) */
+#define RSN_AKM_UNSPECIFIED	1	/* Over 802.1x */
+#define RSN_AKM_PSK		2	/* Pre-shared Key */
+#define RSN_AKM_FBT_1X		3	/* Fast Bss transition using 802.1X */
+#define RSN_AKM_FBT_PSK		4	/* Fast Bss transition using Pre-shared Key */
+#define RSN_AKM_MFP_1X		5	/* SHA256 key derivation, using 802.1X */
+#define RSN_AKM_MFP_PSK		6	/* SHA256 key derivation, using Pre-shared Key */
+#define RSN_AKM_TPK			7	/* TPK(TDLS Peer Key) handshake */
+
+/* Key related defines */
+#define DOT11_MAX_DEFAULT_KEYS	4	/* number of default keys */
+#define DOT11_MAX_KEY_SIZE	32	/* max size of any key */
+#define DOT11_MAX_IV_SIZE	16	/* max size of any IV */
+#define DOT11_EXT_IV_FLAG	(1<<5)	/* flag to indicate IV is > 4 bytes */
+#define DOT11_WPA_KEY_RSC_LEN   8       /* WPA RSC key len */
+
+#define WEP1_KEY_SIZE		5	/* max size of any WEP key */
+#define WEP1_KEY_HEX_SIZE	10	/* size of WEP key in hex. */
+#define WEP128_KEY_SIZE		13	/* max size of any WEP key */
+#define WEP128_KEY_HEX_SIZE	26	/* size of WEP key in hex. */
+#define TKIP_MIC_SIZE		8	/* size of TKIP MIC */
+#define TKIP_EOM_SIZE		7	/* max size of TKIP EOM */
+#define TKIP_EOM_FLAG		0x5a	/* TKIP EOM flag byte */
+#define TKIP_KEY_SIZE		32	/* size of any TKIP key */
+#define TKIP_MIC_AUTH_TX	16	/* offset to Authenticator MIC TX key */
+#define TKIP_MIC_AUTH_RX	24	/* offset to Authenticator MIC RX key */
+#define TKIP_MIC_SUP_RX		TKIP_MIC_AUTH_TX	/* offset to Supplicant MIC RX key */
+#define TKIP_MIC_SUP_TX		TKIP_MIC_AUTH_RX	/* offset to Supplicant MIC TX key */
+#define AES_KEY_SIZE		16	/* size of AES key */
+#define AES_MIC_SIZE		8	/* size of AES MIC */
+#define BIP_KEY_SIZE		16	/* size of BIP key */
+
+/* WCN */
+#define WCN_OUI			"\x00\x50\xf2"	/* WCN OUI */
+#define WCN_TYPE		4	/* WCN type */
+
+
+/* 802.11r protocol definitions */
+
+/* Mobility Domain IE */
+BWL_PRE_PACKED_STRUCT struct dot11_mdid_ie {
+	uint8 id;
+	uint8 len;
+	uint16 mdid;		/* Mobility Domain Id */
+	uint8 cap;
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_mdid_ie dot11_mdid_ie_t;
+
+#define FBT_MDID_CAP_OVERDS	0x01	/* Fast Bss transition over the DS support */
+#define FBT_MDID_CAP_RRP	0x02	/* Resource request protocol support */
+
+/* Fast Bss Transition IE */
+BWL_PRE_PACKED_STRUCT struct dot11_ft_ie {
+	uint8 id;
+	uint8 len;
+	uint16 mic_control;		/* Mic Control */
+	uint8 mic[16];
+	uint8 anonce[32];
+	uint8 snonce[32];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_ft_ie dot11_ft_ie_t;
+
+#define TIE_TYPE_RESERVED		0
+#define TIE_TYPE_REASSOC_DEADLINE	1
+#define TIE_TYPE_KEY_LIEFTIME		2
+#define TIE_TYPE_ASSOC_COMEBACK		3
+BWL_PRE_PACKED_STRUCT struct dot11_timeout_ie {
+	uint8 id;
+	uint8 len;
+	uint8 type;		/* timeout interval type */
+	uint32 value;		/* timeout interval value */
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_timeout_ie dot11_timeout_ie_t;
+
+/* GTK ie */
+BWL_PRE_PACKED_STRUCT struct dot11_gtk_ie {
+	uint8 id;
+	uint8 len;
+	uint16 key_info;
+	uint8 key_len;
+	uint8 rsc[8];
+	uint8 data[1];
+} BWL_POST_PACKED_STRUCT;
+typedef struct dot11_gtk_ie dot11_gtk_ie_t;
+
+#define BSSID_INVALID           "\x00\x00\x00\x00\x00\x00"
+#define BSSID_BROADCAST         "\xFF\xFF\xFF\xFF\xFF\xFF"
+
+
+/* ************* WMM Parameter definitions. ************* */
+#define WMM_OUI			"\x00\x50\xF2"	/* WNN OUI */
+#define WMM_OUI_LEN		3		/* WMM OUI length */
+#define WMM_OUI_TYPE	2		/* WMM OUT type */
+#define WMM_VERSION		1
+#define WMM_VERSION_LEN	1
+
+/* WMM OUI subtype */
+#define WMM_OUI_SUBTYPE_PARAMETER	1
+#define WMM_PARAMETER_IE_LEN		24
+
+/* Link Identifier Element */
+BWL_PRE_PACKED_STRUCT struct link_id_ie {
+	uint8 id;
+	uint8 len;
+	struct ether_addr	bssid;
+	struct ether_addr	tdls_init_mac;
+	struct ether_addr	tdls_resp_mac;
+} BWL_POST_PACKED_STRUCT;
+typedef struct link_id_ie link_id_ie_t;
+#define TDLS_LINK_ID_IE_LEN		18
+
+/* Link Wakeup Schedule Element */
+BWL_PRE_PACKED_STRUCT struct wakeup_sch_ie {
+	uint8 id;
+	uint8 len;
+	uint32 offset;			/* in ms between TSF0 and start of 1st Awake Window */
+	uint32 interval;		/* in ms bwtween the start of 2 Awake Windows */
+	uint32 awake_win_slots;	/* in backof slots, duration of Awake Window */
+	uint32 max_wake_win;	/* in ms, max duration of Awake Window */
+	uint16 idle_cnt;		/* number of consecutive Awake Windows */
+} BWL_POST_PACKED_STRUCT;
+typedef struct wakeup_sch_ie wakeup_sch_ie_t;
+#define TDLS_WAKEUP_SCH_IE_LEN		18
+
+/* Channel Switch Timing Element */
+BWL_PRE_PACKED_STRUCT struct channel_switch_timing_ie {
+	uint8 id;
+	uint8 len;
+	uint16 switch_time;		/* in ms, time to switch channels */
+	uint16 switch_timeout;	/* in ms */
+} BWL_POST_PACKED_STRUCT;
+typedef struct channel_switch_timing_ie channel_switch_timing_ie_t;
+#define TDLS_CHANNEL_SWITCH_TIMING_IE_LEN		4
+
+/* PTI Control Element */
+BWL_PRE_PACKED_STRUCT struct pti_control_ie {
+	uint8 id;
+	uint8 len;
+	uint8 tid;
+	uint16 seq_control;
+} BWL_POST_PACKED_STRUCT;
+typedef struct pti_control_ie pti_control_ie_t;
+#define TDLS_PTI_CONTROL_IE_LEN		3
+
+/* PU Buffer Status Element */
+BWL_PRE_PACKED_STRUCT struct pu_buffer_status_ie {
+	uint8 id;
+	uint8 len;
+	uint8 status;
+} BWL_POST_PACKED_STRUCT;
+typedef struct pu_buffer_status_ie pu_buffer_status_ie_t;
+#define TDLS_PU_BUFFER_STATUS_IE_LEN	1
+#define TDLS_PU_BUFFER_STATUS_AC_BK		1
+#define TDLS_PU_BUFFER_STATUS_AC_BE		2
+#define TDLS_PU_BUFFER_STATUS_AC_VI		4
+#define TDLS_PU_BUFFER_STATUS_AC_VO		8
+
+/* This marks the end of a packed structure section. */
+#include <packed_section_end.h>
+
+#endif /* _802_11_H_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/proto/802.1d.h b/drivers/bcmdrivers/gmac/src/include/proto/802.1d.h
new file mode 100755
index 0000000..3749214
