--- /dev/null
+++ b/arch/arm/plat-iproc/include/mach/bridge-regs.h
@@ -0,0 +1,68 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+/*
+ * Mbus-L to Mbus Bridge Registers
+ *
+ */
+
+#ifndef __ASM_ARCH_BRIDGE_REGS_H
+#define __ASM_ARCH_BRIDGE_REGS_H
+
+#include <mach/iproc.h>
+
+#define CPU_CONFIG		(BRIDGE_VIRT_BASE | 0x0000)
+
+#define CPU_CONTROL		(BRIDGE_VIRT_BASE | 0x0104)
+#define  CPU_CTRL_PCIE0_LINK	0x00000001
+#define  CPU_RESET		0x00000002
+#define  CPU_CTRL_PCIE1_LINK	0x00000008
+
+#define RSTOUTn_MASK		(BRIDGE_VIRT_BASE | 0x0108)
+#define  SOFT_RESET_OUT_EN	0x00000004
+
+#define SYSTEM_SOFT_RESET	(BRIDGE_VIRT_BASE | 0x010c)
+#define  SOFT_RESET		0x00000001
+
+#define BRIDGE_CAUSE		(BRIDGE_VIRT_BASE | 0x0110)
+#define BRIDGE_MASK		(BRIDGE_VIRT_BASE | 0x0114)
+#define  BRIDGE_INT_TIMER0	0x0002
+#define  BRIDGE_INT_TIMER1	0x0004
+#define  BRIDGE_INT_TIMER1_CLR	(~0x0004)
+
+#define IRQ_VIRT_BASE		(BRIDGE_VIRT_BASE | 0x0200)
+#define IRQ_CAUSE_LOW_OFF	0x0000
+#define IRQ_MASK_LOW_OFF	0x0004
+#define FIQ_MASK_LOW_OFF	0x0008
+#define ENDPOINT_MASK_LOW_OFF	0x000c
+#define IRQ_CAUSE_HIGH_OFF	0x0010
+#define IRQ_MASK_HIGH_OFF	0x0014
+#define FIQ_MASK_HIGH_OFF	0x0018
+#define ENDPOINT_MASK_HIGH_OFF	0x001c
+#define PCIE_INTERRUPT_MASK_OFF	0x0020
+
+#define IRQ_MASK_LOW		(IRQ_VIRT_BASE + IRQ_MASK_LOW_OFF)
+#define FIQ_MASK_LOW		(IRQ_VIRT_BASE + FIQ_MASK_LOW_OFF)
+#define ENDPOINT_MASK_LOW	(IRQ_VIRT_BASE + ENDPOINT_MASK_LOW_OFF)
+#define IRQ_MASK_HIGH		(IRQ_VIRT_BASE + IRQ_MASK_HIGH_OFF)
+#define FIQ_MASK_HIGH		(IRQ_VIRT_BASE + FIQ_MASK_HIGH_OFF)
+#define ENDPOINT_MASK_HIGH	(IRQ_VIRT_BASE + ENDPOINT_MASK_HIGH_OFF)
+#define PCIE_INTERRUPT_MASK	(IRQ_VIRT_BASE + PCIE_INTERRUPT_MASK_OFF)
+
+#define POWER_MANAGEMENT	(BRIDGE_VIRT_BASE | 0x011c)
+
+#define TIMER_VIRT_BASE		(BRIDGE_VIRT_BASE | 0x0300)
+
+#endif
diff --git a/arch/arm/plat-iproc/include/mach/clkdev.h b/arch/arm/plat-iproc/include/mach/clkdev.h
new file mode 100644
index 0000000..d77f186
