--- /dev/null
+++ b/arch/arm/net/bpf_jit_32.h
@@ -0,0 +1,190 @@
+/*
+ * Just-In-Time compiler for BPF filters on 32bit ARM
+ *
+ * Copyright (c) 2011 Mircea Gherzan <mgherzan@gmail.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; version 2 of the License.
+ */
+
+#ifndef PFILTER_OPCODES_ARM_H
+#define PFILTER_OPCODES_ARM_H
+
+#define ARM_R0	0
+#define ARM_R1	1
+#define ARM_R2	2
+#define ARM_R3	3
+#define ARM_R4	4
+#define ARM_R5	5
+#define ARM_R6	6
+#define ARM_R7	7
+#define ARM_R8	8
+#define ARM_R9	9
+#define ARM_R10	10
+#define ARM_FP	11
+#define ARM_IP	12
+#define ARM_SP	13
+#define ARM_LR	14
+#define ARM_PC	15
+
+#define ARM_COND_EQ		0x0
+#define ARM_COND_NE		0x1
+#define ARM_COND_CS		0x2
+#define ARM_COND_HS		ARM_COND_CS
+#define ARM_COND_CC		0x3
+#define ARM_COND_LO		ARM_COND_CC
+#define ARM_COND_MI		0x4
+#define ARM_COND_PL		0x5
+#define ARM_COND_VS		0x6
+#define ARM_COND_VC		0x7
+#define ARM_COND_HI		0x8
+#define ARM_COND_LS		0x9
+#define ARM_COND_GE		0xa
+#define ARM_COND_LT		0xb
+#define ARM_COND_GT		0xc
+#define ARM_COND_LE		0xd
+#define ARM_COND_AL		0xe
+
+/* register shift types */
+#define SRTYPE_LSL		0
+#define SRTYPE_LSR		1
+#define SRTYPE_ASR		2
+#define SRTYPE_ROR		3
+
+#define ARM_INST_ADD_R		0x00800000
+#define ARM_INST_ADD_I		0x02800000
+
+#define ARM_INST_AND_R		0x00000000
+#define ARM_INST_AND_I		0x02000000
+
+#define ARM_INST_BIC_R		0x01c00000
+#define ARM_INST_BIC_I		0x03c00000
+
+#define ARM_INST_B		0x0a000000
+#define ARM_INST_BX		0x012FFF10
+#define ARM_INST_BLX_R		0x012fff30
+
+#define ARM_INST_CMP_R		0x01500000
+#define ARM_INST_CMP_I		0x03500000
+
+#define ARM_INST_LDRB_I		0x05d00000
+#define ARM_INST_LDRB_R		0x07d00000
+#define ARM_INST_LDRH_I		0x01d000b0
+#define ARM_INST_LDR_I		0x05900000
+
+#define ARM_INST_LDM		0x08900000
+
+#define ARM_INST_LSL_I		0x01a00000
+#define ARM_INST_LSL_R		0x01a00010
+
+#define ARM_INST_LSR_I		0x01a00020
+#define ARM_INST_LSR_R		0x01a00030
+
+#define ARM_INST_MOV_R		0x01a00000
+#define ARM_INST_MOV_I		0x03a00000
+#define ARM_INST_MOVW		0x03000000
+#define ARM_INST_MOVT		0x03400000
+
+#define ARM_INST_MUL		0x00000090
+
+#define ARM_INST_POP		0x08bd0000
+#define ARM_INST_PUSH		0x092d0000
+
+#define ARM_INST_ORR_R		0x01800000
+#define ARM_INST_ORR_I		0x03800000
+
+#define ARM_INST_REV		0x06bf0f30
+#define ARM_INST_REV16		0x06bf0fb0
+
+#define ARM_INST_RSB_I		0x02600000
+
+#define ARM_INST_SUB_R		0x00400000
+#define ARM_INST_SUB_I		0x02400000
+
+#define ARM_INST_STR_I		0x05800000
+
+#define ARM_INST_TST_R		0x01100000
+#define ARM_INST_TST_I		0x03100000
+
+#define ARM_INST_UDIV		0x0730f010
+
+#define ARM_INST_UMULL		0x00800090
+
+/* register */
+#define _AL3_R(op, rd, rn, rm)	((op ## _R) | (rd) << 12 | (rn) << 16 | (rm))
+/* immediate */
+#define _AL3_I(op, rd, rn, imm)	((op ## _I) | (rd) << 12 | (rn) << 16 | (imm))
+
+#define ARM_ADD_R(rd, rn, rm)	_AL3_R(ARM_INST_ADD, rd, rn, rm)
+#define ARM_ADD_I(rd, rn, imm)	_AL3_I(ARM_INST_ADD, rd, rn, imm)
+
+#define ARM_AND_R(rd, rn, rm)	_AL3_R(ARM_INST_AND, rd, rn, rm)
+#define ARM_AND_I(rd, rn, imm)	_AL3_I(ARM_INST_AND, rd, rn, imm)
+
+#define ARM_BIC_R(rd, rn, rm)	_AL3_R(ARM_INST_BIC, rd, rn, rm)
+#define ARM_BIC_I(rd, rn, imm)	_AL3_I(ARM_INST_BIC, rd, rn, imm)
+
+#define ARM_B(imm24)		(ARM_INST_B | ((imm24) & 0xffffff))
+#define ARM_BX(rm)		(ARM_INST_BX | (rm))
+#define ARM_BLX_R(rm)		(ARM_INST_BLX_R | (rm))
+
+#define ARM_CMP_R(rn, rm)	_AL3_R(ARM_INST_CMP, 0, rn, rm)
+#define ARM_CMP_I(rn, imm)	_AL3_I(ARM_INST_CMP, 0, rn, imm)
+
+#define ARM_LDR_I(rt, rn, off)	(ARM_INST_LDR_I | (rt) << 12 | (rn) << 16 \
+				 | (off))
+#define ARM_LDRB_I(rt, rn, off)	(ARM_INST_LDRB_I | (rt) << 12 | (rn) << 16 \
+				 | (off))
+#define ARM_LDRB_R(rt, rn, rm)	(ARM_INST_LDRB_R | (rt) << 12 | (rn) << 16 \
+				 | (rm))
+#define ARM_LDRH_I(rt, rn, off)	(ARM_INST_LDRH_I | (rt) << 12 | (rn) << 16 \
+				 | (((off) & 0xf0) << 4) | ((off) & 0xf))
+
+#define ARM_LDM(rn, regs)	(ARM_INST_LDM | (rn) << 16 | (regs))
+
+#define ARM_LSL_R(rd, rn, rm)	(_AL3_R(ARM_INST_LSL, rd, 0, rn) | (rm) << 8)
+#define ARM_LSL_I(rd, rn, imm)	(_AL3_I(ARM_INST_LSL, rd, 0, rn) | (imm) << 7)
+
+#define ARM_LSR_R(rd, rn, rm)	(_AL3_R(ARM_INST_LSR, rd, 0, rn) | (rm) << 8)
+#define ARM_LSR_I(rd, rn, imm)	(_AL3_I(ARM_INST_LSR, rd, 0, rn) | (imm) << 7)
+
+#define ARM_MOV_R(rd, rm)	_AL3_R(ARM_INST_MOV, rd, 0, rm)
+#define ARM_MOV_I(rd, imm)	_AL3_I(ARM_INST_MOV, rd, 0, imm)
+
+#define ARM_MOVW(rd, imm)	\
+	(ARM_INST_MOVW | ((imm) >> 12) << 16 | (rd) << 12 | ((imm) & 0x0fff))
+
+#define ARM_MOVT(rd, imm)	\
+	(ARM_INST_MOVT | ((imm) >> 12) << 16 | (rd) << 12 | ((imm) & 0x0fff))
+
+#define ARM_MUL(rd, rm, rn)	(ARM_INST_MUL | (rd) << 16 | (rm) << 8 | (rn))
+
+#define ARM_POP(regs)		(ARM_INST_POP | (regs))
+#define ARM_PUSH(regs)		(ARM_INST_PUSH | (regs))
+
+#define ARM_ORR_R(rd, rn, rm)	_AL3_R(ARM_INST_ORR, rd, rn, rm)
+#define ARM_ORR_I(rd, rn, imm)	_AL3_I(ARM_INST_ORR, rd, rn, imm)
+#define ARM_ORR_S(rd, rn, rm, type, rs)	\
+	(ARM_ORR_R(rd, rn, rm) | (type) << 5 | (rs) << 7)
+
+#define ARM_REV(rd, rm)		(ARM_INST_REV | (rd) << 12 | (rm))
+#define ARM_REV16(rd, rm)	(ARM_INST_REV16 | (rd) << 12 | (rm))
+
+#define ARM_RSB_I(rd, rn, imm)	_AL3_I(ARM_INST_RSB, rd, rn, imm)
+
+#define ARM_SUB_R(rd, rn, rm)	_AL3_R(ARM_INST_SUB, rd, rn, rm)
+#define ARM_SUB_I(rd, rn, imm)	_AL3_I(ARM_INST_SUB, rd, rn, imm)
+
+#define ARM_STR_I(rt, rn, off)	(ARM_INST_STR_I | (rt) << 12 | (rn) << 16 \
+				 | (off))
+
+#define ARM_TST_R(rn, rm)	_AL3_R(ARM_INST_TST, 0, rn, rm)
+#define ARM_TST_I(rn, imm)	_AL3_I(ARM_INST_TST, 0, rn, imm)
+
+#define ARM_UDIV(rd, rn, rm)	(ARM_INST_UDIV | (rd) << 16 | (rn) | (rm) << 8)
+
+#define ARM_UMULL(rd_lo, rd_hi, rn, rm)	(ARM_INST_UMULL | (rd_hi) << 16 \
+					 | (rd_lo) << 12 | (rm) << 8 | rn)
+
+#endif /* PFILTER_OPCODES_ARM_H */
diff --git a/arch/arm/plat-iproc/Kconfig b/arch/arm/plat-iproc/Kconfig
new file mode 100644
index 0000000..5b8675f
