--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/shared/siutils_priv.h
@@ -0,0 +1,259 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Include file private to the SOC Interconnect support files.
+ *
+ * $Id: siutils_priv.h 302333 2011-12-11 01:47:49Z $
+ */
+
+#ifndef	_siutils_priv_h_
+#define	_siutils_priv_h_
+
+#ifdef BCMDBG_ERR
+#define	SI_ERROR(args)	printf args
+#else
+#define	SI_ERROR(args)
+#endif	/* BCMDBG_ERR */
+
+#ifdef BCMDBG
+#define	SI_MSG(args)	printf args
+#else
+#define	SI_MSG(args)
+#endif	/* BCMDBG */
+
+#ifdef BCMDBG_SI
+#define	SI_VMSG(args)	printf args
+#else
+#define	SI_VMSG(args)
+#endif
+
+#define	IS_SIM(chippkg)	((chippkg == HDLSIM_PKG_ID) || (chippkg == HWSIM_PKG_ID))
+
+
+typedef uint32 (*si_intrsoff_t)(void *intr_arg);
+typedef void (*si_intrsrestore_t)(void *intr_arg, uint32 arg);
+typedef bool (*si_intrsenabled_t)(void *intr_arg);
+
+typedef struct gpioh_item {
+	void			*arg;
+	bool			level;
+	gpio_handler_t		handler;
+	uint32			event;
+	struct gpioh_item	*next;
+} gpioh_item_t;
+
+/* misc si info needed by some of the routines */
+typedef struct si_info {
+	struct si_pub pub;		/* back plane public state (must be first field) */
+
+	void	*osh;			/* osl os handle */
+	void	*sdh;			/* bcmsdh handle */
+
+	uint	dev_coreid;		/* the core provides driver functions */
+	void	*intr_arg;		/* interrupt callback function arg */
+	si_intrsoff_t intrsoff_fn;	/* turns chip interrupts off */
+	si_intrsrestore_t intrsrestore_fn; /* restore chip interrupts */
+	si_intrsenabled_t intrsenabled_fn; /* check if interrupts are enabled */
+
+	void *pch;			/* PCI/E core handle */
+
+	gpioh_item_t *gpioh_head; 	/* GPIO event handlers list */
+
+	bool	memseg;			/* flag to toggle MEM_SEG register */
+
+	char *vars;
+	uint varsz;
+
+	void	*curmap;		/* current regs va */
+	void	*regs[SI_MAXCORES];	/* other regs va */
+
+	uint	curidx;			/* current core index */
+	uint	numcores;		/* # discovered cores */
+	uint	coreid[SI_MAXCORES];	/* id of each core */
+	uint32	coresba[SI_MAXCORES];	/* backplane address of each core */
+	void	*regs2[SI_MAXCORES];	/* va of each core second register set (usbh20) */
+	uint32	coresba2[SI_MAXCORES];	/* address of each core second register set (usbh20) */
+	uint32	coresba_size[SI_MAXCORES]; /* backplane address space size */
+	uint32	coresba2_size[SI_MAXCORES]; /* second address space size */
+
+	void	*curwrap;		/* current wrapper va */
+	void	*wrappers[SI_MAXCORES];	/* other cores wrapper va */
+	uint32	wrapba[SI_MAXCORES];	/* address of controlling wrapper */
+
+	uint32	cia[SI_MAXCORES];	/* erom cia entry for each core */
+	uint32	cib[SI_MAXCORES];	/* erom cia entry for each core */
+	uint32	oob_router;		/* oob router registers for axi */
+} si_info_t;
+
+#define	SI_INFO(sih)	(si_info_t *)(uintptr)sih
+
+#define	GOODCOREADDR(x, b) (((x) >= (b)) && ((x) < ((b) + SI_MAXCORES * SI_CORE_SIZE)) && \
+		ISALIGNED((x), SI_CORE_SIZE))
+#define	GOODREGS(regs)	((regs) != NULL && ISALIGNED((uintptr)(regs), SI_CORE_SIZE))
+#define BADCOREADDR	0
+#define	GOODIDX(idx)	(((uint)idx) < SI_MAXCORES)
+#define	NOREV		-1		/* Invalid rev */
+
+#define PCI(si)		((BUSTYPE((si)->pub.bustype) == PCI_BUS) &&	\
+			 ((si)->pub.buscoretype == PCI_CORE_ID))
+
+#define PCIE_GEN1(si)	((BUSTYPE((si)->pub.bustype) == PCI_BUS) &&	\
+			 ((si)->pub.buscoretype == PCIE_CORE_ID))
+
+#define PCIE_GEN2(si)	((BUSTYPE((si)->pub.bustype) == PCI_BUS) &&	\
+			 ((si)->pub.buscoretype == PCIE2_CORE_ID))
+
+#define PCIE(si)	(PCIE_GEN1(si) || PCIE_GEN2(si))
+
+#define PCMCIA(si)	((BUSTYPE((si)->pub.bustype) == PCMCIA_BUS) && ((si)->memseg == TRUE))
+
+/* Newer chips can access PCI/PCIE and CC core without requiring to change
+ * PCI BAR0 WIN
+ */
+#define SI_FAST(si) (PCIE(si) || (PCI(si) && ((si)->pub.buscorerev >= 13)))
+
+#define PCIEREGS(si) (((char *)((si)->curmap) + PCI_16KB0_PCIREGS_OFFSET))
+#define CCREGS_FAST(si) (((char *)((si)->curmap) + PCI_16KB0_CCREGS_OFFSET))
+
+/*
+ * Macros to disable/restore function core(D11, ENET, ILINE20, etc) interrupts before/
+ * after core switching to avoid invalid register accesss inside ISR.
+ */
+#define INTR_OFF(si, intr_val) \
+	if ((si)->intrsoff_fn && (si)->coreid[(si)->curidx] == (si)->dev_coreid) {	\
+		intr_val = (*(si)->intrsoff_fn)((si)->intr_arg); }
+#define INTR_RESTORE(si, intr_val) \
+	if ((si)->intrsrestore_fn && (si)->coreid[(si)->curidx] == (si)->dev_coreid) {	\
+		(*(si)->intrsrestore_fn)((si)->intr_arg, intr_val); }
+
+/* dynamic clock control defines */
+#define	LPOMINFREQ		25000		/* low power oscillator min */
+#define	LPOMAXFREQ		43000		/* low power oscillator max */
+#define	XTALMINFREQ		19800000	/* 20 MHz - 1% */
+#define	XTALMAXFREQ		20200000	/* 20 MHz + 1% */
+#define	PCIMINFREQ		25000000	/* 25 MHz */
+#define	PCIMAXFREQ		34000000	/* 33 MHz + fudge */
+
+#define	ILP_DIV_5MHZ		0		/* ILP = 5 MHz */
+#define	ILP_DIV_1MHZ		4		/* ILP = 1 MHz */
+
+#define PCI_FORCEHT(si)	\
+	(((PCIE_GEN1(si)) && (si->pub.chip == BCM4311_CHIP_ID) && ((si->pub.chiprev <= 1))) || \
+	((PCI(si) || PCIE_GEN1(si)) && (si->pub.chip == BCM4321_CHIP_ID)) || \
+	(PCIE_GEN1(si) && (si->pub.chip == BCM4716_CHIP_ID)) || \
+	(PCIE_GEN1(si) && (si->pub.chip == BCM4748_CHIP_ID)))
+
+/* GPIO Based LED powersave defines */
+#define DEFAULT_GPIO_ONTIME	10		/* Default: 10% on */
+#define DEFAULT_GPIO_OFFTIME	90		/* Default: 10% on */
+
+#ifndef DEFAULT_GPIOTIMERVAL
+#define DEFAULT_GPIOTIMERVAL  ((DEFAULT_GPIO_ONTIME << GPIO_ONTIME_SHIFT) | DEFAULT_GPIO_OFFTIME)
+#endif
+
+#define sb_scan(a, b, c) do {} while (0)
+#define sb_coreid(a) (0)
+#define sb_intflag(a) (0)
+#define sb_flag(a) (0)
+#define sb_setint(a, b) do {} while (0)
+#define sb_corevendor(a) (0)
+#define sb_corerev(a) (0)
+#define sb_corereg(a, b, c, d, e) (0)
+#define sb_iscoreup(a) (false)
+#define sb_setcoreidx(a, b) (0)
+#define sb_core_cflags(a, b, c) (0)
+#define sb_core_cflags_wo(a, b, c) do {} while (0)
+#define sb_core_sflags(a, b, c) (0)
+#define sb_commit(a) do {} while (0)
+#define sb_base(a) (0)
+#define sb_size(a) (0)
+#define sb_core_reset(a, b, c) do {} while (0)
+#define sb_core_disable(a, b) do {} while (0)
+#define sb_addrspace(a, b)  (0)
+#define sb_addrspacesize(a, b) (0)
+#define sb_numaddrspaces(a) (0)
+#define sb_set_initiator_to(a, b, c) (0)
+#define sb_taclear(a, b) (false)
+#define sb_view(a, b) do {} while (0)
+#define sb_viewall(a, b) do {} while (0)
+#define sb_dump(a, b) do {} while (0)
+#define sb_dumpregs(a, b) do {} while (0)
+
+/* Wake-on-wireless-LAN (WOWL) */
+extern bool sb_pci_pmecap(si_t *sih);
+struct osl_info;
+extern bool sb_pci_fastpmecap(struct osl_info *osh);
+extern bool sb_pci_pmeclr(si_t *sih);
+extern void sb_pci_pmeen(si_t *sih);
+extern uint sb_pcie_readreg(void *sih, uint addrtype, uint offset);
+
+/* AMBA Interconnect exported externs */
+extern si_t *ai_attach(uint pcidev, osl_t *osh, void *regs, uint bustype,
+                       void *sdh, char **vars, uint *varsz);
+extern si_t *ai_kattach(osl_t *osh);
+extern void ai_scan(si_t *sih, void *regs, uint devid);
+
+extern uint ai_flag(si_t *sih);
+extern void ai_setint(si_t *sih, int siflag);
+extern uint ai_coreidx(si_t *sih);
+extern uint ai_corevendor(si_t *sih);
+extern uint ai_corerev(si_t *sih);
+extern bool ai_iscoreup(si_t *sih);
+extern void *ai_setcoreidx(si_t *sih, uint coreidx);
+extern uint32 ai_core_cflags(si_t *sih, uint32 mask, uint32 val);
+extern void ai_core_cflags_wo(si_t *sih, uint32 mask, uint32 val);
+extern uint32 ai_core_sflags(si_t *sih, uint32 mask, uint32 val);
+extern uint ai_corereg(si_t *sih, uint coreidx, uint regoff, uint mask, uint val);
+extern void ai_core_reset(si_t *sih, uint32 bits, uint32 resetbits);
+extern void ai_core_disable(si_t *sih, uint32 bits);
+extern int ai_numaddrspaces(si_t *sih);
+extern uint32 ai_addrspace(si_t *sih, uint asidx);
+extern uint32 ai_addrspacesize(si_t *sih, uint asidx);
+extern void ai_coreaddrspaceX(si_t *sih, uint asidx, uint32 *addr, uint32 *size);
+extern uint ai_wrap_reg(si_t *sih, uint32 offset, uint32 mask, uint32 val);
+
+#ifdef BCMDBG
+extern void ai_view(si_t *sih, bool verbose);
+extern void ai_viewall(si_t *sih, bool verbose);
+#endif
+#if defined(BCMDBG)
+extern void ai_dumpregs(si_t *sih, struct bcmstrbuf *b);
+#endif
+
+#ifdef SI_ENUM_BASE_VARIABLE
+extern void si_enum_base_init(si_t *sih, uint bustype);
+#endif /* SI_ENUM_BASE_VARIABLE */
+
+#define ub_scan(a, b, c) do {} while (0)
+#define ub_flag(a) (0)
+#define ub_setint(a, b) do {} while (0)
+#define ub_coreidx(a) (0)
+#define ub_corevendor(a) (0)
+#define ub_corerev(a) (0)
+#define ub_iscoreup(a) (0)
+#define ub_setcoreidx(a, b) (0)
+#define ub_core_cflags(a, b, c) (0)
+#define ub_core_cflags_wo(a, b, c) do {} while (0)
+#define ub_core_sflags(a, b, c) (0)
+#define ub_corereg(a, b, c, d, e) (0)
+#define ub_core_reset(a, b, c) do {} while (0)
+#define ub_core_disable(a, b) do {} while (0)
+#define ub_numaddrspaces(a) (0)
+#define ub_addrspace(a, b)  (0)
+#define ub_addrspacesize(a, b) (0)
+#define ub_view(a, b) do {} while (0)
+#define ub_dumpregs(a, b) do {} while (0)
+
+#endif	/* _siutils_priv_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/shared/wl_config b/drivers/bcmdrivers/gmac/src/shared/wl_config
new file mode 100755
index 0000000..aded587
