--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/linuxver.h
@@ -0,0 +1,662 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Linux-specific abstractions to gain some independence from linux kernel versions.
+ * Pave over some 2.2 versus 2.4 versus 2.6 kernel differences.
+ *
+ * $Id: linuxver.h 312774 2012-02-03 22:20:14Z $
+ */
+
+#ifndef _linuxver_h_
+#define _linuxver_h_
+
+#include <linux/version.h>
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0))
+#include <linux/config.h>
+#else
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 33))
+#include <generated/autoconf.h>
+#else
+#include <linux/autoconf.h>
+#endif
+#endif /* (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0)) */
+#include <linux/module.h>
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 0))
+/* __NO_VERSION__ must be defined for all linkables except one in 2.2 */
+#ifdef __UNDEF_NO_VERSION__
+#undef __NO_VERSION__
+#else
+#define __NO_VERSION__
+#endif
+#endif	/* LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 0) */
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2, 5, 0)
+#define module_param(_name_, _type_, _perm_)	MODULE_PARM(_name_, "i")
+#define module_param_string(_name_, _string_, _size_, _perm_) \
+		MODULE_PARM(_string_, "c" __MODULE_STRING(_size_))
+#endif
+
+/* linux/malloc.h is deprecated, use linux/slab.h instead. */
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 9))
+#include <linux/malloc.h>
+#else
+#include <linux/slab.h>
+#endif
+
+#include <linux/types.h>
+#include <linux/init.h>
+#include <linux/mm.h>
+#include <linux/string.h>
+#include <linux/pci.h>
+#include <linux/interrupt.h>
+#include <linux/netdevice.h>
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 27))
+#include <linux/semaphore.h>
+#else
+#include <asm/semaphore.h>
+#endif /* (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 27)) */
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 28))
+#undef IP_TOS
+#endif /* (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 28)) */
+#include <asm/io.h>
+
+#if (LINUX_VERSION_CODE > KERNEL_VERSION(2, 5, 41))
+#include <linux/workqueue.h>
+#else
+#include <linux/tqueue.h>
+#ifndef work_struct
+#define work_struct tq_struct
+#endif
+#ifndef INIT_WORK
+#define INIT_WORK(_work, _func, _data) INIT_TQUEUE((_work), (_func), (_data))
+#endif
+#ifndef schedule_work
+#define schedule_work(_work) schedule_task((_work))
+#endif
+#ifndef flush_scheduled_work
+#define flush_scheduled_work() flush_scheduled_tasks()
+#endif
+#endif	/* LINUX_VERSION_CODE > KERNEL_VERSION(2, 5, 41) */
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 19)
+#define	MY_INIT_WORK(_work, _func)	INIT_WORK(_work, _func)
+#else
+#define	MY_INIT_WORK(_work, _func)	INIT_WORK(_work, _func, _work)
+typedef void (*work_func_t)(void *work);
+#endif	/* >= 2.6.20 */
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0))
+/* Some distributions have their own 2.6.x compatibility layers */
+#ifndef IRQ_NONE
+typedef void irqreturn_t;
+#define IRQ_NONE
+#define IRQ_HANDLED
+#define IRQ_RETVAL(x)
+#endif
+#else
+typedef irqreturn_t(*FN_ISR) (int irq, void *dev_id, struct pt_regs *ptregs);
+#endif	/* LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0) */
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 18)
+#define IRQF_SHARED	SA_SHIRQ
+#endif /* < 2.6.18 */
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 17)
+#ifdef	CONFIG_NET_RADIO
+#define	CONFIG_WIRELESS_EXT
+#endif
+#endif	/* < 2.6.17 */
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 5, 67)
+#define MOD_INC_USE_COUNT
+#define MOD_DEC_USE_COUNT
+#endif /* LINUX_VERSION_CODE >= KERNEL_VERSION(2, 5, 67) */
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 32)
+#include <linux/sched.h>
+#endif
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 29)
+#include <net/lib80211.h>
+#endif
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 29)
+#include <linux/ieee80211.h>
+#else
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 14)
+#include <net/ieee80211.h>
+#endif
+#endif /* LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 30) */
+
+#if defined(CONFIG_PCMCIA) || defined(CONFIG_PCMCIA_MODULE)
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 27)
+#include <pcmcia/version.h>
+#endif /* LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 27) */
+
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 36)
+#include <pcmcia/cs_types.h>
+#include <pcmcia/cs.h>
+#endif
+#include <pcmcia/cistpl.h>
+#include <pcmcia/cisreg.h>
+#include <pcmcia/ds.h>
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 5, 69))
+/* In 2.5 (as of 2.5.69 at least) there is a cs_error exported which
+ * does this, but it's not in 2.4 so we do our own for now.
+ */
+static inline void
+cs_error(client_handle_t handle, int func, int ret)
+{
+	error_info_t err = { func, ret };
+	CardServices(ReportError, handle, &err);
+}
+#endif
+
+#if (LINUX_VERSION_CODE > KERNEL_VERSION(2, 6, 16))
+
+typedef	struct pcmcia_device dev_link_t;
+
+#endif
+
+#endif /* CONFIG_PCMCIA */
+
+#ifndef __exit
+#define __exit
+#endif
+#ifndef __devexit
+#define __devexit
+#endif
+#ifndef __devinit
+#define __devinit	__init
+#endif
+#ifndef __devinitdata
+#define __devinitdata
+#endif
+#ifndef __devexit_p
+#define __devexit_p(x)	x
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 0))
+
+#define pci_get_drvdata(dev)		(dev)->sysdata
+#define pci_set_drvdata(dev, value)	(dev)->sysdata = (value)
+
+/*
+ * New-style (2.4.x) PCI/hot-pluggable PCI/CardBus registration
+ */
+
+struct pci_device_id {
+	unsigned int vendor, device;		/* Vendor and device ID or PCI_ANY_ID */
+	unsigned int subvendor, subdevice;	/* Subsystem ID's or PCI_ANY_ID */
+	unsigned int class, class_mask;		/* (class,subclass,prog-if) triplet */
+	unsigned long driver_data;		/* Data private to the driver */
+};
+
+struct pci_driver {
+	struct list_head node;
+	char *name;
+	const struct pci_device_id *id_table;	/* NULL if wants all devices */
+	int (*probe)(struct pci_dev *dev,
+	             const struct pci_device_id *id); /* New device inserted */
+	void (*remove)(struct pci_dev *dev);	/* Device removed (NULL if not a hot-plug
+						 * capable driver)
+						 */
+	void (*suspend)(struct pci_dev *dev);	/* Device suspended */
+	void (*resume)(struct pci_dev *dev);	/* Device woken up */
+};
+
+#define MODULE_DEVICE_TABLE(type, name)
+#define PCI_ANY_ID (~0)
+
+/* compatpci.c */
+#define pci_module_init pci_register_driver
+extern int pci_register_driver(struct pci_driver *drv);
+extern void pci_unregister_driver(struct pci_driver *drv);
+
+#endif /* PCI registration */
+
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 18))
+#define pci_module_init pci_register_driver
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 2, 18))
+#ifdef MODULE
+#define module_init(x) int init_module(void) { return x(); }
+#define module_exit(x) void cleanup_module(void) { x(); }
+#else
+#define module_init(x)	__initcall(x);
+#define module_exit(x)	__exitcall(x);
+#endif
+#endif	/* LINUX_VERSION_CODE < KERNEL_VERSION(2, 2, 18) */
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 31)
+#define WL_USE_NETDEV_OPS
+#else
+#undef WL_USE_NETDEV_OPS
+#endif
+
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 31)) && defined(CONFIG_RFKILL)
+#define WL_CONFIG_RFKILL
+#else
+#undef WL_CONFIG_RFKILL
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 48))
+#define list_for_each(pos, head) \
+	for (pos = (head)->next; pos != (head); pos = pos->next)
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 13))
+#define pci_resource_start(dev, bar)	((dev)->base_address[(bar)])
+#elif (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 44))
+#define pci_resource_start(dev, bar)	((dev)->resource[(bar)].start)
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 23))
+#define pci_enable_device(dev) do { } while (0)
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 14))
+#define net_device device
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 42))
+
+/*
+ * DMA mapping
+ *
+ * See linux/Documentation/DMA-mapping.txt
+ */
+
+#ifndef PCI_DMA_TODEVICE
+#define	PCI_DMA_TODEVICE	1
+#define	PCI_DMA_FROMDEVICE	2
+#endif
+
+typedef u32 dma_addr_t;
+
+/* Pure 2^n version of get_order */
+static inline int get_order(unsigned long size)
+{
+	int order;
+
+	size = (size-1) >> (PAGE_SHIFT-1);
+	order = -1;
+	do {
+		size >>= 1;
+		order++;
+	} while (size);
+	return order;
+}
+
+static inline void *pci_alloc_consistent(struct pci_dev *hwdev, size_t size,
+                                         dma_addr_t *dma_handle)
+{
+	void *ret;
+	int gfp = GFP_ATOMIC | GFP_DMA;
+
+	ret = (void *)__get_free_pages(gfp, get_order(size));
+
+	if (ret != NULL) {
+		memset(ret, 0, size);
+		*dma_handle = virt_to_bus(ret);
+	}
+	return ret;
+}
+static inline void pci_free_consistent(struct pci_dev *hwdev, size_t size,
+                                       void *vaddr, dma_addr_t dma_handle)
+{
+	free_pages((unsigned long)vaddr, get_order(size));
+}
+#ifdef ILSIM
+extern uint pci_map_single(void *dev, void *va, uint size, int direction);
+extern void pci_unmap_single(void *dev, uint pa, uint size, int direction);
+#else
+#define pci_map_single(cookie, address, size, dir)	virt_to_bus(address)
+#define pci_unmap_single(cookie, address, size, dir)
+#endif
+
+#endif /* DMA mapping */
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 3, 43))
+
+#define dev_kfree_skb_any(a)		dev_kfree_skb(a)
+#define netif_down(dev)			do { (dev)->start = 0; } while (0)
+
+/* pcmcia-cs provides its own netdevice compatibility layer */
+#ifndef _COMPAT_NETDEVICE_H
+
+/*
+ * SoftNet
+ *
+ * For pre-softnet kernels we need to tell the upper layer not to
+ * re-enter start_xmit() while we are in there. However softnet
+ * guarantees not to enter while we are in there so there is no need
+ * to do the netif_stop_queue() dance unless the transmit queue really
+ * gets stuck. This should also improve performance according to tests
+ * done by Aman Singla.
+ */
+
+#define dev_kfree_skb_irq(a)	dev_kfree_skb(a)
+#define netif_wake_queue(dev) \
+		do { clear_bit(0, &(dev)->tbusy); mark_bh(NET_BH); } while (0)
+#define netif_stop_queue(dev)	set_bit(0, &(dev)->tbusy)
+
+static inline void netif_start_queue(struct net_device *dev)
+{
+	dev->tbusy = 0;
+	dev->interrupt = 0;
+	dev->start = 1;
+}
+
+#define netif_queue_stopped(dev)	(dev)->tbusy
+#define netif_running(dev)		(dev)->start
+
+#endif /* _COMPAT_NETDEVICE_H */
+
+#define netif_device_attach(dev)	netif_start_queue(dev)
+#define netif_device_detach(dev)	netif_stop_queue(dev)
+
+/* 2.4.x renamed bottom halves to tasklets */
+#define tasklet_struct				tq_struct
+static inline void tasklet_schedule(struct tasklet_struct *tasklet)
+{
+	queue_task(tasklet, &tq_immediate);
+	mark_bh(IMMEDIATE_BH);
+}
+
+static inline void tasklet_init(struct tasklet_struct *tasklet,
+                                void (*func)(unsigned long),
+                                unsigned long data)
+{
+	tasklet->next = NULL;
+	tasklet->sync = 0;
+	tasklet->routine = (void (*)(void *))func;
+	tasklet->data = (void *)data;
+}
+#define tasklet_kill(tasklet)	{ do {} while (0); }
+
+/* 2.4.x introduced del_timer_sync() */
+#define del_timer_sync(timer) del_timer(timer)
+
+#else
+
+#define netif_down(dev)
+
+#endif /* SoftNet */
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 3))
+
+/*
+ * Emit code to initialise a tq_struct's routine and data pointers
+ */
+#define PREPARE_TQUEUE(_tq, _routine, _data)			\
+	do {							\
+		(_tq)->routine = _routine;			\
+		(_tq)->data = _data;				\
+	} while (0)
+
+/*
+ * Emit code to initialise all of a tq_struct
+ */
+#define INIT_TQUEUE(_tq, _routine, _data)			\
+	do {							\
+		INIT_LIST_HEAD(&(_tq)->list);			\
+		(_tq)->sync = 0;				\
+		PREPARE_TQUEUE((_tq), (_routine), (_data));	\
+	} while (0)
+
+#endif	/* LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 3) */
+
+/* Power management related macro & routines */
+#if LINUX_VERSION_CODE > KERNEL_VERSION(2, 6, 9)
+#define	PCI_SAVE_STATE(a, b)	pci_save_state(a)
+#define	PCI_RESTORE_STATE(a, b)	pci_restore_state(a)
+#else
+#define	PCI_SAVE_STATE(a, b)	pci_save_state(a, b)
+#define	PCI_RESTORE_STATE(a, b)	pci_restore_state(a, b)
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 6))
+static inline int
+pci_save_state(struct pci_dev *dev, u32 *buffer)
+{
+	int i;
+	if (buffer) {
+		for (i = 0; i < 16; i++)
+			pci_read_config_dword(dev, i * 4, &buffer[i]);
+	}
+	return 0;
+}
+
+static inline int
+pci_restore_state(struct pci_dev *dev, u32 *buffer)
+{
+	int i;
+
+	if (buffer) {
+		for (i = 0; i < 16; i++)
+			pci_write_config_dword(dev, i * 4, buffer[i]);
+	}
+	/*
+	 * otherwise, write the context information we know from bootup.
+	 * This works around a problem where warm-booting from Windows
+	 * combined with a D3(hot)->D0 transition causes PCI config
+	 * header data to be forgotten.
+	 */
+	else {
+		for (i = 0; i < 6; i ++)
+			pci_write_config_dword(dev,
+			                       PCI_BASE_ADDRESS_0 + (i * 4),
+			                       pci_resource_start(dev, i));
+		pci_write_config_byte(dev, PCI_INTERRUPT_LINE, dev->irq);
+	}
+	return 0;
+}
+#endif /* PCI power management */
+
+/* Old cp0 access macros deprecated in 2.4.19 */
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 4, 19))
+#define read_c0_count() read_32bit_cp0_register(CP0_COUNT)
+#endif
+
+/* Module refcount handled internally in 2.6.x */
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 24))
+#ifndef SET_MODULE_OWNER
+#define SET_MODULE_OWNER(dev)		do {} while (0)
+#define OLD_MOD_INC_USE_COUNT		MOD_INC_USE_COUNT
+#define OLD_MOD_DEC_USE_COUNT		MOD_DEC_USE_COUNT
+#else
+#define OLD_MOD_INC_USE_COUNT		do {} while (0)
+#define OLD_MOD_DEC_USE_COUNT		do {} while (0)
+#endif
+#else /* LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 24) */
+#ifndef SET_MODULE_OWNER
+#define SET_MODULE_OWNER(dev)		do {} while (0)
+#endif
+#ifndef MOD_INC_USE_COUNT
+#define MOD_INC_USE_COUNT			do {} while (0)
+#endif
+#ifndef MOD_DEC_USE_COUNT
+#define MOD_DEC_USE_COUNT			do {} while (0)
+#endif
+#define OLD_MOD_INC_USE_COUNT		MOD_INC_USE_COUNT
+#define OLD_MOD_DEC_USE_COUNT		MOD_DEC_USE_COUNT
+#endif /* LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 24) */
+
+#ifndef SET_NETDEV_DEV
+#define SET_NETDEV_DEV(net, pdev)	do {} while (0)
+#endif
+
+#ifndef HAVE_FREE_NETDEV
+#define free_netdev(dev)		kfree(dev)
+#endif
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0))
+/* struct packet_type redefined in 2.6.x */
+#define af_packet_priv			data
+#endif
+
+/* suspend args */
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 11)
+#define DRV_SUSPEND_STATE_TYPE pm_message_t
+#else
+#define DRV_SUSPEND_STATE_TYPE uint32
+#endif
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 19)
+#define CHECKSUM_HW	CHECKSUM_PARTIAL
+#endif
+
+typedef struct {
+	void 	*parent;  /* some external entity that the thread supposed to work for */
+	struct	task_struct *p_task;
+	long 	thr_pid;
+	int 	prio; /* priority */
+	struct	semaphore sema;
+	int	terminated;
+	struct	completion completed;
+} tsk_ctl_t;
+
+
+/* requires  tsk_ctl_t tsk  argument, the caller's priv data is passed in owner ptr */
+/* note this macro assumes there may be only one context waiting on thread's completion */
+#ifdef DHD_DEBUG
+#define DBG_THR(x) printk x
+#else
+#define DBG_THR(x)
+#endif
+
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 0))
+#define SMP_RD_BARRIER_DEPENDS(x) smp_read_barrier_depends(x)
+#else
+#define SMP_RD_BARRIER_DEPENDS(x) smp_rmb(x)
+#endif
+
+
+#define PROC_START(thread_func, owner, tsk_ctl, flags) \
+{ \
+	sema_init(&((tsk_ctl)->sema), 0); \
+	init_completion(&((tsk_ctl)->completed)); \
+	(tsk_ctl)->parent = owner; \
+	(tsk_ctl)->terminated = FALSE; \
+	(tsk_ctl)->thr_pid = kernel_thread(thread_func, tsk_ctl, flags); \
+	if ((tsk_ctl)->thr_pid > 0) \
+		wait_for_completion(&((tsk_ctl)->completed)); \
+	DBG_THR(("%s thr:%lx started\n", __FUNCTION__, (tsk_ctl)->thr_pid)); \
+}
+
+#define PROC_STOP(tsk_ctl) \
+{ \
+	(tsk_ctl)->terminated = TRUE; \
+	smp_wmb(); \
+	up(&((tsk_ctl)->sema));	\
+	wait_for_completion(&((tsk_ctl)->completed)); \
+	DBG_THR(("%s thr:%lx terminated OK\n", __FUNCTION__, (tsk_ctl)->thr_pid)); \
+	(tsk_ctl)->thr_pid = -1; \
+}
+
+/*  ----------------------- */
+
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 31))
+#define KILL_PROC(nr, sig) \
+{ \
+struct task_struct *tsk; \
+struct pid *pid;    \
+pid = find_get_pid((pid_t)nr);    \
+tsk = pid_task(pid, PIDTYPE_PID);    \
+if (tsk) send_sig(sig, tsk, 1); \
+}
+#else
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 27)) && (LINUX_VERSION_CODE <= \
+	KERNEL_VERSION(2, 6, 30))
+#define KILL_PROC(pid, sig) \
+{ \
+	struct task_struct *tsk; \
+	tsk = find_task_by_vpid(pid); \
+	if (tsk) send_sig(sig, tsk, 1); \
+}
+#else
+#define KILL_PROC(pid, sig) \
+{ \
+	kill_proc(pid, sig, 1); \
+}
+#endif
+#endif /* LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 31) */
+
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 0))
+#include <linux/time.h>
+#include <linux/wait.h>
+#else
+#include <linux/sched.h>
+
+#define __wait_event_interruptible_timeout(wq, condition, ret)		\
+do {									\
+	wait_queue_t __wait;						\
+	init_waitqueue_entry(&__wait, current);				\
+									\
+	add_wait_queue(&wq, &__wait);					\
+	for (;;) {							\
+		set_current_state(TASK_INTERRUPTIBLE);			\
+		if (condition)						\
+			break;						\
+		if (!signal_pending(current)) {				\
+			ret = schedule_timeout(ret);			\
+			if (!ret)					\
+				break;					\
+			continue;					\
+		}							\
+		ret = -ERESTARTSYS;					\
+		break;							\
+	}								\
+	current->state = TASK_RUNNING;					\
+	remove_wait_queue(&wq, &__wait);				\
+} while (0)
+
+#define wait_event_interruptible_timeout(wq, condition, timeout)	\
+({									\
+	long __ret = timeout;						\
+	if (!(condition))						\
+		__wait_event_interruptible_timeout(wq, condition, __ret); \
+	__ret;								\
+})
+
+#endif /* (LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 0)) */
+
+/*
+For < 2.6.24, wl creates its own netdev but doesn't
+align the priv area like the genuine alloc_netdev().
+Since netdev_priv() always gives us the aligned address, it will
+not match our unaligned address for < 2.6.24
+*/
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 24))
+#define DEV_PRIV(dev)	(dev->priv)
+#else
+#define DEV_PRIV(dev)	netdev_priv(dev)
+#endif
+
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 20)
+#define WL_ISR(i, d, p)         wl_isr((i), (d))
+#else
+#define WL_ISR(i, d, p)         wl_isr((i), (d), (p))
+#endif  /* < 2.6.20 */
+
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0))
+#define netdev_priv(dev) dev->priv
+#endif /* (LINUX_VERSION_CODE < KERNEL_VERSION(2, 6, 0)) */
+
+#endif /* _linuxver_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/osl.h b/drivers/bcmdrivers/gmac/src/include/osl.h
new file mode 100755
index 0000000..6b961d9
