--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmenetmib.h
@@ -0,0 +1,88 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Hardware-specific MIB definition for
+ * Broadcom Home Networking Division
+ * BCM44XX and BCM47XX 10/100 Mbps Ethernet cores.
+ *
+ * $Id: bcmenetmib.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef _bcmenetmib_h_
+#define _bcmenetmib_h_
+
+/* cpp contortions to concatenate w/arg prescan */
+#ifndef PAD
+#define	_PADLINE(line)	pad ## line
+#define	_XSTR(line)	_PADLINE(line)
+#define	PAD		_XSTR(__LINE__)
+#endif	/* PAD */
+
+/*
+ * EMAC MIB Registers
+ */
+typedef volatile struct {
+	uint32 tx_good_octets;
+	uint32 tx_good_pkts;
+	uint32 tx_octets;
+	uint32 tx_pkts;
+	uint32 tx_broadcast_pkts;
+	uint32 tx_multicast_pkts;
+	uint32 tx_len_64;
+	uint32 tx_len_65_to_127;
+	uint32 tx_len_128_to_255;
+	uint32 tx_len_256_to_511;
+	uint32 tx_len_512_to_1023;
+	uint32 tx_len_1024_to_max;
+	uint32 tx_jabber_pkts;
+	uint32 tx_oversize_pkts;
+	uint32 tx_fragment_pkts;
+	uint32 tx_underruns;
+	uint32 tx_total_cols;
+	uint32 tx_single_cols;
+	uint32 tx_multiple_cols;
+	uint32 tx_excessive_cols;
+	uint32 tx_late_cols;
+	uint32 tx_defered;
+	uint32 tx_carrier_lost;
+	uint32 tx_pause_pkts;
+	uint32 PAD[8];
+
+	uint32 rx_good_octets;
+	uint32 rx_good_pkts;
+	uint32 rx_octets;
+	uint32 rx_pkts;
+	uint32 rx_broadcast_pkts;
+	uint32 rx_multicast_pkts;
+	uint32 rx_len_64;
+	uint32 rx_len_65_to_127;
+	uint32 rx_len_128_to_255;
+	uint32 rx_len_256_to_511;
+	uint32 rx_len_512_to_1023;
+	uint32 rx_len_1024_to_max;
+	uint32 rx_jabber_pkts;
+	uint32 rx_oversize_pkts;
+	uint32 rx_fragment_pkts;
+	uint32 rx_missed_pkts;
+	uint32 rx_crc_align_errs;
+	uint32 rx_undersize;
+	uint32 rx_crc_errs;
+	uint32 rx_align_errs;
+	uint32 rx_symbol_errs;
+	uint32 rx_pause_pkts;
+	uint32 rx_nonpause_pkts;
+} bcmenetmib_t;
+
+#endif	/* _bcmenetmib_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmenetphy.h b/drivers/bcmdrivers/gmac/src/include/bcmenetphy.h
new file mode 100755
index 0000000..19c9c86
