--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmsdh.h
@@ -0,0 +1,226 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * SDIO host client driver interface of Broadcom HNBU
+ *     export functions to client drivers
+ *     abstract OS and BUS specific details of SDIO
+ *
+ * $Id: bcmsdh.h 299859 2011-12-01 03:53:27Z $
+ */
+
+/**
+ * @file bcmsdh.h
+ */
+
+#ifndef	_bcmsdh_h_
+#define	_bcmsdh_h_
+
+#define BCMSDH_ERROR_VAL	0x0001 /* Error */
+#define BCMSDH_INFO_VAL		0x0002 /* Info */
+extern const uint bcmsdh_msglevel;
+
+#ifdef BCMDBG
+#define BCMSDH_ERROR(x)	do { if (bcmsdh_msglevel & BCMSDH_ERROR_VAL) printf x; } while (0)
+#define BCMSDH_INFO(x)	do { if (bcmsdh_msglevel & BCMSDH_INFO_VAL) printf x; } while (0)
+#else /* BCMDBG */
+#define BCMSDH_ERROR(x)
+#define BCMSDH_INFO(x)
+#endif /* BCMDBG */
+
+
+/* forward declarations */
+typedef struct bcmsdh_info bcmsdh_info_t;
+typedef void (*bcmsdh_cb_fn_t)(void *);
+
+/* Attach and build an interface to the underlying SD host driver.
+ *  - Allocates resources (structs, arrays, mem, OS handles, etc) needed by bcmsdh.
+ *  - Returns the bcmsdh handle and virtual address base for register access.
+ *    The returned handle should be used in all subsequent calls, but the bcmsh
+ *    implementation may maintain a single "default" handle (e.g. the first or
+ *    most recent one) to enable single-instance implementations to pass NULL.
+ */
+extern bcmsdh_info_t *bcmsdh_attach(osl_t *osh, void *cfghdl, void **regsva, uint irq);
+
+/* Detach - freeup resources allocated in attach */
+extern int bcmsdh_detach(osl_t *osh, void *sdh);
+
+/* Query if SD device interrupts are enabled */
+extern bool bcmsdh_intr_query(void *sdh);
+
+/* Enable/disable SD interrupt */
+extern int bcmsdh_intr_enable(void *sdh);
+extern int bcmsdh_intr_disable(void *sdh);
+
+/* Register/deregister device interrupt handler. */
+extern int bcmsdh_intr_reg(void *sdh, bcmsdh_cb_fn_t fn, void *argh);
+extern int bcmsdh_intr_dereg(void *sdh);
+
+#if defined(DHD_DEBUG) || defined(BCMDBG)
+/* Query pending interrupt status from the host controller */
+extern bool bcmsdh_intr_pending(void *sdh);
+#endif
+
+/* Register a callback to be called if and when bcmsdh detects
+ * device removal. No-op in the case of non-removable/hardwired devices.
+ */
+extern int bcmsdh_devremove_reg(void *sdh, bcmsdh_cb_fn_t fn, void *argh);
+
+/* Access SDIO address space (e.g. CCCR) using CMD52 (single-byte interface).
+ *   fn:   function number
+ *   addr: unmodified SDIO-space address
+ *   data: data byte to write
+ *   err:  pointer to error code (or NULL)
+ */
+extern uint8 bcmsdh_cfg_read(void *sdh, uint func, uint32 addr, int *err);
+extern void bcmsdh_cfg_write(void *sdh, uint func, uint32 addr, uint8 data, int *err);
+
+/* Read/Write 4bytes from/to cfg space */
+extern uint32 bcmsdh_cfg_read_word(void *sdh, uint fnc_num, uint32 addr, int *err);
+extern void bcmsdh_cfg_write_word(void *sdh, uint fnc_num, uint32 addr, uint32 data, int *err);
+
+/* Read CIS content for specified function.
+ *   fn:     function whose CIS is being requested (0 is common CIS)
+ *   cis:    pointer to memory location to place results
+ *   length: number of bytes to read
+ * Internally, this routine uses the values from the cis base regs (0x9-0xB)
+ * to form an SDIO-space address to read the data from.
+ */
+extern int bcmsdh_cis_read(void *sdh, uint func, uint8 *cis, uint length);
+
+/* Synchronous access to device (client) core registers via CMD53 to F1.
+ *   addr: backplane address (i.e. >= regsva from attach)
+ *   size: register width in bytes (2 or 4)
+ *   data: data for register write
+ */
+extern uint32 bcmsdh_reg_read(void *sdh, uint32 addr, uint size);
+extern uint32 bcmsdh_reg_write(void *sdh, uint32 addr, uint size, uint32 data);
+
+/* set sb address window */
+extern int bcmsdhsdio_set_sbaddr_window(void *sdh, uint32 address, bool force_set);
+
+/* Indicate if last reg read/write failed */
+extern bool bcmsdh_regfail(void *sdh);
+
+/* Buffer transfer to/from device (client) core via cmd53.
+ *   fn:       function number
+ *   addr:     backplane address (i.e. >= regsva from attach)
+ *   flags:    backplane width, address increment, sync/async
+ *   buf:      pointer to memory data buffer
+ *   nbytes:   number of bytes to transfer to/from buf
+ *   pkt:      pointer to packet associated with buf (if any)
+ *   complete: callback function for command completion (async only)
+ *   handle:   handle for completion callback (first arg in callback)
+ * Returns 0 or error code.
+ * NOTE: Async operation is not currently supported.
+ */
+typedef void (*bcmsdh_cmplt_fn_t)(void *handle, int status, bool sync_waiting);
+extern int bcmsdh_send_buf(void *sdh, uint32 addr, uint fn, uint flags,
+                           uint8 *buf, uint nbytes, void *pkt,
+                           bcmsdh_cmplt_fn_t complete_fn, void *handle);
+extern int bcmsdh_recv_buf(void *sdh, uint32 addr, uint fn, uint flags,
+                           uint8 *buf, uint nbytes, void *pkt,
+                           bcmsdh_cmplt_fn_t complete_fn, void *handle);
+
+/* Flags bits */
+#define SDIO_REQ_4BYTE	0x1	/* Four-byte target (backplane) width (vs. two-byte) */
+#define SDIO_REQ_FIXED	0x2	/* Fixed address (FIFO) (vs. incrementing address) */
+#define SDIO_REQ_ASYNC	0x4	/* Async request (vs. sync request) */
+#define SDIO_BYTE_MODE	0x8	/* Byte mode request(non-block mode) */
+
+/* Pending (non-error) return code */
+#define BCME_PENDING	1
+
+/* Read/write to memory block (F1, no FIFO) via CMD53 (sync only).
+ *   rw:       read or write (0/1)
+ *   addr:     direct SDIO address
+ *   buf:      pointer to memory data buffer
+ *   nbytes:   number of bytes to transfer to/from buf
+ * Returns 0 or error code.
+ */
+extern int bcmsdh_rwdata(void *sdh, uint rw, uint32 addr, uint8 *buf, uint nbytes);
+
+/* Issue an abort to the specified function */
+extern int bcmsdh_abort(void *sdh, uint fn);
+
+/* Start SDIO Host Controller communication */
+extern int bcmsdh_start(void *sdh, int stage);
+
+/* Stop SDIO Host Controller communication */
+extern int bcmsdh_stop(void *sdh);
+
+/* Wait system lock free */
+extern int bcmsdh_waitlockfree(void *sdh);
+
+/* Returns the "Device ID" of target device on the SDIO bus. */
+extern int bcmsdh_query_device(void *sdh);
+
+/* Returns the number of IO functions reported by the device */
+extern uint bcmsdh_query_iofnum(void *sdh);
+
+/* Miscellaneous knob tweaker. */
+extern int bcmsdh_iovar_op(void *sdh, const char *name,
+                           void *params, int plen, void *arg, int len, bool set);
+
+/* Reset and reinitialize the device */
+extern int bcmsdh_reset(bcmsdh_info_t *sdh);
+
+/* helper functions */
+
+extern void *bcmsdh_get_sdioh(bcmsdh_info_t *sdh);
+
+/* callback functions */
+typedef struct {
+	/* attach to device */
+	void *(*attach)(uint16 vend_id, uint16 dev_id, uint16 bus, uint16 slot,
+	                uint16 func, uint bustype, void * regsva, osl_t * osh,
+	                void * param);
+	/* detach from device */
+	void (*detach)(void *ch);
+} bcmsdh_driver_t;
+
+/* platform specific/high level functions */
+extern int bcmsdh_register(bcmsdh_driver_t *driver);
+extern void bcmsdh_unregister(void);
+extern bool bcmsdh_chipmatch(uint16 vendor, uint16 device);
+extern void bcmsdh_device_remove(void * sdh);
+
+#if defined(OOB_INTR_ONLY)
+extern int bcmsdh_register_oob_intr(void * dhdp);
+extern void bcmsdh_unregister_oob_intr(void);
+extern void bcmsdh_oob_intr_set(bool enable);
+#endif /* defined(OOB_INTR_ONLY) */
+
+/* Function to pass device-status bits to DHD. */
+extern uint32 bcmsdh_get_dstatus(void *sdh);
+
+/* Function to return current window addr */
+extern uint32 bcmsdh_cur_sbwad(void *sdh);
+
+/* Function to pass chipid and rev to lower layers for controlling pr's */
+extern void bcmsdh_chipinfo(void *sdh, uint32 chip, uint32 chiprev);
+
+#ifdef BCMSPI
+extern void bcmsdh_dwordmode(void *sdh, bool set);
+#endif /* BCMSPI */
+
+extern int bcmsdh_sleep(void *sdh, bool enab);
+
+/* GPIO support */
+extern int bcmsdh_gpio_init(void *sd);
+extern bool bcmsdh_gpioin(void *sd, uint32 gpio);
+extern int bcmsdh_gpioouten(void *sd, uint32 gpio);
+extern int bcmsdh_gpioout(void *sd, uint32 gpio, bool enab);
+
+#endif	/* _bcmsdh_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmsdpcm.h b/drivers/bcmdrivers/gmac/src/include/bcmsdpcm.h
new file mode 100755
index 0000000..c1a320c
