--- /dev/null
+++ b/arch/arm/plat-iproc/include/mach/hardware.h
@@ -0,0 +1,43 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+#ifndef __PLAT_IPROC_HARDWARE_H
+#define __PLAT_IPROC_HARDWARE_H
+
+#include <asm/sizes.h>
+#include <mach/memory.h>
+#include <mach/io_map.h>
+
+/* Hardware addresses of major areas.
+ *  *_START is the physical address
+ *  *_SIZE  is the size of the region
+ *  *_BASE  is the virtual address
+ */
+#define RAM_START		PHYS_OFFSET
+
+#define RAM_BASE		PAGE_OFFSET
+
+#define IO_START IO_START_PA
+#define IO_BASE  IO_START_VA
+
+/* In case we use physical addresses */
+#define IO_ADDRESS(x)   (x)
+
+#define pcibios_assign_all_busses() 1
+
+#define PCIBIOS_MIN_IO			0x1000
+#define PCIBIOS_MIN_MEM			0x01000000
+
+#endif /* __PLAT_IPROC_HARDWARE_H */
diff --git a/arch/arm/plat-iproc/include/mach/io.h b/arch/arm/plat-iproc/include/mach/io.h
new file mode 100644
index 0000000..b980406
