{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Service"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Service","index":0,"n_rows":8,"n_cols":12,"rows_kept":8,"flags":["formulas_cached_only"]}
[]
[]
[]
[{"$nulls":8},"optional","Optional  (list of nodes to be crossed)","Optional - Yes means relaxes path constraint"]
["route id","Source","Destination","TRX type","Mode","System: spacing","System: input power (dBm)","System: nb of channels","routing: disjoint from","routing: path","routing: is loose?","path bandwidth"]
[0,"Lorient_KMA","Vannes_KBE","Voyager","mode 1",50,null,80,{"$nulls":3},100]
[1,"Brest_KLA","Vannes_KBE","Voyager","mode 1",50,1,{"$nulls":4},10]
[3,"Lannion_CAS","Rennes_STA","vendorA_trx-type1","mode 1",50,1,80,{"$nulls":3},60]