From c5749de8927e1b64eaf5e6c7401a24d1ee0fdc68 Mon Sep 17 00:00:00 2001
From: Florian Meier <florian.meier@koalo.de>
Date: Fri, 22 Nov 2013 19:21:34 +0100
Subject: [PATCH 39/54] BCM2708: Add HifiBerry DAC to board file

This adds the initalization of the HifiBerry DAC
to the mach-bcm2708 board file.

Signed-off-by: Florian Meier <florian.meier@koalo.de>
---
 arch/arm/mach-bcm2708/bcm2708.c | 19 +++++++++++++++++++
 1 file changed, 19 insertions(+)

diff --git a/arch/arm/mach-bcm2708/bcm2708.c b/arch/arm/mach-bcm2708/bcm2708.c
index 07da1fd..82b09a5 100644
--- a/arch/arm/mach-bcm2708/bcm2708.c
+++ b/arch/arm/mach-bcm2708/bcm2708.c
@@ -637,6 +637,20 @@ static struct platform_device bcm2708_i2s_device = {
 };
 #endif
 
+#if defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC) || defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC_MODULE)
+static struct platform_device snd_hifiberry_dac_device = {
+        .name = "snd-hifiberry-dac",
+        .id = 0,
+        .num_resources = 0,
+};
+
+static struct platform_device snd_pcm5102a_codec_device = {
+        .name = "pcm5102a-codec",
+        .id = -1,
+        .num_resources = 0,
+};
+#endif
+
 int __init bcm_register_device(struct platform_device *pdev)
 {
 	int ret;
@@ -764,6 +778,11 @@ void __init bcm2708_init(void)
 	bcm_register_device(&bcm2708_i2s_device);
 #endif
 
+#if defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC) || defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC_MODULE)
+        bcm_register_device(&snd_hifiberry_dac_device);
+        bcm_register_device(&snd_pcm5102a_codec_device);
+#endif
+
 	for (i = 0; i < ARRAY_SIZE(amba_devs); i++) {
 		struct amba_device *d = amba_devs[i];
 		amba_device_register(d, &iomem_resource);
-- 
1.9.1

