--- a/drivers/net/wireless/ath/ath9k/hw.c
+++ b/drivers/net/wireless/ath/ath9k/hw.c
@@ -215,6 +215,19 @@ void ath9k_hw_get_channel_centers(struct
 		centers->synth_center + (extoff * HT40_CHANNEL_CENTER_SHIFT);
 }
 
+static inline void ath9k_hw_disable_pll_lock_detect(struct ath_hw *ah)
+{
+	/* On AR9330 and AR9340 devices, some PHY registers must be
+	 * tuned to gain better stability/performance. These registers
+	 * might be changed while doing wlan reset so the registers must
+	 * be reprogrammed after each reset.
+	 */
+	REG_CLR_BIT(ah, AR_PHY_USB_CTRL1, BIT(20));
+	REG_RMW(ah, AR_PHY_USB_CTRL2,
+		(1 << 21) | (0xf << 22),
+		(1 << 21) | (0x3 << 22));
+}
+
 /******************/
 /* Chip Revisions */
 /******************/
@@ -1351,6 +1364,9 @@ static bool ath9k_hw_set_reset(struct at
 	if (AR_SREV_9100(ah))
 		udelay(50);
 
+	if (AR_SREV_9330(ah) || AR_SREV_9340(ah))
+		ath9k_hw_disable_pll_lock_detect(ah);
+
 	return true;
 }
 
@@ -1450,6 +1466,9 @@ static bool ath9k_hw_chip_reset(struct a
 		ar9003_hw_internal_regulator_apply(ah);
 	ath9k_hw_init_pll(ah, chan);
 
+	if (AR_SREV_9330(ah) || AR_SREV_9340(ah))
+		ath9k_hw_disable_pll_lock_detect(ah);
+
 	return true;
 }
 
@@ -1744,8 +1763,14 @@ static int ath9k_hw_do_fastcc(struct ath
 	if (AR_SREV_9271(ah))
 		ar9002_hw_load_ani_reg(ah, chan);
 
+	if (AR_SREV_9330(ah) || AR_SREV_9340(ah))
+		ath9k_hw_disable_pll_lock_detect(ah);
+
 	return 0;
 fail:
+	if (AR_SREV_9330(ah) || AR_SREV_9340(ah))
+		ath9k_hw_disable_pll_lock_detect(ah);
+
 	return -EINVAL;
 }
 
@@ -1995,6 +2020,9 @@ int ath9k_hw_reset(struct ath_hw *ah, st
 		ath9k_hw_set_radar_params(ah);
 	}
 
+	if (AR_SREV_9330(ah) || AR_SREV_9340(ah))
+		ath9k_hw_disable_pll_lock_detect(ah);
+
 	return 0;
 }
 EXPORT_SYMBOL(ath9k_hw_reset);
--- a/drivers/net/wireless/ath/ath9k/phy.h
+++ b/drivers/net/wireless/ath/ath9k/phy.h
@@ -48,6 +48,9 @@
 #define AR_PHY_PLL_CONTROL 0x16180
 #define AR_PHY_PLL_MODE 0x16184
 
+#define AR_PHY_USB_CTRL1	0x16c84
+#define AR_PHY_USB_CTRL2	0x16c88
+
 enum ath9k_ant_div_comb_lna_conf {
 	ATH_ANT_DIV_COMB_LNA1_MINUS_LNA2,
 	ATH_ANT_DIV_COMB_LNA2,
