From d9bf66aadd1f0238d2f055a9204e892f3b8d9366 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Fri, 28 Feb 2014 15:26:33 +0000
Subject: [PATCH 175/196] ASoc: Don't report S24_LE support, it produces white
 noise with xbmc

---
 sound/soc/codecs/pcm5102a.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/codecs/pcm5102a.c b/sound/soc/codecs/pcm5102a.c
index 126f1e9..7812d34 100644
--- a/sound/soc/codecs/pcm5102a.c
+++ b/sound/soc/codecs/pcm5102a.c
@@ -28,7 +28,7 @@ static struct snd_soc_dai_driver pcm5102a_dai = {
 		.channels_max = 2,
 		.rates = SNDRV_PCM_RATE_8000_192000,
 		.formats = SNDRV_PCM_FMTBIT_S16_LE |
-			   SNDRV_PCM_FMTBIT_S24_LE |
+			   // SNDRV_PCM_FMTBIT_S24_LE | : disable for now, it causes white noise with xbmc
 			   SNDRV_PCM_FMTBIT_S32_LE
 	},
 };
-- 
1.9.1

