From 3aa7ff0de5bddc825406ffff49dc4a38b13ebac3 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Wed, 5 Feb 2014 14:05:07 +0100
Subject: [PATCH] ARM: sunxi: Enable A31 SPI and SID in the defconfig

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/configs/sunxi_defconfig | 3 +++
 1 file changed, 3 insertions(+)

--- a/arch/arm/configs/sunxi_defconfig
+++ b/arch/arm/configs/sunxi_defconfig
@@ -24,6 +24,7 @@ CONFIG_IP_PNP_BOOTP=y
 # CONFIG_WIRELESS is not set
 CONFIG_DEVTMPFS=y
 CONFIG_DEVTMPFS_MOUNT=y
+CONFIG_EEPROM_SUNXI_SID=y
 CONFIG_NETDEVICES=y
 CONFIG_SUN4I_EMAC=y
 # CONFIG_NET_CADENCE is not set
@@ -48,6 +49,8 @@ CONFIG_I2C=y
 # CONFIG_I2C_COMPAT is not set
 CONFIG_I2C_CHARDEV=y
 CONFIG_I2C_MV64XXX=y
+CONFIG_SPI=y
+CONFIG_SPI_SUN6I=y
 CONFIG_GPIO_SYSFS=y
 # CONFIG_HWMON is not set
 CONFIG_WATCHDOG=y
