From 92fde23153240a6173645dabe4d99f4aa6570bb7 Mon Sep 17 00:00:00 2001
From: Stephen Boyd <sboyd@codeaurora.org>
Date: Mon, 28 Apr 2014 16:01:03 -0700
Subject: [PATCH 129/182] clk: qcom: Add support for NSS/GMAC clocks and
 resets

The NSS driver expects one virtual clock that actually represents
two clocks (one for each UBI32 core). Register the ubi32 core
clocks and also make a wrapper virtual clock called nss_core_clk
to be used by the driver. This will properly handle switching the
rates of both clocks at the same time like how the NSS driver
expects it. Also add the TCM clock and the NSS resets.

Signed-off-by: Stephen Boyd <sboyd@codeaurora.org>
---
 drivers/clk/qcom/gcc-ipq806x.c               |  710 +++++++++++++++++++++++++-
 include/dt-bindings/clock/qcom,gcc-ipq806x.h |    3 +
 include/dt-bindings/reset/qcom,gcc-ipq806x.h |   43 ++
 3 files changed, 755 insertions(+), 1 deletion(-)

--- a/drivers/clk/qcom/gcc-ipq806x.c
+++ b/drivers/clk/qcom/gcc-ipq806x.c
@@ -32,6 +32,33 @@
 #include "clk-branch.h"
 #include "reset.h"
 
+static struct clk_pll pll0 = {
+	.l_reg = 0x30c4,
+	.m_reg = 0x30c8,
+	.n_reg = 0x30cc,
+	.config_reg = 0x30d4,
+	.mode_reg = 0x30c0,
+	.status_reg = 0x30d8,
+	.status_bit = 16,
+	.clkr.hw.init = &(struct clk_init_data){
+		.name = "pll0",
+		.parent_names = (const char *[]){ "pxo" },
+		.num_parents = 1,
+		.ops = &clk_pll_ops,
+	},
+};
+
+static struct clk_regmap pll0_vote = {
+	.enable_reg = 0x34c0,
+	.enable_mask = BIT(0),
+	.hw.init = &(struct clk_init_data){
+		.name = "pll0_vote",
+		.parent_names = (const char *[]){ "pll0" },
+		.num_parents = 1,
+		.ops = &clk_pll_vote_ops,
+	},
+};
+
 static struct clk_pll pll3 = {
 	.l_reg = 0x3164,
 	.m_reg = 0x3168,
@@ -102,11 +129,46 @@ static struct clk_regmap pll14_vote = {
 	},
 };
 
+#define NSS_PLL_RATE(f, _l, _m, _n, i) \
+	{  \
+		.freq = f,  \
+		.l = _l, \
+		.m = _m, \
+		.n = _n, \
+		.ibits = i, \
+	}
+
+static struct pll_freq_tbl pll18_freq_tbl[] = {
+	NSS_PLL_RATE(550000000, 44, 0, 1, 0x01495625),
+	NSS_PLL_RATE(733000000, 58, 16, 25, 0x014b5625),
+};
+
+static struct clk_pll pll18 = {
+	.l_reg = 0x31a4,
+	.m_reg = 0x31a8,
+	.n_reg = 0x31ac,
+	.config_reg = 0x31b4,
+	.mode_reg = 0x31a0,
+	.status_reg = 0x31b8,
+	.status_bit = 16,
+	.post_div_shift = 16,
+	.post_div_width = 1,
+	.freq_tbl = pll18_freq_tbl,
+	.clkr.hw.init = &(struct clk_init_data){
+		.name = "pll18",
+		.parent_names = (const char *[]){ "pxo" },
+		.num_parents = 1,
+		.ops = &clk_pll_ops,
+	},
+};
+
 #define P_PXO	0
 #define P_PLL8	1
 #define P_PLL3	1
 #define P_PLL0	2
 #define P_CXO	2
+#define P_PLL14	3
+#define P_PLL18	4
 
 static const u8 gcc_pxo_pll8_map[] = {
 	[P_PXO]		= 0,
@@ -157,6 +219,22 @@ static const char *gcc_pxo_pll8_pll0_map
 	"pll0",
 };
 
+static const u8 gcc_pxo_pll8_pll14_pll18_pll0_map[] = {
+	[P_PXO]		= 0,
+	[P_PLL8]	= 4,
+	[P_PLL0]	= 2,
+	[P_PLL14]	= 5,
+	[P_PLL18]	= 1,
+};
+
+static const char *gcc_pxo_pll8_pll14_pll18_pll0[] = {
+	"pxo",
+	"pll8_vote",
+	"pll0_vote",
+	"pll14",
+	"pll18",
+};
+
 static struct freq_tbl clk_tbl_gsbi_uart[] = {
 	{  1843200, P_PLL8, 2,  6, 625 },
 	{  3686400, P_PLL8, 2, 12, 625 },
@@ -2132,12 +2210,567 @@ static struct clk_branch usb_fs1_h_clk =
 	},
 };
 
+static const struct freq_tbl clk_tbl_gmac[] = {
+	{ 133000000, P_PLL0, 1, 50, 301 },
+	{ }
+};
+
+static struct clk_dyn_rcg gmac_core1_src = {
+	.ns_reg[0] = 0x3cac,
+	.ns_reg[1] = 0x3cb0,
+	.md_reg[0] = 0x3ca4,
+	.md_reg[1] = 0x3ca8,
+	.bank_reg = 0x3ca0,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_gmac,
+	.clkr = {
+		.enable_reg = 0x3ca0,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core1_src",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+		},
+	},
+};
+
+static struct clk_branch gmac_core1_clk = {
+	.halt_reg = 0x3c20,
+	.halt_bit = 4,
+	.hwcg_reg = 0x3cb4,
+	.hwcg_bit = 6,
+	.clkr = {
+		.enable_reg = 0x3cb4,
+		.enable_mask = BIT(4),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core1_clk",
+			.parent_names = (const char *[]){
+				"gmac_core1_src",
+			},
+			.num_parents = 1,
+			.ops = &clk_branch_ops,
+			.flags = CLK_SET_RATE_PARENT,
+		},
+	},
+};
+
+static struct clk_dyn_rcg gmac_core2_src = {
+	.ns_reg[0] = 0x3ccc,
+	.ns_reg[1] = 0x3cd0,
+	.md_reg[0] = 0x3cc4,
+	.md_reg[1] = 0x3cc8,
+	.bank_reg = 0x3ca0,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_gmac,
+	.clkr = {
+		.enable_reg = 0x3cc0,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core2_src",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+		},
+	},
+};
+
+static struct clk_branch gmac_core2_clk = {
+	.halt_reg = 0x3c20,
+	.halt_bit = 5,
+	.hwcg_reg = 0x3cd4,
+	.hwcg_bit = 6,
+	.clkr = {
+		.enable_reg = 0x3cd4,
+		.enable_mask = BIT(4),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core2_clk",
+			.parent_names = (const char *[]){
+				"gmac_core2_src",
+			},
+			.num_parents = 1,
+			.ops = &clk_branch_ops,
+			.flags = CLK_SET_RATE_PARENT,
+		},
+	},
+};
+
+static struct clk_dyn_rcg gmac_core3_src = {
+	.ns_reg[0] = 0x3cec,
+	.ns_reg[1] = 0x3cf0,
+	.md_reg[0] = 0x3ce4,
+	.md_reg[1] = 0x3ce8,
+	.bank_reg = 0x3ce0,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_gmac,
+	.clkr = {
+		.enable_reg = 0x3ce0,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core3_src",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+		},
+	},
+};
+
+static struct clk_branch gmac_core3_clk = {
+	.halt_reg = 0x3c20,
+	.halt_bit = 6,
+	.hwcg_reg = 0x3cf4,
+	.hwcg_bit = 6,
+	.clkr = {
+		.enable_reg = 0x3cf4,
+		.enable_mask = BIT(4),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core3_clk",
+			.parent_names = (const char *[]){
+				"gmac_core3_src",
+			},
+			.num_parents = 1,
+			.ops = &clk_branch_ops,
+			.flags = CLK_SET_RATE_PARENT,
+		},
+	},
+};
+
+static struct clk_dyn_rcg gmac_core4_src = {
+	.ns_reg[0] = 0x3d0c,
+	.ns_reg[1] = 0x3d10,
+	.md_reg[0] = 0x3d04,
+	.md_reg[1] = 0x3d08,
+	.bank_reg = 0x3d00,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_gmac,
+	.clkr = {
+		.enable_reg = 0x3d00,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core4_src",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+		},
+	},
+};
+
+static struct clk_branch gmac_core4_clk = {
+	.halt_reg = 0x3c20,
+	.halt_bit = 7,
+	.hwcg_reg = 0x3d14,
+	.hwcg_bit = 6,
+	.clkr = {
+		.enable_reg = 0x3d14,
+		.enable_mask = BIT(4),
+		.hw.init = &(struct clk_init_data){
+			.name = "gmac_core4_clk",
+			.parent_names = (const char *[]){
+				"gmac_core4_src",
+			},
+			.num_parents = 1,
+			.ops = &clk_branch_ops,
+			.flags = CLK_SET_RATE_PARENT,
+		},
+	},
+};
+
+static const struct freq_tbl clk_tbl_nss_tcm[] = {
+	{ 266000000, P_PLL0, 3, 0, 0 },
+	{ 400000000, P_PLL0, 2, 0, 0 },
+	{ }
+};
+
+static struct clk_dyn_rcg nss_tcm_src = {
+	.ns_reg[0] = 0x3dc4,
+	.ns_reg[1] = 0x3dc8,
+	.bank_reg = 0x3dc0,
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 4,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 4,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_nss_tcm,
+	.clkr = {
+		.enable_reg = 0x3dc0,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "nss_tcm_src",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+		},
+	},
+};
+
+static struct clk_branch nss_tcm_clk = {
+	.halt_reg = 0x3c20,
+	.halt_bit = 14,
+	.clkr = {
+		.enable_reg = 0x3dd0,
+		.enable_mask = BIT(6) | BIT(4),
+		.hw.init = &(struct clk_init_data){
+			.name = "nss_tcm_clk",
+			.parent_names = (const char *[]){
+				"nss_tcm_src",
+			},
+			.num_parents = 1,
+			.ops = &clk_branch_ops,
+			.flags = CLK_SET_RATE_PARENT,
+		},
+	},
+};
+
+static const struct freq_tbl clk_tbl_nss[] = {
+	{ 110000000, P_PLL18, 1, 1, 5 },
+	{ 275000000, P_PLL18, 2, 0, 0 },
+	{ 550000000, P_PLL18, 1, 0, 0 },
+	{ 733000000, P_PLL18, 1, 0, 0 },
+	{ }
+};
+
+static struct clk_dyn_rcg ubi32_core1_src_clk = {
+	.ns_reg[0] = 0x3d2c,
+	.ns_reg[1] = 0x3d30,
+	.md_reg[0] = 0x3d24,
+	.md_reg[1] = 0x3d28,
+	.bank_reg = 0x3d20,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_nss,
+	.clkr = {
+		.enable_reg = 0x3d20,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "ubi32_core1_src_clk",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+			.flags = CLK_SET_RATE_PARENT | CLK_GET_RATE_NOCACHE,
+		},
+	},
+};
+
+static struct clk_dyn_rcg ubi32_core2_src_clk = {
+	.ns_reg[0] = 0x3d4c,
+	.ns_reg[1] = 0x3d50,
+	.md_reg[0] = 0x3d44,
+	.md_reg[1] = 0x3d48,
+	.bank_reg = 0x3d40,
+	.mn[0] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.mn[1] = {
+		.mnctr_en_bit = 8,
+		.mnctr_reset_bit = 7,
+		.mnctr_mode_shift = 5,
+		.n_val_shift = 16,
+		.m_val_shift = 16,
+		.width = 8,
+	},
+	.s[0] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.s[1] = {
+		.src_sel_shift = 0,
+		.parent_map = gcc_pxo_pll8_pll14_pll18_pll0_map,
+	},
+	.p[0] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.p[1] = {
+		.pre_div_shift = 3,
+		.pre_div_width = 2,
+	},
+	.mux_sel_bit = 0,
+	.freq_tbl = clk_tbl_nss,
+	.clkr = {
+		.enable_reg = 0x3d40,
+		.enable_mask = BIT(1),
+		.hw.init = &(struct clk_init_data){
+			.name = "ubi32_core2_src_clk",
+			.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+			.num_parents = 5,
+			.ops = &clk_dyn_rcg_ops,
+			.flags = CLK_SET_RATE_PARENT | CLK_GET_RATE_NOCACHE,
+		},
+	},
+};
+
+static int nss_core_clk_set_rate(struct clk_hw *hw, unsigned long rate,
+				 unsigned long parent_rate)
+{
+	int ret;
+
+	ret = clk_dyn_rcg_ops.set_rate(&ubi32_core1_src_clk.clkr.hw, rate,
+				    parent_rate);
+	if (ret)
+		return ret;
+
+	return clk_dyn_rcg_ops.set_rate(&ubi32_core2_src_clk.clkr.hw, rate,
+				    parent_rate);
+}
+
+static int
+nss_core_clk_set_rate_and_parent(struct clk_hw *hw, unsigned long rate,
+				 unsigned long parent_rate, u8 index)
+{
+	int ret;
+
+	ret = clk_dyn_rcg_ops.set_rate_and_parent(
+			&ubi32_core1_src_clk.clkr.hw, rate, parent_rate, index);
+	if (ret)
+		return ret;
+
+	ret = clk_dyn_rcg_ops.set_rate_and_parent(
+			&ubi32_core2_src_clk.clkr.hw, rate, parent_rate, index);
+	return ret;
+}
+
+static long nss_core_clk_determine_rate(struct clk_hw *hw, unsigned long rate,
+				 unsigned long *p_rate, struct clk **p)
+{
+	return clk_dyn_rcg_ops.determine_rate(&ubi32_core1_src_clk.clkr.hw,
+						 rate, p_rate, p);
+}
+
+static unsigned long
+nss_core_clk_recalc_rate(struct clk_hw *hw, unsigned long parent_rate)
+{
+	return clk_dyn_rcg_ops.recalc_rate(&ubi32_core1_src_clk.clkr.hw,
+						 parent_rate);
+}
+
+static u8 nss_core_clk_get_parent(struct clk_hw *hw)
+{
+	return clk_dyn_rcg_ops.get_parent(&ubi32_core1_src_clk.clkr.hw);
+}
+
+static int nss_core_clk_set_parent(struct clk_hw *hw, u8 i)
+{
+	int ret;
+
+	ret = clk_dyn_rcg_ops.set_parent(&ubi32_core1_src_clk.clkr.hw, i);
+	if (ret)
+		return ret;
+
+	return clk_dyn_rcg_ops.set_parent(&ubi32_core2_src_clk.clkr.hw, i);
+}
+
+static struct clk *nss_core_clk_get_safe_parent(struct clk_hw *hw)
+{
+	return clk_get_parent_by_index(hw->clk,
+			ubi32_core2_src_clk.s[0].parent_map[P_PLL8]);
+}
+
+static const struct clk_ops clk_ops_nss_core = {
+	.set_rate = nss_core_clk_set_rate,
+	.set_rate_and_parent = nss_core_clk_set_rate_and_parent,
+	.determine_rate = nss_core_clk_determine_rate,
+	.recalc_rate = nss_core_clk_recalc_rate,
+	.get_parent = nss_core_clk_get_parent,
+	.set_parent = nss_core_clk_set_parent,
+	.get_safe_parent = nss_core_clk_get_safe_parent,
+};
+
+/* Virtual clock for nss core clocks */
+static struct clk_regmap nss_core_clk = {
+	.hw.init = &(struct clk_init_data){
+		.name = "nss_core_clk",
+		.ops = &clk_ops_nss_core,
+		.parent_names = gcc_pxo_pll8_pll14_pll18_pll0,
+		.num_parents = 5,
+		.flags = CLK_SET_RATE_PARENT,
+	},
+};
+
 static struct clk_regmap *gcc_ipq806x_clks[] = {
+	[PLL0] = &pll0.clkr,
+	[PLL0_VOTE] = &pll0_vote,
 	[PLL3] = &pll3.clkr,
 	[PLL8] = &pll8.clkr,
 	[PLL8_VOTE] = &pll8_vote,
 	[PLL14] = &pll14.clkr,
 	[PLL14_VOTE] = &pll14_vote,
+	[PLL18] = &pll18.clkr,
 	[GSBI1_UART_SRC] = &gsbi1_uart_src.clkr,
 	[GSBI1_UART_CLK] = &gsbi1_uart_clk.clkr,
 	[GSBI2_UART_SRC] = &gsbi2_uart_src.clkr,
@@ -2232,6 +2865,19 @@ static struct clk_regmap *gcc_ipq806x_cl
 	[USB_FS1_XCVR_SRC] = &usb_fs1_xcvr_clk_src.clkr,
 	[USB_FS1_XCVR_CLK] = &usb_fs1_xcvr_clk.clkr,
 	[USB_FS1_SYSTEM_CLK] = &usb_fs1_sys_clk.clkr,
+	[GMAC_CORE1_CLK_SRC] = &gmac_core1_src.clkr,
+	[GMAC_CORE1_CLK] = &gmac_core1_clk.clkr,
+	[GMAC_CORE2_CLK_SRC] = &gmac_core2_src.clkr,
+	[GMAC_CORE2_CLK] = &gmac_core2_clk.clkr,
+	[GMAC_CORE3_CLK_SRC] = &gmac_core3_src.clkr,
+	[GMAC_CORE3_CLK] = &gmac_core3_clk.clkr,
+	[GMAC_CORE4_CLK_SRC] = &gmac_core4_src.clkr,
+	[GMAC_CORE4_CLK] = &gmac_core4_clk.clkr,
+	[UBI32_CORE1_CLK_SRC] = &ubi32_core1_src_clk.clkr,
+	[UBI32_CORE2_CLK_SRC] = &ubi32_core2_src_clk.clkr,
+	[NSSTCM_CLK_SRC] = &nss_tcm_src.clkr,
+	[NSSTCM_CLK] = &nss_tcm_clk.clkr,
+	[NSS_CORE_CLK] = &nss_core_clk,
 };
 
 static const struct qcom_reset_map gcc_ipq806x_resets[] = {
@@ -2350,6 +2996,48 @@ static const struct qcom_reset_map gcc_i
 	[USB30_1_PHY_RESET] = { 0x3b58, 0 },
 	[NSSFB0_RESET] = { 0x3b60, 6 },
 	[NSSFB1_RESET] = { 0x3b60, 7 },
+	[UBI32_CORE1_CLKRST_CLAMP_RESET] = { 0x3d3c, 3},
+	[UBI32_CORE1_CLAMP_RESET] = { 0x3d3c, 2 },
+	[UBI32_CORE1_AHB_RESET] = { 0x3d3c, 1 },
+	[UBI32_CORE1_AXI_RESET] = { 0x3d3c, 0 },
+	[UBI32_CORE2_CLKRST_CLAMP_RESET] = { 0x3d5c, 3 },
+	[UBI32_CORE2_CLAMP_RESET] = { 0x3d5c, 2 },
+	[UBI32_CORE2_AHB_RESET] = { 0x3d5c, 1 },
+	[UBI32_CORE2_AXI_RESET] = { 0x3d5c, 0 },
+	[GMAC_CORE1_RESET] = { 0x3cbc, 0 },
+	[GMAC_CORE2_RESET] = { 0x3cdc, 0 },
+	[GMAC_CORE3_RESET] = { 0x3cfc, 0 },
+	[GMAC_CORE4_RESET] = { 0x3d1c, 0 },
+	[GMAC_AHB_RESET] = { 0x3e24, 0 },
+	[NSS_CH0_RST_RX_CLK_N_RESET] = { 0x3b60, 0 },
+	[NSS_CH0_RST_TX_CLK_N_RESET] = { 0x3b60, 1 },
+	[NSS_CH0_RST_RX_125M_N_RESET] = { 0x3b60, 2 },
+	[NSS_CH0_HW_RST_RX_125M_N_RESET] = { 0x3b60, 3 },
+	[NSS_CH0_RST_TX_125M_N_RESET] = { 0x3b60, 4 },
+	[NSS_CH1_RST_RX_CLK_N_RESET] = { 0x3b60, 5 },
+	[NSS_CH1_RST_TX_CLK_N_RESET] = { 0x3b60, 6 },
+	[NSS_CH1_RST_RX_125M_N_RESET] = { 0x3b60, 7 },
+	[NSS_CH1_HW_RST_RX_125M_N_RESET] = { 0x3b60, 8 },
+	[NSS_CH1_RST_TX_125M_N_RESET] = { 0x3b60, 9 },
+	[NSS_CH2_RST_RX_CLK_N_RESET] = { 0x3b60, 10 },
+	[NSS_CH2_RST_TX_CLK_N_RESET] = { 0x3b60, 11 },
+	[NSS_CH2_RST_RX_125M_N_RESET] = { 0x3b60, 12 },
+	[NSS_CH2_HW_RST_RX_125M_N_RESET] = { 0x3b60, 13 },
+	[NSS_CH2_RST_TX_125M_N_RESET] = { 0x3b60, 14 },
+	[NSS_CH3_RST_RX_CLK_N_RESET] = { 0x3b60, 15 },
+	[NSS_CH3_RST_TX_CLK_N_RESET] = { 0x3b60, 16 },
+	[NSS_CH3_RST_RX_125M_N_RESET] = { 0x3b60, 17 },
+	[NSS_CH3_HW_RST_RX_125M_N_RESET] = { 0x3b60, 18 },
+	[NSS_CH3_RST_TX_125M_N_RESET] = { 0x3b60, 19 },
+	[NSS_RST_RX_250M_125M_N_RESET] = { 0x3b60, 20 },
+	[NSS_RST_TX_250M_125M_N_RESET] = { 0x3b60, 21 },
+	[NSS_QSGMII_TXPI_RST_N_RESET] = { 0x3b60, 22 },
+	[NSS_QSGMII_CDR_RST_N_RESET] = { 0x3b60, 23 },
+	[NSS_SGMII2_CDR_RST_N_RESET] = { 0x3b60, 24 },
+	[NSS_SGMII3_CDR_RST_N_RESET] = { 0x3b60, 25 },
+	[NSS_CAL_PRBS_RST_N_RESET] = { 0x3b60, 26 },
+	[NSS_LCKDT_RST_N_RESET] = { 0x3b60, 27 },
+	[NSS_SRDS_N_RESET] = { 0x3b60, 28 },
 };
 
 static const struct regmap_config gcc_ipq806x_regmap_config = {
@@ -2378,6 +3066,8 @@ static int gcc_ipq806x_probe(struct plat
 {
 	struct clk *clk;
 	struct device *dev = &pdev->dev;
+	struct regmap *regmap;
+	int ret;
 
 	/* Temporary until RPM clocks supported */
 	clk = clk_register_fixed_rate(dev, "cxo", NULL, CLK_IS_ROOT, 25000000);
@@ -2388,7 +3078,25 @@ static int gcc_ipq806x_probe(struct plat
 	if (IS_ERR(clk))
 		return PTR_ERR(clk);
 
-	return qcom_cc_probe(pdev, &gcc_ipq806x_desc);
+	ret = qcom_cc_probe(pdev, &gcc_ipq806x_desc);
+	if (ret)
+		return ret;
+
+	regmap = dev_get_regmap(dev, NULL);
+	if (!regmap)
+		return -ENODEV;
+
+	/* Setup PLL18 static bits */
+	regmap_update_bits(regmap, 0x31a4, 0xffffffc0, 0x40000400);
+	regmap_write(regmap, 0x31b0, 0x3080);
+
+	/* Set GMAC footswitch sleep/wakeup values */
+	regmap_write(regmap, 0x3cb8, 8);
+	regmap_write(regmap, 0x3cd8, 8);
+	regmap_write(regmap, 0x3cf8, 8);
+	regmap_write(regmap, 0x3d18, 8);
+
+	return 0;
 }
 
 static int gcc_ipq806x_remove(struct platform_device *pdev)
--- a/include/dt-bindings/clock/qcom,gcc-ipq806x.h
+++ b/include/dt-bindings/clock/qcom,gcc-ipq806x.h
@@ -289,5 +289,8 @@
 #define UBI32_CORE2_CLK_SRC			277
 #define UBI32_CORE1_CLK				278
 #define UBI32_CORE2_CLK				279
+#define NSSTCM_CLK_SRC				280
+#define NSSTCM_CLK				281
+#define NSS_CORE_CLK				282 /* Virtual */
 
 #endif
--- a/include/dt-bindings/reset/qcom,gcc-ipq806x.h
+++ b/include/dt-bindings/reset/qcom,gcc-ipq806x.h
@@ -129,4 +129,47 @@
 #define USB30_1_PHY_RESET				112
 #define NSSFB0_RESET					113
 #define NSSFB1_RESET					114
+#define UBI32_CORE1_CLKRST_CLAMP_RESET			115
+#define UBI32_CORE1_CLAMP_RESET				116
+#define UBI32_CORE1_AHB_RESET				117
+#define UBI32_CORE1_AXI_RESET				118
+#define UBI32_CORE2_CLKRST_CLAMP_RESET			119
+#define UBI32_CORE2_CLAMP_RESET				120
+#define UBI32_CORE2_AHB_RESET				121
+#define UBI32_CORE2_AXI_RESET				122
+#define GMAC_CORE1_RESET				123
+#define GMAC_CORE2_RESET				124
+#define GMAC_CORE3_RESET				125
+#define GMAC_CORE4_RESET				126
+#define GMAC_AHB_RESET					127
+#define NSS_CH0_RST_RX_CLK_N_RESET			128
+#define NSS_CH0_RST_TX_CLK_N_RESET			129
+#define NSS_CH0_RST_RX_125M_N_RESET			130
+#define NSS_CH0_HW_RST_RX_125M_N_RESET			131
+#define NSS_CH0_RST_TX_125M_N_RESET			132
+#define NSS_CH1_RST_RX_CLK_N_RESET			133
+#define NSS_CH1_RST_TX_CLK_N_RESET			134
+#define NSS_CH1_RST_RX_125M_N_RESET			135
+#define NSS_CH1_HW_RST_RX_125M_N_RESET			136
+#define NSS_CH1_RST_TX_125M_N_RESET			137
+#define NSS_CH2_RST_RX_CLK_N_RESET			138
+#define NSS_CH2_RST_TX_CLK_N_RESET			139
+#define NSS_CH2_RST_RX_125M_N_RESET			140
+#define NSS_CH2_HW_RST_RX_125M_N_RESET			141
+#define NSS_CH2_RST_TX_125M_N_RESET			142
+#define NSS_CH3_RST_RX_CLK_N_RESET			143
+#define NSS_CH3_RST_TX_CLK_N_RESET			144
+#define NSS_CH3_RST_RX_125M_N_RESET			145
+#define NSS_CH3_HW_RST_RX_125M_N_RESET			146
+#define NSS_CH3_RST_TX_125M_N_RESET			147
+#define NSS_RST_RX_250M_125M_N_RESET			148
+#define NSS_RST_TX_250M_125M_N_RESET			149
+#define NSS_QSGMII_TXPI_RST_N_RESET			150
+#define NSS_QSGMII_CDR_RST_N_RESET			151
+#define NSS_SGMII2_CDR_RST_N_RESET			152
+#define NSS_SGMII3_CDR_RST_N_RESET			153
+#define NSS_CAL_PRBS_RST_N_RESET			154
+#define NSS_LCKDT_RST_N_RESET				155
+#define NSS_SRDS_N_RESET				156
+
 #endif
