From 0af3258f87d590864187b0187c7aa7428801ef80 Mon Sep 17 00:00:00 2001
From: Alexander Bersenev <bay@hackerdom.ru>
Date: Mon, 9 Jun 2014 00:08:12 +0600
Subject: [PATCH] ARM: sunxi: Add IR controllers on A20 to dtsi

This patch adds records for two IR controllers on A20

Signed-off-by: Alexander Bersenev <bay@hackerdom.ru>
Signed-off-by: Alexsey Shestacov <wingrime@linux-sunxi.org>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 18 ++++++++++++++++++
 1 file changed, 18 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index 4e4d6ce..3050369 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -784,6 +784,24 @@
 			#pwm-cells = <3>;
 		};
 
+		ir0: ir@01c21800 {
+			compatible = "allwinner,sun7i-a20-ir";
+			clocks = <&apb0_gates 6>, <&ir0_clk>;
+			clock-names = "apb", "ir";
+			interrupts = <0 5 4>;
+			reg = <0x01c21800 0x40>;
+			status = "disabled";
+		};
+
+		ir1: ir@01c21c00 {
+			compatible = "allwinner,sun7i-a20-ir";
+			clocks = <&apb0_gates 7>, <&ir1_clk>;
+			clock-names = "apb", "ir";
+			interrupts = <0 6 4>;
+			reg = <0x01c21c00 0x40>;
+			status = "disabled";
+		};
+
 		lradc: lradc@01c22800 {
 			compatible = "allwinner,sun4i-lradc-keys";
 			reg = <0x01c22800 0x100>;
