From f70ff551596e371431a05ab5678fb12f2dfc282a Mon Sep 17 00:00:00 2001
From: Daniel Matuschek <info@crazy-audio.com>
Date: Thu, 16 Jan 2014 07:27:28 +0100
Subject: [PATCH 46/54] BCM2708: Added HiFiBerry Digi configuration option It
 will be compiled as a module by default. This also includes the WM8804
 driver.

Signed-off-by: Daniel Matuschek <daniel@matuschek.net>
---
 arch/arm/configs/bcmrpi_defconfig | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/configs/bcmrpi_defconfig b/arch/arm/configs/bcmrpi_defconfig
index f877ab2..3d3c8ab 100644
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -742,8 +742,10 @@ CONFIG_SND_USB_6FIRE=m
 CONFIG_SND_SOC=m
 CONFIG_SND_SOC_DMAENGINE_PCM=y
 CONFIG_SND_SOC_GENERIC_DMAENGINE_PCM=y
+CONFIG_SND_SOC_WM8804=m
 CONFIG_SND_BCM2708_SOC_I2S=m
 CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC=m
+CONFIG_SND_BCM2708_SOC_HIFIBERRY_DIGI=m
 CONFIG_SND_BCM2708_SOC_RPI_DAC=m
 CONFIG_SND_SOC_I2C_AND_SPI=m
 CONFIG_SND_SOC_PCM5102A=m
-- 
1.9.1

