From cb78955cb0bedd81351bbe017dd5642f1358148d Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Wed, 20 Nov 2013 11:22:05 +0000
Subject: [PATCH 107/196] sdhci: Only do one iteration of PIO reading loop

---
 drivers/mmc/host/sdhci.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/mmc/host/sdhci.c b/drivers/mmc/host/sdhci.c
index 9c93e00..b4faaff 100644
--- a/drivers/mmc/host/sdhci.c
+++ b/drivers/mmc/host/sdhci.c
@@ -539,6 +539,7 @@ static void sdhci_transfer_pio(struct sdhci_host *host, u32 intstate)
 			break;
 		state = sdhci_readl(host, SDHCI_PRESENT_STATE);
 		available = state & mask;
+		break;
 	}
 
 	DBG("PIO transfer complete - %d blocks left.\n", host->blocks);
-- 
1.9.1

