From fee1501c494954f6e889563ca44aadfe4a83a643 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Tue, 14 Oct 2014 00:05:42 +0200
Subject: [PATCH] bcma: register SoC later (as a module)
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is temporary workaround required for easier debugging.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/bcma/host_soc.c | 12 ++++++++++--
 1 file changed, 10 insertions(+), 2 deletions(-)

diff --git a/drivers/bcma/host_soc.c b/drivers/bcma/host_soc.c
index 335cbcf..c7e12f2 100644
--- a/drivers/bcma/host_soc.c
+++ b/drivers/bcma/host_soc.c
@@ -265,14 +265,22 @@ static struct platform_driver bcma_host_soc_driver = {
 	.probe		= bcma_host_soc_probe,
 	.remove		= bcma_host_soc_remove,
 };
+/* FIXME: Using module_platform_driver is a temp hack to get bcma SoC
+ * initialzed *after* serial console. This way we get some logs in case of hang
+ * inside bcma or related driver. We need that for debugging problems and it's
+ * also useful for development. Otherwise any hang (in flash driver, PCIe
+ * driver, USB driver, etc.) would result in not getting logs at all.
+ */
+module_platform_driver(bcma_host_soc_driver);
 
 int __init bcma_host_soc_register_driver(void)
 {
-	return platform_driver_register(&bcma_host_soc_driver);
+	/* return platform_driver_register(&bcma_host_soc_driver); */
+	return 0;
 }
 
 void __exit bcma_host_soc_unregister_driver(void)
 {
-	platform_driver_unregister(&bcma_host_soc_driver);
+	/* platform_driver_unregister(&bcma_host_soc_driver); */
 }
 #endif /* CONFIG_OF */
-- 
1.8.4.5

