From cac3c4d67c80c4895d0d44e609beb535d66af6a3 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 22 Feb 2014 22:35:55 +0100
Subject: [PATCH] ARM: dt: sun4i: Add A10 SPI controller nodes

The A10 has 4 SPI controllers that are now supported. Add them in the DT.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi | 44 ++++++++++++++++++++++++++++++++++++++++
 1 file changed, 44 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -339,6 +339,28 @@
 		#size-cells = <1>;
 		ranges;
 
+		spi0: spi@01c05000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c05000 0x1000>;
+			interrupts = <10>;
+			clocks = <&ahb_gates 20>, <&spi0_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi1: spi@01c06000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c06000 0x1000>;
+			interrupts = <11>;
+			clocks = <&ahb_gates 21>, <&spi1_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		emac: ethernet@01c0b000 {
 			compatible = "allwinner,sun4i-a10-emac";
 			reg = <0x01c0b000 0x1000>;
@@ -353,6 +375,28 @@
 			status = "disabled";
 			#address-cells = <1>;
 			#size-cells = <0>;
+		};
+
+		spi2: spi@01c17000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c17000 0x1000>;
+			interrupts = <12>;
+			clocks = <&ahb_gates 22>, <&spi2_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi3: spi@01c1f000 {
+			compatible = "allwinner,sun4i-a10-spi";
+			reg = <0x01c1f000 0x1000>;
+			interrupts = <50>;
+			clocks = <&ahb_gates 23>, <&spi3_clk>;
+			clock-names = "ahb", "mod";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		intc: interrupt-controller@01c20400 {
