From 05cffcda932b0914d78a08891c13e61593a6ce02 Mon Sep 17 00:00:00 2001
From: Alexander Bersenev <bay@hackerdom.ru>
Date: Mon, 9 Jun 2014 00:08:13 +0600
Subject: [PATCH] ARM: sunxi: Enable IR controller on cubieboard 2 and
 cubietruck in dts

This patch enables two IR devices in dts:
- One IR device physically found on Cubieboard 2
- One IR device physically found on Cubietruck

Signed-off-by: Alexander Bersenev <bay@hackerdom.ru>
Signed-off-by: Alexsey Shestacov <wingrime@linux-sunxi.org>
---
 arch/arm/boot/dts/sun7i-a20-cubieboard2.dts | 6 ++++++
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts  | 6 ++++++
 2 files changed, 12 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
index 97bcb2a..81bf3df 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -66,6 +66,12 @@
 			};
 		};
 
+		ir0: ir@01c21800 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&ir0_pins_a>;
+			status = "okay";
+		};
+
 		uart0: serial@01c28000 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&uart0_pins_a>;
diff --git a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
index 624e0a5..3931986 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -114,6 +114,12 @@
 			status = "okay";
 		};
 
+		ir0: ir@01c21800 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&ir0_pins_a>;
+			status = "okay";
+		};
+
 		uart0: serial@01c28000 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&uart0_pins_a>;
