From 886f41537ad5e873caee522704e96e844a485961 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Wed, 5 Mar 2014 20:41:17 +0100
Subject: [PATCH] ARM: sun7i: dt: Add AXP209 support to cubietruck

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts      | 10 ++++++++++
 arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts | 10 ++++++++++
 2 files changed, 20 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -89,6 +89,16 @@
 			pinctrl-names = "default";
 			pinctrl-0 = <&uart0_pins_a>;
 			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupt-parent = <&nmi_intc>;
+				interrupts = <0 8>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
 		};
 
 		gmac: ethernet@01c50000 {
--- a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
@@ -127,6 +127,16 @@
 			pinctrl-names = "default";
 			pinctrl-0 = <&i2c0_pins_a>;
 			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupt-parent = <&nmi_intc>;
+				interrupts = <0 8>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
 		};
 
 		i2c1: i2c@01c2b000 {
