From f97cc1b1a4c868500cee6b016f54d78bdd3cdc26 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Sat, 8 Sep 2012 15:17:53 +0100
Subject: [PATCH 030/196] Avoid dynamic memory allocation for channel lock in
 USB driver. Thanks ddv2005.

---
 drivers/usb/host/dwc_otg/dwc_otg_hcd.c      | 6 +++---
 drivers/usb/host/dwc_otg/dwc_otg_hcd.h      | 2 +-
 drivers/usb/host/dwc_otg/dwc_otg_hcd_ddma.c | 3 +--
 drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c | 3 +--
 4 files changed, 6 insertions(+), 8 deletions(-)

diff --git a/drivers/usb/host/dwc_otg/dwc_otg_hcd.c b/drivers/usb/host/dwc_otg/dwc_otg_hcd.c
index 20f989e..0ce7e46 100644
--- a/drivers/usb/host/dwc_otg/dwc_otg_hcd.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_hcd.c
@@ -822,6 +822,7 @@ static void dwc_otg_hcd_free(dwc_otg_hcd_t * dwc_otg_hcd)
 	} else if (dwc_otg_hcd->status_buf != NULL) {
 		DWC_FREE(dwc_otg_hcd->status_buf);
 	}
+	DWC_SPINLOCK_FREE(dwc_otg_hcd->channel_lock);
 	DWC_SPINLOCK_FREE(dwc_otg_hcd->lock);
 	/* Set core_if's lock pointer to NULL */
 	dwc_otg_hcd->core_if->lock = NULL;
@@ -848,6 +849,7 @@ int dwc_otg_hcd_init(dwc_otg_hcd_t * hcd, dwc_otg_core_if_t * core_if)
 	dwc_hc_t *channel;
 
 	hcd->lock = DWC_SPINLOCK_ALLOC();
+	hcd->channel_lock = DWC_SPINLOCK_ALLOC();
         DWC_DEBUGPL(DBG_HCDV, "init of HCD %p given core_if %p\n",
                     hcd, core_if);
 	if (!hcd->lock) {
@@ -1248,7 +1250,7 @@ dwc_otg_transaction_type_e dwc_otg_hcd_select_transactions(dwc_otg_hcd_t * hcd)
 	dwc_otg_qh_t *qh;
 	int num_channels;
 	dwc_irqflags_t flags;
-	dwc_spinlock_t *channel_lock = DWC_SPINLOCK_ALLOC();
+	dwc_spinlock_t *channel_lock = hcd->channel_lock;
 	dwc_otg_transaction_type_e ret_val = DWC_OTG_TRANSACTION_NONE;
 
 #ifdef DEBUG_SOF
@@ -1348,8 +1350,6 @@ dwc_otg_transaction_type_e dwc_otg_hcd_select_transactions(dwc_otg_hcd_t * hcd)
 #ifdef DEBUG_HOST_CHANNELS
 	last_sel_trans_num_avail_hc_at_end = hcd->available_host_channels;
 #endif /* DEBUG_HOST_CHANNELS */
-
-	DWC_SPINLOCK_FREE(channel_lock);
 	return ret_val;
 }
 
diff --git a/drivers/usb/host/dwc_otg/dwc_otg_hcd.h b/drivers/usb/host/dwc_otg/dwc_otg_hcd.h
index dd30f47..6d82127 100644
--- a/drivers/usb/host/dwc_otg/dwc_otg_hcd.h
+++ b/drivers/usb/host/dwc_otg/dwc_otg_hcd.h
@@ -548,7 +548,7 @@ struct dwc_otg_hcd {
 
 	/*  */
 	dwc_spinlock_t *lock;
-
+	dwc_spinlock_t *channel_lock;
 	/**
 	 * Private data that could be used by OS wrapper.
 	 */
diff --git a/drivers/usb/host/dwc_otg/dwc_otg_hcd_ddma.c b/drivers/usb/host/dwc_otg/dwc_otg_hcd_ddma.c
index d0d5fa1..a2ceb77 100644
--- a/drivers/usb/host/dwc_otg/dwc_otg_hcd_ddma.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_hcd_ddma.c
@@ -276,7 +276,7 @@ void dump_frame_list(dwc_otg_hcd_t * hcd)
 static void release_channel_ddma(dwc_otg_hcd_t * hcd, dwc_otg_qh_t * qh)
 {
 	dwc_irqflags_t flags;
-	dwc_spinlock_t *channel_lock = DWC_SPINLOCK_ALLOC();
+	dwc_spinlock_t *channel_lock = hcd->channel_lock;
 
 	dwc_hc_t *hc = qh->channel;
 	if (dwc_qh_is_non_per(qh)) {
@@ -306,7 +306,6 @@ static void release_channel_ddma(dwc_otg_hcd_t * hcd, dwc_otg_qh_t * qh)
 		dwc_memset(qh->desc_list, 0x00,
 			   sizeof(dwc_otg_host_dma_desc_t) * max_desc_num(qh));
 	}
-	DWC_SPINLOCK_FREE(channel_lock);
 }
 
 /** 
diff --git a/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c b/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
index f1658fa..21e8f09 100644
--- a/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_hcd_intr.c
@@ -922,7 +922,7 @@ static void release_channel(dwc_otg_hcd_t * hcd,
 	dwc_otg_transaction_type_e tr_type;
 	int free_qtd;
 	dwc_irqflags_t flags;
-	dwc_spinlock_t *channel_lock = DWC_SPINLOCK_ALLOC();
+	dwc_spinlock_t *channel_lock = hcd->channel_lock;
 
 	DWC_DEBUGPL(DBG_HCDV, "  %s: channel %d, halt_status %d, xfer_len %d\n",
 		    __func__, hc->hc_num, halt_status, hc->xfer_len);
@@ -1009,7 +1009,6 @@ cleanup:
 	if (tr_type != DWC_OTG_TRANSACTION_NONE) {
 		dwc_otg_hcd_queue_transactions(hcd, tr_type);
 	}
-	DWC_SPINLOCK_FREE(channel_lock);
 }
 
 /**
-- 
1.9.1

