#!/bin/sh
. /etc/config/network

WAN="$wan_ifname"
LAN="$lan_ifname"

iptables -F input_rule
iptables -F output_rule
iptables -F forwarding_rule
iptables -t nat -F prerouting_rule
iptables -t nat -F postrouting_rule

### BIG FAT DISCLAIMER
## The "-i $WAN" is used to match packets that come in via the $WAN interface.
## it WILL NOT MATCH packets sent from the $WAN ip address -- you won't be able
## to see the effects from within the LAN.

### Open port to WAN
## -- This allows port 22 to be answered by (dropbear on) the router
# iptables -t nat -A prerouting_rule -i $WAN -p tcp --dport 22 -j ACCEPT 
# iptables        -A input_rule      -i $WAN -p tcp --dport 22 -j ACCEPT

### Port forwarding
## -- This forwards port 8080 on the WAN to port 80 on 192.168.1.2
# iptables -t nat -A prerouting_rule -i $WAN -p tcp --dport 8080 -j DNAT --to 192.168.1.2:80
# iptables        -A forwarding_rule -i $WAN -p tcp --dport 80 -d 192.168.1.2 -j ACCEPT

### DMZ
## -- Connections to ports not handled above will be forwarded to 192.168.1.2
# iptables -t nat -A prerouting_rule -i $WAN -j DNAT --to 192.168.1.2
# iptables        -A forwarding_rule -i $WAN -d 192.168.1.2 -j ACCEPT
