--- a/drivers/net/tg3.c
+++ b/drivers/net/tg3.c
@@ -41,6 +41,7 @@
 #include <linux/prefetch.h>
 #include <linux/dma-mapping.h>
 #include <linux/firmware.h>
+#include <linux/ssb/ssb_driver_gige.h>
 
 #include <net/checksum.h>
 #include <net/ip.h>
@@ -446,8 +447,9 @@ static void _tw32_flush(struct tg3 *tp, 
 static inline void tw32_mailbox_flush(struct tg3 *tp, u32 off, u32 val)
 {
 	tp->write32_mbox(tp, off, val);
-	if (!(tp->tg3_flags & TG3_FLAG_MBOX_WRITE_REORDER) &&
-	    !(tp->tg3_flags2 & TG3_FLG2_ICH_WORKAROUND))
+	if ((tp->tg3_flags3 & TG3_FLG3_FLUSH_POSTED_WRITES) ||
+	    (!(tp->tg3_flags & TG3_FLAG_MBOX_WRITE_REORDER) &&
+	     !(tp->tg3_flags2 & TG3_FLG2_ICH_WORKAROUND)))
 		tp->read32_mbox(tp, off);
 }
 
@@ -457,7 +459,7 @@ static void tg3_write32_tx_mbox(struct t
 	writel(val, mbox);
 	if (tp->tg3_flags & TG3_FLAG_TXD_MBOX_HWBUG)
 		writel(val, mbox);
-	if (tp->tg3_flags & TG3_FLAG_MBOX_WRITE_REORDER)
+	if ((tp->tg3_flags & TG3_FLAG_MBOX_WRITE_REORDER) || (tp->tg3_flags3 & TG3_FLG3_FLUSH_POSTED_WRITES))
 		readl(mbox);
 }
 
@@ -729,7 +731,7 @@ static void tg3_switch_clocks(struct tg3
 
 #define PHY_BUSY_LOOPS	5000
 
-static int tg3_readphy(struct tg3 *tp, int reg, u32 *val)
+static int __tg3_readphy(struct tg3 *tp, unsigned int phy_addr, int reg, u32 *val)
 {
 	u32 frame_val;
 	unsigned int loops;
@@ -743,7 +745,7 @@ static int tg3_readphy(struct tg3 *tp, i
 
 	*val = 0x0;
 
-	frame_val  = ((PHY_ADDR << MI_COM_PHY_ADDR_SHIFT) &
+	frame_val  = ((phy_addr << MI_COM_PHY_ADDR_SHIFT) &
 		      MI_COM_PHY_ADDR_MASK);
 	frame_val |= ((reg << MI_COM_REG_ADDR_SHIFT) &
 		      MI_COM_REG_ADDR_MASK);
@@ -778,7 +780,12 @@ static int tg3_readphy(struct tg3 *tp, i
 	return ret;
 }
 
-static int tg3_writephy(struct tg3 *tp, int reg, u32 val)
+static int tg3_readphy(struct tg3 *tp, int reg, u32 *val)
+{
+	return __tg3_readphy(tp, PHY_ADDR, reg, val);
+}
+
+static int __tg3_writephy(struct tg3 *tp, unsigned int phy_addr, int reg, u32 val)
 {
 	u32 frame_val;
 	unsigned int loops;
@@ -794,7 +801,7 @@ static int tg3_writephy(struct tg3 *tp, 
 		udelay(80);
 	}
 
-	frame_val  = ((PHY_ADDR << MI_COM_PHY_ADDR_SHIFT) &
+	frame_val  = ((phy_addr << MI_COM_PHY_ADDR_SHIFT) &
 		      MI_COM_PHY_ADDR_MASK);
 	frame_val |= ((reg << MI_COM_REG_ADDR_SHIFT) &
 		      MI_COM_REG_ADDR_MASK);
@@ -827,6 +834,11 @@ static int tg3_writephy(struct tg3 *tp, 
 	return ret;
 }
 
+static int tg3_writephy(struct tg3 *tp, int reg, u32 val)
+{
+	return __tg3_writephy(tp, PHY_ADDR, reg, val);
+}
+
 static int tg3_bmcr_reset(struct tg3 *tp)
 {
 	u32 phy_control;
@@ -2263,6 +2275,9 @@ static int tg3_nvram_read(struct tg3 *tp
 {
 	int ret;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE)
+		return -ENODEV;
+
 	if (!(tp->tg3_flags & TG3_FLAG_NVRAM))
 		return tg3_nvram_read_using_eeprom(tp, offset, val);
 
@@ -2594,8 +2609,10 @@ static int tg3_set_power_state(struct tg
 	tg3_frob_aux_power(tp);
 
 	/* Workaround for unstable PLL clock */
-	if ((GET_CHIP_REV(tp->pci_chip_rev_id) == CHIPREV_5750_AX) ||
-	    (GET_CHIP_REV(tp->pci_chip_rev_id) == CHIPREV_5750_BX)) {
+	if ((tp->phy_id & PHY_ID_MASK) != PHY_ID_BCM5750_2 &&
+				/* !!! FIXME !!! */
+	    ((GET_CHIP_REV(tp->pci_chip_rev_id) == CHIPREV_5750_AX) ||
+	    (GET_CHIP_REV(tp->pci_chip_rev_id) == CHIPREV_5750_BX))) {
 		u32 val = tr32(0x7d00);
 
 		val &= ~((1 << 16) | (1 << 4) | (1 << 2) | (1 << 1) | 1);
@@ -3087,6 +3104,14 @@ relink:
 
 		tg3_phy_copper_begin(tp);
 
+		if (tp->tg3_flags3 & TG3_FLG3_ROBOSWITCH) {
+			current_link_up = 1;
+			current_speed = SPEED_1000; //FIXME
+			current_duplex = DUPLEX_FULL;
+			tp->link_config.active_speed = current_speed;
+			tp->link_config.active_duplex = current_duplex;
+		}
+
 		tg3_readphy(tp, MII_BMSR, &tmp);
 		if (!tg3_readphy(tp, MII_BMSR, &tmp) &&
 		    (tmp & BMSR_LSTATUS))
@@ -6000,6 +6025,11 @@ static int tg3_poll_fw(struct tg3 *tp)
 	int i;
 	u32 val;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* We don't use firmware. */
+		return 0;
+	}
+
 	if (GET_ASIC_REV(tp->pci_chip_rev_id) == ASIC_REV_5906) {
 		/* Wait up to 20ms for init done. */
 		for (i = 0; i < 200; i++) {
@@ -6257,6 +6287,14 @@ static int tg3_chip_reset(struct tg3 *tp
 		tw32(0x5000, 0x400);
 	}
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* BCM4785: In order to avoid repercussions from using potentially
+		 * defective internal ROM, stop the Rx RISC CPU, which is not
+		 * required. */
+		tg3_stop_fw(tp);
+		tg3_halt_cpu(tp, RX_CPU_BASE);
+	}
+
 	tw32(GRC_MODE, tp->grc_mode);
 
 	if (tp->pci_chip_rev_id == CHIPREV_ID_5705_A0) {
@@ -6409,9 +6447,12 @@ static int tg3_halt_cpu(struct tg3 *tp, 
 		return -ENODEV;
 	}
 
-	/* Clear firmware's nvram arbitration. */
-	if (tp->tg3_flags & TG3_FLAG_NVRAM)
-		tw32(NVRAM_SWARB, SWARB_REQ_CLR0);
+	if (!(tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE)) {
+		/* Clear firmware's nvram arbitration. */
+		if (tp->tg3_flags & TG3_FLAG_NVRAM)
+			tw32(NVRAM_SWARB, SWARB_REQ_CLR0);
+	}
+
 	return 0;
 }
 
@@ -6474,6 +6515,11 @@ static int tg3_load_5701_a0_firmware_fix
 	const __be32 *fw_data;
 	int err, i;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* We don't use firmware. */
+		return 0;
+	}
+
 	fw_data = (void *)tp->fw->data;
 
 	/* Firmware blob starts with version numbers, followed by
@@ -6533,6 +6579,11 @@ static int tg3_load_tso_firmware(struct 
 	unsigned long cpu_base, cpu_scratch_base, cpu_scratch_size;
 	int err, i;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* We don't use firmware. */
+		return 0;
+	}
+
 	if (tp->tg3_flags2 & TG3_FLG2_HW_TSO)
 		return 0;
 
@@ -7444,6 +7495,11 @@ static void tg3_timer(unsigned long __op
 
 	spin_lock(&tp->lock);
 
+	if (tp->tg3_flags3 & TG3_FLG3_FLUSH_POSTED_WRITES) {
+		/* BCM4785: Flush posted writes from GbE to host memory. */
+		tr32(HOSTCC_MODE);
+	}
+
 	if (!(tp->tg3_flags & TG3_FLAG_TAGGED_STATUS)) {
 		/* All of this garbage is because when using non-tagged
 		 * IRQ status the mailbox/status_block protocol the chip
@@ -9217,6 +9273,11 @@ static int tg3_test_nvram(struct tg3 *tp
 	if (tp->tg3_flags3 & TG3_FLG3_NO_NVRAM)
 		return 0;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* We don't have NVRAM. */
+		return 0;
+	}
+
 	if (tg3_nvram_read(tp, 0, &magic) != 0)
 		return -EIO;
 
@@ -10010,7 +10071,7 @@ static int tg3_ioctl(struct net_device *
 			return -EAGAIN;
 
 		spin_lock_bh(&tp->lock);
-		err = tg3_readphy(tp, data->reg_num & 0x1f, &mii_regval);
+		err = __tg3_readphy(tp, data->phy_id & 0x1f, data->reg_num & 0x1f, &mii_regval);
 		spin_unlock_bh(&tp->lock);
 
 		data->val_out = mii_regval;
@@ -10029,7 +10090,7 @@ static int tg3_ioctl(struct net_device *
 			return -EAGAIN;
 
 		spin_lock_bh(&tp->lock);
-		err = tg3_writephy(tp, data->reg_num & 0x1f, data->val_in);
+		err = __tg3_writephy(tp, data->phy_id & 0x1f, data->reg_num & 0x1f, data->val_in);
 		spin_unlock_bh(&tp->lock);
 
 		return err;
@@ -10619,6 +10680,12 @@ static void __devinit tg3_get_57780_nvra
 /* Chips other than 5700/5701 use the NVRAM for fetching info. */
 static void __devinit tg3_nvram_init(struct tg3 *tp)
 {
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE) {
+		/* No NVRAM and EEPROM on the SSB Broadcom GigE core. */
+		tp->tg3_flags &= ~(TG3_FLAG_NVRAM | TG3_FLAG_NVRAM_BUFFERED);
+		return;
+	}
+
 	tw32_f(GRC_EEPROM_ADDR,
 	     (EEPROM_ADDR_FSM_RESET |
 	      (EEPROM_DEFAULT_CLOCK_PERIOD <<
@@ -10877,6 +10944,9 @@ static int tg3_nvram_write_block(struct 
 {
 	int ret;
 
+	if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE)
+		return -ENODEV;
+
 	if (tp->tg3_flags & TG3_FLAG_EEPROM_WRITE_PROT) {
 		tw32_f(GRC_LOCAL_CTRL, tp->grc_local_ctrl &
 		       ~GRC_LCLCTRL_GPIO_OUTPUT1);
@@ -12136,6 +12206,11 @@ static int __devinit tg3_get_invariants(
 	      GET_ASIC_REV(tp->pci_chip_rev_id) == ASIC_REV_5701)))
 		tp->tg3_flags |= TG3_FLAG_SRAM_USE_CONFIG;
 
+	if (tp->tg3_flags3 & TG3_FLG3_FLUSH_POSTED_WRITES) {
+		tp->write32_tx_mbox = tg3_write_flush_reg32;
+		tp->write32_rx_mbox = tg3_write_flush_reg32;
+	}
+
 	/* Get eeprom hw config before calling tg3_set_power_state().
 	 * In particular, the TG3_FLG2_IS_NIC flag must be
 	 * determined before calling tg3_set_power_state() so that
@@ -12513,6 +12588,10 @@ static int __devinit tg3_get_device_addr
 	}
 
 	if (!is_valid_ether_addr(&dev->dev_addr[0])) {
+		if (tp->tg3_flags3 & TG3_FLG3_IS_SSB_CORE)
+			ssb_gige_get_macaddr(tp->pdev, &dev->dev_addr[0]);
+	}
+	if (!is_valid_ether_addr(&dev->dev_addr[0])) {
 #ifdef CONFIG_SPARC
 		if (!tg3_get_default_macaddr_sparc(tp))
 			return 0;
@@ -13004,6 +13083,7 @@ static char * __devinit tg3_phy_string(s
 	case PHY_ID_BCM5704:	return "5704";
 	case PHY_ID_BCM5705:	return "5705";
 	case PHY_ID_BCM5750:	return "5750";
+	case PHY_ID_BCM5750_2:	return "5750-2";
 	case PHY_ID_BCM5752:	return "5752";
 	case PHY_ID_BCM5714:	return "5714";
 	case PHY_ID_BCM5780:	return "5780";
@@ -13214,6 +13294,13 @@ static int __devinit tg3_init_one(struct
 		tp->msg_enable = tg3_debug;
 	else
 		tp->msg_enable = TG3_DEF_MSG_ENABLE;
+	if (pdev_is_ssb_gige_core(pdev)) {
+		tp->tg3_flags3 |= TG3_FLG3_IS_SSB_CORE;
+		if (ssb_gige_must_flush_posted_writes(pdev))
+			tp->tg3_flags3 |= TG3_FLG3_FLUSH_POSTED_WRITES;
+		if (ssb_gige_have_roboswitch(pdev))
+			tp->tg3_flags3 |= TG3_FLG3_ROBOSWITCH;
+	}
 
 	/* The word/byte swap controls here control register access byte
 	 * swapping.  DMA data byte swapping is controlled in the GRC_MODE
--- a/drivers/net/tg3.h
+++ b/drivers/net/tg3.h
@@ -1853,6 +1853,9 @@
 #define  NIC_SRAM_RGMII_STD_IBND_DISABLE 0x00000004
 #define  NIC_SRAM_RGMII_EXT_IBND_RX_EN	 0x00000008
 #define  NIC_SRAM_RGMII_EXT_IBND_TX_EN	 0x00000010
+#define TG3_FLG3_IS_SSB_CORE		0x00000800
+#define TG3_FLG3_FLUSH_POSTED_WRITES	0x00001000
+#define TG3_FLG3_ROBOSWITCH		0x00002000
 
 #define NIC_SRAM_RX_MINI_BUFFER_DESC	0x00001000
 
@@ -2701,6 +2704,7 @@ struct tg3 {
 #define PHY_ID_BCM5714			0x60008340
 #define PHY_ID_BCM5780			0x60008350
 #define PHY_ID_BCM5755			0xbc050cc0
+#define PHY_ID_BCM5750_2		0xbc050cd0
 #define PHY_ID_BCM5787			0xbc050ce0
 #define PHY_ID_BCM5756			0xbc050ed0
 #define PHY_ID_BCM5784			0xbc050fa0
@@ -2745,7 +2749,7 @@ struct tg3 {
 	 (X) == PHY_ID_BCM5780 || (X) == PHY_ID_BCM5787 || \
 	 (X) == PHY_ID_BCM5755 || (X) == PHY_ID_BCM5756 || \
 	 (X) == PHY_ID_BCM5906 || (X) == PHY_ID_BCM5761 || \
-	 (X) == PHY_ID_BCM8002)
+	 (X) == PHY_ID_BCM8002 || (X) == PHY_ID_BCM5750_2)
 
 	struct tg3_hw_stats		*hw_stats;
 	dma_addr_t			stats_mapping;
