From 7b55ff7b9fd37ac8857746603ec580d277208f01 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:29:40 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/053-adc.patch

---
 drivers/misc/Kconfig  |   11 +++++++++++
 drivers/misc/Makefile |    1 +
 2 files changed, 12 insertions(+), 0 deletions(-)

--- a/drivers/misc/Kconfig
+++ b/drivers/misc/Kconfig
@@ -246,6 +246,17 @@ config EP93XX_PWM
 	  To compile this driver as a module, choose M here: the module will
 	  be called ep93xx_pwm.
 
+config JZ4740_ADC
+	tristate "Ingenic JZ4720/JZ4740 SoC ADC driver"
+	depends on SOC_JZ4740
+    help
+      If you say yes here you get support for the Ingenic JZ4720/JZ4740 SoC ADC
+      core. It is required for the JZ4720/JZ4740 battery and touchscreen driver
+      and is used to synchronize access to the adc core between those two.
+
+      This driver can also be build as a module. If so, the module will be
+      called jz4740-adc.
+
 source "drivers/misc/c2port/Kconfig"
 source "drivers/misc/eeprom/Kconfig"
 source "drivers/misc/cb710/Kconfig"
--- a/drivers/misc/Makefile
+++ b/drivers/misc/Makefile
@@ -21,5 +21,6 @@ obj-$(CONFIG_HP_ILO)		+= hpilo.o
 obj-$(CONFIG_ISL29003)		+= isl29003.o
 obj-$(CONFIG_EP93XX_PWM)	+= ep93xx_pwm.o
 obj-$(CONFIG_C2PORT)		+= c2port/
+obj-$(CONFIG_JZ4740_ADC)	+= jz4740-adc.o
 obj-y				+= eeprom/
 obj-y				+= cb710/
