The bootloader now uses additional board type constants.  The
octeon-ethernet driver needs some of the new values.

Signed-off-by: David Daney <ddaney@caviumnetworks.com>
---
 arch/mips/include/asm/octeon/cvmx-bootinfo.h |   13 +++++++++++++
 1 files changed, 13 insertions(+), 0 deletions(-)

--- a/arch/mips/include/asm/octeon/cvmx-bootinfo.h
+++ b/arch/mips/include/asm/octeon/cvmx-bootinfo.h
@@ -157,6 +157,13 @@ enum cvmx_board_types_enum {
 	CVMX_BOARD_TYPE_NIC_XLE_4G = 21,
 	CVMX_BOARD_TYPE_EBT5600 = 22,
 	CVMX_BOARD_TYPE_EBH5201 = 23,
+	CVMX_BOARD_TYPE_EBT5200 = 24,
+	CVMX_BOARD_TYPE_CB5600  = 25,
+	CVMX_BOARD_TYPE_CB5601  = 26,
+	CVMX_BOARD_TYPE_CB5200  = 27,
+	/* Special 'generic' board type, supports many boards */
+	CVMX_BOARD_TYPE_GENERIC = 28,
+	CVMX_BOARD_TYPE_EBH5610 = 29,
 	CVMX_BOARD_TYPE_MAX,
 
 	/*
@@ -228,6 +235,12 @@ static inline const char *cvmx_board_typ
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_NIC_XLE_4G)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_EBT5600)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_EBH5201)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_EBT5200)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_CB5600)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_CB5601)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_CB5200)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_GENERIC)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_EBH5610)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_MAX)
 
 			/* Customer boards listed here */
