--- a/drivers/net/wireless/ath/ath9k/hw.c
+++ b/drivers/net/wireless/ath/ath9k/hw.c
@@ -16,8 +16,10 @@
 
 #include <linux/io.h>
 #include <linux/etherdevice.h>
+#include <linux/ath9k_platform.h>
 #include <asm/unaligned.h>
 
+#include "ath9k.h"
 #include "hw.h"
 #include "rc.h"
 #include "initvals.h"
@@ -428,17 +430,23 @@ static int ath9k_hw_rf_claim(struct ath_
 static int ath9k_hw_init_macaddr(struct ath_hw *ah)
 {
 	struct ath_common *common = ath9k_hw_common(ah);
+	struct ath_softc *sc = (struct ath_softc *) common->priv;
+	struct ath9k_platform_data *pdata = sc->dev->platform_data;
 	u32 sum;
 	int i;
 	u16 eeval;
 
 	sum = 0;
-	for (i = 0; i < 3; i++) {
-		eeval = ah->eep_ops->get_eeprom(ah, AR_EEPROM_MAC(i));
-		sum += eeval;
-		common->macaddr[2 * i] = eeval >> 8;
-		common->macaddr[2 * i + 1] = eeval & 0xff;
-	}
+	if (pdata && pdata->macaddr)
+		memcpy(common->macaddr, pdata->macaddr, ETH_ALEN);
+	else
+		for (i = 0; i < 3; i++) {
+			eeval = ah->eep_ops->get_eeprom(ah, AR_EEPROM_MAC(i));
+			sum += eeval;
+			common->macaddr[2 * i] = eeval >> 8;
+			common->macaddr[2 * i + 1] = eeval & 0xff;
+		}
+
 	if (!is_valid_ether_addr(common->macaddr)) {
 		DECLARE_MAC_BUF(macbuf);
 
--- a/include/linux/ath9k_platform.h
+++ b/include/linux/ath9k_platform.h
@@ -23,6 +23,7 @@
 
 struct ath9k_platform_data {
 	u16 eeprom_data[ATH9K_PLAT_EEP_MAX_WORDS];
+	u8 *macaddr;
 };
 
 #endif /* _LINUX_ATH9K_PLATFORM_H */
