From 045c37b75e13fe84f582627f7e2f68b7fa194909 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:29:41 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/100-battery.patch

---
 drivers/power/Kconfig  |   11 +++++++++++
 drivers/power/Makefile |    1 +
 2 files changed, 12 insertions(+), 0 deletions(-)

--- a/drivers/power/Kconfig
+++ b/drivers/power/Kconfig
@@ -110,4 +110,15 @@ config CHARGER_PCF50633
 	help
 	 Say Y to include support for NXP PCF50633 Main Battery Charger.
 
+config BATTERY_JZ4740
+	tristate "Ingenic JZ4720/JZ4740 battery"
+	depends on SOC_JZ4740
+	depends on JZ4740_ADC
+	help
+	  Say Y to enable support for the battery on Ingenic JZ4720/JZ4740 based
+	  boards.
+
+	  This driver can be build as a module. If so, the module will be
+	  called jz4740-battery.
+
 endif # POWER_SUPPLY
--- a/drivers/power/Makefile
+++ b/drivers/power/Makefile
@@ -29,3 +29,4 @@ obj-$(CONFIG_BATTERY_BQ27x00)	+= bq27x00
 obj-$(CONFIG_BATTERY_DA9030)	+= da9030_battery.o
 obj-$(CONFIG_BATTERY_MAX17040)	+= max17040_battery.o
 obj-$(CONFIG_CHARGER_PCF50633)	+= pcf50633-charger.o
+obj-$(CONFIG_BATTERY_JZ4740)	+= jz4740-battery.o
