--- a/arch/mips/cavium-octeon/pci.c
+++ b/arch/mips/cavium-octeon/pci.c
@@ -102,6 +102,8 @@ const char *octeon_get_pci_interrupts(vo
 		return "AAAAAAAAAAAAAABAAAAAAAAAAAAAAABA";
 	case CVMX_BOARD_TYPE_BBGW_REF:
 		return "AABCD";
+	case CVMX_BOARD_TYPE_CUST_NB5:
+		return "ABDABAAAAAAAAAAAAAAAAAAAAAAAAAAA";
 	default:
 		return "";
 	}
--- a/drivers/staging/octeon/cvmx-helper-board.c
+++ b/drivers/staging/octeon/cvmx-helper-board.c
@@ -699,6 +699,7 @@ cvmx_helper_board_usb_clock_types_t __cv
 {
 	switch (cvmx_sysinfo_get()->board_type) {
 	case CVMX_BOARD_TYPE_BBGW_REF:
+	case CVMX_BOARD_TYPE_CUST_NB5:
 		return USB_CLOCK_TYPE_CRYSTAL_12;
 	}
 	return USB_CLOCK_TYPE_REF_48;
